**3GPP TSG RAN WG1 #110R1-22bbbbb**

**Toulouse, France, August 22nd – 26th, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **[DRAFT] CHANGE REQUEST** |
|  |
|  | **38.214** | **CR** | **xxx** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on UE PDSCH processing procedure time for operation with shared spectrum channel access in FR2-2 in TS 38.214 |
|  |  |
| ***Source to WG:*** | Moderator (vivo), ZTE, Sanechips |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_ext\_to\_71GHz |  | ***Date:*** | 2022-08-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | For operation with shared spectrum channel access in FR2-2, cyclic prefix extension specified in Re-16 NR-U is not supported, thus  for calculating UE PDSCH processing procedure time should be equal to 0. In order to avoid ambiguity, calculated according to TS 38.211 should be restricted to only be applicable to Rel-16 NR-U in FR1. |
|  |  |
| ***Summary of change:*** | Restrict the calculation of  according to TS 38.211 is only applicable to operation with shared spectrum channel access in FR1. |
|  |  |
| ***Consequences if not approved:*** | Incorrect calculation of UE PDSCH processing procedure time |
|  |  |
| ***Clauses affected:*** | 5.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 5.3 UE PDSCH processing procedure time

If the first uplink symbol of the PUCCH which carries the HARQ-ACK information, as defined by the assigned HARQ-ACK timing *K1* and Koffset, if configured, and the PUCCH resource to be used and including the effect of the timing advance, starts no earlier than at symbol *L1*, where *L1* is defined as the next uplink symbol with its CP starting after  after the end of the last symbol of the PDSCH carrying the TB being acknowledged, then the UE shall provide a valid HARQ-ACK message.

*- N1* is based on *µ* of table 5.3-1 and table 5.3-2 for UE processing capability 1 and 2 respectively, where *µ* corresponds to the one of (*µPDCCH*, *µPDSCH*, *µUL*) resulting with the largest *Tproc,1*, where the *µPDCCH* corresponds to the subcarrier spacing of the PDCCH scheduling the PDSCH, the *µPDSCH* corresponds to the subcarrier spacing of the scheduled PDSCH, and *µUL* corresponds to the subcarrier spacing of the uplink channel with which the HARQ-ACK is assumed to be transmitted regardless of whether or not the PDSCH reception provides a transport block for a HARQ process with disabled HARQ-ACK information as indicated by HARQ-feedbackEnabling-disablingperHARQprocess, if provided, and κ is defined in clause 4.1 of [4, TS 38.211].

*-* For operation with shared spectrum channel access in FR1, is calculated according to [4, TS 38.211], otherwise =0.

*-* If the PDSCH DM-RS position $l\_{1}$ for the additional DM-RS in Table 7.4.1.1.2-3 in clause 7.4.1.1.2 of [4, TS 38.211] is $l\_{1}=12$ then *N1,0=14* inTable 5.3-1*,* otherwise *N1,0=13.*

**<Unchanged parts are omitted>**