**3GPP TSG RAN WG1 Meeting #110R1-220XXXX**

**Toulouse, France, August 22 - 26, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **[DRAFT] CHANGE REQUEST** |
|  |
|  | **38.214** | **CR** |  | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Corrections on UE power saving enhancements for NR in TS 38.214 |
|  |  |
| ***Source to WG:*** | MediaTek, ZTE, Sanechips, Huawei, HiSilicon |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_UE\_pow\_sav\_enh-Core |  | ***Date:*** | 2022-08-25 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Some parameter names for Rel-17 UE power saving are not aligned with the parameter names used in TS 38.331. |
|  |  |
| ***Summary of change:*** | Updates on the parameter names to align with TS 38.331：1. Modify the name of the parameter ‘*TRS-ResourceSetConfig*’ in 38.214
2. Update the parameter name of “*numberOfresources*” to “*nrofResources*”;
3. Update “*scramblingID*” to “*ScramblingID*”;
 |
|  |  |
| ***Consequences if not approved:*** | Some parameter names for Rel-17 UE power saving are not aligned with the name used in TS 38.331. |
|  |  |
| ***Clauses affected:*** | 5.1.6.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

5.1.6.1.1 CSI-RS for tracking

#### < Unchanged parts are omitted >

A UE in RRC\_IDLE or RRC\_INACTIVE can receive a higher layer configuration of TRS occasions via a *trs-ResourceSetConfig*.

- For frequency range 1, the UE may be configured with one or more TRS resource set(s), where each TRS resource set configured by a *TRS-ResourceSet* consists of four periodic NZP CSI-RS resources in two consecutive slots with two periodic NZP CSI-RS resources in each slot. If no two consecutive slots are indicated as downlink slots by *tdd-UL-DL-ConfigurationCommon*, then the UE may be configured with one or more NZP CSI-RS set(s), where a *TRS-ResourceSet* consists of two periodic NZP CSI-RS resources in one slot.

- For frequency range 2 the UE may be configured with one or more TRS resource set(s), where each TRS resource set configured by a *TRS-ResourceSet* consists of two periodic NZP CSI-RS resources in one slot or by a *TRS-ResourceSet* of four periodic NZP CSI-RS resources in two consecutive slots with two periodic NZP CSI-RS resources in each slot.

Each NZP CSI-RS resource, defined in Clause 7.4.1.5.3 of [4, TS 38.211], is configured by the higher layer parameter *TRS-ResourceSet* with the following restrictions for a UE in RRC\_IDLE or RRC\_INACTIVE:

- the number of periodic NZP CSI-RS resources configured by a *TRS-ResourceSet* is given by *nrofResources*

- the time-domain locations of the two CSI-RS resources in a slot, or of the four CSI-RS resources in two consecutive slots (which are the same across two consecutive slots), is one of

- , , or for frequency range 1 and frequency range 2,

- , , , , ,  or  for frequency range 2.

- where the first symbol location in a slot is indicated by *firstOFDMSymbolInTimeDomain* in the *TRS-ResourceSet* and the second symbol location in a slot is *firstOFDMSymbolInTimeDomain +* 4

- a single port CSI-RS resource with density  given by Table 7.4.1.5.3-1 from [4, TS 38.211]*.*

- the bandwidth and the frequency location of the NZP CSI-RS resource, is given by the higher layer parameter *nrofRBs*, *startingRB* and *frequencyDomainAllocation* in a *TRS-ResourceSet* and applies to all resources in a *TRS-ResourceSet*. Bandwidth, *nrofRBs*, and the initial CRB index, *startingRB*, of the NZP CSI-RS resource configured by *TRS-ResourceSet* are not restricted by initial DL BWP.

- UE is not required to receive TRS occasions outside the initial DL BWP.

- the periodicity for periodic NZP CSI-RS resources, is given by the higher layer parameter *periodicityAndOffset* configured b*y* a *TRS-ResourceSet*, is one of slots where 10, 20, 40, or 80 and where µ is defined in Clause 4.3 of [4, TS 38.211], applies to all resources in a *TRS-ResourceSet*. The slot offset given by the higher layer parameter *periodicityAndOffset* configured b*y* a *TRS-ResourceSet* provides the location of the first slot containing the periodic NZP CSI-RS resources configured by b*y* a *TRS-ResourceSet.*

- the UE does not expect the *TRS-ResourceSet* to be configured with the periodicity of  slots if the bandwidth of NZP CSI-RS resource is larger than 52 resource blocks.

- the UE may assume the sub-carrier spacing of the NZP CSI-RS resources configured by *TRS-ResourceSet* to be same as the sub-carrier spacing of the initial DL BWP.

- *powerControlOffsetSS* given bya *TRS-ResourceSet* applies to all resources in a *TRS-ResourceSet*.

- the QCL information for periodic NZP CSI-RS resources, is given by the higher layer parameter *ssb-Index* configured by a *TRS-ResourceSet*, is a SS/PBCH block, applies to all resources in a *TRS-ResourceSet*.

- One or more *ScramblingIDs* where if a single *ScramblingID* is configured, it applies to all NZP-CSI-RS resources in the resource set, otherwise, each NZP-CSI-RS resource is provided with a *ScramblingID*.

- the UE may assume the following quasi co-location type(s):

- 'typeC' with an SS/PBCH block and, when applicable, 'typeD' with the same SS/PBCH block.

#### < Unchanged parts are omitted >