**3GPP TSG- RAN WG1 Meeting #110 R1-220xxxx**

**Toulouse, FR, Aug 22th – Aug 26th, 2022**

Agenda Item: 9.2.2.2

Source: Moderator (Apple)

Title: Email discussion on other aspects of AI/ML for CSI

# Introduction

This paper summarizes the discussion for agenda item 9.2.2.2.

# Finalize representative sub use cases for CSI feedback enhancement

## Summary of proposals

Spatial-frequency domain CSI compression using two-sided AI model is selected as one representative sub-use case in RAN1 109-e meeting. Study of other sub use cases is not precluded.

Following table summarizes company’s proposals on other use cases.

|  |  |
| --- | --- |
| **Company** | **Key Proposals/Observations/Positions** |
| Huawei | Proposal 1: For AI/ML-based CSI feedback enhancement, study temporal-spatial-frequency domain CSI compression using two-sided AI/ML model. |
| TCL communication  | Proposal 1: The basic CSI feedback model based on auto-encoder reduces feedback bits through the air-interface, compared to the CSI feedback based on codebook. It is a functional replacement of the CSI feedback based on codebook.Proposal 2: To fix the problem of outdated CSI feedback, the predictive CSI feedback model is necessary to predict CSI at scheduling time.Proposal 3: Multiple CSI measurements can be compressed together and feedback at one shot to further reduces the feedback overhead.Proposal 4: The CSI feedback compression along the frequency dimension, can be designed with new sparser CSI-RS patterns. The resource utilization is improved by allocating more REs to data transmission. |
| vivo | Proposal 1: To ensure the enhancement of CSI at both low and high-speed scenarios, study AI/ML for time domain CSI prediction with high priority. |
| ZTE | Proposal 3: For improving the CSI accuracy based on traditional codebook design using one-sided model, enhancement on Rel-16/17 eType II should be considered as a representative sub-use case for further study.Proposal 4: For CSI prediction, we need to identify at least three aspects for further study: CSI prediction in spatial domain, frequency domain and time domain. However, time domain CSI prediction can be deprioritized in Rel-18 AI PHY, waiting for progress in Rel-18 MIMO session. |
| Sony | Proposal 1: RAN1 study paradigms for CSI measurement prediction to closer to the transmission resources allocated.Proposal 2: RAN1 study paradigms for increasing CSI measurement granularity in both time and frequency for more accurate resource and MCS allocation. Proposal 3: RAN1 study new methods of resource allocation and transport channel processing based on higher CSI measurement granularity. Proposal 4: RAN1 should study how to reduce the transmission data size for both current coarse CSI and finer granularity CSI feedback. |
| Fujitsu | Proposal-1: AI/ML-based CSI feedback prediction in time domain should be selected as a sub-use case of CSI feedback enhancement. Proposal-2: Both CSI prediction at UE side and CSI prediction at gNB side can be studied in this sub-use case. |
| Google | Proposal 7: Study CSI prediction as a use case for AI/ML based CSI feedback.Proposal 8: AI/ML based joint CSI prediction and CSI compression should be deprioritized.Proposal 9: AI/ML based CSI-RS configuration and overhead reduction should be deprioritized. |
| NEC | Proposal 1: Support temporal-domain CSI prediction using one-sided AI/ML model is selected as one representative sub use case.Proposal 2: Support the adjustment of CSI feedback rate/ CSI reporting pattern based on the predicted CSI variation points as one of the final representative sub use cases. |
| Oppo | Proposal 1: The screening of CSI sub use cases needs to meet all the following conditions:1. Potential performance gain.2. Feasible evaluation methodology and valid training data set. 3. Reasonable non-AI/ML-based baseline for performance gain analysis.4. Potential specification impacts.Proposal 2: CSI compression(AE based Spatial-frequency domain CSI compression) should be given the high priority on evaluation and specification impact consideration. Other sub use cases, e.g. CSI prediction, CSI compression in temporal-spatial-frequency domain, or at gNB/UE side only could be given a lower priority until common understanding have been made |
| CATT | Proposal 1: The following sub use cases for CSI feedback are not considered in Rel-18:– Temporal-spatial-frequency domain CSI compression;– Improving the CSI accuracy based on traditional codebook design using one-sided model;– AI/ML based DL/UL CSI prediction via UL/DL RS– AI/ML based spatial/frequency/time domain CSI prediction through partial information;– Resource allocation and scheduling;– Joint CSI prediction and compression.Proposal 2: The sub use case of AI/ML based CSI prediction in time domain is deprioritized in Rel-18. |
| Lenovo  | Proposal 1 Agreements/Conclusions made in agenda 9.2.2.2 on further aspects of AI/ML for CSI feedback should focus on discussing the sub-use cases and corresponding specification impact. Details on the supported AI/ML model should be discussed in agenda 9.2.2.1 on evaluation of AI/ML for CSI feedbackProposal 2 The study of spatial-frequency domain CSI compression using AI/ML should not be restricted by two-sided models in this stage. Decisions on the underlying AI model should be discussed in agenda 9.2.2.1 based on simulation and analytical resultsProposal 3 The study of temporal-spatial-frequency domain CSI compression is deprioritizedProposal 4 CSI feedback overhead reduction and CSI accuracy improvement objectives are not to be treated in isolation, but into one sub use-case of CSI feedback enhancementProposal 5 Defer the discussion on AI-based CSI prediction sub use-case to RAN1#110bis-eProposal 6 CSI-RS configuration enhancement is not considered for study of AI/ML for CSI frameworkProposal 7 Resource allocation and scheduling sub-use case is discussed after the outline of CSI prediction sub-use case is finalizedProposal 8 Use LTE UE-based sub-band selection for CQI reporting as a starting point for the study of AI-based resource allocation and schedulingProposal 9 Joint CSI prediction and compression is not considered |
| NVIDIA | Proposal 1: Autoencoder based CSI feedback enhancement should be selected as one representative sub use case.Proposal 2: Focus on the sub-use case of spatial-frequency domain CSI compression using two-sided AI model to develop a thorough understanding of the performance of the AI model and the associated potential specification impacts.Proposal 3: Potential sub-use cases other than of spatial-frequency domain CSI compression using two-sided AI model may be discussed at a later stage after a thorough understanding of the sub-use case of spatial-frequency domain CSI compression using two-sided AI model is developed. |
| Intel | Proposal 1:• Spatial-frequency domain CSI compression using two-sided AI model should be prioritized |
| Xiaomi | Proposal 1: Other sub-use cases for CSI feedback are studied with lower priority except improving the CSI accuracy based on traditional codebook design using one-sided model due to its less specification impact. |
| CAICT | Proposal 1: CSI prediction and compression is treated as two separate sub use cases. |
| China Telecom | Proposal 1: Study benefits of using AI/ML for CSI compression in spatial and frequency domain compression using Rel-16 eType II codebook as a baseline.Proposal 2: Study benefits of using AI/ML for CSI compression in Temporal-spatial-frequency domain compression.Proposal 3: Further discuss AI/ML for CSI compression in Temporal-spatial-frequency domain compression as a possible sub-use case for CSI feedback enhancement.Proposal 4: The performance gain of AI based CSI prediction may need FFS. |
| Samsung | Proposal 1-1: Study CSI prediction/extrapolation as one sub-use case for AI/ML for CSI feedback enhancement, including signaling requirements, input/output requirements, CSI configurations, and training strategies.Proposal 1-2: Study CSI prediction/extrapolation at the UE under collaboration level (B), where limited information exchanges are required to configure/enable AI/ML.Proposal 2-3: Study and verify model update of the encoder at the UE, where the gNB’s training strategy is not disclosed while transferring/configuring the AE.Proposal 3-1: Study joint CSI prediction and compression as a representative sub-use case of AI/ML based CSI feedback enhancement. • Consider joint CSI prediction and compression as temporal-spatial-frequency-domain compression. |
| LGE | Proposal #1: Prioritize to further study on legacy codebook enhancement and CSI-RS overhead reduction based on AI/ML. |
| Ericsson | Proposal 1 Add the temporal-spatial-frequency (TSF) domain compression as an optional variant of the two-sided model based spatial-frequency (SF) compression. The TSF variant allows multiple CSI-RS measurements over time to be utilized for CSI compression and prediction into the future. The proponent needs to explain whether SF or TSF was used when providing result and analysis.Proposal 2 Study one-sided model-based CSI enhancements using traditional codebooks by investigating the possible benefits of UE to network codebook parameter recommendation and faster than RRC codebook re-configurationProposal 3 Study the performance and standardization impact of one-sided (i.e., UE) model based CSI prediction using the existing CSI framework as a starting point |
| CMCC | Proposal 1: Spatial-frequency domain CSI compression using two-sided AI model should be studied with high priority.Proposal 2: Temporal-spatial-frequency domain CSI compression and CSI prediction could be studied with low priority. |
| Nokia | Proposal 3. Support CSI prediction as a second sub-use case.Proposal 4. Compare channel prediction over broad bandwidth versus based on Type II CSI per sub-band. Proposal 5: Consider UE sided as well as gNB sided channel prediction, as well as potentially include combined prediction between UE and gNB. |
| MediaTek | Proposal 1: Study CSI prediction under Release 18 AI/ML-based CSI enhancement. |
| Interdigital  | Proposal 7: CSI prediction can be studied with lower priority if time allows in Rel-18 but there should be no conclusion/suggestion for CSI prediction as an outcome for normative work.Proposal 8: Study CSI-RS configurations and overhead reduction at least to support CSI compression and prediction sub-use cases. |
| Qualcomm | Proposal 1: The study item should focus on the sub-use-case of spatial-frequency domain CSI compression and reconstruction of observed channel features using two-sided AI model; other sub-use-cases can be studied with lower priority. |
| Apple | Proposal 1: Consider time domain CSI prediction using one-sided AI model as one representative sub use case for R18 AI based CSI study. |
| AT&T | Proposal 1: Include resource allocation and scheduling as a sub-use case for CSI feedback enhancement.Proposal 2: Include CSI prediction as a sub-use case for CSI feedback enhancements in combination with resource allocation and scheduling to further improve MU-MIMO scheduling optimization. |
| NTT DOCOMO | Proposal 1: Prioritize the discussion of spatial-frequency domain CSI compression from other sub-use case in 9.2.2. |

A summary of supporting companies for each sub-use case is listed in the table. (Note: Please update the table if proposals are captured wrong.)

|  |  |
| --- | --- |
|  | Support |
| temporal-spatial-frequency domain CSI compression using two-sided model | Huawei, TCL, China Telecom, Samsung, Ericsson |
| CSI prediction  | TCL, vivo, Sony, Fujitsu, Google, NEC, CAICT, Samsung, Ericsson, Nokia, Apple, AT&T |
| CSI accuracy based on traditional codebook design | ZTE, Xiaomi, Ericsson |
| CSI-RS configuration and overhead reduction | TCL, Samsung, LGE, Interdigital |
| Resource allocation and scheduling | Sony, AT&T |
| Joint CSI prediction and compression | Samsung, Ericsson. (Suggest to merge with Temporal-Spatial-Freq domain CSI compression).  |

It has been mentioned by many companies that one-sided model is easier to implement, with less specification impact and likely to have a much shorter time to market than two-sided model. Therefore, it is proposed to study at least one sub use case with one-sided model for CSI feedback enhancement.

## ***Proposal 2-1:***

***Include at least one sub-use case with one-sided model under Release 18 AI/ML-based CSI enhancement use case.***

Please provide your view in the following two tables. 1st table please enter whether support or not support. The second table is for additional comments.

|  |  |
| --- | --- |
| Supporting companies |  |
| Objecting companies |  |

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

It has been mentioned that the potential specification impact of the temporal-spatial-frequency domain CSI compression using two-sided model is very similar to spatial-frequency domain CSI compression, and the temporal-spatial-frequency domain CSI compression can be an optional sub-use case for CSI compression using two-sided model. It would be beneficial to understand if any additional specification impact is identified to enable the temporal-spatial-frequency domain CSI compression sub-use case.

## ***Proposal 2-2:***

***Identify additional specification impact, if any, to support temporal-spatial-frequency domain CSI compression on top of spatial-frequency domain CSI compression using two-sided model.***

Please provide your view in the following two tables. 1st table please enter whether support or not support. The second table is for additional comments.

|  |  |
| --- | --- |
| Supporting companies |  |
| Objecting companies |  |

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

# Potential specification impact for CSI compression with two-sided model

## Training collaboration

Following table summarize company’s proposals related to training collaboration.

|  |  |
| --- | --- |
| Huawei | Proposal 2: Study the potential specification impact for following training types:• Type 1: On-network training with model transfer to UE• Type 2: On-UE training with model transfer to network• Type 3: Joint training across network and UE without model transfer, where the UE-side CSI generation part and the network-side CSI reconstruction part are trained in one forward propagation (FP) & backward propagation (BP) loop with necessary gradients exchange• Type 4: Separate training at network and UE without model transfer, where the UE-side CSI generation part and the network-side CSI reconstruction part are trained by UE and network, respectively, in their own FP & BP loops |
| vivo | Proposal 6: Adopt either Definition Alt 1 or Definition Alt 2 to elaborate the process of joint training and separate training in CSI compression, although Definition Alt 2 is clearer with more detailed description.• Clarification: Joint training could be done both at single NW node and multiple NW nodes (e.g., through gradient exchange between nodes).Proposal 7: Study all 4 training options for CSI compression in short and long term, including performance, life cycle management, expected spec impacts, pros/cons, etc. |
| ZTE | Proposal 1: In CSI compression using two-sided model, the following mechanisms for AI/ML model training will be further studied:▪ Type 1: On-network training of two-sided model with model transfer to UE▪ Type 2: On-UE training of two-sided model with model transfer to NW▪ Type 3: Joint training of two-sided model without specified interactions between UE and NW▪ Type 4: Joint training of two-sided model with specified interactions between UE and NW▪ Type 5: Separate training at UE side and NW side for CSI feedback generation model / CSI reconstruction model respectivelyNote: Joint training means the generation model and reconstruction model should be trained in the same loop for forward propagation and backward propagation. However, generation model and reconstruction model for separate training are trained in different loops for forward propagation and backward propagation. |
| Fujitsu | Proposal-3: For the two-sided AI/ML-based method, the study of STD impacts may start from: Studying the CSI report configurations and the procedures related to the two-sided AI/ML model. Studying the procedures related to pairing the AI/ML CSI generation part and the AI/ML CSI reconstruction part. Studying the AI/ML ON/OFF switching and the AI/ML operation alignment for the two-sided AI/ML model. |
| Panasonic | Proposal 1: The following training collaboration should be studied. Option 1: Joint training of the two-sided model with model transfer to UE. Option 2: Joint training of the two-sided model with model transfer to network Option 3: Joint training in offline engineering with multi-vendor agreements Option 4: Separate offline training at UE side and network side for CSI feedback generation model / CSI reconstruction model respectively |
| Oppo | Proposal 3: A clear distinction between the training phase and the deployment phase would be helpful.Training – The training procedure is to obtain a new AI/ML model. It starts from data collection and end up with an AI/ML model well trained and delivered to a given node, e.g. UE or gNB. Deployment – The deployment phase refers to that after a node receives a model, some engineering operations are required to make the model available to use at that node, e.g. specific optimization, compiling and testing.Proposal 5: In Rel-18, discussions on training collaboration should be handled with low priority.- No collaboration needs in 3GPP could be treated as the basic assumption- Collaboration needs for joint training with model transfer could be discussed with lower priority- Collaboration needs for separate training with intermediate results interaction should be handled in subsequent releases. |
| Futurewei | Proposal 1: Study potential standards impact related to training collaboration Type 1, 2 and 4 for AI/ML model training.Note: the assumption is that training collaboration Type 3 doesn’t incur specification impact in the model training phase. |
| CATT | Proposal 4: Study whether separate training for spatial-frequency domain CSI compression using two-sided AI/ML model is feasible, with the following aspects considered:– Whether the same training dataset is used by both sides;– Mechanisms on training dataset collection & transfer;– Whether the two sides can use different AI/ML model structures (e.g. one side uses transformer and the other side uses ResNet);– Whether associated /partial of AI/ML model related information exchange is needed. |
| Lenovo | Proposal 10 Study the advantages/disadvantages of network-based AI model training vs. UE-based AI model training |
| NVIDIA | Proposal 4: Study different training methods for autoencoder based CSI feedback including at least the following options:• Option 1: Network performs autoencoder training• Option 2: UE performs autoencoder training• Option 3: Joint training between network and UE via federated learning• Option 4: Joint training between network and UE via split learning |
| Xiaomi | Proposal 2: The training collaboration type of a two-sided model should be discussed with lower priority. |
| CAICT | Proposal 2: For CSI compression using two-sided AI model, offline training at gNB side with model transfer to UE side could be considered as baseline.Proposal 3: Further discussion on standard impact of separate training and joint training for two-sided AI model is required. |
| China Telecom | Proposal 5: Further evaluation the performance impact of air-interface enhancement without model exchange. |
| Samsung  | Proposal 2-2: Study CSI compression at the UE under collaboration level (D), where model exchanges are required to configure/enable AI, and inference is performed at the UE and the gNB. |
| Ericsson  | Proposal 4 Aim to agree in RAN1#110 on the definitions of the four training collaboration types for CSI enhancements, a starting point is the draft shown above.Proposal 5 For Type 3, study whether somewhat aligning AI/ML modes across different bilateral trainings (e.g. node internal model transfer approaches) with different vendors can reduce the implementation complexity due to the multi-vendor training situation.Proposal 6 Study two-sided AI-based solutions for CSI reporting that enable UE side AI/ML / NW side AI/ML interoperability between different vendors, without the need for joint training. |
| CMCC | Proposal 5: In CSI compression using two-sided model use case, the Type 1 of offline AI/ML model training collaboration could be further studied:• Type 1: Joint training of the two-sided model with model transfer to UEProposal 6: In CSI compression using two-sided model use case, transfer learning-based method could be studied for the training phase. |
| ETRI | Proposal 1: When considering Autoencoder for CSI feedback enhancement, first study the feasible training process of Autoencoder in both UE (Encoder) and gNB (Decoder) side supporting compatibility. |
| MediaTek | Proposal 2: Use the Alt 2 as the definition of joint training and separate training of two-sided modelProposal 3: Discuss spec impact for offline/online training collaboration after the discussion on general UE-gNB collaboration is finalized in AI 9.2.1. |
| Qualcomm | Proposal 3: For the CSI feedback enhancement use-cases, focus on collaboration level “y” based on offline training that would enable a model to be optimized specifically for the device that will run the model.Proposal 4: The distributed or separate offline training scenarios can be considered as a baseline for two-sided AI/ML model training. |
| Apple | Proposal 3: Consider four types of training collaboration for two-sided CSI compression use case. • Type 1: NW trained and at least encoder is transferred to UE. • Type 2: UE trained and at least decoder is transferred to NW• Type 3: Offline engineering event where UE trained encoder/gNB train decoder through split learning • Type 4: Separate training with training collaboration |

Training collaboration has been discussed in RAN1 109-e. It is desirable to agree on the training collaboration in RAN1 110. In 9.2.1 discussion, definition of “on-device training: online training at the UE” is discussed and not agreed yet. To avoid confusion, the proposals using “On-UE training” and “On-NW training” terminology is revised. The proposal reuse the wording before RAN1 109-e summary, with revision from proposals above.

Many companies share the view on prioritization of one or more types of training collaboration over the others. Views are not converging at this early phase. Therefore, we should have a detailed study of pros/cons of each approach.

## ***Proposal 3-1:***

***In CSI compression using two-sided model use case, the following AI/ML model training collaborations will be further studied:***

* ***Type 1: Joint training of the two-sided model with model transfer to UE.***
* ***Type 2: Joint training of the two-sided model with model transfer to NW.***
* ***Type 3: Joint training across network and UE without model transfer.***
* ***Type 4: Separate training at network and UE without model transfer, where the UE-side CSI generation part and the network-side CSI reconstruction part are trained by UE and network, respectively, in their own forward propagation and backward propagation loops.***
* ***FFS: Model fine tune.***
* ***FFS: Type 3 with specified interactions between UE and NW.***

***Note: Joint training means the generation model and reconstruction model should be trained in the same loop for forward propagation and backward propagation. Joint training could be done both at single NW node or across multiple nodes (e.g., through gradient exchange between nodes).***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## Data collection

Following table summarize company’s proposals related to data collection

|  |  |
| --- | --- |
| Huawei | Proposal 3: Study the potential specification impact on enabling network to obtain the ground-truth CSI from the realistic network as training labels for the AI/ML based model training at network. |
| Vivo | Proposal 2: In CSI compression, the following key LCM components for different training collaboration can be studied:• Data collection• Assistance information for model inference• Model transfer• Model activation/deactivation/switch• Performance monitoring• Model updating• Assistance information for trainingroposal 3: For data collection in CSI compression, study the potential specification impacts of:• Data collection via current or potentially enhanced reference signals • Data reporting via current or enhanced mechanism |
| Lenovo | Proposal 11 Study the means of feeding back the CSI training data from the UE to the network for FDD systems |
| NVIDIA | Proposal 5: For AI/ML model training for CSI feedback enhancement, study potential specification impact related to training data type/size, training data source determination, and assistance signalling and procedure for training data collection. |
| Xiaomi | Proposal 3: The signalling enhancements need to be studied for data collection used for training. |
| CMCC | Proposal 3: For AI based CSI enhancement, the potential spec impact on the training data reporting should be studied. |
| Qualcomm | Proposal 2: While generating the training dataset, the target CSI corresponding to a downlink measurement should be derived by the UE side.Proposal 5: Study meta-data assistance signaling for UE’s training data collection for AI/ML Model development. Here, meta-data refers to auxiliary information about data such as an ID assigned for each distinct beam configuration. Meta-data can be used for scenario discovery during offline model development and scenario association during inference.Proposal 6: UE data collection format and procedure is via offline engineering without need to involve 3GPP signaling.Proposal 7: Focus on offline training scenario, where the development and training of the ML model for CSI feedback happens offline without the need to involve 3GPP signaling. |
| Apple | Proposal 2: Consider training assisted information in CSI-RS configuration for different training data set. |
| NEC | Proposal 3: Identify each training procedure. Especially, the exact procedures of separate training at UE and NW should be clarified to discuss the potential specification impacts.  |

## ***Proposal 3-2:***

***In CSI compression using two-sided model use case, further discuss at least the following options for data collection:***

* ***Assistance signaling for UE’s training data collection for AI/ML Model development.***
* ***Transmission/reception of the datasets for training/validation/testing.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## Inference related spec impact

Following table summarize company’s proposals related to inferencing

|  |  |
| --- | --- |
| Huawei | Proposal 4: Study the potential specification impact for configuration and content of AI/ML model input/output for CSI compression. Proposal 5: Study the potential specification impact for the alignment of pre-processing and post-processing approaches between network and UE.Proposal 6: Study the potential specification impact for the quantization/dequantization method for the compressed CSI. |
| Vivo | Proposal 8: The specification impacts of encoder (decoder) input depend on the corresponding training options:• For training collaboration Type 1, 2, and 4, encoder input and decoder input should be specified• For training collaboration Type 3, encoder input could be left to implementation and decoder input should be specifiedProposal 9: The specification impacts of encoder (decoder) output depend on the corresponding training options:• For training collaboration Type 1, 2, and 4, encoder output and decoder output should be specified.• For training collaboration Type 3, encoder output should be specified and decoder output could be left to implementation. Proposal 10: Study the potential modifications in CQI/RI for AI/ML based CSI compression.Proposal 14: Study the specification impact of pre- and post-processing approaches for model input/output to address the issue of adaption to multi-configurations (e.g., bandwidth, number of ports, feedback payloads, antenna configurations, etc.). |
| ZTE | Proposal 2: For spatial-frequency domain CSI compression using two-sided AI model, at least further study and evaluate the following options for different types of AI/ML model input/output,▪ Option 1: The input of AI encoder is a raw channel (i.e obtained directly from CSI-RS) without any further pre-processing and corresponding output is a recovered raw channel: Option 1a: The raw channel is in frequency domain Option 1b: The raw channel is in time domain▪ Option 2: The input of AI encoder is a precoding matrix which is pre-processed from a raw channel and corresponding output is a recovered precoding matrix: Option 2a: The precoding matrix is a group of eigenvectors Option 2b: The precoding matrix is an eType II-like PMI. |
| Panasonic | Proposal 2: For each option of training collaboration, configuration and content for CSI report should be studied.Proposal 3: For each option of training collaboration, handling of rank of AI/ML model should studied. |
| Google | Proposal 2: Study the input of CSI compression based on the eigenvectors of the raw channel with a wideband precoder selected as SD basis, e.g. HW1. |
| Oppo | Proposal 4: The research and potential protocol impact analysis on the training, deployment, inference and management of AI/ML solutions could be discussed separately.- The requirements of AI/ML solutions for standardization in the inference phase should be evaluated with high priority- Corresponding necessary deployment and management issues also need to be analyzedProposal 10: Consider the impact of standards on encoder input, decoder output, as well as pre/post-processing(if needed) together.Proposal 11: Consider the impact of standards on encoder output and decoder input together.Proposal 15: Discussions on Quantization/Loss function should be left to implementation. |
| FutureWei | Proposal 2: Study potential standards impact regarding exchanging/sharing the main encoder input type, e.g., raw CSI feedback or eigenvectors while the exact input format, shape, and other accessory input features may be considered as implementation dependent.Proposal 3: Study potential standards impact related to the new CSI feedback to be transmitted over the air-interface (i.e., in bits) that is generated from the encoder at UE side and may be used as the input to the decoder directly or further processed to generate the input to the decoder at gNB.Proposal 4: Study potential standards impact related to other supporting information that is needed for the gNB to recover the unquantized encoder output from the received bits, e.g., quantization codebook, if such information is not already available.Proposal 8: Study potential standards impact to support AI/ML model inference procedure at UE side and gNB side. |
| Lenovo | Proposal 12 Study CSI reporting configuration enhancement for AI-based CSI feedback under different network-UE collaboration levelsProposal 13 Study CSI reporting content enhancement for AI-based CSI feedback under different network-UE collaboration levelsProposal 14 Study means of signaling the AI model parameters for two-sided AI models |
| NVIDIA | Proposal 8: For AI/ML based CSI feedback, study potential specification impact related to report/feedback of model input for inference, type of model input, and model input acquisition and pre-processing.Proposal 9: For AI/ML based CSI feedback, study potential specification impact related to report/feedback of model inference output and post-processing. |
| Intel | Proposal 2: • Specification impact for the CSI compression using two-sided AI model may include the followingo Introduction of NN concept in specification for PMI bits calculation (encoder part)o Introduction of NN concept in specification for precoder reconstruction for CQI (decoder part)o RRC configuration (including NN parameters configuration and NN coefficients)o UCI design (including new CSI quantity)o UE capabilities (including CPU definition for the AI/ML CSI) |
| Spreadtrum Communications | Proposal 2: AI/ML module at UE side can be delivered from gNB, based on UE’s capability. The input format and output format of the AI/ML module also should be included.Proposal 3: Aperiodic CSI reporting should be considered firstly.Proposal 4: The configuration of CSI-ResourceConfig and/or CSI-ReportConfig should be enhanced. |
| Xiaomi | Proposal 5: Input/output data format of AI/ML model needs to be defined.Proposal 7: In order to avoid performance loss due to mismatch between precoder and RI/CQI, it needs to study how to calculate RI/CQI when decoder is not deployed at UE side. |
| Samsung | Proposal 2-1: For CSI compression, study signaling requirements, input/output requirements, CSI configurations, and training strategies. |
| LGE | Proposal #2: Consider enhancement of CSI-RS/CSI reporting configurations for AI/ML based CSI feedback. |
| Ericsson  | Proposal 7 Study model-based MIMO channel feature extraction methods (pre-processing) based on spatial- and frequency-domain DFT codebooks (using Type-II CSI Rel.16) and associated specification impacts (e.g., additional required signaling over the air interface).Proposal 8 Study MIMO channel normalization methods, and associated specification impacts (e.g., additional required signaling over the air interface).Proposal 9 Include Ais based on both real- and complex-valued NNs in the study, where each proponent report which type was used in evaluaitons (i.e., do not restrict the study to only to real-valued NNs).Proposal 10 Study CSI enhanced reporting options for two-sided AI based solutions. For example, the CSI report may include a preferred rank indication, channel quality information, interference information, feature extraction information, and compression quality indicators.Proposal 11 Study quantization methods for UCI, including quantization aware training and complex-valued activation functions. |
| Nokia | Proposal 1. Study channel-, eigenvector-based and W2-based two-sided models for CSI feedback compression. Proposal 2. For the two-sided models, study the impact of quantizers on CSI feedback compression. |
| MediaTek | Proposal 4: Discuss spec impact for model input (encoder/decoder input) and pre-processing after the discussion on training collaboration is finished. Proposal 5: Discuss spec impact for model output (encoder/decoder output) after the discussion on training collaboration is finished.Proposal 8: Study potential spec impact on quantization for CSI compression with auto-encoder focusing on the followings• Uniform vs Non-uniform quantization• Scalar vs Vector quantization• Derivable (approximated) quantization• Gradient passing• Learnable quantization offset |
| Interdigital | Proposal 5: Study the use of pre-processing in the frequency, spatial and angle-delay domains as means to reduce the AI/ML model complexity.Proposal 6: Study specification impacts of CSI compression using AI/ML including: pre-processing the measurements at the UE, AI/ML model selection at the UE, new CSI report types and new CSI reporting mechanism. |
| Qualcomm | Proposal 8: The input to the UE-side model should be left to UE implementation, the output at the NW-side model can be specifiedProposal 9: Preprocessing at UE side is upto UE-implementation and should not be specified. Proposal 10: For AI-based CSI feedback, the size of the UCI payload and the final CSI format can be specified. Post-processing of CSI decoder output to the final CSI should be specified as part of the final CSI structure.Proposal 11: The discussion on specification impact on input/output of CSI encoder/decoder and CSI report configuration is independent of training collaborations. |
| Apple | Proposal 4: Input to the AI encoder including potential pre-processing needs to be signalled.Proposal 5: Output of the AI encoder needs to be signalled, including RI, CQI, inferencing output and potential encoder neural network ID.Proposal 6: RAN1 further discuss CQI definition for AI based CSI compression. Proposal 7: Output of the AI decoder including potential post-processing needs to be signalled. |
| NTT DOCOMO | Proposal 2: Study the potential specification impacts based on CSI type for input/output. |

## ***Proposal 3-3-1:***

***In CSI compression using two-sided model use case, further study potential specification impact on CSI report, including at least***

* ***Encoder output and decoder input, including size/configuration and potential post/pre-processing of encoder output/decoder input.***
* ***RI***
* ***CQI with potential modification for AI based CSI compression.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## ***Proposal 3-3-2:***

***In CSI compression using two-sided model use case, further study potential specification impact on encoder input, including at least***

* ***Model input type/dimension/configuration***
* ***Model-based MIMO channel feature extraction methods (pre-processing) based on spatial- and frequency-domain DFT codebooks (using Type-II CSI Rel.16) and associated specification impacts (e.g., additional required signaling over the air interface).***
* ***MIMO channel normalization methods, and associated specification impacts (e.g., additional required signaling over the air interface).***
* ***Note: The encoder input can be left for implementation at least for training collaboration type 3.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## ***Proposal 3-3-3:***

***In CSI compression using two-sided model use case, further study potential specification impact on decoder output, including at least***

* ***Model output type/dimension/configuration and potential post processing***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## ***Proposal 3-3-4:***

***In CSI compression using two-sided model use case, further study potential specification impact on the quantization/dequantization method for the compressed CSI.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## Performance monitoring, model update, activation/de-activation/switching

Following table summarize company’s proposals related to model performance monitoring, activation/de-activation/switching.

|  |  |
| --- | --- |
| Huawei | Proposal 7: Study the potential specification impact for life cycle management for AI/ML-based CSI feedback, including dataset collection, model monitoring, model switching, and model updating. Proposal 8: Study the potential specification impact for the co-existence between AI/ML mode and legacy non-AI/ML mode. |
| Vivo | Proposal 4: For model activation/deactivation/switch in CSI compression, study the potential specification impacts of following options:• Model activation/deactivation/switch via model ID Proposal 5: For performance monitoring in CSI compression, study the potential specification impacts of following cases:• Complete model (encoder and decoder) is available at UE • Complete model (encoder and decoder) is available at gNB• Neither UE nor gNB has complete modelProposal 13: Study the schemes and corresponding specification to address issues of scenario (e.g., Umi, UMa, Indoor, etc.) and configuration adaption (e.g., bandwidth, number of ports, feedback payloads, antenna configurations, etc.) in AI/ML for CSI feedback enhancement, including:• Schemes that can be easily adapted to different scenarios and configurations• Procedure and ignaling for scenario- and configuration-specific data collection;• Procedure and ignaling for model selection;• Signalling to indicate the application scope of each model |
| ZTE | Proposal 5: During study phase, companies need to evaluate and identify the solutions to perform model life cycle management in CSI feedback enhancement, at least following perspectives can be further studied:▪ Case 1: A common AI/ML model that is applicable to all scenarios▪ Case 2: AI/ML model switching to adapt different scenarios based on model performance monitoring▪ Case 3: An offline trained AI/ML model to be updated online |
| Fujitsu | Proposal-3: For the two-sided AI/ML-based method, the study of STD impacts may start from: Studying the CSI report configurations and the procedures related to the two-sided AI/ML model. Studying the procedures related to pairing the AI/ML CSI generation part and the AI/ML CSI reconstruction part. Studying the AI/ML ON/OFF switching and the AI/ML operation alignment for the two-sided AI/ML model. |
| Panasonic | Proposal 4: The following options should be studied for life cycle management. Solution 1: gNB side performance monitoring 1-1: UE transmit encoder input as CSI report periodically or occasionally. 1-2: gNB may directly use system throughput or ratio of NACK. Solution 2: UE side performance monitoring 2-1: UE calculate decoder output using virtual decoder in UE. 2-2: UE may obtain the inference results indicated from gNB periodically or occasionally 2-3: UE may use PDSCH decoding performance as KPI. |
| Google | Proposal 6: Study the AI/ML model adaptation for CSI compression, where different AI/ML models may be with different compression ratio. |
| NEC | Proposal 3: Study the mechanism of evaluating model performance to facilitate AI/ML model lifecycle management.Proposal 4: Study the behaviors of UE or (and) gNB after AI/ML model performance deteriorates, e.g., model update (fine-tuning), model switching, fall back to non-AI/ML mechanism.Proposal 5: Study the mechanism of model selection to facilitate AI/ML model lifecycle management. |
| Oppo | Proposal 12: Give high priority to some basic LCM solutions, e.g. the selection and use of the most suitable scheme through reasonable performance monitoring, necessary signaling indication and model switching.Proposal 13: More challenging LCM schemes, e.g. online real-time model training and updating, can be studied in subsequent studies. |
| FutureWei | Proposal 7: Study potential standards impact to support AI/ML model adaptation across various configurations. |
| CATT | Proposal 5: Study mechanisms on model quality monitoring for CSI feedback, with the following aspects considered:– Which side takes responsibility on model quality monitoring, e.g. at UE side, at network side, or both;– The scheme of model quality monitoring when only partial of AI/ML model (i.e. encoder/decoder) is known by one side. |
| NVIDIA | Proposal 6: For AI/ML based CSI feedback, study potential specification impact related to assistance ignaling and procedure for model configuration, model activation/deactivation, model recovery/termination, and model selection.Proposal 7: For AI/ML based CSI feedback, study potential specification impact related to assistance ignaling and procedure for model performance monitoring and model update/tuning. |
| Spreadtrum Communications  | Proposal 6: Both gNB and UE can be considered to monitor AI/ML model.Proposal 7: The better generalization of AI/ML model should be strived, to avoid frequent AI/ML model updating. |
| Xiaomi | Proposal 4: It should be studied which side implementing performance monitoring or what is the metric of performance monitoring. |
| CAICT | Proposal 4: Some original CSI information feedback could be considered for AI/ML model monitoring. |
| Samsung | Proposal 2-3: Study and verify model update of the encoder at the UE, where the gNB’s training strategy is not disclosed while transferring/configuring the AE |
| LGE | Proposal #4: Consider fallback operation when AI/ML based CSI reporting is not valid. |
| CMCC | Proposal 7: For AI based CSI enhancement, the potential spec impact of model selection/model switching should be studied. |
| Interdigital | Proposal 10: Study means to monitor the AI/ML encoder performance at inference time, for CSI enhancements using both two-sided AI/ML model, and one-sided AI/ML at the UE.Proposal 11: Study means to mitigate AI/ML encoder model performance degradation.Proposal 12: Study means to perform model transfer to mitigate AI/ML model performance degradation Proposal 13: Mechanisms to fallback to legacy CSI reporting are needed (e.g. for cases where model transfer or AI/ML model on-line training is performed) |
| Qualcomm | Proposal 12: Study signaling and procedures for X-node CSF performance monitoring, including assistance information, performance report and indication of model deactivation, retraining or switching. |
| Apple | Proposal 8: Activation/de-activation/switching can be enabled by RRC configuration. Proposal 9: Performance monitoring can be done at the UE and the gNB based on DL throughput or PDSCH BLER.  |
| NTT DOCOMO | Proposal 4: Study NW-based model monitoring and UE-based model monitoring for spatial-frequency domain CSI compression. |

## ***Proposal 3-3-4:***

***In CSI compression using two-sided model use case, study potential specification impact for performance monitoring, considering at least the following aspects:***

* ***NW-based AI model performance monitoring and UE-based AI model performance monitoring***
* ***Performance monitoring KPIs***
* ***Assisted information and performance report***
* ***Co-existence and fall-back mechanisms between AI/ML mode and legacy non-AI/ML mode.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## ***Proposal 3-3-5:***

***In CSI compression using two-sided model use case, further study potential specification for model selection, model configuration, model activation/de-activation, model adaptation across various configurations.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| xxx |  |

## Model transfer

Following table summarize company’s proposals related to model transfer.

|  |  |
| --- | --- |
| Vivo |  Proposal 11: Study the specification impacts of following model transfer cases:• Option 0: Network sends updated parameters and does not change the AI/ML model structure. (Already supported by nowadays typical chipset implementations)• Option 1: Network sends AI/ML model parameter and structure information. (Dependent on how much the model structure is changed, recompilation may be needed.)Proposal 12: Further study model transfer format in both short and long term. We suggest to consider the following options:• Negotiation between networks nodes• Definition of a common format recognizable by multiple parties• Definition of a new model description format by 3GPP |
|  Futurewei |  Proposal 5: For solution options required model transfer, study potential standards impact associated with:o Exchanging model information, including protocol/ignaling mechanism that enables the model transfero Exchanging additional functional modules (if not integrated with the model) and/or other supporting information between gNB and UE to help the receiving node to perform the encoding/decoding function and/or interpret the modelProposal 6: Study potential standards impact related to deploying/supporting different encoders based on UE capability while keeping the main decoder architecture unchanged at gNB. |
| CMCC | Proposal 4: For AI based CSI enhancement, the potential spec impact on AI model transfer need to be studied. |
| MediaTek | Proposal 7: Discuss potential spec impact on model exchange focusing on the followings• Content of the model exchange including model format, pre/post-processing choice, model parameters, hyper-parameters, etc.• Signalling format for the model exchange• Related UE capability |

Model exchange can be discussed at least initially at 9.2.1. CSI specific model exchange will be discussed later after high level discussion in 9.2.1.

## Framework, UE capability, and other topics

Following table summarize company’s proposals related to framework.

|  |  |
| --- | --- |
| Google | Proposal 1: The study of AI/ML based CSI compression should be based on the CSI framework in Rel-17.Proposal 3: The study of the report of compressed CSI should be based on Rel-15 CSI report mechanism, where the CSI is reported in a single part in short PUCCH, and the CSI can be reported in two parts in long PUCCH and PUSCH.Proposal 4: Study the priority rule for AI/ML based CSI report and non-AI/ML based CSI report with regard to CSI collision handling and CSI omission.Proposal 5: The AI/ML based CSI compression should consider the following types of UE: • Type 1 UE (low performance UE): CSI compression is based on general processing unit (GPU)• Type 2 UE (high performance UE): CSI compression is based on neural processing unit (NPU) |
|  Oppo  | Proposal 6: Discussions on AI/ML model deployment and AI/ML model training should be decoupled.Proposal 7: In Rel-18, fully analyze the difficulty and requirement of AI/ML model deployment, and distinguish the impact of different conditions and assumptions, including: - Real-time deployment- Non real-time deployment- Whole new model deployment- Partial new model deployment (e.g. the deployment of only updating model weights)- Deployment of complex models- Deployment of simple modelsProposal 8: Scenarios for non real-time, partial model deployment and simple model deployment can be considered as the basic deployment assumption for subsequent research in Rel-18. - FFS Other scenarios - Scenarios with high deployment complexity can wait until it could be handled by companies with reasonable solutionsProposal 9: Both protocol visible interfaces and protocol invisible interfaces can be used in subsequent AI/ML applications and need to be studied. |
| CATT | Proposal 6: Study the scalable and flexible frameworks for AI/ML based approaches for CSI feedback.Proposal 7: On evaluation of scalability of AI/ML model for CSI feedback, the following configurations can be considered as the starting point:- Different number of antenna ports, e.g. 32 ports, 16 ports.- Different number of reporting subbands.- Different bandwidths, e.g. 10MHz vs. 20MHz.- Different numerologies, e.g. 15kHz vs. 30kHz.- Different CSI feedback payloads. |
| Spreadtrum Communications | Proposal 1: Legacy CSI framework can be reused for the sub use case - Spatial-frequency domain CSI compression. Additional enhancement can be considered.Proposal 5: How to define/reflect the complexity of the AI/ML operation in the specification should be considered. |
| Samsung | Proposal 4-1: Study UE processing time impact on online training for update, transfer, and download. |
| LGE | Proposal #3: Consider enhancement of UE CSI processing procedure including CPU and CSI reference resource for AI/ML based CSI reporting. |
| ETRI | Proposal 2: Study the feasibility of the PCA based two-sided AI model for CSI compression sub use case. |

UE capability and other topics will be discussed later. High level agreement on framework can be benifical for future discussion.

## ***Proposal 3-6:***

***The study of AI/ML based CSI compression should be based on the legacy CSI feedback framework.***

Please provide your view below:

|  |  |
| --- | --- |
| **Company** | **View** |
| Xxx |  |

# Potential specification impact for other use cases

The following table summarizes proposals on potential specification impact on other sub-use cases. The summary can be used as reference for discussion of section 2.

|  |  |
| --- | --- |
| vivo | Proposal 15: Study the specification impact of both gNB- and UE-based CSI prediction.Proposal 16: For UE-based CSI prediction, study on specification impact at least includes the following aspects• Capability report of CSI prediction• gNB’s activation, deactivation, configuration and adjustment of AI based CSI prediction, and UE’s request on such actions• gNB and UE’s alignment on prediction related time domain configuration information• Supported CSI-RS configurations (e.g., CSI-RS time domain type(s))• Correct CSI reference resource definitionProposal 17: To support gNB-based prediction with high accuracy, the CSI feedback enhancement should be carefully designed to reserve Doppler information or time varying information as much as possible.Proposal 18: Study on LCM aspects of CSI prediction at least includes the following• For performance monitoring, functionality of using dedicated CSI-RS and reporting process to derive label with lower noise and interference• LCM of chained AI model (e.g., for AI-based prediction and compression)• Finetuning process of AI-based CSI prediction |
| Fujitsu | Proposal-4: For the one-sided AI/ML-based method, the study of STD impacts may start from: Studying the time-domain CSI-RS configurations to enable accurate CSI prediction. Studying CSI-RS overhead reduction for CSI prediction. Studying assistance information needed for CSI prediction. |
| NEC | Proposal 6: Support the location/CQI report timing set mapping table based on AI/ML.Proposal 7: Support the location/CQI periodicity mapping table based on AI/ML. |
| Apple | Proposal 10: For CSI prediction use case, potential specification impact including UE capability signaling, UE request and NW activation/de-activation signaling.  |
| Interdigital | Proposal 9: Specification impacts of reduced CSI-RS overhead include new RS configurations, new RS triggers, and UE feedback. |

# Reference

[R1-2205891](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2205891.zip) Discussion on AI/ML for CSI feedback enhancement Huawei, HiSilicon

[R1-2205967](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2205967.zip) Discussions on Sub-Use Cases in AI/ML for CSI Feedback Enhancement TCL Communication

[R1-2206033](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206033.zip) Other aspects on AI/ML for CSI feedback enhancement vivo

[R1-2206069](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206069.zip) Discussion on other aspects for AI CSI feedback enhancement ZTE

[R1-2206114](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206114.zip) Considerations on CSI measurement enhancements via AI/ML Sony

[R1-2206165](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206165.zip) Discussion on other aspects of AI/ML for CSI feedback enhancement Fujitsu

[R1-2206185](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206185.zip) Discussion on AI/ML for CSI feedback enhancement Panasonic

[R1-2206196](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206196.zip) On Enhancement of AI/ML based CSI Google

[R1-2206241](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206241.zip) Discussion on AI/ML for CSI feedback enhancement NEC

[R1-2206316](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206316.zip) On sub use cases and other aspects of AI/ML for CSI feedback enhancement OPPO

[R1-2206337](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206337.zip) Continued discussion on other aspects of AI/ML for CSI feedback enhancement FUTUREWEI

[R1-2206392](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206392.zip) Other aspects on AI/ML for CSI feedback CATT

[R1-2206511](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206511.zip) Further aspects of AI/ML for CSI feedback Lenovo

[R1-2206521](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206521.zip) AI and ML for CSI feedback enhancement NVIDIA

[R1-2206579](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206579.zip) Use-cases and specification for CSI feedback Intel Corporation

[R1-2206605](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206605.zip) Discussion on other aspects on AIML for CSI feedback Spreadtrum Communications

[R1-2206636](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206636.zip) Discussion on potential specification impact for CSI feedback based on AI/ML Xiaomi

[R1-2206676](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206676.zip) Discussions on AI-ML for CSI feedback CAICT

[R1-2206687](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206687.zip) Discussion on AI/ML for CSI feedback enhancement China Telecom

[R1-2206821](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206821.zip) Representative sub use cases for CSI feedback enhancement Samsung

[R1-2206875](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206875.zip) Other aspects on AI/ML for CSI feedback enhancement LG Electronics

[R1-2206884](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206884.zip) Discussion on AI-CSI Ericsson

[R1-2206903](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206903.zip) Discussion on other aspects on AI/ML for CSI feedback enhancement CMCC

[R1-2206954](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206954.zip) Discussion on other aspects on AI/ML for CSI feedback enhancement ETRI

[R1-2206969](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206969.zip) Other aspects on ML for CSI feedback enhancement Nokia, Nokia Shanghai Bell

[R1-2206989](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2206989.zip) Other aspects on AI/ML for CSI feedback enhancement MediaTek Inc.

[R1-2207153](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2207153.zip) Discussion on AI/ML for CSI feedback enhancement InterDigital, Inc.

[R1-2207225](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2207225.zip) Other aspects on AI/ML for CSI feedback enhancement Qualcomm Incorporated

[R1-2207329](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2207329.zip) Other aspects on AI/ML for CSI Apple

[R1-2207370](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2207370.zip) Sub-use cases for AI/ML feedback enhancements AT&T

[R1-2207402](file:///C%3A%5CUsers%5Cyounsun%5CDocuments%5C3GPP%20documents%5CRAN1%20tdocs%5CTSGR1_110%5CDocs%5CR1-2207402.zip) Discussion on other aspects on AI/ML for CSI feedback enhancement NTT DOCOMO, INC.