**3GPP TSG RAN WG1 #110bis-e** **R1-221xxxx**

**e-Meeting, October 10th – 19th, 2022**

**Agenda item:** 7.1

**Source:** Moderator (Samsung)

**Title:** Summary of [110bis-e-NR-R15-01] Discussion on PUCCH collision handling for more than two overlapped PUCCHs with repetition

**Document for:** Discussion and Decision

# Introduction

This contribution provides the summary for the following email discussion in RAN1#110bis-e:

[110bis-e-NR-R15-01] Discussion on PUCCH collision handling for more than two overlapped PUCCHs with repetition by Oct 17 – Sa (Samsung)

Section 3 provides the background information. Section 4 captures the detailed email discussions. Section 5 summarizes the outcome of the email discussion.

# Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
| Moderator (Samsung) | Sa Zhang | sa.zhang@samsung.com |
| Qualcomm  | Yi Huang | yihuang@qti.qualcomm.com |
| Intel  | Yi Wang  | yi5.wang@Intel.com |
| OPPO | Yi Zhang | zhangy@oppo.com |
| CATT | Yanping Xing | xingyanping@catt.cn |
| ZTE | Junfeng Zhang | Zhang.junfeng@zte.com.cn |
| MTK | James Hsieh | CH.Hsieh@mediatek.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Background

In RAN1#109-e, more than two overlapping PUCCHs with repetitions was discussed [1] and the following conclusions were made [2].

|  |
| --- |
| Conclusion:For resolving overlapping PUCCHs with and/or without repetitions in a slot in Rel-16, a UE first performs clause 9.2.6 (TS 38.213) to resolve overlapping PUCCHs where at least one PUCCH is with repetitions, and then UE performs clause 9.2.5 (TS 38.213) to resolve overlapping PUCCHs without repetitions.* Note: The above is performed per slot.

Conclusion:For resolving overlapping PUCCHs with repetitions in clause 9.2.6 of TS 38.213 in Rel-16, PUCCHs with repetitions and PUCCHs overlapping with a PUCCH with repetitions are considered. PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not considered.* Note 1: The above is for clarifying the determination of the overlapping PUCCHs resolved in clause 9.2.6 of TS 38.213 and does not impact the determination of “a set of overlapping PUCCHs” when performing clause 9.2.6 of TS 38.213 discussed in [109-e-NR-CRs-03].
* Note 2: The above has no spec impact. This is also assumed in discussion to solve issue in [109-e-NR-CRs-03].

Conclusion:For resolving the overlapping PUCCHs with repetitions in Rel-16, the procedure of 9.2.6 of TR38.213 only performs prioritization, multiplexing is not performed in 9.2.6 of TR38.213.* Note: the above has no spec impact.

ConclusionFor resolving overlapping PUCCHs of a same priority in Rel-16, a UE performs the following steps* Step1, the UE resolves overlapping PUCCHs with repetitions as described in TS 38.213 clause 9.2.6, if any.
	+ Step 1-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.6.
		- o    PUCCHs with repetitions and PUCCHs overlapping with a PUCCH with repetitions are involved.
		- o    PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved.
	+ Step 1-2: the UE resolves overlapping PUCCHs determined in Step 1-1 by performing TS 38.213 clause 9.2.6.
		- o    Only prioritization is performed.
* Step2, the UE resolves overlapping PUCCHs without repetitions as described in TS 38.213 clause 9.2.5, if any.
	+ Step 2-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.5.
		- PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are involved.
		- Resulting PUCCHs without repetitions of resolving overlapping PUCCHs determined in Step 1-2 are involved.
	+ Step 2-2: the UE resolves overlapping PUCCHs determined in Step 2-1 by performing TS 38.213 clause 9.2.5.

Note: The above conclusion on the generic framework with high-level steps has no spec impact. The details of certain steps, e.g. step 1-2, may have spec impact subject to outcome of the ongoing and future discussion on the issues identified in email thread [109-e-NR-CRs-03].  |

In RAN1#110, the issue was further discussed and the following working assumption was made [4].

|  |
| --- |
| Working AssumptionFor resolving overlapping PUCCHs with repetitions of a same priority in Rel-16, a UE performs the following steps* Step 1-2-1: the UE determines a set of overlapping PUCCHs.
* Step 1-2-2: the UE performs prioritization among PUCCHs in the set of overlapping PUCCHs.
	+ The priority order for different UCI types is defined as: HARQ-ACK > SR > CSI with higher priority > CSI with lower priority
	+ For overlapping PUCCHs of the same UCI priority, the priority order for a same UCI type is defined as：PUCCH starting at an earlier slot > PUCCH starting at a later slot
* Step 1-2-3: the UE repeats step 1-2-1 and step 1-2-2 until the overlapping PUCCHs with repetitions is resolved.
 |

8 companies discuss the remaining issues of the overlapping PUCCHs with repetitions in the submitted contributions [5] ~ [13] and the proposals are summarized below.

|  |  |
| --- | --- |
| Company | Proposal |
| HW | ***Proposal 1: For a group of more than two overlapping PUCCHs at Step 1-2-1, “a set of overlapping PUCCHs” is determined by the following two steps:**** ***Step i, a reference PUCCH is selected from all PUCCHs with repetition that overlap with at least one PUCCH in the current slot with the order of earliest symbol followed by longest duration.***
* ***Step ii, the “a set of overlapping PUCCHs” is determined as the reference PUCCH and all PUCCHs (with/without repetitions) that are overlapping with this reference PUCCH.***

***Proposal 2: For a group of more than two overlapping PUCCHs in Step 1-2-2, the PUCCH with the highest priority/earliest slot of “a set of overlapping PUCCHs” is transmitted, while the PUCCH with any lower priority/later slot of “a set of overlapping PUCCHs” is dropped.**** ***If there are at least two PUCCHs with the same highest priority in the “a set of overlapping PUCCHs”, the PUCCH starting at the earliest slot among the at least two PUCCHs is transmitted, while other PUCCHs are dropped.***
* ***UE does not expect any two PUCCHs of the “a set of overlapping PUCCHs” have the same UCI type as well as start at the same slot***

9.2.6 PUCCH repetition procedure< Unchanged parts are omitted >A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and at least a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect any two PUCCHs from the first PUCCH and the second PUCCHs to start at a same slot and include a UCI type with same priority - if the first PUCCH and each of the second PUCCHs include a UCI type with same priority, the UE transmits the PUCCH starting at an earliest slot and does not transmit the PUCCH starting at any later slot- if the first PUCCH and any of the second PUCCHs do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with highest priority followed by starting at an earliest slot and does not transmit the PUCCH that include the UCI type with any lower priority or any later slot- the UE performs the above rules by selecting the first PUCCH with the order of earliest symbol followed by longest duration from the PUCCHs with repetition that overlap with at least one PUCCH, and the at least a second PUCCH includes all PUCCHs overlapping with the first PUCCH< Unchanged parts are omitted > |
| SPRD | 1. ***The reference PUCCH is a PUCCH with repetitions to determine a set of overlapping PUCCHs.***
2. ***The collision of all PUCCHs within the set of overlapping PUCCHs are resolved at a time, PUCCH resource with higher /highest priority or earlier/earliest slot is transmitted and the others are dropped in Step 1-2-2.***
 |
| OPPO | ***Proposal 1: In step 1-2-1 for determining a set of overlapping PUCCHs, the reference PUCCH should be a PUCCH with repetitions.******Proposal 2: In step 1-2-1, “a set of overlapping PUCCHs” can contain at least two PUCCHs including “a first PUCCH” with repetitions and “at least a second PUCCH” overlapping with the “first PUCCH”.******Proposal 3: In step 1-2-2, within “a set of overlapping PUCCHs”, UE transmits the PUCCH with UCI type with the highest priority or earliest starting slot (when same priority) and drops all other PUCCHs.******Proposal 4: In step 1-2-3, the UE repeats step 1-2-1 and step 1-2-2 until there is no PUCCH overlapping with a PUCCH with repetitions.******Observation 1: There exists ambiguity on the selection order of the “reference PUCCH/first PUCCH” when there are more than one PUCCH with repetitions in a slot.******Proposal 5: When there are more than one PUCCH with repetitions in a slot, RAN1 to discuss the following alternatives:******Alt 1:*** ***Step a: UE selects a PUCCH with rep as the “reference PUCCH/first PUCCH” that overlap with at least one PUCCH according to the order of earliest starting symbol followed by longest duration.*** ***Step b: “A set of overlapping PUCCHs” include the “reference PUCCH/first PUCCH” and all the PUCCHs overlapping with the “reference PUCCH/first PUCCH”. UE transmits the PUCCH with UCI type with the highest priority or earliest starting slot (when same priority) and drops all other PUCCHs.******Step c: repeat step a and step b until there is no PUCCH overlapping with a PUCCH with repetitions.******Alt 2:*** ***Step a: UE selects a PUCCH with rep as the “reference PUCCH/first PUCCH” that overlap with at least one PUCCH according to the order of UCI priority followed by earliest starting slot then by longest duration.*** ***Step b: “A set of overlapping PUCCHs” include the “reference PUCCH/first PUCCH” and all the PUCCHs overlapping with the “reference PUCCH/first PUCCH”. UE transmits the PUCCH with UCI type with the highest priority or earliest starting slot (when same priority) and drops all other PUCCHs.******Step c: repeat step a and step b until there is no PUCCH overlapping with a PUCCH with repetitions.******Alt 3:*** ***UE does not expect to be configured or scheduled more than one PUCCH with repetitions in a slot.*** |
| CATT | **Observation 1: UE behavior is not clear for Option 1, 2 and 6 for the case shown in Figure 1.****Observation 2: For the case shown in Figure 2, only Option 4 keeps both PUCCH 1 and PUCCH 3 and other options (i.e. Option 1/2/3/5/6) additionally drop PUCCH 3.****Observation 3: For the case shown in Figure 3, Option 4/5/6 keep both PUCCH 1 and PUCCH 3 and other options (i.e. Option 1/2/3) additionally drop PUCCH 1.****Observation 4: For the case shown in Figure 4, Option 4/5 keep both PUCCH 1 and PUCCH 3 and other options (i.e. Option 1/2/3/6) additionally drop PUCCH 1.****Proposal: For collision handling of more than two overlapping PUCCHs with repetition, consider following Option 4 and Option 5.*** **Option 4:**
* **Step 1-2-1: Determine a first PUCCH with repetition based on UCI priority followed by starting slot/sub-slot as defined in TS 38.213 clause 9.2.6 and “a set of overlapping PUCCHs” including the first PUCCH and all the PUCCHs overlapping with the first PUCCH;**
* **Step 1-2-2: Perform pair-wise prioritization between the first PUCCH and a second PUCCH until there is no overlapping between the first PUCCH and another PUCCH, where the second PUCCH is selected based on UCI priority followed by starting slot/sub-slot as defined in TS 38.213 clause 9.2.6 within “a set of overlapping PUCCHs”.**
* **Option 5:**
* **Step 1-2-1: Determine a first PUCCH based on UCI priority followed by starting slot/sub-slot as defined in TS 38.213 clause 9.2.6 and “a set of overlapping PUCCHs” including the first PUCCH and all the PUCCHs overlapping with the first PUCCH**
* **Step 1-2-2: Keep the first PUCCH and drop all the other PUCCHs within “a set of overlapping PUCCHs”.**
 |
| Intel | **Proposal 1: For resolving overlapping PUCCHs of a same priority in Rel-16, a UE performs the following steps*** **Step 1-2-1: the UE determines a set of overlapping PUCCHs according to existing pseudo-code in clause 9.2.5**
* **Step 1-2-2: the UE performs prioritization among PUCCHs in the set of overlapping PUCCHs with only one survived PUCCH**
	+ **The priority order for different UCI types is defined as: HARQ-ACK > SR > CSI with higher priority > CSI with lower priority**
	+ **For overlapping PUCCHs of the same UCI priority, the priority order for a same UCI type is defined as：PUCCH starting at an earlier slot > PUCCH starting at a later slot**
* **Step 1-2-3: the UE repeats step 1-2-1 and step 1-2-2 until the overlapping PUCCHs with repetitions is resolved.**
 |
| ZTE | ***Proposal 1:*** *To perform prioritization among PUCCHs in the set of overlapping PUCCHs, UE would transmit the highest priority channel(s) in the set of overlapping PUCCHs. If there are two or more non-overlapping PUCCHs with UCI of highest priority, all of them will be transmitted.****Proposal 2****: For the determination of reference PUCCH in the set of overlapping PUCCHs with repetitions, the reference PUCCH can be a PUCCH with or without repetitions.*  |
| Samsung | **Proposal: For resolving more than two overlapping PUCCHs of the same priority, reuse the pseudo-code in TS 38.213 9.2.5 with the restriction of selecting up to 2 PUCCH resources and apply the rules defined in clause 9.2.6 if there is repetition or clause 9.2.5, otherwise. Adopt the following TP for section 9.2.5 and 9.2.6 of TS38.213.**-------------------------------------------------- Start of text proposal ---------------------------------------------------**9.2.5 UE procedure for reporting multiple UCI types**<Unchanged text omitted>Set  to the cardinality of Set to be the first symbol of resource  in the slotSet  to be the number of symbols of resource  in the slotSet  - index of first resource in set Set  - counter of overlapped resourceswhile if  and resource  overlaps with resource  and the resources in set $Q$ do not include a PUCCH with repetitions, or $j<C\left(Q\right)-1$ and resource $Q(j-o)$ overlaps with resource $Q(j+1)$, $o=0$, and the resources in set $Q$ include at least one PUCCH with repetitionselseif determine a single resource for multiplexing UCI associated with resources  as described in clauses 9.2.5.0, 9.2.5.1, ~~and~~ 9.2.5.2 and 9.2.6set the index of the single resource to   % start from the beginning after reordering unmerged resources at next step % function that re-orders resources in current set Set  to the cardinality of elseend ifend ifend while<Unchanged text omitted>**9.2.6 PUCCH repetition procedure**<Unchanged text omitted>A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and ~~at least~~ a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect the first PUCCH and ~~any of~~ the second PUCCH~~s~~ to start at a same slot and include a UCI type with same priority - if the first PUCCH and ~~any of~~ the second PUCCH~~s~~ include a UCI type with same priority, the UE transmits the PUCCH starting at an earlier slot and does not transmit the PUCCH starting at a later slot- if the first PUCCH and ~~any of~~ the second PUCCH~~s~~ do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with higher priority and does not transmit the PUCCH that include the UCI type with lower priority If a UE would transmit more than two overlapping PUCCH transmissions in a slot, where at least one PUCCH transmission is with repetitions over $N\_{PUCCH}^{repeat}>1$ slots, the UE resolves the overlapping for PUCCH transmissions in the slot using the pseudo-code in clause 9.2.5.<Unchanged text omitted>----------------------------------------------------- End of text proposal ------------------------------------------------ |
| QC | ***Proposal 1: Adopt the following TP for Rel-***9.2.6 PUCCH repetition procedure\*\*\*\* unchanged text omitted \*\*\*\*\*\*A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and at least a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect the first PUCCH and any of the second PUCCHs to start at a same slot and include a UCI type with same priority - if the first PUCCH and any of the second PUCCHs include a UCI type with same priority, the UE transmits the PUCCH starting at an earlier slot and does not transmit the PUCCH starting at a later slot- if the first PUCCH and any of the second PUCCHs do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with higher priority and does not transmit the PUCCH that include the UCI type with lower priority If a UE would transmit a group of overlapping PUCCH channels {Q(j-o+1),…,Q(j)} with a same priority index as described in Clause 9.2.5 in a slot, and if at least one of the PUCCH in the group is repeated over more than one slots, the UE transmits the PUCCH with the highest priority in the group in the slot using the procedures described above and does not transmit the other PUCCH(s) in the group.  |

# Email Discussion

In RAN1#110e 7 candidate options were proposed by companies and companies’ preferences are quite diverse. It seems not possible to directly converge to a candidate option. In this meeting, moderator’s suggestion is separately discussing each of the remaining issues and try to better align companies’ view. Considering this is the late CR phase, the solution should aim for minimizing specification impact.

## First round

## Determination of a set of overlapping PUCCHs

All the submitted contributions [5] ~ [13] discussed the details of Step 1-2-1 of the following WA. The common understanding is that the set of overlapping PUCCHs consist of a reference PUCCH and PUCCH(s) overlapping with the reference PUCCH. A UE first determines a reference PUCCH and then determines the PUCCHs overlapping with the reference PUCCH.

|  |
| --- |
| Working AssumptionFor resolving overlapping PUCCHs with repetitions of a same priority in Rel-16, a UE performs the following steps* Step 1-2-1: the UE determines a set of overlapping PUCCHs.
* Step 1-2-2: the UE performs prioritization among PUCCHs in the set of overlapping PUCCHs.
	+ The priority order for different UCI types is defined as: HARQ-ACK > SR > CSI with higher priority > CSI with lower priority
	+ For overlapping PUCCHs of the same UCI priority, the priority order for a same UCI type is defined as：PUCCH starting at an earlier slot > PUCCH starting at a later slot
* Step 1-2-3: the UE repeats step 1-2-1 and step 1-2-2 until the overlapping PUCCHs with repetitions is resolved.
 |

One controversial issue is whether the reference PUCCH should be a PUCCH with repetitions. The input is summarized below.

Alt 1: The reference PUCCH is a PUCCH with repetitions.

 Proponents: HW, SPRD, OPPO, CATT

Alt 2: The reference PUCCH is a PUCCH with or without repetitions.

Proponents: CATT, Intel, QC, Samsung, ZTE

The proponents of Alt 1 think ‘the first PUCCH’ in clause 9.2.6 is the reference PUCCH, to align with clause 9.2.6 the reference PUCCH should be with repetitions. The proponents of Alt 2 would like to reuse the pseudo-code in clause 9.2.5 to minimize specification impact. However, the concern of Alt 2 is that the set of overlapping PUCCHs may not include a PUCCH with repetitions and UE may resolve overlapping PUCCHs without repetitions first. Alt 2 contradicts with the conclusion copied below.

|  |
| --- |
| Conclusion:For resolving overlapping PUCCHs with and/or without repetitions in a slot in Rel-16, a UE first performs clause 9.2.6 (TS 38.213) to resolve overlapping PUCCHs where at least one PUCCH is with repetitions, and then UE performs clause 9.2.5 (TS 38.213) to resolve overlapping PUCCHs without repetitions.* Note: The above is performed per slot.
 |

This issue was discussed in RAN1#110, Alt 1 was also supported by vivo and MTK. Moderator suggest to go with the majority view.

Another issue is whether up to one or all the PUCCHsoverlapping with the reference PUCCH should be included in the set of overlapping PUCCHs**.** The inputs are summarized below.

Option 1: All the overlapping PUCCH

Proponents: HW, SPRD, OPPO, QC, Intel

Option 2: Up to one overlapping PUCCH

Proponents: Samsung

Considering there is a clear majority view, moderator would suggest to go with Option 1.

#### **P1:**

**For resolving overlapping PUCCHs with repetitions of a same priority in Rel-16, a set of overlapping PUCCHs consist of a reference PUCCH and all the PUCCHs overlapping with the reference PUCCH.**

* **A UE first determines a reference PUCCH and then determines all the PUCCHs overlapping with the reference PUCCH.**
* **The reference PUCCH is a PUCCH overlaps with at least another PUCCH.**
* **FFS: The reference PUCCH is a PUCCH with repetitions.**

|  |  |
| --- | --- |
| Support or can live with | QC, Intel, OPPO, Apple, CATT, ZTE, Samsung (can live with), MTK, Huawei/HiSi |
| Object |  |

|  |  |
| --- | --- |
| Company | View |
| Apple | The last sub-bullet does not have to be an FFS. The reference PUCCH shall be a PUCCH with repetition otherwise we may end up a new procedure even for PUCCHs without repetition (for which spec is already clear in 9.2.5) |
| vivo | Agree with Apple to remove FFS in the last bullet. The reference PUCCH shall be a PUCCH with repetition. |
| Samsung | Although we prefer a pair-wise solution to determine the set of PUCCHs but we can live with the proposal to make progress. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

#### **Q1**

**Can you** **live with the restriction that the reference PUCCH is a PUCCH with repetitions? If not, please address the concern that Alt 2 may contradict previous conclusion.**

|  |  |
| --- | --- |
| Company | View |
| QC | We just want to minimize the spec. Therefore we prefer not restricting the reference PUCCH as a PUCCH with repetition. We actually don’t think Alt2 contracts with previous conclusion. Step 1-2-1/1-2-2/1-2-3 are all sub-steps of step 1-2, which is part of the following framework (conclusion agreed in RAN1 109e). As we can see, step 1-2 is part of step 1 which is for PUCCHs with repetitions. Actually, after step 1-1, the PUCCHs being processed by step 1-2 is either a PUCCH with repetition, or a PUCCH overlap with another PUCCH with repetitions, because a sub-bullet clearly states that “PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved”. In other words, this “However, the concern of Alt 2 is that the set of overlapping PUCCHs may not include a PUCCH with repetitions and UE may resolve overlapping PUCCHs without repetitions first” is not a correct statement. A set of overlapping PUCCHs determined in step 1-2-1 will always has a PUCCH with repetitions. **Conclusion (in RAN1 109e)**For resolving overlapping PUCCHs of a same priority in Rel-16, a UE performs the following steps* Step1, the UE resolves overlapping PUCCHs with repetitions as described in TS 38.213 clause 9.2.6, if any.
	+ Step 1-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.6.
		- o    PUCCHs with repetitions and PUCCHs overlapping with a PUCCH with repetitions are involved.
		- o    PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved.
	+ Step 1-2: the UE resolves overlapping PUCCHs determined in Step 1-1 by performing TS 38.213 clause 9.2.6.
		- o    Only prioritization is performed.
* Step2, the UE resolves overlapping PUCCHs without repetitions as described in TS 38.213 clause 9.2.5, if any.
	+ Step 2-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.5.
		- PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are involved.
		- Resulting PUCCHs without repetitions of resolving overlapping PUCCHs determined in Step 1-2 are involved.
	+ Step 2-2: the UE resolves overlapping PUCCHs determined in Step 2-1 by performing TS 38.213 clause 9.2.5.

Note: The above conclusion on the generic framework with high-level steps has no spec impact. The details of certain steps, e.g. step 1-2, may have spec impact subject to outcome of the ongoing and future discussion on the issues identified in email thread [109-e-NR-CRs-03].  |
| Intel  | We share same view with QC to minimize standard impact. We think no need to restrict reference PUCCH as PUCCH with repetitions, because we think the case that ‘the set of overlapping PUCCHs may not include a PUCCH with repetitions’ is not a valid case to be considered here.  |
| OPPO | We support the reference PUCCH is a PUCCH with repetitions for the following three reasons:1. align with clause 9.2.6 the reference PUCCH is the first PUCCH and should be with repetitions;
2. Alt 2 may contradict previous conclusion, further clarification is as following:

In the following case: first UE selects PUCCH 1 and PUCCH 2 as “a set of overlapping PUCCHs”, then UE drop PUCCH 2. After that, UE will select PUCCH 3 and PUCCH 4 as “a set of overlapping PUCCHs” but PUCCH 3 and PUCCH4 are all without repetitions. 1. We see the spec impact for Alt 1 and Alt 2 is similar.
 |
| Apple | We share similar view as FL/OPPO |
| CATT | In general, we provided solutions to minimize the unnecessary PUCCH dropping. But based on the discussions, it seems that companies do not care the performance much but would like to go with the solution with minimal specification changes.In that case, for the reference PUCCH, we agree with OPPO and Apple that the first PUCCH should be a PUCCH with repetition as defined in current 9.2.6. The case identified by OPPO is also valid in our view. |
| ZTE | We support Alt.2. The concern on Alt.2 is not an issue as Qualcomm and Intel said. Even if that is so, if the set of overlapping PUCCHs does not include a PUCCH with repetitions and UE will skip the set and to find the next available set with PUCCH repetitions.There is another solution to solve the divergence between Alt.1 and Alt.2, but may affect the conclusion of the processing order of 9.2.6 and 9.2.5.For example, in a slot, UE determines the set according to the reference PUCCH, and then there may be PUCCH with repetitions in the set or there may not be PUCCH with repetitions in the set. If there is at least a PUCCH with repetition in the set, then process according to 9.2.6 (step 1), otherwise, process according to 9.2.5 (step 1). It is simpler than 2-step procedure but need additional interpretation of previous conclusion. |
| ZTE2 | To explain the less spec impact from Alt.2, the possible TP is shown below:----------------------------------------- Start of text proposal ------------------------------------------------**9.2.5 UE procedure for reporting multiple UCI types**<Unchanged text omitted>Set  to the set of resources for transmission of corresponding PUCCHs in a single slot ~~without repetitions~~ where- a resource with earlier first symbol is placed before a resource with later first symbol- for two resources with same first symbol, the resource with longer duration is placed before the resource with shorter duration- for two resources with same first symbol and same duration, the placement is arbitrary- the above three steps for the set  are according to a subsequent pseudo-code for a function - a resource for negative SR transmission that does not overlap with a resource for HARQ-ACK or CSI transmission is excluded from set  - if the UE is not provided *simultaneousHARQ-ACK-CSI* and resources for transmission of HARQ-ACK information include PUCCH format 0 or PUCCH format 2, resources that include PUCCH format 2, or PUCCH format 3, or PUCCH format 4 for transmission of CSI reports are excluded from the set  if they overlap with any resource from the resources for transmission of HARQ-ACK information- if the UE is not provided *simultaneousHARQ-ACK-CSI* and at least one of the resources for transmission of HARQ-ACK information includes PUCCH format 1, PUCCH format 3, or PUCCH format 4- resources that include PUCCH format 3 or PUCCH format 4 for transmission of CSI reports are excluded from the set - resources that include PUCCH format 2 for transmission of CSI reports are excluded from the set  if they overlap with any resource from the resources for transmission of HARQ-ACK informationSet  to the cardinality of Set to be the first symbol of resource  in the slotSet  to be the number of symbols of resource  in the slotSet  - index of first resource in set Set  - counter of overlapped resourceswhile if  and resource  overlaps with resource  elseif determine a single resource for multiplexing UCI associated with resources  as described in clauses 9.2.5.0, 9.2.5.1, ~~and~~ 9.2.5.2 and 9.2.6set the index of the single resource to   % start from the beginning after reordering unmerged resources at next step % function that re-orders resources in current set Set  to the cardinality of elseend ifend ifend while}For each PUCCH resource in the set  that satisfies the aforementioned timing conditions, when applicable,- the UE transmits a PUCCH using the PUCCH resource if the PUCCH resource does not overlap in time with a PUSCH transmission after multiplexing UCI following the procedures described in clauses 9.2.5.1, ~~and~~ 9.2.5.2 and 9.2.6.- the UE multiplexes HARQ-ACK information and/or CSI reports in a PUSCH if the PUCCH resource overlaps in time with a PUSCH transmission, as described in clause 9.3, and does not transmit SR. In case the PUCCH resource overlaps in time with multiple PUSCH transmissions, the PUSCH for multiplexing HARQ-ACK information and/or CSI is selected as described in clause 9. If the PUSCH transmission by the UE is not in response to a DCI format detection and the UE multiplexes only CSI reports, the timing conditions are not applicable- the UE does not expect the resource to overlap with a second resource of a PUCCH transmission over multiple slots if the resource is obtained from a group of resources that do not overlap with the second resource. <Unchanged text omitted>**9.2.6 PUCCH repetition procedure**<Unchanged text omitted>A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect the first PUCCH and the second PUCCHs to start at a same slot and include a UCI type with same priority - if the first PUCCH and the second PUCCHs include a UCI type with same priority, the UE transmits the PUCCH starting at an earlier slot and does not transmit the PUCCH starting at a later slot- if the first PUCCH and the second PUCCHs do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with ~~higher~~highest priority and does not transmit the PUCCH that include the UCI type with lower priority <Unchanged text omitted>---------------------------------------- End of text proposal ------------------------------------------------ |
| vivo | We share similar view as FL/OPPO/Apple.  |
| Samsung | Our preference is not to have such restriction but can live with it to make progress. |
| MTK | We can live with the restriction that the reference PUCCH is a PUCCH with repetitions |
| Huawei/HiSi | We support the reference PUCCH is PUCCH with repetition. If there is no such restriction, it is conflict with the agreement that 9.2.6 is performed in prior to 9.2.5, since if the reference PUCCH is w/o repetition, and all its overlapping PUCCHs are also w/o repetitions, then it will jump from 9.2.6 to 9.2.5; when performing a next reference PUCCH with repetition in the same slot, it will jump back to 9.2.6.

|  |
| --- |
| AgreementFor resolving overlapping PUCCHs and/or PUSCHs of a same priority in Rel-16, a UE performs the following steps* Step1, the UE resolves overlapping PUCCHs with repetitions as described in TS 38.213 clause 9.2.6, if any.
* Step2, the UE resolves overlapping PUCCHs without repetitions as described in TS 38.213 clause 9.2.5, if any.
* Step3, the UE resolves overlapping PUSCH(s) and PUCCH(s) with repetitions as described in TS 38.213 clause 9, if any.
* Step4, the UE resolves overlapping PUSCH(s) and PUCCH(s) without repetitions as described in TS 38.213 clause 9, if any.
 |

On the contrary, we think it is with smaller spec impact to restrict the reference PUCCH to be w/ repetitions. Our draft TP is in the following.=====================================================A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and at least a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect any two PUCCHs from the first PUCCH and the second PUCCHs to start at a same slot and include a UCI type with same priority - if the first PUCCH and each of the second PUCCHs include a UCI type with same priority, the UE transmits the PUCCH starting at an earliest slot and does not transmit the PUCCH starting at any later slot- if the first PUCCH and any of the second PUCCHs do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with highest priority followed by starting at an earliest slot and does not transmit the PUCCH that include the UCI type with any lower priority or any later slot- the UE performs the above rules by selecting the first PUCCH with the order of earliest symbol followed by longest duration from the PUCCHs with repetition that overlap with at least one PUCCH, and the at least a second PUCCH includes all PUCCHs overlapping with the first PUCCH===================================================== |
|  |  |
|  |  |
|  |  |

Another remaining issue is the order of reference PUCCH determination. The inputs are summarized below.

Alt 1: Earliest starting symbol followed by longest duration

Proponents: HW OPPO, QC, Samsung, Intel

Alt 2: UCI with the highest priority

Proponents: OPPO, CATT

Alt 3: UE does not expect to be configured or scheduled more than one PUCCH with repetitions in a slot.

Proponents: OPPO

The proponents of Alt 1 aim to minimize specification impact by reusing the rules defined in clause 9.2.5. Alt 2 has additional specification impact compared with Alt 1. Alt 3 is very restrictive for the scenario of multiple traffic types. For such scenario, a SR configuration can be associated with a logic channel and multiple SR configurations can be configured in a same slot. Alt 3 prevents such scheduling flexibility. Moderator suggest to go with the majority view.

#### **P2:**

**For resolving overlapping PUCCHs with repetitions of a same priority in Rel-16, the PUCCH resources are ordered as following for determining the reference PUCCH.**

**- a resource with earlier first symbol is placed before a resource with later first symbol**

**- for two resources with same first symbol, the resource with longer duration is placed before the resource with shorter duration**

**- for two resources with same first symbol and same duration, the placement is arbitrary**

**Note: the above does not imply that the reference PUCCH is with or without repetitions.**

|  |  |
| --- | --- |
| Support or can live with | QC, Intel, OPPO, Apple (see comments), CATT (can live with), ZTE, vivo, Samsung, MTK Huawei/HiSi |
| Object |  |

|  |  |
| --- | --- |
| Company | View |
| Apple | For the (for example) two overlapping PUCCHs both with repetitions, the reference is first determined based on UCI priority. Why the proposal does not consider different UCI priorities? |
| CATT | That is not our preference as we analyzed in our contribution, it would lead to unnecessary PUCCH dropping. But for the sake of progress, we can compromise with majority views. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Prioritization among PUCCHs in the set of overlapping PUCCHs

There are two alternatives for determining the PUCCHs overlapping with the reference PUCCH. The inputs are summarized below.

Alt 1: UE transmit the PUCCH with the highest priority.

Proponents: HW, SPRD, OPPO, QC, Intel, CATT, Samsung

Alt 2: Perform pair-wise prioritization between the first PUCCH (reference) and a second PUCCH until there is no overlapping between the first PUCCH and another PUCCH, where the second PUCCH is selected based on UCI priority followed by starting slot/sub-slot.

Proponents: CATT

#### **P3:**

**For resolving overlapping PUCCHs with repetitions of a same priority in Rel-16, UE transmits the PUCCH with the highest priority when performing prioritization among PUCCHs in a set of overlapping PUCCHs.**

* **The priority order for different UCI types is defined as: HARQ-ACK > SR > CSI with higher priority > CSI with lower priority**
* **For overlapping PUCCHs of the same UCI priority, the priority order for a same UCI type is defined as: PUCCH starting at an earlier slot > PUCCH starting at a later slot**

|  |  |
| --- | --- |
| Support or can live with | QC, Intel, OPPO, ZTE, vivo (can live with), Samsung, MTK, Huawei/HiSi |
| Object | Apple |

|  |  |
| --- | --- |
| Company | View |
| Apple | We tend to go with pair-wise solution which is more compliant with 9.2.6, in our view. Basically, once the set is determined, as long as the reference PUCCH (which has repetitions) is not dropped, it is compared in a pair-wise way with other PUCCHs within the set. If the reference PUCCH is dropped, all the PUCCH resources within the set (except the reference PUCCH) may survive (subject to the existing specification). |
| CATT | We agree with Apple that pair-wise solution is more compliant with 9.2.6. Pair-wise solution is also better from performance perspective thus we prefer pair-wise prioritization. But if majority companies want to go with one-shot approach, we can live with it for the sake of progress. |
| vivo | Although this alt may result in unnecessary dropping, we can live with it for the sake of progress. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

In addition, ZTE raised a case that there are more than one non-overlapping PUCCHs with the highest priority in a set of overlapping PUCCH, in this case, all the non-overlapping PUCCHs with the highest priority should be transmitted. Companies are encouraged to provide the view on this case.

#### **Q2:**

What is your option on the case that there are more than one non-overlapping PUCCHs with the highest priority in a set of overlapping PUCCH?

|  |  |
| --- | --- |
| Company | View |
| QC | No strong view here. But I am not sure we have to solve all the corner case of a corner case, given that this issue that we have been discussed for a few meetings is already a corner case by itself… |
| Intel  | We share exactly same view with QC 😊 |
| CATT | We do not have a strong preference but we think we need a conclusion/agreement for this case. |
| ZTE | For this issue, we should have a conclusion or agreement even if it is a corner case as the behavior is not defined in case it happens. |
| vivo | This issue can be solved by changing P3 as UE transmits the PUCCH(s) with the highest priority when performing prioritization among PUCCHs in a set of overlapping PUCCHs where the PUCCHs with the highest priority are non-overlapped if any. Of course, we do not have a strong view. We are fine to treat it as an corner case and have a conclusion/agreement for it. |
| MTK | Similar view as QC. However, we are fine to adopt ZTE’s proposal if necessary. |
| Huawei/HiSi | UE does not expect. In the legacy spec, it already specifies that UE does not expect the first PUCCH and the second PUCCH does not expect to start at the same slot and include the same priority UCI. We can simply extend the rule to any two PUCCHs in the set of PUCCH of the first PUCCH and multiple second PUCCHs.As in our draft TP (“first PUCCH” in below denotes the reference PUCCH):- the UE does not expect any two PUCCHs from the first PUCCH and the second PUCCHs to start at a same slot and include a UCI type with same priority  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Second round

In the first round discussion, companies view are quite aligned for P1~P3 except Apple raised a concern on P3. Pair-wise operation was discussed in the last meeting, however, companies had concerns on it. As clarified in previous meetings, in current spec, the second PUCCH can consist of multiple PUCCHs, some companies do not agree that pair-wise operation is the current behaviour. Hopefully, Apple could reconsider it and be flexible.

In the 2nd round, the discussion will focus on the FFS of P1.

Regarding the concern on whether Alt 2 contradicts with previous conclusion, moderator would like to clarify a bit more about the two conclusions below.

|  |
| --- |
| **Conclusion #1**For resolving overlapping PUCCHs with and/or without repetitions in a slot in Rel-16, a UE first performs clause 9.2.6 (TS 38.213) to resolve overlapping PUCCHs where at least one PUCCH is with repetitions, and then UE performs clause 9.2.5 (TS 38.213) to resolve overlapping PUCCHs without repetitions.* Note: The above is performed per slot.
 |

|  |
| --- |
| **Conclusion #2**For resolving overlapping PUCCHs of a same priority in Rel-16, a UE performs the following steps* Step1, the UE resolves overlapping PUCCHs with repetitions as described in TS 38.213 clause 9.2.6, if any.
	+ Step 1-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.6.
		- o    PUCCHs with repetitions and PUCCHs overlapping with a PUCCH with repetitions are involved.
		- o    PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved.
	+ Step 1-2: the UE resolves overlapping PUCCHs determined in Step 1-1 by performing TS 38.213 clause 9.2.6.
		- o    Only prioritization is performed.
* Step2, the UE resolves overlapping PUCCHs without repetitions as described in TS 38.213 clause 9.2.5, if any.
	+ Step 2-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.5.
		- PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are involved.
		- Resulting PUCCHs without repetitions of resolving overlapping PUCCHs determined in Step 1-2 are involved.
	+ Step 2-2: the UE resolves overlapping PUCCHs determined in Step 2-1 by performing TS 38.213 clause 9.2.5.

Note: The above conclusion on the generic framework with high-level steps has no spec impact. The details of certain steps, e.g. step 1-2, may have spec impact subject to outcome of the ongoing and future discussion on the issues identified in email thread [109-e-NR-CRs-03]. |

Conclusion #2 further clarifies the details of Conclusion #1. The issue under discussion here belongs to the details of Step 1-2 of Conclusion #2. Please note the main bullet of P1 ‘For resolving overlapping PUCCHs with repetitions of a same priority in Rel-16’ is aligned with Step 1. According to the highlight part of Step 1-2, only prioritization is performed, there is no intention to change this behaviour. UE will not perform multiplexing during the procedure of Step 1. With this understanding, it does not contradict with Conclusion #1. Regarding Oppo’s example in Q1, UE will perform prioritization for PUCCH#3 and PUCCH#4. Although prioritization may result in PUCCH dropping, we should aim for minimizing spec impact instead of best performance in the CR phase. Besides, this is a very corner case, the performance loss should be acceptable. Moderator’s suggestion is not focusing on the extreme corner case. The impact of the extreme corner case should not be taken as essential in the CR phase.

#### **Q3:**

Do you agree that only prioritization is performed during the procedure of Step 1-2 of Conclusion #2? If not, please clarify the reason why the conclusion should be violated.

|  |  |
| --- | --- |
| Company | View |
| vivo | Regarding FL’s following comment, we have different view.Regarding Oppo’s example in Q1, UE will perform prioritization for PUCCH#3 and PUCCH#4. Although prioritization may result in PUCCH dropping, we should aim for minimizing spec impact instead of best performance in the CR phase.Note that in Conclusion #2, in Step 1-1, it says that PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved. So, PUCCH 3 and PUCCH 4 should not be involved based on Conclusion #2.**Conclusion #2**For resolving overlapping PUCCHs of a same priority in Rel-16, a UE performs the following steps* Step1, the UE resolves overlapping PUCCHs with repetitions as described in TS 38.213 clause 9.2.6, if any.
	+ Step 1-1: the UE determines the PUCCHs involved in TS 38.213 clause 9.2.6.
		- o    PUCCHs with repetitions and PUCCHs overlapping with a PUCCH with repetitions are involved.
		- o    PUCCHs without repetitions that do not overlap with a PUCCH with repetitions are not involved.

…Regarding Q3, YES. |
| CATT | Yes, we agree that only prioritization is performed during the procedure of Step 1-2 of Conclusion #2.Regarding OPPO’s example, our understanding is that both PUCCH 3 and PUCCH 4 are involved in Step 1-2 because both PUCCH 3 and PUCCH 4 overlap with a PUCCH with repetition and are included in Step 1-1. But we are not sure whether proponents of Alt 2 consider prioritization or multiplexing for PUCCH 3 and PUCCH 4.  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

#### **Q4:**

If only prioritization is performed during the procedure of Step 1-2 of Conclusion #2, do you still think Alt 2 contradicts with Conclusion #1? If yes, please clarify.

|  |  |
| --- | --- |
| Company | View |
| vivo | Yes. As comment in Q3. PUCCH 3 and PUCCH 4 should not be involved based on Conclusion #2. But Alt 2 would perform preoptimization between PUCCH 3 and PUCCH 4. |
| CATT | No. But as commented above, it is not clear that whether all the proponents of Alt 2 think that prioritization instead of multiplexing is performed between PUCCH 3 and PUCCH 4 in OPPO’s example. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

From moderator’s understanding, the down-selection of Alt 1 and Alt 2 should mainly focus on the spec impact and UE implementation complexity. In previous meeting, the understanding of the spec below was clarified. A first PUCCH consists of only one PUCCH while the second PUCCH(s) consists of one or more PUCCHs. All the second PUCCH(s) overlap with the first PUCCH. Comparing with P1, a set of overlapping PUCCHs correspond to the first PUCCH and the second PUCCH(s), the first PUCCH is aligned with the reference PUCCH and the second PUCCH(s) is aligned with the PUCCH(s) overlapping with the reference PUCCH. With this understanding, ‘the reference PUCCH is a PUCCH with repetitions’ is aligned with clause 9.2.6.

|  |
| --- |
| A UE does not multiplex different UCI types in a PUCCH transmission with repetitions over $N\_{PUCCH}^{repeat}>1$ slots. If a UE would transmit a first PUCCH over more than one slot and at least a second PUCCH over one or more slots, and the transmissions of the first PUCCH and the second PUCCH would overlap in a number of slots then, for each slot of the number of slots and with UCI type priority of HARQ-ACK > SR > CSI with higher priority > CSI with lower priority- the UE does not expect the first PUCCH and any of the second PUCCHs to start at a same slot and include a UCI type with same priority - if the first PUCCH and any of the second PUCCHs include a UCI type with same priority, the UE transmits the PUCCH starting at an earlier slot and does not transmit the PUCCH starting at a later slot- if the first PUCCH and any of the second PUCCHs do not include a UCI type with same priority, the UE transmits the PUCCH that includes the UCI type with higher priority and does not transmit the PUCCH that include the UCI type with lower priority  |

#### **Q5:**

Do you agree that ‘the reference PUCCH is a PUCCH with repetitions’ is aligned with clause 9.2.6? If not, please clarify the reason.

|  |  |
| --- | --- |
| Company | View |
| vivo | YES |
| CATT | Yes, we agree with FL. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

The proponents of Alt 2 aim for reusing the pseudo-code of 9.2.5 for determine a set of overlapping PUCCHs to minimize spec impact. The repetition is not considered when determining the reference PUCCH. On the contrary, for Alt 1, the pseudo-code of 9.2.5 needs to be changed at least with adding the repetition restriction for selecting a reference PUCCH. From moderator’s understanding, the pseudo-code of 9.2.5 may not be a must. The difference between prioritization and multiplexing is that the result PUCCH of multiplexing may overlap with other PUCCHs not in the selected set but for prioritization such situation does not exists. In the pseudo-code of 9.2.5 the result PUCCH is put back to the set Q and then redo the ordering. These steps can be avoided for prioritization operation because the result PUCCH would not overlap with other PUCCHs in Step 1-2.

#### **Q6:**

What is your preference on reusing the pseudo-code of clause 9.2.5 for resolving overlapping PUCCHs with repetitions?

|  |  |
| --- | --- |
| Reuse |  |
| NOT reuse |  |

|  |  |
| --- | --- |
| Company | View |
| CATT | For collision handling of PUCCH with repetition, the existing rules should be followed (i.e. the first PUCCH is a PUCCH with repetition and the second PUCCH(s) are the PUCCHs with or without repetition overlapping with the first PUCCH). What is missing is to define a processing order for multiple first PUCCHs within a slot. In this regard, we follow the same rule as in Clause 9.2.5.We should not break the existing rules just for reusing the pseudo-code of clause 9.2.5.  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

#### **Q7:**

What is your preference on the following two alternatives?

Alt 1: The reference PUCCH is a PUCCH with repetitions.

Alt 2: The reference PUCCH is a PUCCH with or without repetitions.

|  |  |  |
| --- | --- | --- |
| Alt 1 | Support or can live with | Vivo, CATT |
| Object |  |
| Alt 2 | Support or can live with |  |
| Object | CATT |

|  |  |
| --- | --- |
| Company | View |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Summary and conclusions

# Reference

1. [R1-2205342](file:///F%3A%5C%5C3GPP%5C%5CRAN1%5C%5CTSGR1_109-e%5C%5CDocs%5C%5CR1-2205342.zip), Summary of [109-e-NR-CRs-03] Collision of more than two overlapped PUCCHs with repetition, Moderator (Samsung), RAN1#109-e, May, 2022.
2. RAN1 Chairman’s Notes, 3GPP TSG RAN WG1 Meeting #109-e, May, 2022.
3. R1-2207913, Summary of Collision handling for overlapping PUCCHs with repetitions, Moderator (Samsung), RAN1#110, Aug., 2022.
4. RAN1 Chairman’s Notes, 3GPP TSG RAN WG1 Meeting #110, Aug., 2022.
5. [R1-2208446](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2208446.zip), Discussion on the collision of overlapped PUCCHs with repetition, Huawei, HiSilicon
6. R1-2208447, Correction on the collision of overlapped PUCCHs with repetition, Huawei, HiSilicon
7. [R1-2208533](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2208533.zip), Collision of overlapped PUCCHs with repetition, Spreadtrum Communications
8. [R1-2208867](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2208867.zip), Discussion on collision handling for overlapping PUCCHs with repetitions, OPPO
9. [R1-2208915](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2208915.zip), Collision handling of more than two overlapping PUCCHs with repetition, CATT
10. [R1-2209030](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2209030.zip), PUCCH collision handling for more than two overlapped PUCCHs with repetition, Intel Corporation
11. [R1-2209463](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2209463.zip), Discussion on more than two overlapping PUCCHs with repetitions, ZTE
12. [R1-2209688](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2209688.zip), Discussion on more than two overlapping PUCCHs with repetitions, Samsung
13. [R1-2209932](file:///F%3A%5C3GPP%5CRAN1%5CTSGR1_110b-e%5CDocs%5CR1-2209932.zip), Issue on PUCCH overlapping with PUCCH with repeatitions, Qualcomm Incorporated