**3GPP TSG RAN WG1 #110bis-e R1-22xxxxx**

**Electronic Meeting, October 10th – 19th, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **[DRAFT] CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.213** | **CR** | **xxxx** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| Title: | Correction on conditions for UE to be UE-B for Condition 2-A-2 of Scheme 2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Moderator (LG Electronics) | | | | | | | | | |
| ***Source to TSG:*** | RAN WG1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_SL\_enh-Core | | | | |  | ***Date:*** | | | 2022-10-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | For Condition 2-A-2 of inter-UE coordination scheme 2, further clarification on conditions for UE to be UE-B is needed, since it is infeasible to transmit the conflict indication if the PSFCH occasion for resource conflict information of the second UE is not valid. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the related description on conditions for UE to be UE-B for Condition 2-A-2 in TS 38.213. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Potential transmission of the conflict indication in an incorrect PSFCH occasion. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 16.3.0 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**<Unchanged parts omitted>**

### 16.3.0 UE procedure for transmitting PSFCH with control information

**<Unchanged parts omitted>**

A first UE determines a second UE for providing the conflict information to in a PSFCH as follows

- if the first UE is an intended receiver of the second UE for a reserved resource of a PSSCH transmission in a slot,

- does not expect to perform reception on the sidelink due to half-duplex operation in the slot,

- the PSFCH occasion for resource conflict information of the second UE is valid, and

- determines to transmit to the second UE the PSFCH with the conflict information.

**<Unchanged parts omitted>**