**3GPP TSG-RAN WG1 Meeting #110bis-eR1-221xxxx**

**e-Meeting, October 10– 19, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** | **xxxx** | **rev** |  | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on dci-enabler for Type1 HARQ-ACK CB for multicast |
|  |  |
| ***Source to WG:*** |  Moderator (Huawei), Qualcomm, Lenovo |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_MBS-Core |  | ***Date:*** | 2022-10-19 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | When UE is configured with 'dci-enabler' and Type-1 HARQ-ACK codebook, UE behaviour is missing.  |
|  |  |
| ***Summary of change:*** | If a UE is provided *pdsch-HARQ-ACK-Codebook = semi-static* for multicast HARQ-ACK information, the UE does not expect to be provided *harq-FeedbackEnablerMulticast* with value set to 'dci-enabler' for a G-RNTI or a G-CS-RNTI. |
|  |  |
| ***Consequences if not approved:*** | UE behavior is unclear if the UE is configured with Type-1 HARQ-ACK codebook and 'dci-enabler'.  |
|  |  |
| ***Clauses affected:*** | 18 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

# 18 Multicast Broadcast Services

< Unchanged parts are omitted >

A UE can be configured per G-RNTI or per G-CS-RNTI, by *harq-FeedbackEnablerMulticast* with value set to 'enabled', to provide HARQ-ACK information for PDSCH receptions. When the UE is not provided *harq-FeedbackEnablerMulticast* for a G-RNTI or G-CS-RNTI, the UE does not provide HARQ-ACK information for respective PDSCH receptions. If a UE is provided *harq-FeedbackEnablerMulticast* with value set to 'dci-enabler' for a G-RNTI or a G-CS-RNTI, the UE determines whether or not to provide the HARQ-ACK information for PDSCH receptions based on an indication by the multicast DCI format associated with the G-RNTI or the G-CS-RNTI [4, TS 38.212]. If a UE is provided *pdsch-HARQ-ACK-Codebook = semi-static* for multicast HARQ-ACK information, the UE does not expect to be provided *harq-FeedbackEnablerMulticast* with value set to 'dci-enabler' for a G-RNTI or a G-CS-RNTI.

< Unchanged parts are omitted >