**3GPP TSG RAN WG1 #110bis-e R1-22xxxx**

**e-Meeting, October 10th – 19th, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **[DRAFT] CHANGE REQUEST** |
|  |
|  | **38.214** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on SPS and dynamic scheduling PDSCH(s) collision for MBS to Ts 38.214 |
|  |  |
| ***Source to WG:*** | Moderator (CMCC) |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_MBS-Core |  | ***Date:*** | 2022-10-12 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The UE behaviour of collision handling of unicast/multicast/broadcast DG PDSCH(s) and unicast/multicast SPS PDSCH(s) is unclear in TS 38.214. |
|  |  |
| ***Summary of change:*** | Add G-RNTI, G-CS-RNTI and MCCH-RNTI in the UE behaviour of collision handling of DG PDSCH(s) and SPS PDSCH(s) similar to unicast SPS and DG PDSCH(s) collision handling. |
|  |  |
| ***Consequences if not approved:*** | Mis-alignment between gNB and UE about the collision handling of unicast/multicast/broadcast DG PDSCH(s) and unicast/multicast SPS PDSCH(s). |
|  |  |
| ***Clauses affected:*** | 5.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 5.1 UE procedure for receiving the physical downlink shared channel

========================= Unchanged parts =========================

The UE is not expected to decode a PDSCH in a serving cell scheduled by a PDCCH with C-RNTI, CS-RNTI, MCS-C-RNTI, G-RNTI, G-CS-RNTI or MCCH-RNTI and one or multiple PDSCH(s) required to be received according to this Clause in the same serving cell without a corresponding PDCCH transmission if the PDSCHs partially or fully overlap in time except if the PDCCH scheduling the PDSCH ends at least 14 symbols before the earliest starting symbol of the PDSCH(s) without the corresponding PDCCH transmission, where *m* and the symbol duration are based on the smallest numerology between the scheduling PDCCH and the PDSCH, in which case the UE shall decode the PDSCH scheduled by the PDCCH. When the PDCCH reception incudes two PDCCH candidates from two respectvie search space sets, as described in clause 10 of [6, TS 38.213], for the purpose of determining the PDCCH with C-RNTI, CS-RNTI, MCS-C-RNTI, G-RNTI, G-CS-RNTI or MCCH-RNTI scheduling the PDSCH ends at least 14 symbols before the earliest starting symbol of the PDSCH(s) without the corresponding PDCCH transmission, the PDCCH candidate that ends later in time is used.

========================= Unchanged parts =========================