**RAN1#110bis-e: Email Endorsement 1**

|  |
| --- |
| **Proposal 1.I**: For the Rel-18 Type-II codebook for CJT mTRP, the switching between mode-1 and mode-2 is gNB-initiated via RRC signalling  **FL Note**: Could CATT please compromise and accept? 🡪 resolved   * **Support/fine (proposal 1.I)**: Xiaomi, Samsung (RRC only), MediaTek, Qualcomm, Nokia/NSB (RRC only), Intel (RRC only), AT&T, Ericsson, vivo, OPPO, ZTE (RRC only), DOCOMO (RRC only), CMCC (RRC only), Huawei/HiSi, Google, Fraunhofer IIS/HHI, NEC, Spreadtrum, Sharp, CATT (ok) * **Not support**: |
| **Proposal 2.B**: For the Rel-18 Type-II codebook refinement for high/medium velocities, support RI={1,2,3,4}.  **FL Note**: Could Lenovo please compromise and accept? 🡪 resolved   * **Support/fine:** Xiaomi, Fraunhofer IIS/HHI, Apple, Samsung, Qualcomm, Nokia/NSB, IDC, vivo, OPPO, Google, ZTE, Ericsson, Huawei/HiSi, CMCC, MediaTek, Spreadtrum, Sharp, Intel (can discuss 1,2, first), Lenovo (ok) * **Not support:** |
| **Proposal 2.D**: For the Rel-18 Type-II codebook refinement for high/medium velocities, support the following codebook structure where N4 is gNB-configured via higher-layer signaling:   * For N4=1, Doppler-domain basis is the identity (no Doppler-domain compression) reusing the legacy *, ,* and *, e.g.* * For N4>1, Doppler-domain orthogonal DFT basis commonly selected for all SD/FD bases reusing the legacyand *,* e.g.   + Only Q (denoting the number of selected DD basis vectors) >1 is allowed   + TBD (by RAN1#110bis): whether rotation is used or not   + FFS: identical or different rotation factors for different SD components   + FFS: Whether *Q* is RRC-configured or reported by the UE   Note: Detailed designs for SD/FD bases including the associated UCI parameters follow the legacy specification  FFS: Whether one CSI reporting instance includes multiple and a single and report.  **FL Note**: Could Nokia, Ericsson, and vivo please compromise and accept the above proposal as is (super-majority which is already a compromise)? 🡪 Ericsson and vivo can accept. Lenovo added to concern. Still waiting for Nokia if they still have concern.   * **Support/fine (N4=2 DFT):** Samsung, ZTE, Qualcomm, Apple, Google, OPPO, Huawei/HiSi, Intel, Spreadtrum, CATT, DOCOMO, NEC, Fraunhofer IIS/HHI, Sharp, IDC, Sony, MediaTek, CEWiT, LG, ZTE, CMCC, Ericsson (ok), vivo (ok) * **Concern (want N4=2 identity):** Lenovo, [Nokia/NSB?] |
| **Proposal 2.E**: On the CSI reporting and measurement for the Rel-18 Type-II codebook refinement for high/medium velocities, when UE-side prediction is assumed, support UE “predicting” channel/CSI after slot *l* where the location of slot *l* is configured (from multiple candidate values) by gNB via higher-layer signalling   * Candidates of slot *l* location include the legacy CSI reference resource location (*n* – *nCSI,ref* ) and slot (*n*+*δ*) where *δ* ≥ 0 * FFS: Possible value(s) of *δ* and possible value(s) of WCSI   Note: Per legacy behavior, the legacy CSI reference resource, i.e., (*n* – *nCSI,ref* ), is reused for locating the last CSI-RS occasion used for a CSI report  For a UE that supports UE-side prediction, the support of *l* = (*n* – *nCSI,ref* ) is UE optional.  **FL Note**: Can Apple please provide some tangible proposal to resolve your concern? Please keep in mind that this proposal keeps the legacy reference resource definition. 🡪 resolved by adding red underlined text (no company raised concern)   * **Support/fine:** Samsung, vivo, Qualcomm (questionable regarding CQI prediction), DOCOMO, Lenovo, IDC, ZTE, Spreadtrum, vivo, LG (ok), CATT, Intel, NEC, Xiaomi, CMCC, MediaTek, Ericsson, [Nokia/NSB], OPPO, Huawei, HiSi, Fraunhofer IIS/HHI, Google (ok), Sharp, Apple (ok) * **Not support:** |
| **Proposal 2.I:** For the Type-II codebook refinement for high/medium velocities, down-select from the following alternatives:   * Alt1. *Q* different 2-dimensional bitmaps are introduced for indicating the location of the NZCs, where the qth (q=1,…., *Q*) 2-dimensional bitmap corresponds to qth selected DD basis vector   + The number of selected DD basis vectors is denoted as *Q*   + This implies that for each layer, the location of NZCs in SD-FD can be different for different selected DD basis vectors. * Alt2. A DD-basis-common per-layer 2-dimensional bitmap for indicating the location of NZCs used in Rel-16/17 Type-II is used   + This implies that for each layer, the location of NZCs in SD-FD is common across all the Q selected DD basis vectors   FFS: Further overhead reduction on bitmap(s)  FFS: Whether the number of NZCs is upper bounded across all DD basis vectors or per DD basis vector  No issue raised   * **Support/fine:** Qualcomm, Samsung (Alt2), Intel (Alt1), IDC (Alt2), vivo, OPPO, ZTE(Alt1)**,** Xiaomi(Alt1), DOCOMO, CATT, Ericsson (Alt1), CMCC (Alt1), Huawei/HiSi, Sharp * **Not support:** |