**3GPP TSG RAN WG1 #110bis-e R1-2210566**

**e-Meeting, October 10th – 19th, 2022**

**Agenda item:** 9.1.2

**Source:** Moderator (Samsung)

**Title:** Moderator Summary#4 on Rel-18 CSI enhancements: ROUND 3

**Document for:** Discussion and Decision

## Introduction

The scope given in the Rel-18 NR Evolved MIMO WID pertaining to CSI enhancement is as follows:

|  |
| --- |
| 1. Study, and if justified, specify CSI reporting enhancement for high/medium UE velocities by exploiting time-domain correlation/Doppler-domain information to assist DL precoding, targeting FR1, as follows:
	* Rel-16/17 Type-II codebook refinement, without modification to the spatial and frequency domain basis
	* UE reporting of time-domain channel properties measured via CSI-RS for tracking
2. Study, and if justified, specify enhancements of CSI acquisition for Coherent-JT targeting FR1 and up to 4 TRPs, assuming ideal backhaul and synchronization as well as the same number of antenna ports across TRPs, as follows:
	1. Rel-16/17 Type-II codebook refinement for CJT mTRP targeting FDD and its associated CSI reporting, taking into account throughput-overhead trade-off
 |

## Summary of companies’ views

### Issue 1: Type-II codebook refinement for CJT

Table 1A Summary: issue 1

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 1.4 | [110bis-e] **Agreement**On the Type-II codebook refinement for CJT mTRP, following legacy (Rel-16 regular eType-II and Rel-17 PS FeType-II), for a given CSI-RS resource:* SD basis selection is layer-common and polarization-common, with *N*1, *N*2, *O*1, *O*2 defined per Rel-16 specification for refinement based on Rel-16 regular eType-II, and per Rel-17 specification for refinement based on Rel-17 PS FeType-II
* FD basis selection is
	+ For refinement based on Rel-16 regular eType-II: per-layer with *M*v, *p*v, *N*3, and *R* defined per Rel-16 specification
	+ For refinement based on Rel-17 PS FeType-II: layer-common with *M*, *N*3, and *R* defined per Rel-17 specification
	+ FFS: Details on FD basis selection window

Note: The supported value(s) for each of the defined parameters are to be discussed separately (e.g. possibilities of adding new or removing existing value(s) in addition to those supported by legacy specification).**Question**: Please share your views on supported value(s) for each of the above parameters, e.g. whether the legacy supported value(s) can be fully reused, or what refinement (removing and/or adding new values) is needed* This is irrespective of the outcome of supported parameter combinations. For now, each parameter should be considered separately from other
 | **{Added later once a proposal is added}** |
| 1.6 | [110bis-e] **Agreement**On the Type-II codebook refinement for CJT mTRP, following legacy (Rel-16 regular eType-II and Rel-17 PS FeType-II), regarding the location of non-zero coefficients (NZCs) indicated by bitmap (following legacy mechanism), for each layer, support separate bitmap per each CSI-RS resource * Total size = $\sum\_{n=1}^{N}B\_{n}$ where $B\_{n}$ is the bitmap size for CSI-RS resource *n*
	+ TBD: Whether $B\_{n}=2L\_{n}M\_{v,n}$ ($M\_{v,n}=M\_{v}$ for mode 2) analogous to legacy, or further reduction of bitmap size is supported.
	+ …

**Question**: Other than the legacy-based scheme (where $B\_{n}=2L\_{n}M\_{v,n}$), what other scheme(s) do you intend to propose for down-selection consideration? | **{Added later once a proposal is added}** |
| 1.9 | **Proposal 1.I.2**: For the Rel-18 Type-II codebook for CJT mTRP, for mode-1, the number of FD basis vectors (Mv related to pv for Rel-16, M for Rel-17) is common across all N CSI-RS resources**FL Note**: While FD basis selection can be TRP-specific for mode-1, a number of companies perceive the number of selected FD basis vectors can be common across all the N TRPs. | **Support/fine:** Huawei/HiSi, Qualcomm, Nokia/NSB, Intel, AT&T, Ericsson, Samsung,**Not support:** [ZTE], [DOCOMO] |

Table 2 Additional inputs: issue 1

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **PLEASE READ THE FL NOTES** 1. **Check and, if needed, update your view in Table 1A especially on the moderator proposals.**
2. **Share additional inputs here, if needed**

**More moderator proposals may be added in the next revision** |
| Apple | **Issue 1.4**Legacy value can be start point, except we prefer to have R=1 only **Issue 1.9**We are fine with the same number of selected FD basis for each TRP/TRP group |
| vivo | **Issue 1.4**We support refinement of the legacy parameter values to cover the lower payload range. On the values of the codebook parameters, the minimum value of K\_0 is ⌈0.25M\_1 ⌉, where L=2, and β=0.25. However, for CJT PMI, the number of rows in W\_2 is greater, e.g.,2LT, where T denotes the number of TRPs. Therefore, the value of K\_0 is ⌈2M\_1 ⌉ which has large gap compared to the value of STRP, when T=4, L=2, and β=0.25. Therefore, we think the value of Beta needs to be further reduced to cover the lower payload range, e.g. 0.125, 0.0625. **Issue 1.6**We support the following alternative for further evaluation/down-selection. One example can be for all the (Ltot) SD basis and all the FD basis across N CSI-RS resources, the bitmap length is 2Ltot for FD basis vector 0 where SCI locates, and bitmap length is 2Ltot- n \* d for the rest, where n denotes the scaling value and d denotes the modulo difference (e.g., mod Mv/2) between the index of each selected FD basis vector and FD basis vector 0.* Alt x: Non-rectangular bitmap, i.e., NZC bitmap allowing different lengths for different basis vectors.
	+ TBD: How to determine the lengths for different basis vectors

**Proposal 1.I.2**Support |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 2: Type-II codebook refinement for high/medium UE velocities (with time/Doppler-domain compression)

Table 3A Summary: issue 2

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 2.1 | [109-e] **Agreement**The work scope of Type-II codebook refinement for high/medium velocities includes refinement of the following codebooks, based on a common design framework:* Rel-16 eType-II regular codebook
* Rel-17 FeType-II port selection (PS) codebook

FFS: Whether to prioritize/down-select from the two**Proposal 2.A**: The Rel-18 Type-II codebook refinement for high/medium velocities comprises refinement of the following codebooks:* Refinement of the Rel-16 eType-II regular codebook
* Refinement of the Rel-17 FeType-II port selection (PS) codebook, based on the same design details as the Refinement of the Rel-16 eType-II regular codebook, except for the supported set of parameter combinations
	+ Time-/Doppler-domain reciprocity is not assumed

**FL Note**: This proposal has been discussed in RAN1#110  | **Support (equal priority for) both Rel-16 eType-II and Rel-17 FeType-II:** Huawei/HiSi, ZTE (Rel-16 first), Fraunhofer IIS/HHI* **Concern:** vivo, Lenovo, LG, Apple, DOCOMO, Spreadtrum

**Down-select to only Rel-16 eType-II:** Apple, DOCOMO, MediaTek, NEC, Xiaomi, Samsung, Lenovo, Intel (if Rel-17, no DD reciprocity), Xiaomi. Qualcomm, Apple, DOCOMO, Ericsson, Nokia/NSB, LG, Spreadtrum, CMCC, vivo, OPPO, Google, Sharp **Proposal 2.A:*** **Support/fine:** IDC, ZTE, Huawei/HiSi, Fraunhofer IIS/HHI
* **Concern (Rel-16 only):** vivo, LG, Apple, DOCOMO, Spreadtrum, Qualcomm, Lenovo
 |
| 2.4 | [109-e] **Agreement**For the Rel-18 Type-II codebook refinement for high/medium velocities, support the following codebook structure where N4 is gNB-configured via higher-layer signaling:* For N4=1, Doppler-domain basis is the identity (no Doppler-domain compression) reusing the legacy$W\_{1}$*,* $\tilde{W}\_{2}$*,* and$W\_{f}$*, e.g.* $W\_{1}\tilde{W}\_{2}(W\_{f})^{H}$
* For N4>1, Doppler-domain orthogonal DFT basis commonly selected for all SD/FD bases reusing the legacy$W\_{1}$and$W\_{f}$*,* e.g.$W\_{1}\tilde{W}\_{2}\left(W\_{f}⨂W\_{d}\right)^{H}$
	+ Only Q (denoting the number of selected DD basis vectors) >1 is allowed
	+ TBD (by RAN1#110bis): whether rotation is used or not
	+ FFS: identical or different rotation factors for different SD components
	+ FFS: Whether *Q* is RRC-configured or reported by the UE

Note: Detailed designs for SD/FD bases including the associated UCI parameters follow the legacy specificationFFS: Whether one CSI reporting instance includes multiple $W\_{2}$ and a single $W\_{1}$ and $W\_{f}$ report.**Proposal 2.D.3**: For the Rel-18 Type-II codebook refinement for high/medium velocities, when N4>1, down-select from the following alternatives (by RAN1#111) for the orthogonal DFT DD basis:* Alt1. No rotation factor
* Alt2. A common rotation factor is selected for all SD basis vector
	+ FFS: Supported values of rotation factor
* Alt3. A rotation factor is select for each SD basis vector
	+ FSS: Supported values of rotation factor

**FL Note**: Please share your preference Alt1 vs Alt2 | **Proposal 2.D.3:*** **Support/fine:**
* **Not support:**
 |
| 2.4 | [110bis-e] **Agreement**For the Type-II codebook refinement for high/medium velocities, the selection of DD basis vectors is layer-specific* The number of selected DD basis vector (denoted as *Q*) is layer-common

**Question**: Please share your views on the possible value(s) of *δ* and possible value(s) of *Q* | **{Added later once a proposal is added}** |
| 2.5 | [110bis-e] **Agreement**On the CSI reporting and measurement for the Rel-18 Type-II codebook refinement for high/medium velocities, when UE-side prediction is assumed, support UE “predicting” channel/CSI after slot *l* where the location of slot *l* is configured (from multiple candidate values) by gNB via higher-layer signalling* Candidates of slot *l* location include the legacy CSI reference resource location (*n* – *nCSI,ref* ) and slot (*n*+*δ*) where *δ* ≥ 0
* FFS: Possible value(s) of *δ* and possible value(s) of WCSI

Note: Per legacy behavior, the legacy CSI reference resource, i.e., (*n* – *nCSI,ref* ), is reused for locating the last CSI-RS occasion used for a CSI reportFor a UE that supports UE-side prediction, the support of *l* = (*n* – *nCSI,ref* ) is UE optional.**Question**: Please share your views on the possible value(s) of *δ* and possible value(s) of WCSI | **{Added later once a proposal is added}** |

Table 4 Additional inputs: issue 2

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **PLEASE READ THE FL NOTES** 1. **Check and, if needed, update your view in Table 3A especially on the moderator proposals.**
2. **Share additional inputs here, if needed**

**More moderator proposals may be added in the next revision** |
| Apple | **Issue 2.1**We prefer to prioritize Rel-16 eType-II over Rel-17 FeType-II PS **Issue 2.4**We prefer Alt1, no rotation factor**Issue 2.5**It depends on the channel coherent time. Assume it is around 30ms, corresponding to roughly 30Hz coherent BW. Consider 30kHz SCS of 0.5ms slot.δ can be up to 64?We are open to more discussion as well |
| vivo | **Issue 2.1**We don’t support proposal 2.A. We support to enhance Rel-16 eType II only.**Proposal 2.D.3**Support. Further evaluation is needed. We prefer Alt 1 at the current stage.**Issue 2.4**We suggest to define Q=ceil(N4/2) for N4>2.For N4=2, the only case we can have now is Q=2.**Issue 2.5**For delta, we support {0, 2, 4} as the candidate values for configuration.For W\_CSI, we think one value is sufficient. Either W\_CSI =1 or N4 is fine. We slightly prefer W\_CSI =1 for lower UE complexity.  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 3: TRS-based reporting of time-domain channel properties (TDCP)

{No issue to be discussed in this round}

Table 5A Summary: issue 3

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
|  |  |
|  |  |  |

Table 6 Additional inputs: issue 3

|  |  |
| --- | --- |
| **Company** | **Input** |
|  |  |
|  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2209715 | Summary of OFFLINE discussion on Rel-18 MIMO CSI | Moderator (Samsung) |
| 2 | R1-2208441 | CSI enhancement for coherent JT and mobility | Huawei, HiSilicon |
| 3 | R1-2208495 | Enhanced CSI for CJT and High Doppler Operations | InterDigital, Inc. |
| 4 | R1-2208504 | CSI enhancement for high/medium UE velocities and CJT | ZTE |
| 5 | R1-2208541 | Discussion on CSI enhancement for high/medium UE velocities and coherent JT | Spreadtrum Communications |
| 6 | R1-2208628 | Discussion on CSI enhancement for high-medium UE velocities and coherent JT | vivo |
| 7 | R1-2208742 | Discussion of CSI enhancement for high speed UE and coherent JT | Lenovo |
| 8 | R1-2208794 | CSI enhancement for high/medium UE velocities and coherent JT | OPPO |
| 9 | R1-2208872 | On CSI Enhancement | Google |
| 10 | R1-2208893 | Potential CSI enhancement for high/medium UE velocities and coherent JT | LG Electronics |
| 11 | R1-2208947 | Discussion on CSI enhancements | CATT |
| 12 | R1-2209041 | On CSI enhancements | Intel Corporation |
| 13 | R1-2209090 | Further considerations on CSI enhancement for high/medium UE velocities and CJT | Sony |
| 14 | R1-2209140 | Discussion on CSI enhancement | NEC |
| 15 | R1-2209247 | Discussion on CSI enhancement | Mavenir |
| 16 | R1-2209258 | Discussion on CSI enhancement for high/medium UE velocities and CJT | xiaomi |
| 17 | R1-2209322 | Discussion on CSI enhancement for high/medium UE velocities and CJT | CMCC |
| 18 | R1-2209381 | CSI enhancement | Sharp |
| 19 | R1-2209494 | CSI enhancement | MediaTek Inc. |
| 20 | R1-2209545 | CSI enhancements for medium UE velocities and coherent JT | Fraunhofer IIS, Fraunhofer HHI |
| 21 | R1-2209570 | Views on Rel-18 MIMO CSI enhancement | Apple |
| 22 | R1-22010241 | Views on CSI enhancements | Samsung |
| 23 | R1-2209793 | Views on CSI Enhancements for CJT | AT&T |
| 24 | R1-2209852 | On CSI enhancements for Rel-18 NR MIMO evolution | Ericsson |
| 25 | R1-2209890 | Discussion on CSI enhancement | NTT DOCOMO, INC. |
| 26 | R1-2209969 | CSI enhancements for high/medium UE velocities and Coherent-JT | Qualcomm Incorporated |
| 27 | R1-2210063 | CSI enhancement for high/medium UE velocities and CJT | Nokia, Nokia Shanghai Bell |
| 28 | R1-2210105 | Discussion on CSI Enhancements for high/medium UE velocities and coherent JT | CEWiT |
|  |  |  |  |