3GPP TSG-RAN WG1 Meeting #110bis-e R1- 2210411

E-meeting, October 10th-19th, 2022

Agenda Item: 9.10.2

Source: Moderator (Ericsson)

Title: Moderator Summary#2 – Study on XR Specific Capacity Improvements

Document for: Discussion, Decision

# 1 Introduction

This document provides a summary of the contributions submitted to RAN1#110bis-e under Agenda item 9.10.2 regarding the study of candidate enhancement techniques for XR capacity improvements, together with an overview and high level key questions to facilitate the discussions under the following email discussion assigned by Chair:

[110bis-e-R18-XR-02] Email discussion on XR capacity enhancement by October 19 – Sorour (Ericsson)

* Check points: October 14, October 19

Moderator presents the views on the candidate capacity enhancements techniques, based on the “common principle for assessment” that was agreed during the last meeting.

|  |
| --- |
| **Agreement:*** For each candidate capacity enhancement technique for XR traffic, companies are encouraged to consider the following common principle for assessment of the candidate capacity enhancement technique:
	+ Identify the XR-specific issue(s) that the enhancement technique is addressing
	+ Identify the necessity of the enhancement technique to address the issues
	+ Identify whether/how the enhancements provide benefit/performance capacity gain.
		- Consider at least feasibility, complexity, and system level performance evaluations in comparing the enhancement techniques. Power saving gains for a given enhancement technique can optionally be evaluated and considered in addition to these other aspects.
* The baseline scheduling scheme when comparing the proposed capacity enhancements techniques is:
	+ Dynamic scheduling and/or
	+ Semi-persistent scheduling / Configured grant scheduling
		- Note: Companies are encouraged to additionally use DG scheduling as the baseline scheduling scheme when showing the capacity performance gain

**Agreement:*** To support a candidate capacity enhancement technique for XR traffic, capacity performance gain by the technique as compared to baseline should be shown.
	+ Capacity performance gain by the candidate technique as compared to baseline is a necessary condition to consider supporting the candidate technique.

**Agreement:**Rel-17 evaluation methodology for XR capacity enhancement captured in TR 38.838 is used as the baseline evaluation methodology for XR capacity enhancement of Rel-18 SI on XR enhancements.**For future meetings:**Companies are **requested to follow** the following agreement and conclusion from RAN1#109-e. Check final FL summary for details.**Agreement:*** Rel-17 evaluation methodology for XR capacity enhancement captured in TR 38.838 is used as the baseline evaluation methodology for XR capacity enhancement of Rel-18 SI on XR enhancements.

**Conclusion:**Companies are encouraged to use the capacity Excel sheet attached with TR 38.838 in [RP-213652](https://www.3gpp.org/ftp/TSG_RAN/TSG_RAN/TSGR_94e/Docs/RP-213652.zip)  for recording the simulation results that are provided in their contributions |

In the following sections, high level summary of companies’ preferences with respect to different enhancement areas are provided. The aim of the discussion is to assess the candidate enhancement techniques and provide valuable inputs for the technical report.

When feasible, few key questions are raised according to the agreed “assessment principle” that is summarized below.

**Summary of assessment principle:**

* **Q1: What are XR-specific issue(s) addressed by the enhancements?**
* **Q2: Whether the enhancement is necessary to address the issues(s)?**
* **Q3: Whether/how the enhancements benefit/performance capacity gain are provided?**
* **Note that capacity performance gain is necessary condition for supporting the enhancements**

This document is the updated version of R1-221040.

# 2 SPS and CG enhancements

The followings are agreed/concluded previously:

|  |
| --- |
| **Agreement (RAN1#109-e)**To study whether/how to support a candidate capacity enhancement technique for XR traffic based SPS/CG transmissions, companies are encouraged to consider the following studies:* + - Study enhancements related to multiple PDSCHs SPStransmission occasions in a period
		- Study enhancements related to multiple PUSCHs CG transmission occasions in a period
		- Study enhancements related to dynamic adaptation of SPS/CG parameters/configurations
		- Study enhancements related to non-integer periodicity for SPS/CG transmissions.
		- Note: Other studies are not precluded, as well as the combination of the above studies.
* Follow the *common principle for assessment of the candidate capacity enhancement technique*

**Conclusion (RAN1#110)**There is no consensus in RAN1 on the benefits of enhancing SPS for the purpose of XR capacity enhancement |

The views regarding SPS/CG enhancements for serving XR traffic are summarized and discussed in the following sections.

## 2.1 Capacity performance evaluations for CG enhancements

The Table A in section 2.1 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Companies with simulation results on CG enhancements (5):**

* **Ericsson, Huawei/HiSilicon, vivo, CATT, ZTE/Sanechips**
* **Supportive of CG enahncements:**
	+ **Yes (4): Huawei/HiSilicon, vivo, CATT, ZTE/Sanechips**
	+ **No (1): Ericsson**

**High-level observations:**

* **Only 5 companies have provided simulation results among 24 companies with views on eCG.**
* **The issue for dynamic scheduling is SR delay and/or BSR delay, specialy for low PDB (10-15ms). Hence CG enhancements is discussed.**
* **Key observations:**
* **Ericsson:**
	+ Pre-scheduling DG provides higher capacity than DG, close to Genie. No need for eCG.
		- The assumptions for pre-scheding are considered based on XR wareness and/or learning based implementation.
	+ Hybird CG-DG provides higher capacity than DG, close to Genie. No need for eCG.
		- CG resources are used to indicated incoming data and BSR. Non-empty BSR triggers DG.
* **Huawei/HiSilicon:**
	+ Pre-scheduling DG improves DG performance (no delay due to SR/BSR).
		- The assumptions are considered ideal and not realistic. Hence, need for eCG.
* **Vivo:**
	+ eCG (CG recycling) provides higher capacity than DG. Need for eCG.
* **ZTE/Sanechips**
	+ eCG (adaptation/CG recycling) provides higher capacity than DG. Need for eCG.
* **CATT:**
	+ XR specific CG resources followed by DG enables serving XR UL traffic during DRX off. Claimed benefits are power saving gain and serving XR traffic during DRX off. No capacity gain is provided.

### 2.1.1 First round of Discussion

**Moderator’s suggestiosn for First round of Discussions:**

* **Q1:** Discuss your view on at least the practicality of assumptions for pre-scheduling, hybrid CG-DG and in comparison, with eCG (recycling/adaptation based)
* **Q2:** Discuss your view on eCG proposed by CATT, and whether it should be considered for this agenda item due to lack of capacity performance gain.
* **Q3:** Discuss your view on the necessity/benefit of eCG with considerations on simulation results**.**
* **Q4:** Discuss your view regarding the evaluation results and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TP.
* **Q5:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1: It is clear that DG always outperforms CG for capacity, especially for XR, with or without any CG enhancements; otherwise, the whole NR design is wrong. For latency, there is no issue in FR2 and possibly in FR1 in the NR bands having “sufficient” BW for XR that use 30 kHz. Pre-scheduling may be used as a complementary mechanism in FR1.Q2: Almost all proposals can be analytically considered and that is preferable as it offers clarity. Regarding CATT’s proposal, if XR traffic arrives when the UE is not in Active Time, it is rather clear that the proposal can be beneficial. The question in our opinion is whether the scenario considered by CATT is a valid one and, if so, what is the point of having DRX.Q3: No need for eCG – same reasons as for no need for eSPS.Q4: Results not considering DG should not be captured. Results considering DG need to be discussed in detail for simulation assumptions and their overall relevance. We think that it would be beneficial to allocate some time for such discussions which may anyway be required in order to capture individual results in the TR.  |
| **Futurewei** | Q1: PDCCH/DCI overhead is not the bottleneck for XR capacity as the number of UEs per cell is relatively small. DG should always provide better capacity than CG except when considering the latency introduced by SR/BSR. We are open to study CG related enhancement(s) when capacity improvement is shown.Q2: In CATT simulation results, no performance gain over DG was able to show. And the gain over the baseline CG is due to additional DG. Therefore, we do not see the enhancement proposed it as one for capacity improvement.Q3: We are open to study eCG if capacity gain over DG can be shown.Q4: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| CATT | Q1: The pre-scheduling DG is similar to CATT’s proposed UL XR-PMW shown in Table 3 of R1-2208953 (also captured in section 3.5). The hybrid CG-DG is similar to CATT’s proposed eCG in Q2. We believe these two schemes are good techniques for XR system capacity enhancementQ2: No system capacity gain of enhanced CG is due to the assumption of no SR delay of baseline dynamic scheduling with very dense SR resource configuration. We don’t have time to provide additional results of baseline dynamic scheduling with SR delay. CATT proposal of UL XR-PMW for dynamic scheduling (capatured in section 3.5) comparing with dynamic scheduling with 5 ms delay showed 33.3% system performance gain. We will provide additional results next time for comparing the baseline results with SR delay. Q3: The study should include all evaluation results regarless gain or loss in system capacity in order to make conclusion of the study Q4: All evaluation results should be captured. If there are questions on certain results, such as counter intuitive good performance results, such as UL capacity over 10 UEs, it should have notes to address the analysis and observation.Q5: We like to clarify on vivo’s results of capacity over 10 users with/without resource recycling. Are the results based on MU-MIMO? |
| MTK | Q1: We tend to think hybrid CG-DG in current spec can already achieve good results. We also tend to agree with Samsung that by intuition DG should outperform CG for capacity. We can be open to discuss CG enhancement if RAN1 has common understanding that SR delay and BSR delay is inevitable and dominates PDB. (While this may be possible to be resolved by pre-scheduling as menionted by Samsung and tdoc from Ericsson)Q2: The eCG proposed by CATT seems to suffer 1.7% capacity loss compared to DG. We can be open to consider it after CATT updated their results with SR delay in next meeting.Q3: Currently we do not see the necessity due to lacke of demonstrated compacity gain.Q4: We can capture results which considers DG in TR 38.835.Q5: Whether SR delay and BSR delay is inevitable and dominates PDB. (While this may be possible to be resolved by pre-scheduling as menionted by Samsung and tdoc from Ericsson) |
| **ZTE, Sanechips** | Q1: For pre-scheduling DG, it is dependant of XR awareness information, which is too ideal. Moreover, which kind of information e.g., packet size statistics, actual packet arrival occasion can be obtained is unknown till SA’s conclusion.Secondly, we need to further think that, i.e.,if the periodicity of UL grant of pre-scheduling DG was not aligned with the periodicity of packet arrival, there exists following problems:* Transmission delay (e.g. the pre-granted resource is before the packet arrival)
* Resource waste due to some periodic blank UL grant scheduling no data.

Besides, legacy BSR is conveyed in MAC CE transmitting in PUSCH with target BLER = 1%, implying BSR has a risk of transmission failure and cause extra transmission delay if SR is not transmitted in this case. As to hybrid CG-DG, as CATT points out, in fact it is a kind of eCG.Then, for CG, to be honest, if companies check the summaried results including ZTE,Huawei,CATT,vivo, it really doesn’t make sense to me to say that DG always outperforms CG for capacity.(DG compares with eCG).Q2: Agree with CATT that more results can be provided to justify the benefit of eCG. Given collected result in this time, we think the benefit is from power saving metric. And it’s clear there is a trade-off between capacity and power saving. Q3: According the simulation results, the drawback of dynamic grant baseline is SR-BSR/PUSCH procedure, which cause transmission delay. While **CG has natural advantage of reducing the scheduling/transmission delay.** In our view some CG enhancements have small specification impact, including e.g. multiple CG PUSCHs in a period, resource recycling etc. In additional, we also observed that eCG could bring capacity gain compared to pre-scheduling DG according with realistic simulation assumptions.Q4: From our perspective, all enhancement techniques with reasonable evaluation results should be capture in TR 38.835, no matter they are high priority or low priority. Moreover, the reason for de-prioritizing the techniques should be stated in the document. |
| **LG** | **Q1:** DG always can be utilize suppliementally for CG. However, we think pre-scheduling is a kind of optimistic assumption. Based on current BSR, gNB may not acquire UE buffer information before traffic arrival. If gNB scheduling based on XR-awareness information, DG may not have significant benefit comparing to CG. Scheduling additional resource by dynamic UL grant is always possible even in current specification. **Q2:** In existing system gNB can scheduling additional resource by UL grant or override configured CG resource as well. If CG resources need to be changed permernently, re-activation could be used. We don’t think proposed eCG has significant difference from those exisiting methodology. **Q3:** Same as Q2. **Q4:** Fine to capture. **Q5:** In our view, main use case of CG is pose data traffic, which have static data size with short period. In this case, jitter handling would be the main issue to be solved.  |
| **Panasonic** | Q1: We think the combination of CG and DG is a feasible approach for supporting XR traffics, considering the jitter of data arrivals.Q2: The proposed technique could be further studied and considered.Q3: We think there is no need for further CG enhancements. |
| **Google** | **Q1**: * Pre-Scheduling: The pre-scheduling DG is relying on the gNB full awareness of the UL video frame arrival time and packet size to anticipate with a Pre-Scheduling. The awareness could be via signalling or via UE/gNB learning based implementation. These assumptions could be very difficult to agree at the moment with the lack of inputs from SA2/RAN2 on XR awareness. Also, the learning-based implementation is a very ideal assumption difficult to make at this stage. In terms of capacity enhancement, it shows less than 1% capacity enhancement compared to normal DG for the 30ms PDB required for the UL AR video traffic, which doesn’t justify this enhancement.
* Hybrid CG-DG: UL pose and control information is a periodic traffic with no jitter and can use periodic CG configuration with no enhancement needed. The hybrid CG-DG can be useful for the UL AR video traffic. However, the PDB latency requirement for UL AR traffic is 30ms and the scheme seems to show less than 3% capacity gain compared to the normal DG, which is not enough to justify this enhancement.
* eCG recycling/adaptation based: We think the use of multiple CG PUSCHS is beneficial and the use of adaptation and recycling techniques to improve this scheme is useful. The UE can request to cancel some occasions, add some occasions or to modify some occasions based on the arrival and the awareness of the UL traffic. However, the capacity gain is not very clear from ZTE’s results for the 30ms PDB requirement and vs. DG.

**Q2**: eCG as proposed by CATT where the CG is used and the remaining data is scheduled by DG and the UE switch to monitor PDCCH after sending a non-empty BSR. The capacity results dhow a degradation of 1.7% compared to DG. The enhancement can probably offer power saving gain compared to DG with continuous PDCCH monitoring but doesn’t seem to offer capacity gain**Q3**: We are OK to study eCG if it offers capacity gain compared to DG. **Q4**: Yes, we think the evaluation results should be captured as long as they use the agreed simulation assumptions.  |
| **vivo** | Q1: In our opinion, pre-scheduling can be a feasible way for UL latency reduction, but realistic assumption should be made considering recycling of pre-allocated resources, resource efficiency, etc. Regarding the solution of hybrid CG-DG, it is a natural choice when CG resources are adopted to serve UL traffic. In summary, hybrid CG-DG, as well as DG, can be regarded as the baseline(s) to assess CG related enhancments, i.e. eCG.Q2: Regarding the eCG solution proposed by CATT, since no capacity gain can be achieved compared to DG, we tend to not consider it for capacity enhancement.Q5: Regarding CATT’s comment for clarification, in the simulation, SU-MIMO is assumed for evaluation of the performance of recycling of unused CG resources. |
| **Ericsson** | Q1: * Hybrid CG-DG is based on existing specification. Hence no enhancement is needed and it is not an eCG.
	+ CATT proposal is similar to Hybrid CG-DG, BUT in CATT proposal, UE monitors PDCCH during DRX-OFF (spec impact). That is not the case for hybrid CG-DC (monitoring PDCCH during DRX-ON).
* On Pre-scheduling and assumption of XR awarensse, we don’t think ideal/exact information is needed. A rough understand on XR packet sizes (which can be also obtained by learning imlementaiton is sufficient). What is important is to have an intital grant of reasonable size (not too small). Please see below when we simulated using initial grant as MIN/AVG/Max of XR traffic and obtaining similar results (in contribution, we showed only MIN)

* **ZTE:** On BSR comment on ZTE, it is unclear for us the reason. Consider URLLC where CG is used. If BLER was an issue, it should have been addressed fro URLLC.
* **ZTE:** Ericsson also shows for low PDB, Baseline DG is not always better than CG (note that we used best case of CG for comparison). The issue is SR delay. That’s why we tried to show for XR traffic, we can address SR delay:
	+ Pre-scheduling is statistics of XR is available
	+ Hybird CG-DG (during DRX-ON) is no information is available. Please note we used in this case small CG resources in UL slots.

Q2: CATT proposal is suitable for power saving. No capacity gain is achieved.Q3: We don’t think any eCG is needed. For the recycling schemes, if the additional information is considered in CG-UCI instead of multi-bit, then it is fine. Because this track is more consistent with current spec than changing SR to extend it to multi-bit. Etc.Q4: We think at least the results showing meaningful capacity gain should be captured.  |
| **Sony** | **Q1:** Pre-scheduling and hybrid CG-DG consume a lot of DL capacity (e.g., PDCCH) as well as DL power consumption. These issues have not been taken into account when companies provided simulation results for Pre-scheduling and hybrid CG-DG. For eCG, some eCG proposals do not impact on DL capacity and DL power consumption at all. In addition, eCG has a benefit of mitigating the scheduling delays. **Q2:** All proposals should be on the table until Nov. Companies still have more time to provide more results.**Q3:** The benefits of eCG are to mitigate the scheduling delays while providing performance similar or close to DG, as well as reduction of DL resource consumption (a plus sign). **Q4:** We think we should have a fair treatment where all reasonable simulation results are captured in the TR provided that the baseline DG and CG are also simulated, and regardless of whether some are more favourable than others. |
| **InterDigital** | Q1: In our view, eCG is benefial for improving capacity and can be considered under enhancements related to adaptations of CG, e.g. for indicating any excess CG resources. We share similar understanding with ZTE that Hybrid CG-DG is a type of eCG, where DG resources can be requested when the allocated CG resources are insufficient, e.g. by including BSR when transmitting data with CG resources. Regarding performance gains of CG over DG, from the evaluation results provided by some companies such as Huawei, vivo and ZTE, clearly the savings due to SR/BSR latency are useful for realizing capacity gains, particularly when considering PDB of 10ms for UL video. Q2:We are open for discussing the benefits of eCG with more results as indicated by CATT under the capacity agenda, even though the gains may be in power savings.Q3 - Q4:We think the latency reduction by avoiding SR/BSR are useful for realizing capacity gains for eCG compared to the legacy DG. We think the TR 38.835 should capture the evaluation results of any of the CG enhancement schemes that show gains over the baseline DG, including the conditions when eCG outperforms DG  |
| **OPPO** | Q1: Although PDCCH overhead is not the bottleneck for XR, less detection of PDCCH can reduce the UE power consumption. Therefore, we think eCG can provide benefits for short latency and power saving.Q2: We think CATT’s proposal is a hybrid CG-DG solution.Q3: We are open to study eCG. |
| **Lenovo** | Pre-scheduling, at least if it is not single DCI scheduling multi-PUSCHs in cases that there is any jitter/inaccuracy w.r.t. XR traffic awareness may result in resource wastage.Hybrid CG-DG may impact power saving (e.g., if DRX is configured) due to having CG resources in [many] slots. If gNB knows some traffic statistics or range of some XR paarmeters, the scheme may be more useful. |
| **Huawei/HiSilicon** | Q1: we think Ericsson’s “Hybrid CG-DG” seems to be legacy CG behavior, i.e.g, UE transmits on CG, and wait for dynamic scheduling if there is still remaining data, which is allowed by current spec. We are unclear about the “normal CG” in Ericsson’s simulation, it seems to be a new UE behavior.In short, several companies’ simulation results prove that eCG can provide higher capacity compared with dynamic grant that requires SR/BSR by reducing the transmission delay. And re-allocate the unused PUSCH occasions to other UEs to avoid resource waste can improve capacity performance. Therefore, support eCG.Q3: According to simulation results, eCG can provide higher capacity compared with dynamic grant that requires SR/BSR, especially in tighter PDB.Q4: Simulation results of CG should be captured in TR.  |
| **Nokia, NSB** | **Q1:** The simulation results provided by companies demonstrated that the scheduling delay caused by SR can significantly degrade the performance of XR users. Thus, solutions that minimizes the scheduling delay is of special importance.From the simulation studies provided by companies, Pre-Scheduling DG and CG show the best results over conventional DG. As mentioned by HW, in case of pre-scheduling DG, UE may not be available to receive DCI in every slot (e.g., due to C-DRX, search space set, PDCCH skipping, etc.). Note that use of CG also comes with the advantage of avoiding failure due to UE PDCCH decoding failures as is the case for DG cases. **Q2:** Therefore, CG is shown to be beneficial for XR use cases. During this meeting we need to agree whether the CG enhancements are necessary or not. Currently, two main problems were identified: (1) non-integer periodicity of video and (2) large video frame that can be conveyed over multiple slots.Problem 1 need to be solved to help CG work properly when supporting XR. Problem 2 can be solved by various means, e.g., by allocating multiple TBs per period, multiple CG configurations or by allocating extra resources with DG. We thus propose to concentrate on the proposed solutions and discuss the pros and cons o each of those and decide whether the enhancements are needed to support large video frame.**Q4:** We also agree to capture the results and the observations related to CG following the assesment to TR 38.835. |
| **Intel** | Q1: Similar view as other companies that pre-scheduling assumes some XR traffic related awareness information which is not clear at the moment to what extent it can be assumed available. Hybrid CG-DG is not new scheme and can be implementend based on specification.Q2: We agreed that capacity gain is a necessary condition for RAN1 endorsementQ3: Open if capacity gain is shownQ4: Results showing meaningful capacity gain with reasonable/practical assumptions should be captured |
| **Qualcomm** | **Q1.** Some of the simulated schemes have ideal assumptions or assumptions with underlying standards impact. For example, the prescheduling scheme assume the gNB knows the packet distribution and arrival time. The simulations from Huawei show that CG is useful.  **Q2.** Considering that simulation results showed no performance gains then suggest to down prioritize. However, this is similar to one of our earlier proposals to have increased PDCCH monitoring around SPS/CG. The idea was to save power (and capacity wrt CG). Would be interesting to see PSG for this. **Q3.** We think CG enhancements are useful for capacity and power savings **Q4.** Agree that simulation results should be captured.  |

### 2.1.2 Second round of Discussion

**Summary of comments/clarifcations:**

* + For large PDB, DG always overperform CG. For small PDB, some areas CG perform better.
	+ Hybrid DG-CG by Ericsson is not an eCG scheme. It does not rely on XR awareness.
	+ XR-PMW by CATT is an eCG scheme (due to support of PDCCh monitoring during DRX off).
	+ Pre-scheduling by Ericsson does not require ideal/exact information of XR traffic (see MIN/AVG/MAX) results.
	+ All simulations try to address at least SR and/or BSR delay.
	+ Two different observations:
		- Ericsson results: See e.g. Hybrid CG-DC. No need for eCG.
		- Vivo/ZTE/Huawei/HiSilcon/CATT: Not considered e.g. hybrid CG-DG. Need for CG eCG.
	+ Performance should be compared to DG.
	+ Question to CATT (by Samsung): Whether the scenario considered by CATT is a valid one and, if so, what is the point of having DRX.
	+ Note: CATT simulations: SR-less. Hence larger capacity in baseline DG as compared to others. CATT plans to provde updated simulation results next meeting.

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Continue discussion for the 2nd round**
	+ **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
	+ **If no consensus on support of eCG is achieved by the ends of 2nd round, down-priorotize this topic for further study.**
	+ **Capture the description of simulated schemes with corresponding simulation results and key assumptions and findings, in this meeting.**
* **Note that CATT plans to update the baseline simulation results next meeting.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.2 Adaptation of CG parameters/configurations

The Table B in section 2.2 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions. Please note that for some enhancements techniques, companies have provided simulations results.

**Status of inputs in the contributions:**

* **Companies with view (16):** Huawei/HiSilicon\*, vivo\*, Nokia/NSB, IDC, QC, ZTE/Sanechips\*, Ericsson\*, CATT, ChinaTelecomm, OPPO, TCL, Sony, CMCC, Apple, Samsung, DCM
	+ **Supportive (13)**: Huawei/HiSilicon\*, vivo\*, Nokia/NSB, IDC, QC, ZTE/Sanechips\*, ChinaTelecomm, OPPO, TCL, Sony, CMCC, Apple, DCM
	+ **Not supportive (3):** Ericsson\*, CATT, Samsung
* **Companies with evalution results (4):** Huawei/HiSilicon\*, vivo\*, ZTE/Sanechips\*, Ericsson\*

**High-level observations:**

* **Only 4 companies have provided simulation results among 16 companies with views on eCG based on dynamic adaptation.**
* **Variety of adaptation schemes are proposed. Not clear how to relate the performance evaluation results to a specific proposed enhancement.**
* **High-level categorization of the proposals on dynamic adaptations of CG configuraitons**
	+ **Group 1:** Dynamic indication of the unused CG PUSCH occasions by the UE to improve XR capacity performance
		- **Supported:** HW/HiSi\*, vivo\*, ZTE/Sanechips\*, Nokia/NSB, QC, IDC, China Telecom
		- **Not supported:** Ericsson\*, CATT, Samsung
	+ **Group 2:** Dynamic indication to the UE to adjust CG parameters (e.g. MCS, number of symbols, number of PRBs, number of layers) to improve XR capacity performance
		- **Supported:** DCM, ZTE/Sanechips\*, TCL, CMCC
		- **Not supported:** Ericsson\*, CATT, Samsung
	+ **Group 3:** Dynamic indication to the UE to modify PUSCH occasions (increase/descrease and/or advance/delay) to improve XR capacity performance
		- **Supported:** IDC, [QC]
		- **Not supported:** Ericsson\*, CATT, Samsung
	+ **Group 4:** Dynamic indication from the UE for adjusted CG parameters (e.g. MCS, number of symbols, number of PRBs, number of layers) to improve XR capacity performance
		- **Supported:** Sony, Appple, QC, OPPO, [Lenovo]
		- **Not supported:** Ericsson\*, CATT, Samsung

### 2.2.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 2-2-1:** Dynamic indication of the unused CG PUSCH occasions by the UE to improve XR capacity performance is beneficial.
* **Proposal 2-2-2:** Dynamic indication to the UE to adjust CG parameters (e.g. MCS, number of symbols, number of PRBs, number of layers) to improve XR capacity performance is beneficial.
* **Proposal 2-2-3:** Dynamic indication to the UE to modify PUSCH occasions (increase/descrease and/or advance/delay) to improve XR capacity performance is beneficial.
* **Proposal 2-2-4:** Dynamic indication from the UE for adjusted CG parameters (e.g. MCS, number of symbols, number of PRBs, number of layers) to improve XR capacity performance is beneficial.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** Moderator recommends to down prioritize Proposal 2-2-3 and Proposal 2-2-4 due to lack of supporting capacity performance evaluation results by propoents.
	+ What is your view on Moderator’s recommendation?
* **Q2:** What is your view on direction of Proposal 2-2-1 and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q3:** What is your view on direction of Proposal 2-2-2 and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q4:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q5:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1/Q2/Q3: We do not agree with further consideration for any of the proposals as there cannot be any benefit over DG, particularly for XR. For example, what is the benefit over DG for “Dynamic indication to the UE to adjust CG parameters (e.g. MCS, number of symbols, number of PRBs, number of layers)”? RAN1 may first discuss any benefits of few selected eCG proposals over DG.A specification impact and how a proposal can be implementable/testable needs to be dscribed. For example, how will a UE determine that it needs fewer resources? Packet size is not enough for such determination and robustness of such UE estimation (e.g. to variations in link quality) need to be discussed for impact on capacity/QoS. How can a gNB trust various UEs to make decisions for spectrum allocation? How will the UE behavior be tested and what motivation does a UE have to not always indicate need for maximum resources? Given that a NW needs to plan for worst case, how many UEs can be supported with CGs based on maximum resources? How will link adaptation be performed differently from DG? There are several more aspects to be discussed for each individual eCG proposal.Q4: Advantages over DG need to first be described/explained and agreed before capturing any results in TR 38.835. |
| **Futurewei** | Q1: WE are ok to down prioritize 2-2-3 and 2-2-4. Q2: For 2-2-1, a few questions on the proposed scheme. For example, how often the dynamic indication needs to be sent and how fast it should be applied to obtain the potential benefit? What should be the criteria for the UE to send such indication?Q3: For 2-2-2, a few questions on the proposed scheme. For example, how often the dynamic indication needs to be sent? What should be the criteria for the gNB to decide the adjustment? How is this better than directly using DG?Q4: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately.  |
| **CATT** | Q1: WE are ok to down prioritize 2-2-3 and 2-2-4. Q2/Q3: We have question on how gNB sends the dynamic indication and how/when UE would receive the indication if there is no UL grant for retransmission. Q4: All results should be captured. If there are questions on some results, they should have a note for clarification.  |
| MTK | **Q1:** We are ok to down prioritize 2-2-3 and 2-2-4.**Q2:** For Proposal 2-2-1, we think UE assistantce information (UAI) to indicate unused CG resource to NW may be useful for NW to more efficiently manage the scheduling resource. However, we this this is better to be discussed in RAN2 since UAI belongs to RAN2.**Q3:** We do not see necessity/benefit for Proposal 2-2-2. If NW wants to dynamically adjust the MCS, number of symbols, …, NW can just use DG.**Q4:** Results can be captured with description about advantages over DG to be described/explained. |
| **ZTE, Sanechips** | In our opinion, we should firstly focus on the necessity of CG enhancement, instead of down selecting the detailed techniques.Q1: Disagree. We are open to study Proposal 2-2-3 and 2-2-4Q2: Support Proposal 2-2-1Q3: Support Proposal 2-2-2Q4: From our perspective, all enhancement techniques with reasonable evaluation results should be capture in TR 38.835, no matter they are high priority or low priority. Moreover, the reason for de-prioritization should be clarified in brief, for the enhancement techniques with low priority. Q5: We should firstly focus on the necessity of CG enhancement, instead of down selecting the detailed techniques |
| **LG** | **Q1:** We are fine to accept FL’s recommendation. One following question is whether 2-2-4 can be considered in SR/BSR enhancement if the indication of UE is formed as SR or BSR. **Q2/Q3:** Same as 2.1.1, In existing system gNB can scheduling additional resource by UL grant or override configured CG resource as well. If CG resources need to be changed permernently, re-activation could be used. We don’t think proposed CG proposal has significant difference from those exisiting methodology.**Q4:** With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. |
| **Panasonic** | Q1: We are fine with the recommendation.Q2: The inidication for releasing the upcoming CG PUSCH requires knowing the exact time of data arrival, which is not feasible according to the agreement.Q3: We do not see a need for dyanimic adjustment for CG resources, such as MCS.Q5: We think the Proposal 2-2-3 could be further studied to align the CG PUSCH to XR traffic. |
| **Google** | **Q1**: We see benefit in Proposal 2-2-3 and Proposal 2-2-4 and we agree with ZTE. The listed proposals are detailed techniques for CG enhancement and we need first to agree whether CG enhancement is beneficial/needed and should be studied (like we did for SPS) and then decide about the detailed techniques to explore and ask for evaluation for each technique.**Q2**: UE sends BSR information on the first CG PUSCH. Hence gNB can have the information of the data waiting for scheduling and can know which CG PUSCH occasions will be unused and can be re-used for other scheduling. Unless the UE is doing some discarding (e.g. close to expiry data) that the gNB is not aware of and the UE indicates that it can release some CG PUSCHs. Alternatively, the UE can provide further assistance information like amount of high and low priority data (e.g. based on the PDU set importance and PSDB) in the buffer and gNB can cancel/add resources based on that.**Q3**: We Proposal 2-2-2 and think it is useful if the gNB get information about the priority of the data, the remaining delay, … For example, an enhanced BSR can signal such assistance information and based on that the gNB can adjust CG parameters. **Q4**: Yes, we think the evaluation results should be captured as long as they use the agreed simulation assumptions.  |
| **vivo** | Q1: WE are OK to down prioritize 2-2-3 and 2-2-4.Q2: Based on our simulation results, we support Proposal 2-2-1.Q3: In our opinion, CG (re-)activation in existing NR specification can achieve the target of adjusting CG parameters. Besides, how frequent to perform CG (re-)activation is up to gNB implementation. It is unclear to us what the enhancement is and how much additional capacity gain it can achieve compare to legacy mechanism. |
| **Ericsson** | Q1: Support to down prioritize 22.3/4.Q2: If the indication is via CG-UCI, we could be OK to study further, since the container is already exists and spec impct is minimum. Having said that, we don’t see it improves capacity over DG, but in principle, providing assistance to gNB via CG-UCI can be useful.Q3: Not supporting 2-2-2. As we showed, DG already provided best performance. No need to introduce adaptation in CG, when we can achieve the same goal with other means as we showed. |
| **Sony** | **Q1:** Disagree. We are open to study proposals 2-2-3 and 2-2-4. Companies still have more time to provide results.**Q2:** Support Proposal 2-2-1**Q3:** In our view proposal 2-2-2 is like CG Type 2 where network can modify the resource allocation of the CG resource. So it is not an enhancement. **Q4:** Simulation Results should be captured in the TR 38.835 provided that the baseline DG and CG are also simulated. |
| **InterDigital** | **Q1:** We share same view with ZTE and Google; proposals 2-2-3 and 2-2-4 should not be down-prioritized at this stage, and should be considered as part of enhancements related to eCG. **Q2:** Support proposal 2-2-1**Q3:** Support proposal 2-2-2**Q4:** We prefer capturing the evaluation results of the enhancement schemes related to adaptation of CG in the TR |
| **OPPO** | Q1: We are OK to down-prioritize Proposal 2-2-3 and 2-2-4. Q2: We support Proposal 2-2-1 if multiple PUSCH transmission occasions in each period is supported. The unused CG PUSCH occasions can be indicated by CG-UCI transmitted in the first CG PUSCH in each period.Q3: We are OK to down-prioritize Proposal 2-2-2, since it can be achcived by current DG overriding CG. |
| **Lenovo** | Schemes with simulation results should be prioritized. Proposal can be updated to include “if CG enhancement for XR is supported”. |
| **Huawei/HiSilicon** | Q1: we are ok to down prioritize 2-2-3 and 2-2-4. Q2: For 2-2-1, we support. When an UL XR video frame arrives, the UE can know the video frame size and thus the number of PUSCH occasions needed to transmit the video frame. If there are one or more unused PUSCH occasions, the UE can indicate the unused CG PUSCH occasions to the gNB to avoid resource waste, which has capacity gain.Q3: For 2-2-2, companies should clarify how often the dynamic indication needs to be sent? How is this better than directly using DG?Q4: Results for Proposal 2-2-1 should be captured. |
| **Nokia, NSB** | Q1: We do not agree with proposal 2-2-4: UE can continue sending the CSI reports and gNB will be able to adjust the parameters via DCI if necessary. Not clear what is needed on top of already supported solution.More clarification about Proposal 2-2-3 is needed to understand the motivation of the proposal.Q2: We agree with proposal 2-2-1. However, we first need to decide on the solution to support large frame size in order to recommend this to WI.Q3: We do not agree with proposal 2-2-2: The currect CG design allows to send DCI and modify the parameters if necessary. Not clear what is needed on top of already supported solution.Q4: We support capturing the results of proposal 2-2-1 and related observations to TR 38.835. |
| **Intel** | Q1/Q2/Q3: Agree to down prioritize.Q4: Results showing meaningful capacity gain with reasonable/practical assumptions should be captured |
| **Qualcomm** | Q1: We are not ok with deprioritizing 2-2-4. We agree with Apple that this has potential capacity and power saving enhancements Q2: for 2-2-1, this may be very useful in terms of freeing up CG resources that were previously reserved for a UE when not needed by that UE. This can be beneficial in terms with regards to the resource overhead as well as UL beam reservation for FR2, since freeing up that resource would un-reserve the beam in that direction and gNB can use some other beam for some other UE.  Q3: for 2-2-2, this may be useful for 1. reducing the need for additional DG resources if preconfigured CG is not enough for the data by allowing flexible CG resources, and 2. Avoid overbooking resources if data is less than the CG resource allocation. Q4: We think companies evaluation results should be captured  |

### 2.2.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| **P2-2-1** | **Companies (9):**ZTE, Google, vivo, Sony, IDC, OPPO, HW/HiSi, Nokia/NSB, QC | **Companies (4):**Samsung, LG, Panasonic, Intel | **Companies (4):**FW, CATT, MTK, Ericsson |
| **P2-2-2** | **Companies (5):**ZTE, Google, Sony, IDC, QC | **Companies (10):**Samsung, MTK, LG, Panasonic, vivo, Ericsson, OPPO, HW/HiSi, Nokia/NSB, Intel | **Companies (2):**FW, CATT |
| **P2-2-3** | **Companies (5):**ZTE, Panasonic, Google, Sony, IDC | **Companies (11):**Samsung, FW, CATT, MTK, LG, Panasonic, vivo, Ericsson, OPPO, HW/HiSi, Intel | **Companies (1):**Nokia/NSB |
| **P2-2-4** | **Companies (5):**ZTE, Google, Sony, IDC, QC | **Companies (12):**Samsung, FW, CATT, MTK, LG, Panasonic, vivo, Ericsson, OPPO, HW/HiSi, Nokia/NSB, Intel |   |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Continue discussion for the 2nd round**
	+ **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
	+ **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.3 Multiple PUSCHs transmission occasions in a CG period

The Table C in section 2.2 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions. Please note that for some enhancements techniques, companies have provided simulations results.

**Status of inputs in the contributions:**

* **Companies with view (14):** CATT, vivo\*, Intel, IDC, QC, ZTE/Sanechips\*, Ericsson\*, China Telcom, OPPO, Lenovo, CMCC, LG, Google, Samsung, DCM
	+ **Supportive of enhancements (11)**: vivo\*, Intel, IDC, QC, ZTE/Sanechips\*, China Telecom, Lenovo, CMCC, LG, Google, DCM
	+ **Not supportive (3):** Ericsson\*, CATT, Samsung
* **Companies with evalution results (3):** vivo\*, ZTE/Sanechips\*, Ericsson\*

### 2.3.1 First round of Discussion

**High level proposals based on input contributions:**

**Proposal 2-3-1:**

* The following enhancement techniqure(s) is beneficial to improve XR capacity performance
	+ Alt-1: single CG configuration with multiple PUSCH occasions per CG period
	+ Alt-2: single DCI based activation of multiple CG configurations.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 2-3-1 and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details/alternatives for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Do not support. Similar comments as for 2.2.1 apply for Q1 and Q2. |
| **Futurewei** | It is not clear to us how these multiple PUSCH occasions will be utilized by the UE and how it will perform better than DG.  |
| **CATT** | We are not clear on the system capacity gain from proposal.  |
| **MTK** | We are not clear on the system capacity gain for this proposal. |
| **ZTE, Sanechips** | Q1: Support Proposal 2-3-1. We are open to study both Alt-1 and Alt-2.We should firstly focus on the necessity of CG enhancement, instead of down selecting the detailed techniques. |
| **LG** | **Q1: Support.** We think it could be useful to jitter handling and serving video traffic.**Q2:** Same as before, fine to capture. |
| **Panasonic** | We think the mentioned enhancements could be beneficial and should be further studied. |
| **Google** | We support Proposal 2-3-1 and both alternatives can be studied.  |
| **vivo** | We support Alt-1 of proposal 2-3-1. For Alt-2, we think the motivation for Alt-2 is for signaling overhead reduction. Meanwhile the complexity involved in DCI format design should be considered. |
| **Ericsson** | Same view as Samsung, FW, others. Not support. |
| **Sony** | We think the enhancements as described in Proposal 2-3-1 can still be considered and further studied. |
| **InterDigital** | Support proposal 2-3-1 (both Alt-1 and Alt-2) |
| **OPPO** | As mentioned in 2.1.1, less detection of PDCCH can reduce the UE power consumption, so we support Alt-1 and open to Alt-2. |
| **Lenovo** | If CG enhancement is supported (e.g., gains shown w.r.t. a hybrid CG-DG), the alternatives are fine. |
| **Huawei/HiSilicon** | Q1: We support Alt-1. Results should be captured.Alt-2 seems just saving DCI overhead, and does not bring capacity gain. |
| **Nokia, NSB** | We do not support Alt-2 since single activation will require a lot of DCI overhead as every CG configuration can have different PRBs, MCS, etc. Alt-1 with the design similar to multi-PUSCH scheduling with single DCI seems more reasonable if we want to support multi TB per period to transmit video frame. |
| **Intel** | We think it is beneficial. For UL video, e.g., in case it arrives outside DRX ON, at least initial PUSCHs transmissions can be made by CG. Open to consider both Alt-1/2  |
| **Qualcomm** | We think it is useful, the first Alt-1 is useful when for single flow with larger burst size and the second Alt-2 is useful for multiple flow case. In order to take full advantage of these enhancements, a study of more dynamic PUSCH occasions parameters may be needed (e.g., cancelling un-used occasions, etc.)  |

### 2.3.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P2-3-1 | **Companies (11):**ZTE, Panasonic, Google, Intel, Sony, IDC, OPPO, QC, vivo(Alt1 ), HW/HiSi(Alt 1), Nokia/NSB(Alt 1) | **Companies (6):**Samsung, FW, CATT, MTK, Ericsson, Nokia/NSB(Alt 2) | **Companies (10):**Lenovo |

**Among the proponets, some companies prefer only Alt-1, and disagree with Alt-2. Moderator suggests considering only Alt-1.**

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Continue discussion for the 2nd round**
	+ **Proponets are requested to indicate if Alt 1 can be prioritized.**
	+ **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

**Moderator’s recommendation:**

## 2.4 Non-integer periodicity for CG transmissions

The Table D in section 2.4 of R1-2214010 lists the proposals in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions. Please note that for some enhancements techniques, companies have provided simulations results.

**Status of inputs in the contributions:**

* **Companies with view (20):** Huawei/HiSilicon\*, vivo\*, Nokia/NSB, IDC, QC, ZTE/Sanechips\*, Ericsson\*, China Telcom, OPPO, TCL, Sony, Lenovo, NEC, CMCC, Panasonic, LG, Apple, Google, Samsung, DCM
	+ **Supportive of enhancements (17)**: vivo\*, Nokia/NSB, IDC, QC, ZTE/Sanechips\*, China Telcom, OPPO, TCL, Sony, Lenovo, NEC, CMCC, Panasonic, LG, Apple, Google, Samsung, DCM
	+ **Not supportive (3):** Huawei/HiSilicon\*, Ericsson\*, Samsung
* **Companies with evalution results (4):** Huawei/HiSilicon\*, vivo\*, ZTE/Sanechips\*, Ericsson\*

### 2.4.1 First round of Discussion

**High level proposals based on input contributions:**

**Proposal 2-4-1:**

* Enhancements related to match the periodicity for CG transmissions with non-interger periodicity of XR traffic is beneficial to improve XR capacity performance.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 2-4-1 and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details/alternatives for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Do not support. Similar comments as for 2.2.1 apply for Q1 and Q2. |
| **Futurewei** | This is also discussed under power saving agenda item. Though it may have power saving benefit, we do not see it as capacity improvement scheme. |
| **CATT** | We don’t see the benefit in capacity enhancement |
| **MTK** | We tend to agree with Futurewei. We do not see clear benefit in capacity enhancement. |
| **ZTE, Sanechips** | Q1: Suppport Proposal 2-4-1. |
| **LG** | **Q1:** Support. Non-interger periodicity has clear benefit to serve periodic traffic by avoiding redundant resource allocation with reducing latency. Based on the contributions, the flexibility of periodicity can be obtain by only few minor specification changes. **Q2**: Same as before, fine to capture the proposal.  |
| **Panasonic** | We think the relevant enhancement could bring power saving gain but not much capacity gain. |
| **Google** | We support the Proposal. |
| **vivo** | We think non-integer periodicity for CG needs to be considered. |
| **Ericsson** | Q1: Not support. We showed with our simulations that non-interger periodicity is not an issue. |
| **Sony** | Q1: Suppport Proposal 2-4-1. The quasi-periodicity of XR transmissions can also be reflected in layer 1 operation (e.g., enhancements of CG). |
| **InterDigital** | We support proposal 2-4-1 |
| **OPPO** | Support Proposal 2-4-1. We think eCG can provide benefits for short latency and power saving. |
| **Lenovo** | Ok |
| **Huawei/HiSilicon** | Non-integer periodicity issue can be solved by configuring multiple CG configurations. No need for more enhancements. |
| **Nokia, NSB** | Simulation results have shown the benefits from CG. It is therefore important to identify the necessary enhancements to support XR with CG. Non-integer periodicity is already considered as an issue for C-DRX in Power saving domain. This enhancement is also necessary for CG and should be considered. The solution can be the same as for non-integer periodicity in C-DRX. We support Proposal 2-4-1. |
| **Intel** | Not a critical issue |
| **Qualcomm** | We support non-integer periodicity for CG to match with XR traffic  |

### 2.4.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P2-4-1 | **Companies (10):**ZTE, LG, Google, vivo, Sony, IDC, OPPO, Lenovo, Nokia/NSB, QC | **Companies (8):**Samsung, FW, CATT, MTK, Panasonic, Ericsson, HW/HiSi, Intel |   |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Continue discussion for the 2nd round**
	+ **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
	+ **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.5 Other enhancements

The Table E in section 2.5 of R1-2214010 lists the proposals in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions. Please note that for some enhancements techniques, companies have provided simulations results.

**Status of inputs in the contributions:**

* **Topic 1: SPS enhancements:**
* **Supporting SPS enhancements (5): CATT\*, ZTE/Sanechips\*, IDC, Sony, China Telcomm**
* **Not supporting SPS enhancements (4): Futurewei, Huawei/HiSilicon, Ericsson, Samsung**
* **Topic 2: PDCCH monitoring occasions during DRX-OFF:**
* **Supported: TCL, CATT\*, Panasonic**
* **Topic 3: XR multiple flows differentiation with CG transmission**
* **Supported: Intel\*, Sony**

### 2.5.1 First round of Discussion

**High level proposals based on input contributions:**

**Topic 1: SPS enhancements:**

* The proposed enhancements suggest configuring PDCCH monitoring occasions after SPS PDSCH transmission occasions. The performance evaluation results by CATT show power saving gain, but no capacity gain. The performance evaluation results by ZTE show gain as compared to legacy SPS, and not DG. Other enhancemnts such as support of CBG for SPS and Type-1 activation are suggested.
* Few companies have expressed concerns on support of any SPS enhancementsfor XR capacity improvements emphasizing that the DCI overhead is not a bottle-neck for XR capacity.
* **Moderator’s recommendation for Topic 1:**
	+ **Per conclusion in RAN1#110, SPS enhancements for XR capacity improvements is down prioritized.**

**Topic 2: PDCCH monitoring occasion during DRX OFF**

* CATT has provided simulation results for the proposed enhancements for both DL and UL (see section 2-1), showing power saving gain, but no capacity gain.
* **Moderator’s recommendation for Topic 2:**
	+ **Configuration of PDCCH monitoring occasions during DRX-off for XR capacity improvements is down prioritized**

**Topic 3: XR multiple flows differentiation with CG transmission**

* **Moderator’s recommendation for Topic 3:**
	+ **Companies feedback regarding this topic is needed.**

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on **Moderator’s recommendation for Topic 1**?
* **Q2:** What is your view on **Moderator’s recommendation for Topic 2**?
* **Q3:** Discuss your view regarding the proposed enhancements in **for Topic 3**
* **Q4:** Discuss your view regarding the proposed enhancements/recommendations and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q5:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1: Agree with moderator – RAN1 already concluded.Q2: Agree with moderator. Given the almost certainly short DRX cycle for XR, if proposal 2 was to apply, what would be the meaning of having DRX?Q3: No need for the proposed enhancements – CG is even less appropriate for multiple flows as that is another dimension for the dynamic nature of XR.Q4: RAN1 discussion/conclusion for simulation assumptions and feasibility and for the benefits over DG is first needed. |
| **Futurewei** | Q1: Agree that this is already concluded.Q2: Agree with moderatorQ3: With multiple flows, it is even more difficult to see the capacity benefit of CG over DG.Q4: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: We are OK with the proposal deprioritize SPS. Q2: We don’t agree with the proposal. PDCCH monitoring at DRX OFF is the enhancement of dynamic scheduling to support XR and other traffic in the same time. The PDCCH monitoring at DRX OFF is one technique of C-DRX enhancement to align the PDCCH monitoring cycle with the XR traffic cycle. Q3: The trunking efficiency is reduced for XR multiple flow differentiation with CG. We need performance results to justify the proposed techniques. Q4: All results should be captured in the TR |
| **MTK** | Q1: Agree with moderator – RAN1 already concluded. Q2: Tend to agree with moderator. To us this is more like a power enhancement scheme. Besides, RAN2 is desining semi-static DRX periodicity enhancement to match XR traffic, so the XR traffic aligning with CDRX (PDCCH monitoring) may not still be an issueQ3: We do not see evident capacity gain for the proposed enhancementsQ4: Discuss your view regarding the proposed enhancements/recommendations and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.Q5: We are ok to capture the results if the comparison baseline is DG |
| **ZTE, Sanechips** | Q1: Agree with Moderator’s recommendation for Topic 1. But we think the evaluations on SPS enhancement can be captured in TR38.835 as illustrated in Q4.Q3: We are open to study CG enhancement on multiple streams model. However, due to limited time unit, RAN1 has not yet had any conclusions for CG enhancement for single stream model. We suggest to focus on the discussion on 2.1~2.4. Moreover, the XR multiple streams differentiation is more likely for XR-awareness transmission, which is in charged by RAN2. We can wait for RAN2’s conclusions on XR-awareness transmission |
| **LG** | **Q1, Q2:** Agree with moderator’s assement. **Q3:** multi-flow is XR use case clearly, but the issue is hard to be identified since it highly depends on what kind enhancement would be done in this AI. We don’t think it is necessary to down-prioritize at this stage. It would be better to keep this for future discussion. **Q4:** Same as before. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal.  |
| **Panasonic** | Q1: We are fine with the proposal.Q2:We are fine with the proposal.Q3: We are fine with the proposal. Flow differentiation is required to meet different QoS. |
| **Google** | **Q1, Q2**: We agree with the moderator’s recommendation.**Q3**: UL pose and control information is a periodic traffic with no jitter and can use CG configuration with no enhancement needed. UL AR video would need a different CG with some enhancement to handle the varying packet sizes and the jitter.  |
| **vivo** | Q1: Support moderator’s recommendation.Q2: Support moderator’s recommendation.Q3: Currently multi-CG configurations be used to address multi-flow case. What will be enhanced and the spec impact need more clarifications. |
| **Ericsson** | Q1: Agree w ModeratorQ2: Agree with Moderator. To CATT, the fact that there is no capacity gain, it is clear this proposal does not belong to capacity gain agenda. It should be discussed in power saving.Q3: Agree with others. Moreover, such differentiation is more RAN2 topic than RAN1.  |
| **Sony** | The conclusion made in RAN1#110 did not explicitly mention to down-prioritize SPS enhancements. The discussion and evaluation related to SPS enhancement can still be captured in the TR. |
| **InterDigital** | Q1 and Q2:Agree with Moderator’s recommendationQ3:Ok for studying CG enhancements for supporting multiple flows. We think configuring different CG configurations with different periodicties that are aligned with the periodicities of different UL flows (e.g. pose, video) are beneficial for improving capacity. |
| **OPPO** | Q1/Q2: Agree with moderator.Q3: Multiple flows differentiation with CG transmission can be solved if the followings are supported:* Single CG configuration with multiple PUSCH occasions per CG period;
* Dynamic indication of the unused CG PUSCH occasions.
 |
| **Lenovo** | Q1&Q2: agree with ModeratorQ2: can concludeQ3: maybe RAN2 can discuss this first |
| **Huawei/HiSilicon** | Q1: Agree with moderator – RAN1 already concluded.Q2/3: Agree with moderator. |
| **Nokia, NSB** | We support Moderator’s recommendation for Topic 1&2.As per Topic 3, more justification is need to see the benefits from the enhacnements and already existing possibility to activate multiple CGs per different flow if needed. |
| **Qualcomm** | Agree on views.   |

### 2.5.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| Topic1 | All agree w Mod.  |   |   |
| Topic2 | **Companies (14):**Samsung, FW, MTK, LG, Panasonic, Google, vivo, Ericsson, IDC, OPPO, Lenovo, HW/HiSi. Nokia/NSB, QC | **Companies (1):**CATT |   |
| Topic3 | **Companies (5):**ZTE, Panasonic, Google, IDC, OPPO | **Companies (8):**Samsung, FW, [CATT], MTK, LG, vivo, Ericsson, Nokia/NSB | **Companies (3):**CATT, [Lenovo], [Nokia/NSB] |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Topic 1:**
	+ **No need for more discussions.**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**
* **Topic 2:**
	+ **CATT, as the only proponet is requested to provide feedback and discuss for the 2nd round on Topic 2:**
		- **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
		- **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
		- **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**
* **Topic 3:**
	+ **Proponets are requested to provide feedback and discuss for the 2nd round on Topic 3, and share the plans for providing simulatin results, if any:**
		- **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
		- **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
		- **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Dynamic scheduling/grant enhancements

The followings are agreed/concluded previously:

|  |
| --- |
| **Agreement (RAN1#109-e):**To study whether/how to support a candidate capacity enhancement technique for XR traffic based dynamic scheduling/grant transmissions, companies are encouraged to consider the following studies:* + - Study enhancements related to extending capability of single DCI scheduling multi-PDSCHs/PUSCHs for FR2-2 to FR1/FR2.
		- Note: whether and how to discuss enhancements may depend on the outcome of Rel-17 B52.6G UE feature discussion
		- Study enhancements related to HARQ-ACK and/or CBG transmissions for single DCI scheduling one or multi PDSCH(s).
		- Study enhancements related to allowing different configurations per PDSCH/PUSCH
		- Study enhancement related to scheduling request and/or BSR with the focus on L1 enhancements.
		- Note: Other studies are not precluded as well as the combination of the above studies.
* Follow the *common principle for assessment of the candidate capacity enhancement technique.*

**Agreement (RAN1#110):**RAN1 to make decision on the following in RAN1#110bis-e* Support single DCI scheduling multi-PDSCHs/PUSCHs which is currently supported for FR2-2 to other SCS in FR1/FR2.

**Agreement (RAN1#110):**Whether/how to enhance BSR to improve capacity performance of XR traffic is within RAN2 scope and is not handled by RAN1.* Note that companies should indicate if and what BSR enhancement is assumed in their RAN1 proposals on CG and DG enhancements.
* RAN1 can evaluate BSR enhancement to improve capacity performance.
 |

The views regarding DG enhancements for serving XR traffic are summarized and discussed in the following sections.

## 3.1 Extension of multi-slot PxSCHs from FR2-2 to FR1/FR2

The Table F in section 3.1 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (15):** Futurewei, Huawei/HiSilicon, CATT, vivo\*, Intel\*, MTK, Nokia/NSB, IDC, QC, ZTE/Sanechips\*, Ericsson, CMCC, Panasonic, LG, [Samsung]
	+ **Supportive of enhancements (10)**: vivo\*, Intel\*, Nokia/NSB, IDC, QC, Ericsson, CMCC, Panasonic, LG, Samsung
* **Not supportive (5):** Futurewei, Huawei/HiSilicon, CATT, MTK, ZTE/Sanechips\*
* **Companies with evaluation results (3):** vivo\*, Intel\*, ZTE/Sanechips\*

**High-level observations:**

* The Proponents’ main reason is that due to large XR packet sizes, it is reasonable to use a single DCI to schedule the XR TBs in multiple slots. The performance maybe improved by supporting the flexibility.
* The opponents’ main reason is that the PDCCH overhead is not a bottleneck for XR capacity. Hence, supporting multi-slot PxSCHs is not beneficial.
* 3 companies, vivo, ZTE/Sanechips and Intel have provided simulation results.
	+ Vivo shows capacity gain when PDCCH overhead is used by data, however ZTE does not show any gain.

### 3.1.1 First round of Discussion

**High level proposals based on input contributions:**

**Proposal 3-1-1:**

* **Support single DCI scheduling multi-PDSCHs which is currently supported for FR2-2 to other SCS in FR1/FR2-1*.***

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** Provide your analysis to understand the difference between ZTE/Sanechips and vivo simulation results.
* What is your view on direction of Proposal 3-1-1 and the necessity/benefit of the proposed enhancements?
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1: DCI rates (~1 Kbps) are several (4-5) orders of magnitude less than data rates (10s Mbps) for XR. That removes from consideration any PDCCH/DCI enhancements for the purpose of capacity. Therefore, based on simple analytical considerations, there is no need to spend time discussing specific simulation assumptions/accuracy of evaluations for Q1. Q2: We prefer to have the option to apply “as is” the multi-PXSCH scheduling from FR2-2 to FR1/FR2 and to postpone for now a decision to include/exclude (can still be concluded at this meeting). Whether anything needs to be captured in the TR can be discussed later.  |
| **Futurewei** | Q1: Agree with Samsung’s analysis. No need to consider further Proposal 3-1-1.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: We don’t see the benefit of Proposal 3-1-1. The results of performance gain from contributions are way too optimistic even with 2 symbols of PDCCH used for PDSCH in single DCI scheduled multiple PDSCH. The loss of link adaptation gain and inflexible of retransmission among PDSCH HARQ by single DCI scheduling multiple PDSCH would limit the performance. Q2: All results should be captured. Some over-optimistic results should have note and observation for clarification.  |
| **MTK** | Q1: We don’t see clear benefit for Proposal 3-1-1. The results from vivo which assumes “PDCCH overhead is used by data” is not really practical from our perspective. The results from ZTE seems more reasonable to us.Q2: The results can be captured if the evaluation assumption is clearly explained in the TR. |
| **ZTE, Sanechips** | Q1: In fact we have similar observation as vivo in the contributions: the capacity performance of 1 DCI scheduling multiple PDSCHs is highly correlated with the PDCCH overhead assumptions. If ideal assumption for PDCCH overhead saving is considered, considerable capacity gain of 1 DCI scheduling multiple PDSCHs can be obtained, while if realistic assumption for PDCCH overhead saving are considered, marginal capacity gain or no capacity gain of 1 DCI scheduling multiple PDSCHs is obtained.And in our contribution, the two different assumption for PDCCH overhead saving are considered: * Realistic assumption in R1-2209198: Considering multiple UEs are waiting for scheduling in one slot, PDCCH overheads cannot be saved in the PDSCH except the first PDSCH, where there are PDCCH monitoring occasions for other UEs.
* Ideal assumption in R1-2207062: the PDSCHs except the first PDSCHs can re-use the PDCCH overhead to transmit data.

The results for these two assumptions are summarized as follow:

|  |  |  |  |
| --- | --- | --- | --- |
| **Assumption** | **Techniques** | **Capacity** | **Capacity gain** |
| Realistic assumption | 1 DCI scheduling one PDSCH | 9.1 | - |
| 1 DCI scheduling multiple PDSCHs | 9.4 | -13.18% |
| Ideal assumption | 1 DCI scheduling one PDSCH | 9.1 | - |
| 1 DCI scheduling multiple PDSCHs | 7.9 | 3.29% |

We also find that **Ericsson, vivo and ZTE/Sanechips** has provided some negative capacity performance of 1 DCI scheduling multiple PDSCHs compared to 1 DCI scheduling 1 PDSCH in some cases. As a result, basically the observation of negative capacity performance of 1 DCI scheduling multiple PDSCHs in the cases is reasonable.Q2: Disagreed. |
| **LG** | **Q1:** We share similar view to Samsung, as long as the PDCCH/DCI overhead is not an issue for XR services. Regarding evaluation results, based on the current specification, the symbols for PDCCH can be utilized as PDSCH resource by gNB’s scheduling. If it is considered in evaluation, the result should be better than other evaluation not considering that. **Q2:** Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | **Q1**: We support for Proposal 3-1-1. Single DCI scheduling multiple PDSCHs/PUSCHs can have capacity gain thanks to the PDCCH overhead reduction that can be re-used for PDSCHs/PUSCHs scheduling as shown in vivo results. Also, the scheme comes with minimum specification effort as it will be extended from Fr2-2, hence our support for Proposal 3-1-1  |
| **vivo** | Q1: Thanks for ZTE’s clarification.Indeed some ideal assumptions are adopted for our simulation. We would like to further clarify our evaluation results that we did not consider any other PDCCH that may occupy the CORESET(s) than scheduling DCI, e.g. broadcast PDCCH. With the existence of such PDCCH other than scheduling DCI, the reserved X(1 or 2) symbol(s) may not be fully utilized for PDSCH scheduling if not used for scheduling DCI. Therefore the potential performance gain by multi-PDSCH scheduling shown in the evaluation can be viewed as the upper bound. Q2: We think the proposed enhancements with evaluation results, especially those showing potential performance gain, can be captured in the TR. Necessary clarification if any can be included. Whether and how to draw observation and conclusion based on the captured techiques and evaluation results can be discussed separately. |
| **Ericsson** | Q1: We are OK to enable support of multi-PxSCH “as it is”, tha tis without enhancements to FR1/FR2-1. The capacity gain, if any, is limited for any enhancement and we should be consistent in our decisions.  |
| **InterDigital** | Q1: We think the extension of single DCI scheduling multiple-PDSCH is useful for addressing issues related to transmission of large PDU sets, where any savings from PDCCH overhead reduction that can be used for data can result in capacity improvement. In this regard we support proposal 3-1-1. |
| **OPPO** | Q1: Agree with other companies. No need to further enhance the multi-PxSCH scheduling. |
| **Lenovo** | Similar to SPS, PDCCH is not the bottleneck in XR scenario, and such extension is not likely needed. In general, wondering if entire 1 or 2 symbol PDCCH (full BW) overhead assumption is a bit conservative?  |
| **Huawei/HiSilicon** | Q1: disagree with Proposal 3-1-1.Single DCI scheduling multiple PXSCHs has been studied in Rel-17 B52.6GHz with the benefit of control signaling overhead saving. Multiple PDSCHs scheduled by single DCI have the same MCS and frequency domain allocation indication, which may decrease the XR capacity due to the variable channel condition. In addition, inflexible retransmission may cause extra delay which would also limit the capacity. Moreover, according to R17 XR evaluation, the bottleneck of XR capacity lies in the data channel rather than the control channel. Therefore, this topic can be down-prioritized.Q2: This topic can be down-prioritized. |
| **Nokia, NSB** | Q1: the difference is coming from vivo’s assumption of giving the resources for PDCCH to PDSCH if the former is not used. We support Proposal 3-1-1. It helps reduce the DCI overhead and is considered advantages for transmission of larger XR payloads that does not fit into a single TTI. We support having captured single-DCI multi-PDSCH scheduling options for FR1 in the TR.Moreover, when sparse PDCCH monitoring is configured to save power, multi-PxSCH scheduling can greatly affect the capacity since the scheduling delay is significantly reduced.Q2: We agree to capture observations and results to TR 38.835. |
| **Intel** | Q1: Ok to consider support of existing solution as is to FR1/FR 2-1 |
| **Qualcomm** | Q1: We think that the capacity gains from vivo are useful. They are showing that Case 3 is useful for capacity as unoccupied coreset can be used for PDSCH. Something that can already be supported.  We support the proposal 3-1-1. We think it is useful for XR burst transmission and reduces the overhead of DCI scheduling. Q2: We think companies effort should be respected.  |

### 3.1.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P3-1-1 | **Companies (7):**Google, vivo, Ericsson, IDC, Nokia/NSB, Intel, QC | **Companies (9):**[Samsung], FW, CATT, MTK, ZTE, LG, OPPO, Lenovo, HW/HiSi | **Companies (1):**Samsung |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* + - **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
		- **If no consensus is achieved by the ends of 2nd round for any of these proposals, conclude that:**
			* **There is no consensus to support legacy single DCI scheduling multi-PDSCHs for FR2-2 to other SCS in FR1/FR2-1*.***

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 3.2 Enhancements of CBG and/or HARQ-ACK feedback

The Table G in section 3.2 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (11):** vivo\*, QC, ZTE/Sanechips, Lenovo, Rakuten, Nokia/NSB, Samsung, LG, InterDigital, Google, Apple
* **Companies with evaluation results (1):** vivo\*

**High-level observations:**

* **Proposed enhancement for early/Multiple HARQ-ACK feedback reporting for multi-slot PDSCHs scheduling**
	+ Vivo\*, QC, ZTE/Sanechips, Lenovo, Rakuten
* **CBG support for multi-slot PDSCH scheduling (when supported)**
	+ Support: Nokia/NSB, Samsung
	+ Not support: LG
* **Proposed enhancement for CBG based HARQ-ACK feedback reporting**
	+ Alt-1: CBG overhead reduction, e.g., Per CBG HARQ-ACK feedback for erroneous TBs
		- Nokia/NSB, Lenovo
	+ Alt-2: Mapping TB related XR information to corresponding CBG
		- Lenovo
	+ Alt-3: Flexibility in number of CBGs per TB
		- InterDigital, Google
	+ Alt-4: CBG based transmission to support QoS enhancement at lower layers.
		- Apple

### First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 3-2-1:** **Early/Multiple HARQ-ACK feedback reporting for multi-slot PDSCHs scheduling is beneficial to improve XR capacity performance.**
* **Proposal 3-2-2:** **CBG support for multi-slot PDSCH scheduling (when supported) is beneficial to improve XR capacity performance.**
* **Proposal 3-2-3:** **Enhancement for CBG based HARQ-ACK feedback reporting) is beneficial to improve XR capacity performance. Examples of enhancements are listed below.**
	+ Alt-1: CBG overhead reduction, e.g Per CBG HARQ-ACK feedback for erroneous TBs
	+ Alt-2: Mapping TB related XR information to corresponding CBG
	+ Alt-3: Flexibility in number of CBGs per TB
	+ Alt-4: CBG based transmission to support QoS enhancement at lower layers.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** Moderator recommends prioritizing Proposal 3-2-1 and Proposal 3-2-2 for discussions due to availability of simulation results and/or more supporting companies.
	+ What is your view on Moderator’s recommendation?
* **Q2:** What is your view on direction of Proposal 3-2-1, Proposal 3-2-2 and Proposal 3-2-3, and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q3:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q4:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q3: Suggest to first conclude on the support of multi-PXSCH. If concluded, OK to focus on the more fundamental aspects captured in Q1 as they were also discussed in R17 for B52.  |
| **Futurewei** | Q1-Q2: we do not see the need or potential to have multi-PXSCH for XR capacity improvement. Q3: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1-Q2: We need to see the performance gain before we further discuss the proposed schemes. Q3: All results should be captured with note for clarification.  |
| **MTK** | Q1-Q2: (Same as Samsung) Suggest to first conclude on the support of multi-PXSCH. If concluded, OK to focus on the more fundamental aspects captured in Q1 as they were also discussed in R17 for B52. Q3: We are ok to capture the results if the comparison baseline is DG. |
| **LG** | It should be discussed after 3.1.1 Q3: Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | We see benefits in the listed proposals but we are aligned with Samsung to first conclude on the support of multi-PDSCHs/PUSCHs scheduling before diving into the details.  |
| **vivo** | Q1: For Proposal 3-2-1, if there is conclusion in section 3.1.1, further study on the feasibility and potential benefit of earlier HARQ-ACK feedback can be considered.Q2: For proposal 3-2-2 and 3-2-3, the benefit needs to be justified by evaluation. Regarding Proposal 3-2-2, it should be noted that there are a lot of issues for enhancements related to CBG based re-transmission and HARQ-ACK reporting, in conjuction with multi-PDSCH scheduling. Besides, most of these issues were discussed extensively during Rel-16 NR-U and Rel-17 B52.6GHz with the conclusion of not supporting. |
| **Ericsson** | Q1: OK with prioritization suggestion. Then agree with Samsung that we need to focus on support of multi-slot PDSCH (since main use case scenarions are FR1/FR2-2).Q2: We are OK to support 3-2-2 if there is strong majority. Please see our simulation results in section 4.3 shows similar performance between TB based and CBG based. So, the capacity gain is not clear to us.Regarding other proposals, we don’t see the need. For example for 3-2-1, if there is TDD pattern, it can use both single-slot and multi-slot PDSCH scheduling, to enable early feedback. (for example for n=0,..,2 multi-slot, for slot n=4,.. multi/single slot)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Dn=0 | Dn=1 | Dn=2 | U n=3 | Dn=4 | Dn=5 | Dn=6 | Un=7 |

 |
| **InterDigital** | Q1 - Q2:We do not see the need for prioritizing proposals 3-2-1 and 3-2-2 related to multi-slot PDSCH scheduling. We think proposal 3-2-3 on the enhancements for CBG based HARQ-ACK should also be the focus of the study/discussion, as these enhancements apply even for the baseline single PDSCH scheduling. |
| **OPPO** | Q1/Q2: We think there is no need to further enhance the multi-PXSCH scheduling. |
| **Lenovo** | The schemes with simulation results should be prioritized. |
| **Huawei/HiSilicon** | Q1-Q3: Suggest to first conclude on the support of multi-PXSCH. Then, performance gain should be given before we further discuss the topic. |
| **Nokia, NSB** | We support proposals 3-2-1, 3-2-2, 3-2-3 as CBG-based transmission has proven to be useful for XR use cases with transmission of large payloads. This should be supported also for single-DCI multi-PDSCH scheduling options. Having Early/Multiple HARQ-ACK feedback reporting for multi-slot PDSCHs scheduling is beneficial to HARQ loop latencies, and a consequence, help the overall improve XR capacity performance. |
| **Qualcomm** | We think that enhancements for multi-PXSCH are useful. Therefore, we are supporting of multi-HARQ ACK, dynamic indication of change of configuration and adaptive configuration.  |

### 3.2.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P3-2-1 | **Companies (2):**Nokia/NSB, QC | **Companies (4):**FW, CATT, Ericsson, IDC | **Companies (6):**Samsung, MTK, LG, Google, vivo, HW/HiSi |
| P3-2-2 | **Companies (2):**Nokia/NSB, QC | **Companies (4):**FW, CATT, vivo, IDC | **Companies (6):**Samsung, MTK, LG, Google, Ericsson, HW/HiSi |
| P3-2-3 | **Companies (3):**Lenovo, Nokia/NSB, QC | **Companies (4):**FW, CATT, vivo, Ericsson | **Companies (5):**Samsung, MTK, LG, Google, HW/HiSi |

**Moderator’s recommendation for discussion:**

**Moderator suggests postponing this discussion after decision on regarding the proposal in section 3.1.1.**

* **Meanwhile, companies can provide any additional comment below.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 3.3 Enhancements of parameters/configurations of multi-slot PDSCHs

The Table H in section 3.3 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (8):** vivo\*, InterDigital\*, QC, TCL, Ericsson, Sony, Rakuten, CMCC
* **Companies with evaluation results (2):** vivo\*, InterDigital\*

**High-level observations:**

* **Applying different parameters (e.g., MCS, FDRA, TDRA, number of PxSCHs) for multi-PxSCHs scheduled by a single DCI**
	+ Support: Vivo\*, InterDigital\*, QC, TCL, Ericsson, Sony, Rakuten
* **PDCCH skipping indication in the single DCI scheduling multi-PDSCHs allows for PDCCH skipping after decoding of the multi-PDSCHs**
	+ Support: QC
* **For single DCI scheduling multi-PDSCHs/PUSCHs, support of dynamic change between single TB transmission per PDSCH/PUSCH and TB repetition on multiple PDSCHs/PUSCHs**
	+ Support: CMCC
* ..

### 3.3.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 3-3-1:** **Applying different parameters (e.g.,** **MCS, FDRA, TDRA, number of PxSCHs) for multi-PxSCHs scheduled by a single DCI is beneficial to improve XR capacity performance.**
* **Proposal 3-3-2:** **PDCCH skipping indication in the single DCI scheduling multi-PDSCHs allows for PDCCH skipping after decoding of the multi-PDSCHs that is beneficial to improve XR capacity performance.**
* **Proposal 3-3-3:** **For single DCI scheduling multi-PDSCHs/PUSCHs, support of dynamic change between single TB transmission per PDSCH/PUSCH and TB repetition on multiple PDSCHs/PUSCHs, is beneficial to improve XR capacity performance.**

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** Moderator recommends prioritizing Proposal 3-3-1 for discussions due to availability of simulation results and/or more supporting companies.
	+ What is your view on Moderator’s recommendation?
* **Q2:** What is your view on direction of Proposal 3-3-1, Proposal 3-3-2 and Proposal 3-3-3, and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q3:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q4:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1: Do not support proposal 3-3-1. For any further consideration of 3-3-1, proponents should describe the DCI format design together with DCI overhead savings considering possible DCI size matching in order to maintain the “3+1” DCI size budget (and preferably, in conjunction with other Rel-18 WIs that are directly applicable for XR such as multi-cell scheduling using a single DCI). Q1-Q3: Similar comment as for CBG enhancements in 3.2.1 – first need to conclude on whether to support multi-slot PXSCH scheduling.  |
| **Futurewei** | Q1-Q2: we do not see the need or potential to have multi-PXSCH for XR capacity improvement.Q3: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1/Q2: We don’t see the benefit of proposed scheme.Q3: all results should be captured with note.  |
| **MTK** | Q1: We do not see clear benefit for Proposal 3-3-1. If NW wants to dynamically change MCS, FDRA, TDRA, …, why not NW just use single PxSCH scheduling?Q2: We do not see clear benefit for Proposal 3-3-1/3-3-3. If NW wants to dynamically change the paramteters…, why not NW just use single PxSCH scheduling?Q3: We agree with Samsung -- first need to conclude on whether to support multi-slot PXSCH scheduling. If the results are to be captured, the comparison baseline should be reasonable chosen and explained in the TR. |
| **LG** | It should be discussed after 3.1.1 Q3: Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | Same as discussion in 3.2, we see benefits in the listed proposals but we need to first conclude on the support of multi-PDSCHs/PUSCHs scheduling before diving into the details. |
| **vivo** | Q1: If multi-PDSCH scheduling is considered for XR, the proposed enhancement in proposal 3-3-1 can be considered, since they can provide more flexibility of scheduling for multi-PDSCH transmission. Besides, capacity gain can be achieved based on our simulation results.Q2: For proposal 3-3-2, it seems the proposed enhancement is addressing power saving rather than capacity improvement. Maybe it is more proper to discuss whether it is beneficial or not for power saving in agenda 9.10.1. Regarding Proposal 3-3-3, from our perspective, there is no need for considering repetition due to that coverage issue is not the focus of this agenda. |
| **Ericsson** | Q1: OK to prioritized.Q2: * On 3-3-1, as proponet, we are supportive. But, as mentioned earlier, we are OK to enable support of multi-PxSCH “as it is”, that is without enhancements to FR1/FR2-1. The capacity gain, if any, is limited for any enhancement and we should be consistent in our decisions. Therefore, we stay neutral regarding this enhancement.
* On 3-3-2: We don’t support. No capacity gain is shown, and intuitively, it seems to be more a power saving feature than capacity improvement,
* On 3-3-3: We don’t support. NW can already switch using single slot on multi-slot DCI. Repetition is also can be dynamically indicated. It is not clear to use the gain that the proposed enhancement offers.
 |
| **InterDigital** | Support proposal 3-3-1 and Moderator’s recommendation. Using flexible parameters for the different PxSCHs results in better alignment with the XR traffic and matches with the flexibility of DG minus the high PDCCH overhead. |
| **OPPO** | Q1/Q2: We think there is no need to further enhance the multi-PxSCH scheduling. |
| **Lenovo** | The proposals need to be updated to clearly indicate whether they are needed for the extension from FR2-2 to FR1/FR2.Proposal 3-3-2 may not much needed for FR2-2?Proposal 3-3-3 if only applicable to FR2-2, assuming channel conditions do not change much across TBs, may not be needed. |
| **Huawei/HiSilicon** | Q1-Q3: Suggest to first conclude on the support of multi-PXSCH. Then, performance gain should be given before we further discuss the topic. |
| **Nokia, NSB** | The enhancement in Proposal 3-3-1 needs to be further studied to see whether the gains from flexible parameters can motivate the considerable DCI overhead. Proposal 3-3-2 seems more for power saving not fo capacity thus the motivation to further study is not clear. Enhancements in Proposal 3-3-3 are mainly seen important for the uplink where repetition may sometimes be needed due to potential uplink coverage challenges. |
| **Intel** | Q1-Q2: Open to consider if there is performance gain Q3: Results showing meaningful capacity gain with reasonable/practical assumptions should be captured |
| **Qualcomm** | Similar to our reasoning above for the previous two questions. We think enhancements for multi-PXSCHs are useful.  |

### 3.3.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P3-3-1 | **Companies (2):**IDC, QC | **Companies (7):**Samsung, FW, CATT, MTK, OPPO, Nokia/NSB, Lenovo | **Companies (5):**[Ericsson], LG, Google, vivo, Intel |
| P3-3-2 | **Companies (1):**QC | **Companies (7):**FW, CATT, vivo, OPPO, Nokia/NSB, Lenovo, Ericsson | **Companies (5):**Samsung, MTK, LG, Google, Intel |
| P3-3-3 | **Companies (1):**QC | **Companies (8):**Samsung, FW, CATT, MTK, vivo, Ericsson, OPPO, Lenovo | **Companies (4):**LG, Google, Nokia/NSB, Intel |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Continue discussion for the 2nd round**
	+ **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
	+ **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## SR and/or BSR enhancements

The Table I in section 3.4 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (9):** **Huawei/HiSilicon\*, Vivo\*, CATT\*, ZTE\*, TCL, Apple, Ericsson, LG, InterDigitial**
* **Companies with evaluation results (4):** **Huawei/HiSilicon\*, Vivo\*, CATT\*, ZTE\***

**High-level observations:**

* Study enhanced BSR mechanisms for capacity improvement of XR traffic.
	+ Support: Vivo\*, CATT\*, ZTE\*, Ericsson, LG, InterDigital
* **Study multi-bits SR for XR traffic for capacity improvement of XR traffic.**
	+ **Support:** Huawei/HiSilicon\*, Apple, TCL. LG
	+ **Not Support:** Ericsson
* On multi-bits enhancements, additional discussion is needed regarding the concerns raised by opponents.

### 3.4.1 First round of Discussion

**High level proposals based on input contributions:**

* Proposal 3-4-1: It is beneficial to study enhanced BSR mechanisms for capacity improvement of XR traffic.
	+ Support: Vivo\*, CATT\*, ZTE\*, Ericsson, LG, InterDigital
* Proposal 3-4-2: It is beneficial to study multi-bits SR mechanisms for capacity improvement of XR traffic.
	+ **Support:** Huawei/HiSilicon\*, Apple, TCL. LG
	+ **Not Support:** Ericsson

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 3-4-1 and Proposal 3-4-2, and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
	+ **Moderator recommends endorsing** Proposal 3-4-1.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q2: Suggest to leave conclusions to RAN2 – this is outside the RAN1 role/expertise. RAN2 is aware of the topics, they were discussed in the previous RAN2 meeting, and there are RAN2 Tdocs with relevant proposals for this meeting.  |
| **Futurewei** | Q1: BSR enhancement should be discussed in RAN2. About multi-bits SR (proposal 3-4-2), it can be beneficial to indicate from the UE to the gNB the UL traffic information in a timely manner via multi-bits SR.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: The performance results with BSR enhancement had been shown. The final BSR enhancement would be determined by RAN2Q2: Multi-bit BSR would be decided by RAN2 |
| **MTK** | Q1-Q2: (Same view as Samsung) Suggest to leave conclusions to RAN2 – this is outside the RAN1 role/expertise. RAN2 is aware of the topics, they were discussed in the previous RAN2 meeting, and there are RAN2 Tdocs with relevant proposals for this meeting. |
| **ZTE, Sanechips** | Support Proposal 3-4-1 and Proposal 3-4-2. |
| **LG** | Q1: the necessity seems clear since most of proposals assumes gNB knows UE traffic characteristic. SR can support responsive indication from UE side, with simplified information. BSR would have larger information size to indicate detailed traffic property for further scheduling. We think both can be kept in RAN1 and proposal 3-4-2 may need to be discussed in RAN2 first. Q2: Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | We also suggest to leave this topic to RAN2 |
| **vivo** | **Q1:** BSR enhancement can be recommended for XR capacity improvement and the detailed designed can be handled by RAN2.With enhanced BSR report, we don’t see the need for multi-bits SR. |
| **Ericsson** | Q1: Support, but also OK with other companies’ suggestions that record the results. But we also would like to record our concerns, as explained in contribution on multi-bit SR that we are not supportive.Q2: We support 3-4-1 and do not support 3-4-2. |
| **Sony** | Q1-Q2: We support 3-4-1. But, this topic should be lead by RAN2. RAN1 provides comments if there are any requests from RAN2. |
| **InterDigital** | Support Proposal 3-4-1 and moderator’s recommendation. The details/design of enhanced BSR can be handled by RAN2  |
| **OPPO** | Q1: BSR should be discussed in RAN2. We are open to proposal 3-4-2 if performance gain is shown by multi-bits SR. |
| **Lenovo** | BSR enhancements should be discussed in RAN2. We don’t see the need for SR enhancements, e.g. multi-bit SR. The concept of multi-bit SR was already discussed in the beginning of Rel-15. However instead of introducing a multi-bit SR it was concluded to introduce different SR configurations. The current NR scheme, i.e. mapping of LCHs to SR configurations, allows UE to indicate some traffic related information to gNB with a single-bit SR. |
| Huawei/HiSilicon | Q1: For Proposal 3-4-1, although BSR enhancement is RAN2’s impact, RAN1 can evaluate BSR enhancement to show the capacity gain. For Proposal 3-4-2, SR enhancement can be considered since SR has RAN1’s impact. And according to our simulation results, it is beneficial to study multi-bits SR mechanisms for capacity improvement of XR traffic.Q2: The proposed SR/BSR enhancements should be captured in TR 38.835. Our simulation results show that UE indicating the gNB of the data arrival time can improve the XR capacity. |
| Nokia, NSB | Q1: We agree that BSR enhancements are beneficial for XR use cases. Details of BSR enhancements shall be directed to RAN2. RAN1 shall focus on RAN1 part and prioritize it given the limited time left for this SI.We do not support Proposal 3-4-2. The numerical results of Pre-Scheduling DG and CG already showed the capacity close to Genie (when gNB aware about the precise traffic arrival and packet size). Therefore, the challenges coming from changing the SR design are not justified. |
| **Intel** | Q1-Q2: Suggest to leave conclusions to RAN2 – this is outside the RAN1 role/expertise. |
| Qualcomm | Ok to consider BSR enhancements; we think BSR enhancements should be discussed in RAN2. Same comment for SR enhancements. Note that in the past RAN1 meeting the following agreement was made:  Agreement: Whether/how to enhance BSR to improve capacity performance of XR traffic is within RAN2 scope and is not handled by RAN1. Note that companies should indicate if and what BSR enhancement is assumed in their RAN1 proposals on CG and DG enhancements. RAN1 can evaluate BSR enhancement to improve capacity performance  |

### 3.4.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P3-4-1 | **Companies (2):**ZTE, LG |   | **Companies (12):**Impacts RAN2:Samsung, FW, MTK, vivo, Ericsson, Sony, IDC, OPPO, Lenovo, HW/HiSi, Nokia/NSB, Intel, QC |
| P3-4-2 | **Companies (4):**FW, ZTE, LG, HW/HiSi | **Companies (4):**vivo, Ericsson, Lenovo, Nokia/NSB | **Companies (6):**Impacts RAN2:Samsung, CATT, MTK, OPPO, Intel, QC |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **On Proposal 3-4-1:**
	+ **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**
* **On Proposal 3-4-2:**
	+ **Continue discussion for the 2nd round**
		- **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
		- **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
		- **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## Other enhancements

The Table G in section 3.5 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Selection of few additional proposed enhancements:**

* **Introduce XR-dedicated PDCCH monitoring window (XR-PMW) for DL/UL that is monitored irrespective of DRX ON/OFF**
	+ Support: CATT\* (with simulation results)
* **Introduce XR-specific *playoutDelayForMediaStartup* for XR awareness scheduling**
	+ Support: CATT\* (with simulation results)
* **Proposal 7: Study if PHR should be further enhanced based on XR traffic arrival periodicity or UL pose periodicity.**
	+ Support: Lenovo
* ***Study mechanism of packet dropping based on the PDB requirement, in order to avoid resource waste due to the out-of-date packets.***
	+ Support: NEC
* ***Proposal 2: Under CA with different TDD patterns, data retransmission can take place on the carrier different from its initial transmission.***
	+ Support: MediTek
* **Proposal 3: Consider mechanisms to satisfy the PDB in the sub-6 GHz NR (TDD) bands such as enabling HARQ retransmission of a TB on a different cell than the cell of the initial TB transmission.**
	+ Support: Samsung
* …..

### First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 3-5-1: Introduce XR-dedicated PDCCH monitoring window (XR-PMW) for DL/UL that is monitored irrespective of DRX ON/OFF**
	+ Support: CATT\* (with simulation results)
* **Proposal 3-5-2: Introduce XR-specific *playoutDelayForMediaStartup* for XR awareness scheduling**
	+ Support: CATT\* (with simulation results)
* **Proposal 3-5-3: Study if PHR should be further enhanced based on XR traffic arrival periodicity or UL pose periodicity.**
	+ Support: Lenovo
* **Proposal 3-5-4: Study mechanism of packet dropping based on the PDB requirement, in order to avoid resource waste due to the out-of-date packets.**
	+ Support: NEC
* **Proposal 3-5-5: Under CA with different TDD patterns, data retransmission can take place on the carrier different from its initial transmission.**
	+ Support: MediTek
* **Proposal 3-5-6: Consider mechanisms to satisfy the PDB in the sub-6 GHz NR (TDD) bands such as enabling HARQ retransmission of a TB on a different cell than the cell of the initial TB transmission.**
	+ Support: Samsung
* …..

**Moderator’s comments:**

* **Moderator recommends prioritizing Proposal 3-5-1 and Proposal 3-5-2, due to availability of simulation results.**
	+ **Proponent (CATT) is kindly requested to provide clarifications regarding following comments:**
		- **Proposal 3-5-1:** SU-MIMO is used as baseline, but MU-MIMO is used for enhancement schemes. It is not clear if the capacity gain due to MU-MIMO. CATT RAN1#109-e R1-2206385 shows with MU-MIMO as baseline, there is no capacity gain for enhancements but power saving gain.
		- **Proposal 3-5-2:** The proposed enhancements seem to be higher layers. Is the RAN1 design part related to Proposal 5 in the contribution?

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 3-5-1 to Proposal 3-5-6, and the necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
	+ **Moderator recommends prioritizing Proposal 3-5-1 and Proposal 3-5-2.**
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q3: A general comment is that simulation results should not be the only criterion to consider proposals particularly as, even for proposals with simulation results from more than one company, there has been no discussion/agreement/calibration on simulation assumptions for a particular scheme nor on its relevance.Many proposals do not require new simulations. For example, it should be clear that it is beneficial for capacity that a gNB has an up-to-date CSI report in order to schedule a UE when the UE enters Active Time and that CSI report should not be provided ~5 msec later. That was OK for eMBB, it is not OK for XR. Similar with beam management, particularly given that FR2 would be a main deployment scenario for XR given the BW availability (and unavailability in FR1) – it is not possible for a UE to enter Active Time with a poor beam. Asking for simulation results for the above is proactically equivalent to saying that CSI reporting or beam management are unnecessary. Some of the proposals, e.g. 3-5-2/3-5-4, fall under RAN2’s expertise. Proposals 3-5-5 and 3-5-6 are probably the same proposal and aim for a structural mechanism for latency reduction – no simulation results are needed – any tradeoffs can be fully determined by analysis. |
| **Futurewei** | Q1: 3-5-2 / 3-5-4 seems to be RAN2 issue and without RAN1 impact. For 3-5-3It is yet to see how and how much 3-5-3 can improve XR capacity. Are 3-5-5 and 3-5-6 similar proposals? There is potential benefit of cross-carrier/cell HARQ to reduce latency and hence improve capacity. About 3-5-1, similar question as the moderator. In addition, we do not see how the proposed scheme can do better than DG.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | **Q1:** For 3-5-1, the XR-PMW scheme has the benefit of gNB pairing in the optimization of the MU-MIMO performance comparing to normal MU-MIMO scheme. We showed about similar performance of XR-PMW with MU-MIMO comparing to dynamic grant with MU-MIMO. However, we followed RAN1 agreements using SU-MIMO as the baseline. For 3-5-2, the XR-specific playoutDelayForMediaStartup for XR awareness scheduling is the de-jitter techniques at gNB scheduler. The gNB obtains the playoutDelayFor MediaStartup from UE XR application layer via RRC. However, the de-jitter techniques of gNB scheduler is for physical layer to measure the delay jitter at the gNB and dynamic adapt the gNB scheduling algorithm based on the measured delay jitter to optimize link adaptation gain. RAN1 impacts of the proposed scheme is to collect the statistic of XR packet arrival in delay and delay jitter along with UE’s CSI feedback for scheduler to optimize the system performance with the system performance gain from 25.8% - 103.6%. **Q2:** The system performance gain is the strong evidence and the results should be captured in the TR. The results and system performance gain had been clearly analyzed in the contribution. Companies are welcomed to verify the results.  |
| **MTK** | Q1: * 3-5-2 /3-5-4 seems to be RAN2 issue and without RAN1 impact.
* It is yet to see how and how much 3-5-3 can improve XR capacity.
* About 3-5-5 and 3-5-6, there is potential benefit of cross-carrier/cell HARQ to reduce latency and hence improve capacity, and we urge companies to take a look.
* About 3-5-1, we think the table 1 from CATT can use 16.67 ms CDRX period as baseline, similar to table 3 from CATT; at the same time, it would be more certain about the capacity gain if more than one companies can provide input/evaluation.

Q2: We think results can be captured with evaluation assumption clear explained in the TR. |
| **LG** | **Q1:** 3-5-1/2/3 seems releated to RAN2. 3-5-4 are related to SR/BSR enhancement. For 3-5-5/6, we see an amount of specification impact comparing expected benefits. **Q2:** Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | 3-5-2 and 3-5-4 are RAN2 topics. 3-5-5 and 3-5-6 are very similar and have the potential to improve latency and reliability by giving more flexibility for HARQ retransmissions in TDD mode.  |
| **vivo** | Q1: Proposal 3-5-2 and 3-5-4 are related to XR-awareness which is handled by RAN2.It seems proposal 3-5-1 is addressing power issue rather than capacity. Maybe it needs more clarifications. To ensure the capacity, sufficient long on duration needs to be configured for DRX, e.g., to cover the jitter range. It is not clear that how the proposed enhancement in proposal 3-5-1 benefit for capacity improvement.For proposal 3-5-3, 3-5-5 and 3-5-6, the performance gain on XR capacity needs to be clarified by evaluation results, according to the agreements. |
| **Ericsson** | Q1: * Proposal 3-5-1: Consideirng CATT clairfcaiton, we see the enhancement as a power saving feature, and not capacity gain. Hence, for this agenda, we are not supportive of the proposal.
* Proposal 3-5-2: Considering CATt clarification, the RAN1 related procedures is about CSI measurement. So, the question is whether this part (CSI measurement) should be handled differently? We are fine to capture this feature in TR as a scheme that shows how XR awareness is used (higher layer aspects). But it seems there is no RAN1 impact. Feedback from CATT is appreciated.

Q2:* Proposal 3-5-3: Similar to FW, it is not clear to us the necessity and benefit of the feature. So, we cant support this proposal.
* Proposal 3-5-4: We agree with others that the impact is on higher layers. What RAN1 can do is to study performance evaluation results (like other schemes, for example CATT). Due to lack of performance evaluation, the need to disucs sin RAN1 is not clear.
* Proposal 3-5-5/3-5-6: We agree with others that these two proposals can be merged. Our view is that although technically, this feature would be beneficial, we think it has considerable impact on RAN2, as well as current implementations, also at NW side. That’s why we are hesitant at this stage.
 |
| **Nokia, NSB** | We do not support Proposal 3-5-1 to 3-5-6. Proposals 3-5-3 to 3-5-6 does not have simulation results and justification that the enhancements are needed.Proposal 3-5-1 shows worse results if we compare MU-MIMO without and MU-MIMO with enhancements.Proposal 3-5-2 does not seem to have a RAN1 impact. |
| **Qualcomm** | Agree with other companies that 3-5-2 / 3-5-3/ 3-5-4 may be better discussed in RAN2. In regards to 3-5-5 and 3-5-6 it would be good if the supporting companies can provide simulation results that prove benefit. All proposals should be treated similarly when it comes to their consideration with or without simulation results.  |

### 3.5.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P3-5-1 | **Companies (1):**CATT | **Companies (3):**LG, Ericsson, Nokia/NSB | **Companies (3):**FW, MTK, vivo |
| P3-5-2 | **Companies (1):**CATT | **Companies (8):**Samsung, FW, MTK, LG, Google, vivo, QC, Nokia/NSB | **Companies (1):**Ericsson |
| P3-5-3 |   | **Companies (5):**LG, vivo, Ericsson, Nokia/NSB, QC | **Companies (2):**FW, MTK |
| P3-5-4 |   | **Companies (9):**Samsung, FW, MTK, LG, Google, vivo, Ericsson, QC, Nokia/NSB |   |
| P3-5-5/P3-5-6 | **Companies (4):**Samsung, FW, MTK, Google | **Companies (5):**LG, vivo, Ericsson, Nokia/NSB, QC |   |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Proposal 3-5-1 and P3-5-2:**
	+ **CATT, as the only proponet is requested to provide feedback and discuss for the 2nd round, including clarification on RAN1 spec impact regarding P3-5-2 :**
		- **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
		- **If no consensus is achieved by the ends of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
		- **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**
* **Proposal 3-5-3 and Proposal 3-5-4:**
	+ **Down-priorotize these proposals and close the discussion.**
* **Proposal 3-5-5/6:**
	+ **Proponets are requested to provide feedback and discuss for the 2nd round, and share the plans for providing simulatin results, if any.**
		- **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

# 4 Other capacity enhancements

The followings are agreed/concluded previously:

|  |
| --- |
| **Agreement:**The following lists the candidate enhancements techniques for link adaptation to improve XR capacity that are proposed by companies RAN1#109-e. * At least the proponents are encouraged to justify the corresponding capacity benefits for XR traffic for considering potential study of these candidate enhancements techniques.
	+ Delta MCS
	+ Soft HARQ-ACK feedback
	+ Cooperative MIMO scheme via precoding technique - bi-directional training
	+ Enhanced link adaptation for CBG-based transmission
	+ CSI report enhancements to address the different BLER requirements of different XR flows
* Follow the *common principle for assessment of the candidate capacity enhancement technique.*

**Agreement:**The following lists the candidate enhancements techniques based on measurement-gap link to improve XR capacity that are proposed by companies RAN1#109-e. * At least the proponents are encouraged to justify the corresponding capacity benefits for XR traffic for considering potential study of these candidate enhancements techniques.
	+ Dynamic L1 based MG activation/deactivation.
	+ Reuse current R16/R17 RRM relaxation condition to allow scheduling in MG to transform the R16/R17 RRM power saving gain into capacity gain.
* Follow the *common principle for assessment of the candidate capacity enhancement technique.*

**Agreement:**The following lists the candidate enhancements techniques to improve XR capacity that are proposed by companies RAN1#109-e. * At least the proponents are encouraged to justify the corresponding capacity benefits for XR traffic for considering potential study of these candidate enhancements techniques.
	+ Inter-UE/intra-UE multiplexing techniques, including e.g. finer granularity preemption indication
* Follow the *common principle for assessment of the candidate capacity enhancement technique.*

**Agreement:*** Deprioritize the study of CQI report for different BLER and/or different XR traffic to improve XR capacity performance.

**Agreement:*** Deprioritize the study of intra/inter UE prioritization/multiplexing enhancements to improve XR capacity performance.
 |

The views regarding these enhancements for serving XR traffic are summarized and discussed in the following sections.

## 4.1 Delta MCS and Soft HARQ-ACK feedback

The Table K in section 4.1 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (8):** Qualcomm\*, Apple, Nokia/NSB, MediaTek, Futurewei, Ericsson, Samsung, LG
	+ **Supportive ([3])**: Qualcomm\*, Apple, [Nokia/NSB]
	+ **Not supportive (5):** MediaTek, Futurewei, Ericsson, Samsung, LG
* **Capacity performance results (2):** Futurewei, Qualcomm

### 4.1.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 4-1-1: Support of soft HARQ-ACK for capacity enhancement of XR capacity.**

**Moderator’s observation:**

* The proponent (QC) has provided extensive simulation results, showing large capacity gain.
* The opponent, Futurewei has also provided evaluation results showing capacity loss.
	+ Discussion is needed to understand the reason for difference.
* Other companies than Apple/QC are not supportive of this enhancement.
* The proposal can be discussed to address the comments and issues for the initial round of discussions.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 4-1-1, necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q3: That is another case where simulation results from proponents show (large) gains while it is already known from Rel-17 that such gains are questionable (if any), the requirements to achieve them are unrealistic, and the schemes are not testable as everything is up to UE implementation. |
| **Futurewei** | Q1: Our simulation follows strictly the agreed assumption baseline and we explained in our contribution why no gain is observed. Therefore, we do not see the benefit of the proposal and still have the similar questions since R17 discussion.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: Both capacity gain and lose had been shown. We need to understand how the gain is obtained before we could further discuss this proposal. Q2: All results should be captured. |
| **MTK** | Q1: Tend to agree with Samsung. To our understanding this discussion also happens in R17 URLLC and it seems hard to achieve consensus.Q2: We think results can be captured with evaluation assumption clearly explained in the TR, e.g., how the soft values are derived. |
| **ZTE, Sanechips** | Support Proposal 4-4-1. |
| **LG** | **Q1: Not support.** It is already known that the performance gains are totally UE implementation specific, and as Futurewei mentioned, the requirement is also quite high. It is hard to say that the feature would be benefial for the sysyem in the practical situation. **Q2:** Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | We don’t support Proposal 4-4-1. This proposal has been discussed an exhausted in Rel-17 URLLC with no convergence.  |
| **vivo** | Q1: The proposed enhancement in proposal 4-1-1 has been discussed in R17 URLLC session. The main concern is the impact on UE complexity and processing time. It seems the situation is not changed much since then. So we suggest proposal 4-1-1 is deprioritized for XR capacity.Q2: We think the proposed enhancements with evaluation results, especially those showing potential performance gain, can be captured in the TR. Necessary clarification if any can be included. Whether and how to draw observation and conclusion based on the captured techiques and evaluation results can be discussed separately. |
| **Ericsson** | Q1: We believe the main difficulty in Rel-17 (that still exists), is that both measures are relative, and that UE has no knowledge of what target BLER the gNB aimed for which means that a reference point (BLER) is needed. Since companies did not manage to agree on a new reference point and the details of these schemes in Rel-17, we believe there is no hope that this will change in Rel-18. Also considering FW’s feedback, we think we should down-prioritze this topic.   |
| **Nokia, NSB** | We suggest having enhancements in Proposal 4-1-1 compared against CBG-based HARQ transmission cases. We are also fine to deprioritize Proposal 4-1-1 in Rel-18. |
| **Qualcomm** | Q1: our evaluations have followed the agreed evaluation methodologies. We also explained in our contribution text why the proposed solution has capacity gain for the latency stringent XR traffic. Q2: yes, evaluation results should be captured in TR 38.835 if they follow evaluation methodologies.  |

### 4.1.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P4-1-1 | **Companies (3):**QC, Apple, ZTE | **Companies (8):**Samsung, FW, MTK, LG, Google, vivo, Ericsson, [Nokia/NSB] | **Companies (2):**CATT, [Nokia/NSB] |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
* **If no consensus is achieved by the end of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
* **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 4.2 Cooperative MIMO scheme via precoding technique

The Table L in section 4.2 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (2):** Futurewei\*, Ericsson
	+ **Supportive**: Futurewei\*
	+ **Not supportive:** Ericsson (in XR, OK in MIMO)
* **Capacity performance results (1):** Futurewei\*

### 4.2.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 4-2-1: *Cooperative MIMO via DL interference probing based on SRS enhancements to improve XR system capacity for TDD* is beneficial.**

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 4-2-1, necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q3: It is not realistic to consider the proposal in XR.  |
| **Futurewei** | Q1: we’ve provided extensive simulation results, analysis, and description of the proposal. Significant benefits of XR capacity gain are shown. The scheme should be considered for XR capacity improvement.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: The synchronization of data, the transmission state, and HARQ among TRPs is the most challenged issue in the proposed scheme. The proposed scheme coud be used for any traffic data and not limited to XR. Q2: All results should be captured.  |
| **MTK** | Q1: The capacity gain seems good but only reported by one company and not sure whether it is specific to XR. We would be open to consider this enhancement if majority of companies think so.Q2: The results can be captured with evaluation assumptions clearly explained in the TR. |
| **LG** | We think it can be considered as an issue of general MIMO discussion. We don’t think this issue is not XR specific issue.  |
| **Google** | This propsal is not addressing an XR pseicifc limitation and it s generic to any type of data. Not sure if it should be discussed under XR AI. |
| **vivo** | Q1: The proposed enhancement in proposal 4-2-1 should be discussed in MIMO session. Besides, Proposal 4-2-1 is not addressing an XR specific issue based on our understanding.Q2: See the reply in section 4.1.1. |
| **Ericsson** | Q1. We are fine to report this results in TR. Indeed high capacity gain is shown. As we mentioned previously, our concern is more on logistics if this enhancement is to be treated in XR WI where needs the expertise in MIMO.  |
| **InterDigital** | Same view as Google. We no not see how this enhancement is best suited for addressing only XR-specific issues. |
| **Nokia, NSB** | Defer MIMO enhancements to the dedicated 3GPP MIMO item. |

### 4.2.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P4-2-1 | **Companies (1):**FW | **Companies (8):**Samsung, CATT, LG, Google, vivo, Ericsson, IDC, Nokia/NSB |   |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
* **If no consensus is achieved by the end of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
* **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 4.3 Enhanced CQI based on CBG or DMRS

The Table M in section 4.3 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (4):** Nokia/NSB\*, Ericsson\*, Futurewei
	+ **Supportive eCQI based CBG (1)**: Nokia/NSB
		- **Not supportive (3):** Futurewei, Ericsson
	+ **Supportive eCQI based DMRS (1)**: Ericsson\* (new simulation results)
* **Capacity performance results (1):** Nokia/NSB\*, Ericsson\*

### 4.3.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 4-3-1: Enhanced CQI based on CBG transmission improves the link adaptation and is beneficial for improving XR capacity performance.**

* **Proposal 4-3-2: DMRS based CQI improves the link adaptation and is beneficial for improving XR capacity performance.**

**Moderator’s observation:**

* eCQI based CBG:
	+ Both Nokia and Ericsosn have provided extensive analysis and evaluations on eCQI based CBG where have different views. Futurewei as well provided views on this enhancements.
	+ Moderator recommends companies review the input contributions and discuss.
* eCQI based DMRS:
	+ Ericsson has provided extensive analysis and simulation results for this enhancements. It seems the analysis and evaluations jointly covers the eCQI based CBG.
	+ Moderator recommends companies review the input contributions and discuss.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on direction of Proposal 4-3-1 and Proposal 4-3-2, necessity/benefit of the proposed enhancements? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q3: DMRS-based CQI has been considered under MIMO over many releases (going back to LTE) and was not agreed. There are several reasons for that and it is not realistic to re-consider under XR. For CBG-based CQI, unless different CBGs correspond to different QoS flows, TB-based CQI is fundamentally preferable. If different CBGs correspond to different QoS, the DCI format design needs to be discussed together with any benefit over using separate DCIs for separate QoS flows. In our opinion, no further consideration is justified for either proposal.  |
| **Futurewei** | Q1: These proposals were discussed in previous releases extensively. It is preferred not to re-discuss again.Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: We should not re-open the issue dropped in MIMO session. Q2: All results should be captured.  |
| **MTK** | Q1: The capacity gain seems good but only reported by one company. We would be open to consider this enhancement if majority of companies think so.Q2: The results can be captured with evaluation assumptions clearly explained in the TR. |
| **ZTE, Sanechips** | We are open to the Proposal 4-3-1 and Proposal 4-3-2 |
| **LG** | **Q1:** We share views from Samsung and Futurewei. We also think gNB can consider CBG even with existing CQI.**Q2:** Same as others. With repect to companies’ effort, we are fine to capture proposals when the performance has been shown or can be clearly expected. We think the same principle can be applied for all of the proposal. |
| **Google** | With the large UL/DL video packets in XR, the use of CBG is very important to improve the system capacity. Also, enhancements to the CBG mechanisms are needed. CBG-based CQI reporting could be further studied.  |
| **vivo** | Q1: We think proposal 4-3-1 and 4-3-2 should be deprioritized for XR capacity study.For proposal 4-3-1, the benefit of CBG based transmission with CBG based CQI reporting compared to TB based retransmission with legacy subband CQI reporting (at most 4 bits) is not clear, while it may burden UE with more complexity and computation.For proposal 4-3-2, it is showed that with 90% target BLER where there will be high probability for retransmission, DMRS-based CSI reporting with HARQ-ACK (if not impact the latency) may be useful. However, if target BLER is typically set as 10%, then there will be no more than 10% retransmission. UE needs to measure CSI based on DMRS with high probability. When considering the increased latency to generate CQI based on DMRS, the beneifit will be vanished due to the short PDB of XR traffic. Meanwhile, this also causes increased UE power consumption.Q2: Same reply as section 4.1.1 |
| **Ericsson** | Q1: We are not supportive of 4-3-1. As proponets, we are supportive of 4-3-2. Based on the input contribution (Nokia), we would like to provide few feedbacks:* Regarding eCQI based CBG, it is important to see as baseline the performance of legacy CBG (only TB based is provided).
* We would like to know the assumption on target BLER and OL.
* In Nokia’s contribution when SINR distribution for CBG and TB are shown (Figure 1), the difference in SINR for the CB difference is (6-7 dB), but for CBG is **maximum 1 dB** as Nokia shows. To us, this means that some CBs in the CBG has good quality while other has worse. So even if VRBs is not used (not clear for us if it is used in Nokia’s result) it will be rather lucky that frequency selective interference happen such that CBs that suffer all belongs to same CBGs while other CBs in other CBGs succeed.
* We explained in our contribution that the reason why CBG-based re-transmissions only give a small capacity improvement compared to TB-based is due to that error curves versus SINR are “knee-like”. Only a small change in SINR can change BLEP from close to 1 to 1e-5.
	+ This further has the consequence that for almost all transmissions either all CBGs are successfully decoded or none of the CBGs could be correctly decoded. In fact, for less than 3% for InH (6% for Uma) of the transmissions, the number of in-correctly decoded CBGs is different from 0 and $n\_{CBG}$.
	+ This means that the occasions where CBG-based re-transmission can reduce the resource consumption compared to TB-based re-transmission are rather rare for the InH and UMa scenarios.
 |
| **InterDigital** | We are open for discussing Proposal 4-3-1 |
| **Nokia, NSB** | Q1: We support Proposal 4-3-1 as we have shown capacity improvements while using CBG-based transmission with an enhanced CQI scheme compared to TB-based and legacy CQI scheme. We have also introduced the specification impact of the enhanced CQI scheme (mainly on 3GPP TS 38.214 clause 5.2.2.1). We believe that it is necessary to update the current CQI determination mechanism to fit better with CBG based transmission. Specifically, for the XR use cases, most of the times full bandwidth is allocated for one UE and due to large channel fading variation among the code blocks, there is a need for an enhancement that takes this variations and unequal CB (and CBG) error probabilities into account. From the Ericsson tdoc, it seems that i.i.d. errors of CBGs are assumed (?), while our sim results show that CBG errors actually vary within one TB. Regarding Proposal 4-3-2, our understanding is that the DMRS based CQI can only happen when there is a PDSCH transmission. This would result in a periodicity of 16.7 ms for a typical XR UE which could lead to outdated channel measurement data.Q2: Yes, we support capturing the results and related observations to TR 38.835. |
| **Qualcomm** | Similar to other companies views prefer not to reconsider. |

### 4.3.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P4-3-1 | **Companies (4):**Google, Nokia/NSB, IDC, ZTE | **Companies (8):**Samsung, FW, CATT, LG, vivo, Ericsson, MTK, QC |   |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions.**
* **If no consensus is achieved by the end of 2nd round for any of these proposals, down-priorotize the proposed technique for further study.**
* **Capture the description of proposed enhancements techniques with corresponding simulation results, if available, and key assumptions and findings, in this meeting.**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

## 4.4 Enhancements based Measurement gap

The Table N in section 4.4 of R1-2214010 lists short descriptions, and the proposals and observations in the contributions submitted in this meeting. For more detailed descriptions and discussions please refer to the corresponding companies’ contributions.

**Status of inputs in the contributions:**

* **Companies with view (5):** Qualcomm, Nokia/NSB\*, MediaTek\*, Futurewei, Ericsson
	+ **Supportive ([4])**: Qualcomm, Nokia/NSB\*, MediaTek\*
	+ **Not supportive (1):** Futurewei, Ericsson
* **Capacity performance results (2):** Nokia/NSB\*, MediaTek\*

### 4.4.1 First round of Discussion

**High level proposals based on input contributions:**

* **Proposal 4-4-1: Support enhancements on RRM to relax scheduling restcition during MG**
	+ **Proposal (Nokia):** The UE-to-gNB signaling to make the gNB scheduler aware of when s-MeasureConfig induced scheduling restrictions apply could be realized with higher-layer signaling such MAC CE or RRC signaling. RAN2 shall be asked for further guidance.
	+ **Proposal (Nokia):** For UEs configured with inter-frequency measurement gaps, solutions where the gNB can signal the UE to skip a measurement gap (to avoid scheduling restrictions) shall be captured in the TR. The gNB-2-UE signaling for this may be realized via a compact DCI format to have fast signaling
	+ **Proposal (MTK):** Support a more dynamic DCI/MAC-CE based MG activation/deactivation or MG setting (including duration and period) change for XR capacity enhancement**.**
	+ **Proposal (QC):** MG should be enhanced by handling the priority of data packets or dynamically activating/deactivating the MG occasions from gNB.

**Moderator’s observation and suggestions for discussions:**

* Enhancements of scheduling restriction due to RRM is proposed by Nokia/NSB and MTK and Qualcomm.The proponents provided extensive analysis and performance evaluation results.
* Two companies (Futurewei and Ericsson) have raised concern on the applicability of scenarios and impact on other WGs.
* Moderator suggests using the initial discuss to address the concern raised by opponents.

**Moderator’s suggestion for First round of Discussions:**

* **Q1:** What is your view on necessity/benefit of the proposed enhancements under **Proposal 4-4-1** for **scheduling restrictions based on RRM**? Please note that based on your feedbacks, the proposals can be updated with more details for the next round of the discussions.
* **Q2:** Discuss your view regarding the proposed enhancements and whether they should be captured in TR 38.835. If yes, feel free to provide suggestions on corresponding TPs.
* **Q3:** Discuss any clarification/correction/comment/question helping the discussion and needed decisions.

**Note: For discussions, please ensure the information provided in companies contributions are taken into account.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **Samsung** | Q1-Q2: We are supportive to discuss the applicable scenarios. Once that is concluded, it should be clear whether the proposal for scheduling restrictions based on RRM (or probably the reverse – i.e. skip RRM) is beneficial to support.  |
| **Futurewei** | Q1: it is intuitively understandable that with measurement gap the system performance degrades for any traffic including XR traffic and reusing some of the resource configured for MG can potentially bring back some of the performance loss. Note that dynamic indication may not always work for example when the XR data arrives during the MG. In addition, questions like the proper configuration of the MG, applicable scenarios, and the impact to RRM measurement need to be answered and RAN2 and RAN4 may need to get involved. Q2: In general, we think companies’ effort should be respected and captured when evaluations were performed according to the agreed simulation assumptions and the agreed common principles. It is better to have a consistent manner on whether/how to capture results with proper observation and conclusion than discussing each individual proposal/result separately. |
| **CATT** | Q1: This is more implementation issue than standard issue since the measurement gap and the XR resource allocations are controlled by the gNB. Q2: All results should be capatured.  |
| **MTK** | Q1: The simulation results from MTK/Nokia show evident capacity gain with MG/SMTC scheduling enhancement. QC also provides very nicely drawn figure to explain the issue. To us, this issue is worthy of an enhancement in the WI phase, since **this issue is XR-specific**, and the **capacity gain is evident**. As 5G NR is a mobile network, MG is always necessary under some mobility scenarios. Moreover, Nokia mentions SMTC scheduling restriction due to beam management which would also have strong impact on capacity for FR2. **If we want to support XR with mobile user or FR2 user, an enhancement to scheduling availability for MG/SMTC seems helpful.** * As for RAN2/RAN4 involvement, if RAN1 agrees on direction, it can be further discussed in RAN plenary when devising the WI description.

Q2: The restuls can be captured with evaluation assumptions clear explained in the TR. |
| **ZTE, Sanechips** | We are open to Proposal 4-4-1.  |
| **LG** | **Q1:** Fine to discuss in general. However, the trade-off should be identified and need to be answered by other WGs. For example, a contribution proposed that the trade-off is hand-over failure. Cosidering those performance degradation, RAN2 should be involded at least. Otherwise, it would be necessary to leave the issue to RAN2.  |
| **vivo** | Q1: We support to study the enhancements on RRM to relax scheduling restcition during MG. In our opinion, it is beneficial for both network capacity performance and UE power saving by dynamically skipping MG of UE.Q2: We think the proposed enhancements with evaluation results, especially those showing potential performance gain, can be captured in the TR. Necessary clarification if any can be included. Whether and how to draw observation and conclusion based on the captured techiques and evaluation results can be discussed separately. |
| **Ericsson** | Q1: In this case, showing capacity gain when one can use 6ms for scheduling is evident.However, as we mentione din our contributions, we have two main concerns: the applicability of the scenarios, and impact on other WGs. We appreciate if propoents provide feedback.  |
| **Lenovo** | It can be discussed how often such events/measurement occur in typical situations, and whether XR data transmission is important or e.g., inter-frequency measurement (e.g., for cell-edge UEs) also whether communication is restricted in all symbols or e.g., just within SSB symbols and 1 symbol before and after consecutive SSB symbols. RAN4 should be involved. |
| **Nokia, NSB** | We support Proposal 4-4-1. The benefit of having such enhancements is presented in our tdoc with performance results. Support that such enhancements are captured in the TR.We propose to modify the proposal to capture FR2 related restrictions:* **Proposal 4-4-1: Support enhancements on RRM to relax scheduling restcition for intra-frequency RRM without MGs and for inter-frequency RRM with MGs**

Q2: Yes, we support capturing the results and related observations to TR 38.835 |
| **Qualcomm** | We are supportive of studying this. |

### 4.4.2 Second round of Discussion

**Summary of 1st round of discussions:**

|  |  |
| --- | --- |
| **Proposal** | **Companies' preferences** |
| **Yes** | **No** | **Maybe/FFS** |
| P4-4-1 | **Companies (6):**MTK, ZTE, LG, vivo, Nokia/NSB, QC | **Companies (2):**FW?, CATT | **Companies (3):**Samsung, Ericsson, Lenovo |

**Moderator’s recommendation for discussion:**

**Moderator suggests the following.**

* **Companies are encouraged to review the 1st ruound of discussions and follow-up if more clairfications/questions are needed in the 2nd round of discussions. For example:**
	+ **Clarifcaitons on scenarios**
	+ **Impact on other WGs**
	+ **..**

**Note: For discussions, please ensure the information provided in companies contributions and previous round of discussion are considered.**

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

# 5 Others

Few enhancement topics were down-prioritized last meeting; however, companies proposed those enhancements at this meeting.

* SPS enhancements
* Intra-UE/Inter-UE prioritization.

Moderator have not treated those proposals. If proponents have concern, please use this section to share your view.

### First round of Discussions

Please share your views on the proposals that you prefer to be discussed. Please also use this section to share your view on any issue that needs to be discussed.

|  |  |
| --- | --- |
| Company | Comments |
| **ZTE, Sanechips** | **We prefer to discuss section 2.1.1 and section 3.1.1 firstly, which are the critical issues and have the widest interests and evaluation results. And of course it is the right way to provide some proposals for section 2.1.1 after collection of views of the 1st round.** |
| **Moderator** | Hopefully the plan for next phase addresses your preference. |
|  |  |
|  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | [**R1-2208377**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208377.zip) | XR Capacity Evaluation and Enhancements | FUTUREWEI |
| 2 | [**R1-2208402**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208402.zip) | Discussion on capacity enhancements for XR | Ericsson |
| 3 | [**R1-2208421**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208421.zip) | Discussion on XR-specific capacity enhancements techniques | Huawei, HiSilicon |
| 4 | [**R1-2208661**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208661.zip) | Discussion on XR specific capacity enhancements | vivo |
| 5 | [**R1-2208782**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208782.zip) | Discussion on XR specific capacity enhancement for NR | China Telecom |
| 6 | [**R1-2208863**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208863.zip) | Discussion on XR specific capacity enhancements techniques | OPPO |
| 7 | [**R1-2208953**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2208953.zip) | NR enhancement for XR capacity improvement | CATT |
| 8 | [**R1-2209000**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209000.zip) | XR-specific capacity enhancements techniques | TCL Communication Ltd. |
| 9 | [**R1-2209070**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209070.zip) | Discussion on XR specific capacity enhancement techniques | Intel Corporation |
| 10 | [**R1-2209113**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209113.zip) | Considerations on XR-specific capacity enhancements | Sony |
| 11 | [**R1-2209129**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209129.zip) | XR-specific Capacity Enhancement Techniques | Lenovo |
| 12 | [**R1-2209156**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209156.zip) | Discussion on XR-specific capacity enhancements | NEC |
| 13 | [**R1-2209198**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209198.zip) | XR specific capacity enhancements | ZTE, Sanechips |
| 14 | [**R1-2209355**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209355.zip) | Discussion on XR-specific capacity enhancements techniques | CMCC |
| 15 | [**R1-2209388**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209388.zip) | Discussion on XR capacity enhancement techniques  | Panasonic |
| 16 | [**R1-2209457**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209457.zip) | Discussion on XR-specific capacity enhancement techniques | LG Electronics |
| 17 | [**R1-2209518**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209518.zip) | On XR specific capacity improvement enhancements | MediaTek Inc. |
| 18 | [**R1-2209536**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209536.zip) | XR-specific capacity enhancements | Nokia, Nokia Shanghai Bell |
| 19 | [**R1-2209598**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209598.zip) | XR-specific capacity enhancements techniques | Apple |
| 20 | [**R1-2209620**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209620.zip) | Discussion on XR-specific capacity improvements | Rakuten Symphony |
| 21 | [**R1-2209642**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209642.zip) | On XR-specific capacity enhancements techniques | Google Inc. |
| 22 | [**R1-2209658**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209658.zip) | Discussion on XR-specific capacity enhancements techniques | InterDigital, Inc. |
| 23 | [**R1-2209749**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209749.zip) | Considerations on Capacity Improvements for XR | Samsung |
| 24 | [**R1-2209920**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2209920.zip) | Discussion on XR specific capacity improvement enhancements | NTT DOCOMO, INC. |
| 25 | [**R1-2210003**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_110b-e/Docs/R1-2210003.zip) | Capacity enhancement techniques for XR | Qualcomm Incorporated |