**3GPP TSG RAN WG1 #112bis-e R1-23xxxxx**

**e-Meeting, April 17th – April 26th, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **[DRAFT] CHANGE REQUEST** |
|  |
|  | **38.214** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on FDMed PDSCH reception |
|  |  |
| ***Source to WG:*** | Moderator (CMCC), Huawei, HiSilicon, Samsung, ZTE |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_MBS-Core |  | ***Date:*** | 2023-04-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | FDMed between unicast PDSCH and multicast PDSCH was supported in Rel-17, however the following restriction “For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to receive a PDSCH that overlaps in time with another PDSCH” is not consistent with RAN1 agreement. |
|  |  |
| ***Summary of change:*** | Add a condition that “if the UE is not capable of receiving FDMed unicast and multicast PDSCH per slot per caiier. |
|  |  |
| ***Consequences if not approved:*** | The FDMed unicast PDSCH and multicast PDSCH cannot be implemented. |
|  |  |
| ***Clauses affected:*** | 5.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 5.1 UE procedure for receiving the physical downlink shared channel

========================= Unchanged parts =========================

A UE shall upon detection of a PDCCH with a configured DCI format 1\_0, 1\_1, 4\_0, 4\_1, 4\_2 or 1\_2 decode the corresponding PDSCHs as indicated by that DCI. When the UE is scheduled with multiple PDSCHs by a DCI, HARQ process ID indicated by this DCI applies to the first PDSCH not overlapping with a UL symbol indicated by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigurationDedicated* if provided, HARQ process ID is then incremented by 1 for each subsequent PDSCH(s) in the scheduled order, with modulo operation of *nrofHARQ-ProcessesForPDSCH* applied if *nrofHARQ-ProcessesForPDSCH* is provided, or with modulo operation of *nrofHARQ-ProcessesForPDSCH-v1700* applied if or *nrofHARQ-ProcessesForPDSCH-v1700* is provided, or with modulo operation of 8 applied, otherwise. HARQ process ID is not incremented for PDSCH(s) not received if at least one of the symbols indicated by the indexed row of the used resource allocation table in the slot overlaps with a UL symbol indicated by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigurationDedicated* if provided. When a UE is configured by the higher layer parameter *repetitionScheme* set to 'tdmSchemeA’, the PDSCH includes two PDSCH transmission occasions. For each PDSCH, if either PDSCH occasion overlaps with a UL symbol indicated by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigurationDedicated* if provided, the PDSCH is not received and HARQ process ID is not increment for the PDSCH. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to receive a PDSCH that overlaps in time with another PDSCH if the UE is not capable of receiving FDMed unicast and multicast PDSCH per slot per carrier. When HARQ feedback for the HARQ process ID is not disabled, or for the HARQ process associated with the first SPS PDSCH when *HARQ-feedbackEnablingforSPSactive* is provided and enabled, the UE is not expected to receive another PDSCH for a given HARQ process until after the end of the expected transmission of HARQ-ACK for that HARQ process, where the timing is given by Clause 9.2.3 of [6, TS 38.213]. For HARQ-ACK subject to HARQ-ACK deferral described in Clause 9.2.5.4 of [6 TS 38.213], the expected transmission of HARQ-ACK corresponds to the expected transmission HARQ-ACK in a first slot. When HARQ feedback for the HARQ process ID is disabled, the UE is not expected to receive another PDCCH carrying a DCI scheduling a PDSCH or set of slot-aggregated PDSCH scheduled for the given HARQ process or to receive another PDSCH without corresponding PDCCH for the given HARQ process that starts until Tproc,1 after the end of the reception of the last PDSCH or slot-aggregated PDSCH for that HARQ process. Except for the case when a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *coresetPoolIndex* in *ControlResourceSet* and PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex,* in a given scheduled cell, the UE is not expected to receive a first PDSCH and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH, where the two resources are in different slots for the associated HARQ-ACK transmissions, each slot is composed of symbols [4] or a number of symbols indicated by *subslotLengthForPUCCH* if provided, and the HARQ-ACK for the two PDSCHs are associated with the HARQ-ACK codebook of the same priority. Except for the case when a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *coresetPoolIndex* in *ControlResourceSet* and PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex,* in a given scheduled cell, the UE is not expected to receive a first PDSCH, and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH if the HARQ-ACK for the two PDSCHs are associated with HARQ-ACK codebooks of different priorities. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH ending in symbol *i* on a scheduling cell, the UE is not expected to be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH that ends later than symbol *i* of a scheduling cell,. When the PDCCH reception includes two PDCCH candidates from two respective search space sets, as described in clause 10.1 of [6, TS 38.213], the PDCCH ending in symbol *i* is determined based on the PDCCH candidate that ends later in time. In a given scheduled cell, for any PDSCH corresponding to SI-RNTI, the UE is not expected to decode a re-transmission of an earlier PDSCH with a starting symbol less than *N* symbols after the last symbol of that PDSCH, where the value of *N* depends on the PDSCH subcarrier spacing configuration *μ,* with *N*=13 for *μ*=0, *N*=13 for *μ*=1, *N*=20 for *μ*=2, *N*=24 for *μ*=3, *N*=96 for *m*=5, and *N*=192 for *m*=6.

========================= Unchanged parts =========================