**3GPP TSG RAN WG1 #112bis-e R1-23xxxxx**

**E-meeting, April 17th – April 26th, 2023**

**Agenda Item: 7.2**

**Source: Moderator (China Telecom)**

**Title: [112bis-e-R17-CovEnh-01] FL summary of maintenance issues for Rel-17 NR coverage enhancements**

**Document for: Discussion**

1. Introduction

This contribution is a summary of the following email discussion on maintenance issues for Rel-17 NR coverage enhancements.

[112bis-e-R17-CovEnh-01] Email discussion on Rel-17 Coverage Enh maintenance by April 21 – Jianchi (China Telecom)

1. Initial discussion

## Issue #1: Correction on unified TCI state with DMRS bundling

[1] has the following proposal:

**Proposal:** Treat the beam switching via the indicated TCI state during repetition as an event breaking the power consistency and phase continuity.

This issue was discussed in RAN1#112. The latest TP is as follows [2]:

|  |
| --- |
| 6.1.7 UE procedure for determining time domain windows for bundling DM-RS < Unchanged parts are omitted >  Events which cause power consistency and phase continuity not to be maintained across PUSCH transmissions of PUSCH repetition type A scheduled by DCI format 0\_1 or 0\_2, or PUSCH repetition Type A with a configured grant, or PUSCH repetition type B or TB processing over multiple slots, or PUCCH transmissions of PUCCH repetition, within the nominal TDW, are:  < Unchanged parts are omitted >  - A different *TCI-State* and/or *TCI-UL-State* is indicated by DCI for uplink according to Clause 5.1.5.  < Unchanged parts are omitted > |

**Companies are encouraged to answer the following question:**

1. **Is it an essential issue to be discussed in RAN1#112bis-e?**
2. **If the answer to the first question is “yes”, please provide comments on the above proposal and TP.**

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |

## Issue #2: Correction on RRC parameters for DMRS bundling in TS38.213

[3] points out that RRC parameter names *PUCCH-DMRS-Bundling, PUCCH-Frequencyhopping-Interval* and *PUCCH-TimeDomainWindowLength* in TS38.214 are not aligned with TS38.331.

[3] proposes the following TP.

|  |
| --- |
| 9.2.6 PUCCH repetition procedure  **<Unchanged text is omitted>**  For ,  - the UE repeats the PUCCH transmission with the UCI over slots  - a repetition of the PUCCH transmission in each of the slots has a same number of consecutive symbols, as provided by *nrofSymbols*  - a repetition of the PUCCH transmission in each of the slots has a same first symbol, as provided by *startingSymbolIndex* if *subslotLengthForPUCCH* is not provided; otherwise mod(*startingSymbolIndex*, *subslotLengthForPUCCH*)  - the UE is configured by *interslotFrequencyHopping* whether or not to perform frequency hopping for repetitions of the PUCCH transmission in different slots  - if the UE is configured to perform frequency hopping for repetitions of a PUCCH transmission across slots and the UE is not provided *pucch-DMRS-Bundling* = 'enabled'  - the UE performs frequency hopping per slot  - the UE transmits the PUCCH starting from a first PRB, provided by *startingPRB*, in slots with even number and starting from a second PRB, provided by *secondHopPRB*, in slots with odd number. The slot indicated to the UE for the first repetition of the PUCCH transmission has number 0 and each subsequent slot until the UE transmits the PUCCH in slots is counted regardless of whether or not the UE transmits the PUCCH in the slot  - the UE does not expect to be configured to perform frequency hopping for a repetition of the PUCCH transmission within a slot  - if the UE is configured to perform frequency hopping for repetitions of a PUCCH transmission across slots and the UE is provided *pucch-DMRS-Bundling* = 'enabled'  - the UE performs frequency hopping per interval of consecutive slots, that start from a slot indicated to the UE and where the UE would transmit a first repetition of the PUCCH, where is the value of *pucch-FrequencyHoppingInterval*, if provided; otherwise, is the value of *pucch-TimeDomainWindowLength*  - the UE transmits the PUCCH over intervals until the UE transmits the PUCCH in slots, where the first interval has number 0 and each subsequent interval is counted regardless of whether or not the UE transmits the PUCCH in a slot  - the UE transmits the PUCCH starting from a first PRB, provided by *startingPRB*, in intervals with even number and starting from a second PRB, provided by *secondHopPRB*, in intervals of frequency hopping intervals with odd number  - the UE does not expect to be configured to perform frequency hopping for a repetition of the PUCCH transmission within a slot  - if the UE is not configured to perform frequency hopping for repetitions of a PUCCH transmission across slots and the UE is configured to perform frequency hopping for a repetition of the PUCCH transmission within a slot, the frequency hopping pattern between the first PRB and the second PRB is same within each slot  **<Unchanged text is omitted>** |

**Companies are encouraged to provide comments on the above TP.**

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |

## Issue #3: Correction on RRC parameters for DMRS bundling in TS38.214

[4] points out that RRC parameter names *PUCCH-DMRS-Bundling, PUSCH-DMRS-Bundling, PUSCH-Frequencyhopping-Interval,* *PUCCH-TimeDomainWindowLength* and *PUSCH-TimeDomainWindowLength* in TS38.214 are not aligned with TS38.331.

[4] proposes the following TP.

|  |
| --- |
| 6.1.7 UE procedure for determining time domain windows for bundling DM-RS  For PUSCH transmissions of PUSCH repetition Type A scheduled by DCI format 0\_1 or 0\_2, PUSCH repetition Type A with a configured grant, PUSCH repetition Type B and TB processing over multiple slots, when *pusch-DMRS-Bundling* is enabled, and for PUCCH transmissions of PUCCH repetition, when *pucch-DMRS-Bundling* is enabled, the UE determines one or multiple nominal TDWs, as follows:  - For PUSCH transmissions of repetition Type A, PUSCH repetition Type B and TB processing over multiple slots, the duration of each nominal TDW except the last nominal TDW, in number of consecutive slots, is:  - Given by *pusch-TimeDomainWindowLength*, if configured.  - Computed as min (*maxDurationDMRS-Bundling*, M), if *pusch-TimeDomainWindowLength* is not configured, where *maxDurationDMRS-Bundling* is maximum duration for a nominal TDW subject to UE capability [13, TS 38.306], M is the time duration in consecutive slots of PUSCH transmissions, and where:  - For PUSCH transmissions of PUSCH repetition Type A, N=1 and K is the number of repetitions, as defined in Clause 6.1.2.1 or in Clause 6.1.2.3.  - For PUSCH transmissions of PUSCH repetition Type B, N=1 and K is the number of nominal repetitions, as defined in Clause 6.1.2.1 or in Clause 6.1.2.3.  - For PUSCH transmissions of TB processing over multiple slots, N is the number of slots used for TBS determination and K is the number of repetitions of the number of slots N used for TBS determination, as defined in Clause 6.1.2.1 or in Clause 6.1.2.3.  - For PUCCH transmissions of PUCCH repetition, the duration of each nominal TDW except the last nominal TDW, in number of consecutive slots, is:  - Given by *pucch-TimeDomainWindowLength*, if configured.  - Computed as min (*maxDurationDMRS-Bundling*, M), if *pucch-TimeDomainWindowLength* is not configured, where *maxDurationDMRS-Bundling* is maximum duration for a nominal TDW subject to UE capability [13, TS 38.306], M is the time duration in consecutive slots from the first slot determined for PUCCH transmissions of PUCCH repetition to the last slot determined for PUCCH transmissions of PUCCH repetition according to clause 9.2.6 of [6, TS 38.213].  - For PUSCH transmission of a PUSCH repetition Type A scheduled by DCI format 0\_1 or 0\_2 and PUSCH repetition Type A with a configured grant, when *AvailableSlotCounting* is enabled, and for TB processing over multiple slots:  - The start of the first nominal TDW is the first slot determined for the first PUSCH transmission.  - The end of the last nominal TDW is the last slot determined for the last PUSCH transmission.  - The start of any other nominal TDWs is the first slot determined for PUSCH transmission after the last slot determined for PUSCH transmission of a previous nominal TDW.  **<Unchanged text is omitted>**  6.3 UE PUSCH frequency hopping procedure  6.3.1 Frequency hopping for PUSCH repetition Type A and for TB processing over multiple slots  **<Unchanged text is omitted>**  In case of inter-slot frequency hopping and when *pusch-DMRS-Bundling* is not enabled, or for inter-slot frequency hopping for a PUSCH scheduled by RAR UL grant or DCI format 0\_0 with CRC scrambled by TC-RNTI, the starting RB during slot  is given by:  ,  where  is the current slot number within a system radio frame, where a multi-slot PUSCH transmission can take place,  is the starting RB within the UL BWP, as calculated from the resource block assignment information of resource allocation type 1 (described in Clause 6.1.2.2.2) and is the frequency offset in RBs between the two frequency hops.  In case of inter-slot frequency hopping and when *pusch-DMRS-Bundling* is enabled, and when a PUSCH is not scheduled by RAR UL grant or DCI format 0\_0 with CRC scrambled by TC-RNTI, the starting RB during slot  is given by:    where is the current slot number within a system radio frame, is the value of the higher layer parameter *pusch-FrequencyHoppingInterval*,  is the starting RB within the UL BWP, as calculated from the resource block assignment information of resource allocation type 1 (described in Clause 6.1.2.2.2) andis the frequency offset in RBs between the two frequency hops.  **<Unchanged text is omitted>** |

**Companies are encouraged to provide comments on the above TP.**

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |

1. Reference
2. R1-2303693, Discussion on the remaining issues for joint channel estimation, NTT DOCOMO, RAN1#112bis-e, April 17th – April 26th, 2023.
3. R1-2301942, FL summary of discussion on joint channel estimation for Rel-17 NR coverage enhancements, Moderator (China Telecom), February 27th – March 3rd, 2023.
4. R1-2303843, Corrections on RRC parameter name for DMRS bundling in TS38.213, Sharp, RAN1#112bis-e, April 17th – April 26th, 2023.
5. R1-2303844, Corrections on RRC parameter name for DMRS bundling in TS38.214, Sharp, RAN1#112bis-e, April 17th – April 26th, 2023.