**3GPP TSG- Meeting #-eR1-230XXXX**

**, -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **Rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on value range mismatch of p0 for SRS in Rel-17 unified TCI framework |
|  |  |
| ***Source to WG:*** | Moderator (ZTE), , Ericsson, ZTE |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In Rel-17 unified TCI framewrok, UL power control parameters (i.e., p0, alpha, power control adjustment state) for PUSCH/PUCCH/SRS is determined according to a RRC parameter Uplink-powerControl-r17, where the value range (-16..15) dB is considered for p0 configuration.However, for SRS transmit power control in TS38.213 is the absolute target power whose value range is (-202…24), and there is serious mismatch of value range for P0 for SRS transmit power control in the current specification. To solve the issue, following agreement was made in RAN1#112bis-e.**Agreement**Regarding SRS UL power control in Rel-17 unified TCI framework, p0 defined in the SRS resource set is assumed as an P0\_nominal\_SRS , and then target power for a SRS transmission is equal to P0\_nominal\_SRS + p0-r17 in P0AlphaSet-r17 for SRS* Note: No further RRC impact.
 |
|  |  |
| ***Summary of change:*** | Clarified UE behavior to determine for SRS transmit power control in unified TCI framework in clause 7.3.1. |
|  |  |
| ***Consequences if not approved:*** | SRS transmit power control in unified TCI framework is inaccurate. |
|  |  |
| ***Clauses affected:*** | 7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | This is the first version of the CR.  |

### 7 UL power control

Uplink power control determines a power for PUSCH, PUCCH, SRS, and PRACH transmissions.

A UE does not expect to simultaneously maintain more than four pathloss estimates per serving cell for all PUSCH/PUCCH/SRS transmissions as described in clauses 7.1.1, 7.2.1, and 7.3.1, except for SRS transmissions configured by *SRS-PosResourceSet* as described in clause 7.3.1. If the UE is provided a number of RS resources for pathloss estimation for PUSCH/PUCCH/SRS transmissions that is larger than 4, the UE maintains for pathloss estimation RS resources corresponding to RS resource indexes as described in clauses 7.1.1, 7.2.1, and 7.3.1. If an RS resource updated by MAC CE, as described in clauses 7.1.1, 7.2.1 and 7.3.1, is one from the RS resources the UE maintains for pathloss estimation for PUSCH/PUCCH/SRS transmissions, the UE applies the pathloss estimation based on the RS resources starting from the first slot that is after slot where is the slot where the UE would transmit a PUCCH or PUSCH with HARQ-ACK information for the PDSCH providing the MAC CE, is the SCS configuration for the PUCCH or PUSCH, respectively, that is determined in the slot when the MAC CE command is applied and is a number of slots for SCS configuration provided by *kmac* or if *kmac* is not provided*.*

A PUSCH/PUCCH/SRS/PRACH transmission occasion is defined by a slot index within a frame with system frame number , a first symbol within the slot, and a number of consecutive symbols . For a PUSCH transmission with repetition Type B, a PUSCH transmission occasion is a nominal repetition [6, TS 38.214].

In the remaining of this clause, if a UE is provided *TCI-State* in *dl-OrJointTCI-StateList* or *TCI-UL-State* and for an indicated *TCI-State* or *TCI-UL-State* as described in [6, TS 38.214]

- in clauses 7.1.1, 7.2.1, and 7.3.1, the RS index for obtaining the downlink pathloss estimate for PUSCH, PUCCH, and SRS transmission is provided by pathlossReferenceRS-Id-r17 associated with or included in the indicated *TCI-State* or *TCI-UL-State* except for SRS transmission that is not provided *followUnifiedTCI-StateSRS*

- in clause 7.1.1, if *p0AlphaSetforPUSCH* is provided, the values of , , and the PUSCH power control adjustment state are provided by *p0AlphaSetforPUSCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.2.1, if *p0AlphaSetforPUCCH* is provided, the values of and the PUCCH power control adjustment state are provided by *p0AlphaSetforPUCCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.3.1, if *p0AlphaSetforSRS* is provided,

- if *followUnifiedTCI-StateSRS* is provided for a SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with the indicated *TCI-State* or *TCI-UL-State*

- else, if *followUnifiedTCI-StateSRS* is not provided for a SRS resource set and for a SRS resource from the SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set and a RS index for obtaining a pathloss estimate for the SRS transmission is provided by *pathlossReferenceRS-Id-r17* associated with or included in the *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set

 is the sum of the component and a component *p0* provided by *SRS-ResourceSet* corresponding to the SRS resource set.

In the remaining of this clause, if a PDCCH reception by a UE includes two PDCCH candidates from corresponding search space sets, as described in clause 10.1

- a PDCCH monitoring occasion is the union of the PDCCH monitoring occasions for the two PDCCH candidates

- the end of the PDCCH reception is the end of the PDCCH candidate that ends later

The PDCCH reception includes the two PDCCH candidates also when the UE is not required to monitor one of the two PDCCH candidates as described in clauses 10 (except clause 10.4), 11.1, 11.1.1 and 17.2.