**3GPP TSG RAN WG1 #112bis-e R1-230xxxx**

**e-Meeting, April 17th – April 26th, 2023**

**Agenda item:** 7.2

**Source:** Moderator (ZTE)

**Title:** Moderator Summary #0 for Maintenance on Rel-17 Multi-Beam

**Document for:** Discussion and Decision

## Introduction

The following in Section 2 and Section 3 is assigned for discussion on maintenance on normal and editorial issues of Rel-17 Multi-Beam in FeMIMO. Please provide your comments in corresponding sections.

## Summary of normal issues

### Issue 1-1 Draft CR on the power control for SRS resource set for noncodebook (R1-2302733)

|  |  |
| --- | --- |
| ***Reason for change:*** | When separate TCI framework is configured, only CSI-RS for beam management which only has 1 or 2 ports, SSB with single ports or SRS for beam management can be configured in the TCI state for the UE to determine the UL beam, with which the UE cannot obtain the full DL channel matrix to calculate the proper precoder for SRS transmission. In other words, the associated NZP CSI-RS may have more than 2 ports for the UE to obtain the full DL channel matrix, should be configured for the SRS resource set for non-codebook at least when separate TCI framework is configured. And in that case, the SRS shall not be configured with TCI state or be indicated to follow the indicated unified TCI state according to Rel-15 principle.  In summary, when an SRS resource set is configured with an associated NZP CSI-RS, how to determine the power control parameters including PL-RS, P0, alpha, closed loop index should be specified |
|  |  |
| ***Summary of change:*** | 1. Add the UE behavior to obtain the power control parameters for SRS resource set configured with associated NZP CSI-RS. |
|  |  |
| ***Consequences if not approved:*** | The UE does not know how to determine the power control related parameters when the SRS resource for non-codebook is configured with associated NZP CSI-RS. |

Due to above, the following draft CR is provided in R1-2302733:

----------------------------------------------------------------------------------------------

**7 Uplink Power control**

<unrelated part omitted>

In the remaining of this clause, if a UE is provided *TCI-State* in *dl-OrJoint-TCIStateList* or *TCI-UL-State* and for an indicated *TCI-State* or *TCI-UL-State* as described in [6, TS 38.214]

- in clauses 7.1.1, 7.2.1, and 7.3.1, the RS index for obtaining the downlink pathloss estimate for PUSCH, PUCCH, and SRS transmission is provided by pathlossReferenceRS-Id-r17 associated with or included in the indicated *TCI-State* or *TCI-UL-State* except for SRS transmission that is not provided *followUnifiedTCIstateSRS*

- in clause 7.1.1, if *p0AlphaSetforPUSCH* is provided, the values of , , and the PUSCH power control adjustment state are provided by *p0AlphaSetforPUSCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.2.1, if *p0AlphaSetforPUCCH* is provided, the values of and the PUCCH power control adjustment state are provided by *p0AlphaSetforPUCCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.3.1, if *p0AlphaSetforSRS* is provided,

- if the higher layer parameter *usage* in *SRS-ResourceSet* set to 'nonCodebook' and a higher layer parameter *associatedCSI-RS* is configured in *SRS-ResourceSet,* thevalues of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with the indicated *TCI-State* or *TCI-UL-State*

- else, if *followUnifiedTCIstateSRS* is provided for a SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with the indicated *TCI-State* or *TCI-UL-State*

- else, if *followUnifiedTCIstateSRS* is not provided for a SRS resource set and for a SRS resource from the SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set and a RS index for obtaining a pathloss estimate for the SRS transmission is provided by *pathlossReferenceRS-Id-r17* associated with or included in the *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set

<unrelated part omitted>

----------------------------------------------------------------------------------------------

Please provide company’s view in the table below.

|  |  |
| --- | --- |
| Company | Comment |
| Mod\_V00 | FL note: Above is to clarify UL power control of SRS transmission for NCB but which is configured with associated NZP CSI-RS.  Please provide your views for this issue, and then do you have any further views on the draft CR, if identifying the essentiality from your side. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 1-2 Value range mismatch of p0 for SRS/PUCCH in Rel-17 unified TCI framework (R1-2303691, R1-2303692)

In Rel-17 unified TCI framework, the following TPC parameters can be configured by p0-r17, and determined based on the indicated TCI

* for PUSCH transmit power control
* for PUCCH transmit power control
* for SRS transmit power control

**P0 for SRS**

As mentioned in R1-2303691, we have the following observation based on the current RRC for unified TCI (details can be found in the corresponding contribution)

* for PUSCH transmit power control is the differential target power in TS38.213.
  + The value range is (-16..15)
* for SRS transmit power control is the absolute target power in TS38.213.
  + The value range is (-202..24)
* The same RRC parameter of p0-r17 in P0AlphaSet-r17, whose value range is {-16..15}, is used for the indication of for PUSCH and for SRS in TS38.331.

That means that we have a serious mismatch of value range for P0 in SRS transmission, if being based on unified TCI framework.

In R1-2303061, the following candidate solution (option-1/2) are provided. Besides for that, from the Moderator’s perspective, in order to avoid the RRC signaling update, one alternative solution may be like what we did for closed loop procedure for SRS in RAN1#111, i.e., reuse the legacy P0 parameter if legacy P0 for SRS is provided in a SRS resource set. Then, we have the following candidate solution

**Proposal: Down select from the following options:**

* + **Option 1: Existing p0-r17 = {-16..15} in P0AlphaSet-r17 is not used for SRS, and introduce new RRC parameter of p0Srs-r17 = {-202..24} in P0AlphaSet-r17 to indicate the absolute target power for SRS.**
    - **Send LS to RAN2 to inform the above.**
  + **Option 2: Reuse existing p0-r17 = {-16..15} in P0AlphaSet-r17 for SRS, and discuss in RAN1 how to indicate the absolute target power for SRS.**

Please provide company’s view in the table below.

|  |  |
| --- | --- |
| Company | Comment |
| Mod\_V00 | FL note: Above seems essential, otherwise we may have to experience unintended absolute target power (i.e., just from -16..15) for SRS transmission in the unified TCI framework.  Please provide your views for this issue, and then do you have any further views on above candidate solution (or any other recommendation from your side), if identifying the essentiality from your side. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**P0 for PUCCH**

|  |  |
| --- | --- |
| ***Reason for change:*** | In Rel-17 FeMIMO WI, unified TCI framework is supported. One of the related features is to configure/indicate TPC parameters (i.e., p0, alpha, power control adjustment state) for PUSCH/PUCCH/SRS according to a RRC parameter Uplink-powerControl-r17, where the value range (-16..15) dB is considered for p0 configuration. The value range fits for the configuration of “differential target power”, e.g., for PUSCH, or for PUCCH.  In Clause 7, however, it is now described that for PUCCH, “ is provided by *p0AlphaSetforPUCCH* (configured in Uplink-powerControl-r17) associated with the indicated *TCI-State* or *TCI-UL-State”*. is nominal (absolute) target power, whose range is (-202..24) in general.  In our understanding, the intention of p0 configuration/update based on Rel-17 unified TCI is differential value. Therefore, the value range of p0-r17 in *p0AlphaSetforPUCCH* specified in 38.331 seems correct, and Clause 7 of 38.213 aims at the configuration/update of a wrong TPC parameter. |
|  |  |
| ***Summary of change:*** | Change one of the TPC parameters configured/indicated for PUCCH in case Rel-17 unified TCI is configured, from to . |
|  |  |
| ***Consequences if not approved:*** | Unintended transmit power is configured/indicated for PUCCH in case uTCI is configured. |

Due to above, the following draft CR is provided in R1-2303692:

----------------------------------------------------------------------------------------------

**7 UL power control**

**< Unchanged parts are omitted >**

In the remaining of this clause, if a UE is provided *TCI-State* in *dl-OrJointTCI-StateList* or *TCI-UL-State* and for an indicated *TCI-State* or *TCI-UL-State* as described in [6, TS 38.214]

- in clauses 7.1.1, 7.2.1, and 7.3.1, the RS index for obtaining the downlink pathloss estimate for PUSCH, PUCCH, and SRS transmission is provided by *pathlossReferenceRS-Id-r17* associated with or included in the indicated *TCI-State* or *TCI-UL-State* except for SRS transmission that is not provided *followUnifiedTCI-StateSRS*

- in clause 7.1.1, if *p0AlphaSetforPUSCH* is provided, the values of , , and the PUSCH power control adjustment state are provided by *p0AlphaSetforPUSCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.2.1, if *p0AlphaSetforPUCCH* is provided, the values of and the PUCCH power control adjustment state are provided by *p0AlphaSetforPUCCH* associated with the indicated *TCI-State* or *TCI-UL-State*

- in clause 7.3.1, if *p0AlphaSetforSRS* is provided,

- if *followUnifiedTCI-StateSRS* is provided for a SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with the indicated *TCI-State* or *TCI-UL-State*

- else, if *followUnifiedTCI-StateSRS* is not provided for a SRS resource set and for a SRS resource from the SRS resource set, the values of , , and SRS power control adjustment state are provided by *p0AlphaSetforSRS* associated with *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set and a RS index for obtaining a pathloss estimate for the SRS transmission is provided by *pathlossReferenceRS-Id-r17* associated with or included in the *TCI-State* or *TCI-UL-State* of an SRS resource with lowest *SRS-ResourceId* in the SRS resource set

**< Unchanged parts are omitted >**

----------------------------------------------------------------------------------------------

Please provide company’s view in the table below

|  |  |
| --- | --- |
| Company | Comment |
| Mod\_V00 | FL note: Above is to clarify that the unified TCI state is just to indicate UE-specific P0 for PUCCH transmission, as PUSCH. That seems reasonable, and, if approved, we can assume that as an alignment CR.  Please provide your views for this issue, and then do you have any further views on the draft CR, if identifying the essentiality from your side. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Summary of editorial (E) issues

Companies are to share their inputs on the editorial CR for the following issues herein.

### Issue 2-1

* R1-2302734 Draft CR on UL-TCI-State configuration in TS38.214 Lenovo

Table 1 Companies’ inputs

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Conclusion

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | [**R1-2302733**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_112b-e/Docs/R1-2302733.zip) | Draft CR on the power control for SRS resource set for noncodebook | Lenovo |
| 2 | [**R1-2302734**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_112b-e/Docs/R1-2302734.zip) | Draft CR on UL-TCI-State configuration in TS38.214 | Lenovo |
| 3 | [**R1-2303691**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_112b-e/Docs/R1-2303691.zip) | Discussion on value range mismatch of p0 for SRS/PUCCH in Rel-17 unified TCI framework | NTT DOCOMO, INC. |
| 4 | [**R1-2303692**](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_112b-e/Docs/R1-2303692.zip) | Draft CR on value range mismatch of p0 for PUCCH in Rel-17 unified TCI framework | NTT DOCOMO, INC. |