**3GPP TSG RAN WG1 #113** **R1-230xxxx**

**Incheon, Korea, May 22nd – 26th, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** |  | **rev** |  | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of NR sidelink evolution |
|  |  |
| ***Source to WG:*** | Samsung |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_SL\_enh2-Core |  | ***Date:*** | 2023-06-04 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of NR sidelink evolution. |
|  |  |
| ***Summary of change:*** |  Capture NR power control for E-UTRA – NR co-channel coexistence.  |
|  |  |
| ***Consequences if not approved:*** | No support NR sidelink evolution. |
|  |  |
| ***Clauses affected:*** | 16.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  |  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* Unchanged parts are omitted \*\*\*

### 16.2.2 PSCCH

A UE determines a power for a PSCCH transmission on a resource pool in PSCCH-PSSCH transmission occasion as

 [dBm]

where

- is specified in clause 16.2.1

- is a number of resource blocks for the PSCCH transmission in PSCCH-PSSCH transmission occasion

- is a number of resource blocks for PSCCH-PSSCH transmission occasion *i*

For sidelink co-channel coexistence between E-UTRA and NR, and for NR SL PSCCH/PSSCH transmissions with SCS configuration of in slots that overlap with an E-UTRA subframe, the UE transmits NR SL PSSCH/PSCCH in the first overlapping slot with a power that is larger than or equal to the power in the remaining overlapping slots.

\*\*\* Unchanged parts are omitted \*\*\*