**3GPP TSG RAN WG1 #114 R1-230XXXX**

**Toulouse, France, August 21st – August 25th, 2023**

**Agenda item:** 7.1

**Source:** Moderator (Qualcomm Incorporated)

**Title:** Summary for x7899 (Correction on RRC parameter name for SRS carrier switching)

**Document for:** Discussion and Decision

# Proposed change

R1-2307899 proposes the following change to TS 38.214 to align with the correct RRC parameter name:

6.2.1.3 UE sounding procedure between component carriers

For a carrier of a serving cell *c1* with slot formats comprised of DL and UL symbols, not configured for PUSCH/PUCCH transmission, denote as the corresponding carrier of a serving cell whose UL transmissions are temporarily suspended as signalled by higher layer parameter *srs-SwitchFromServCellIndex* and *srs-SwitchFromCarrier*. Define the set as the set of carriers of serving cells that each carrier meets one of the following conditions:

- is in the same band and same TAG as;

- is a carrier of inter-band CA with and is indicated through the capability signalling *srs-SwitchingAffectedBandsListNR-r17* to be affected by the SRS switch from to ;

where .

Companies are encouraged to provide comments on the above change:

|  |  |
| --- | --- |
| Company | Comment |
|  |  |