**3GPP TSG RAN WG1 #114** **R1-230xxxx**

**Toulouse, France, August 21st – 25th, 2023**

**Agenda item:** 9.17

**Source:** Samsung

**Title:** Summary of email discussions [114-R18-38.213-NR\_FR1\_lessthan\_5MHz\_BW]

**Document for:** Discussion and decision

# Introduction

The purpose of this document is to collect inputs/comments on the draft CR for TS 38.213 [draftCR\_38213 Less than 5 MHz BW](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_114/Inbox/drafts/9.17(Other)/%5B38.213%20draft%20CRs%5D/NR_FR1_lessthan_5MHz_BW/R1-230xxxx%20draftCR_38213%20Less%20than%205%20MHz%20BW.docx) on the introduction of NR support for dedicated spectrum less than 5MHz for FR1. If a comment on a particular aspect has been made by another company, please do not repeat it until, if needed, after a response.

The first checkpoint is on September 5, UTC 13:00.

# First Round Discussion

Please provide your comments on the draft CR for TS 38.213 [draftCR\_38213 Less than 5 MHz BW](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_114/Inbox/drafts/9.17(Other)/%5B38.213%20draft%20CRs%5D/NR_FR1_lessthan_5MHz_BW/R1-230xxxx%20draftCR_38213%20Less%20than%205%20MHz%20BW.docx).

|  |  |
| --- | --- |
| Company | Comments |
| Ericsson | Thanks for the draft CR, we have the following comments:   * Clause 13: The new text added as part of the first paragraph should also include the following statement “… in [8-1, TS 38.101 -1]. In Table 13-0, for configurations with indices 0, 1, 10 and 11, Table 5.4.3.1-3 in [8-1, TS 38.101-1] applies.”   [Aris]: Table 5.4.3.1-3 defines GSCN values 41637 and 41638, and Table 5.4.3.3-1 (NOTE 1) and Table 5.4.3.3-2 (NOTE 2) specify how to apply the two GSCN values. So, referring to Table 5.4.3.3-1 (NOTE 1) and Table 5.4.3.3-2 (NOTE 2) is sufficient.   * Clauses 12 and 13: The word “truncation” can be replaced by “puncturing” as to align the wording used in TS 38.213 and TS 38.211.   [Aris]: Yes. |
| FUTUREWEI | Thanks for the draft CR  1. For clause 13, the text “In Table 13-1, the associated SS/PBCH block is not located according to NOTE 12 of Table 5.4.3.3-1 in [8-1, TS 38.101-1].” seems unneeded.  [Aris]: The intention is to say that when an SS/PBCH block is located as in NOTE 12 of Table 5.4.3.3-1, a UE uses Table 13-0 instead of Table 13-1 (clarifies UE behavior - no UE blind detection on which Table to use).  2. For clauses 12/13, “if truncation, if any”. In this case, “puncturing” seems to be the appropriate work. The SS/PBCH and CORESET are punctured.  [Aris]: Yes. |
|  |  |
|  |  |
|  |  |
|  |  |

# Second Round Discussion

Please provide your comments on the draft CR for TS 38.213 at [draftCR\_38213 Less than 5 MHz BW\_v1](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_114/Inbox/drafts/9.17(Other)/%5B38.213%20draft%20CRs%5D/NR_FR1_lessthan_5MHz_BW/R1-230xxxx%20draftCR_38213%20Less%20than%205%20MHz%20BW_v1.docx).

The second checkpoint is on September 6, UTC 15:00.

|  |  |
| --- | --- |
| Company | Comments |
| Ericsson v05 | Editor thanks for the response. The tables and notes cited in your comment do not encompass CORESET 0, because the notes state “punctured PBCH,” and “DCH transmission”. Thus, stating that indices 0, 1, 10 and 11 in Table 13-0 apply for Table 5.4.3.1-3, creates a link between the usage of those CORESET 0 entries and the sync-raster points described in Table 5.4.3.3-1. Having said that, the following still holds:   * Clause 13: The new text added as part of the first paragraph should also include the following statement “… in [8-1, TS 38.101 -1]. In Table 13-0, for configurations with indices 0, 1, 10 and 11, Table 5.4.3.1-3 in [8-1, TS 38.101-1] applies.” |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |