**3GPP TSG RAN WG1 #114** **R1-230xxxx**

**Toulouse, France, August 21st – 25th, 2023**

**Agenda item:** 9.17

**Source:** Samsung

**Title:** Summary of email discussions [114-R18-38.213-NR\_Netw\_Energy\_NR]

**Document for:** Discussion and decision

# Introduction

The purpose of this document is to collect inputs/comments on the draft CR for TS 38.213 [draftCR\_38213 NES](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_114/Inbox/drafts/9.17(Other)/%5B38.213%20draft%20CRs%5D/NR_Netw_Energy_NR/R1-230xxxx%20draftCR_38213%20NES.docx) on the introduction of network energy savings for NR. If a comment on a particular aspect has been made by another company, please do not repeat it until, if needed, after a response.

The first checkpoint is on September 5, UTC 13:00.

# First Round Discussion

Please provide your comments on the draft CR for TS 38.213 [draftCR\_38213 NES](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_114/Inbox/drafts/9.17(Other)/%5B38.213%20draft%20CRs%5D/NR_Netw_Energy_NR/R1-230xxxx%20draftCR_38213%20NES.docx).

|  |  |
| --- | --- |
| Company | Comments |
| ZTE, Sanechips | Thanks for the draft CR. Our comments are as below   |  | | --- | | Comment#1  Based on the agreements, the serving cell that UE monitors DCI format 2\_x is not limited to PCell, it can be SCell.  **Agreement**  From RAN1 point of view, DCI format 2\_X supports activation/deactivation of cell DTX/DRX configuration of multiple serving cells and support activation/deactivation per cell   * UE monitor DCI format 2\_X in one serving cell | | Original text #1  “a Type3-PDCCH CSS set configured by  - *SearchSpace* in *PDCCH-Config* with *searchSpaceType* = *common* for DCI formats with CRC scrambled by INT-RNTI, SFI-RNTI, TPC-PUSCH-RNTI, TPC-PUCCH-RNTI, TPC-SRS-RNTI, or CI-RNTI and, only for the primary cell, C-RNTI, MCS-C-RNTI, CS-RNTI(s), or NES-RNTI, or PS-RNTI, or ” | | Suggested text #1  “a Type3-PDCCH CSS set configured by  - *SearchSpace* in *PDCCH-Config* with *searchSpaceType* = *common* for DCI formats with CRC scrambled by INT-RNTI, SFI-RNTI, TPC-PUSCH-RNTI, TPC-PUCCH-RNTI, TPC-SRS-RNTI, or CI-RNTI or NES-RNTI and, only for the primary cell, C-RNTI, MCS-C-RNTI, CS-RNTI(s), ~~or NES-RNTI,~~ or PS-RNTI, or ”  UE expects to monitoring DCI format 2\_9 in one serving cell. | | Comment#2  Based on the following agreements, the function of DCI format 2\_X is to activation or de-activation of cell DTX/DRX. Furthermore, based on RAN2 agreements, the cell DTX/DRX is determined by the configuration of periodicity, start slot/offset, on duration, and the design in RAN2 focuses on one single configuration.  Therefore, the activation/de-activation function carried by DCI format 2-9 only indicate the following   1. Operate the cell DTX/DRX according to the RRC configured parameters via activation indication or 2. switch to normal cell state (no cell DTX/DRX operation, the cell is always active) via de-activation indication.   However, with the wording of “indicates a start of DTX Active Time or of DRX Active Time”, it seems that the start position of cell DTX/DRX active time is dynamically changed. Meanwhile, with the wording of “indicates an end of DTX Active Time or of DRX Active Time” , it seems the active time of cell DTX/DRX will be terminated. Basically, we think the current wording needs to be update to be consistent with previous agreements.  **Agreement in RAN1#114**   * An information block field of DCI format 2\_X is variable size either 1 or 2 bits.   + Higher layer signaling configures whether the activation/deactivation of cell DTX and/or cell DRX is indicated in DCI format 2\_X for a serving cell.     - If both cell DTX and cell DRX are configured for a serving cell,       * 1st bit corresponds to activation/deactivation of cell DTX configuration, and       * 2nd bit corresponds to activation/deactivation of cell DRX configuration,     - otherwise, the 1 bit corresponds to the configured cell DTX or cell DRX configuration.   **Agreements in RAN2**  The Cell DTX/DRX configuration contains at least: periodicity, start slot/offset, on duration.  **Agreements in RAN2**  Confirm study item agreement that we can have separate DTX and DRX configuration. We will focus on designing DTX/DRX for at least single configuration. FFS whether multiple configuration of cell DTX or DRX will be supported. | | Original text #2  - a '0' value for a bit of the cell operation state indicator field indicates a start of DTX Active Time or of DRX Active Time  - a '1' value for a bit of the cell operation state indicator field indicates an end of DTX Active Time or of DRX Active Time  - if the serving cell is configured with a SUL carrier, the cell operation state indicator field indication for start/end of DRX Active Time applies to both the UL carrier and the SUL carrier  When a UE receives in slot on the active DL BWP of a first serving cell a PDCCH providing DCI format 2\_9 that indicates a change in a current start/end state of DTX Active Time or DRX Active Time for a second serving cell, the UE operates on the second serving cell according to the indicated state of DTX Active Time or of DRX Active Time starting from a slot on the active DL BWP or on the active UL BWP of the second serving cell, respectively, that is not before the beginning of the slot on the active DL BWP of the first serving cell where is a number of slots for the SCS of the active DL BWP of the first serving cell in Table 11.5-1. | | Suggested text #2  - a '0' value for a bit of the cell operation state indicator field indicates the de-activation of cell DTX or cell DRX ~~a start of DTX Active Time or of DRX Active Time~~  - a '1' value for a bit of the cell operation state indicator field indicates the activation of cell DTX or cell DRX ~~an end of DTX Active Time or of DRX Active Time~~  - if the serving cell is configured with a SUL carrier, the cell operation state indicator field indication for the activation or de-activation of cell DRX ~~start/end of DRX Active Time~~ applies to both the UL carrier and the SUL carrier  When a UE receives in slot on the active DL BWP of a first serving cell a PDCCH providing DCI format 2\_9 that indicates a change in a current ~~start/end~~ state of cell DTX or cell DRX ~~DTX Active Time or DRX Active Time~~ for a second serving cell, the UE operates on the second serving cell according to the indicated state of cell DTX or cell DRX ~~DTX Active Time or of DRX Active Time~~ starting from a slot on the active DL BWP or on the active UL BWP of the second serving cell, respectively, that is not before the beginning of the slot on the active DL BWP of the first serving cell where is a number of slots for the SCS of the active DL BWP of the first serving cell in Table 11.5-1. | | Comment #3  The DCI format 2-9 can be monitored in a serving cell, and also indicates the activation/de-activation information for the same serving cell.  If we use the term “first serving cell”, and “second serving cell”, it may be interpreted that the DCI format 2-9 can not carry information for the serving cell that transmits DCI 2-9.  Therefore, a slight change is suggested. | | Original text #3  When a UE receives in slot on the active DL BWP of a first serving cell a PDCCH providing DCI format 2\_9 that indicates a change in a current start/end state of DTX Active Time or DRX Active Time for a second serving cell, the UE operates on the second serving cell according to the indicated state of DTX Active Time or of DRX Active Time starting from a slot on the active DL BWP or on the active UL BWP of the second serving cell, respectively, that is not before the beginning of the slot on the active DL BWP of the first serving cell where is a number of slots for the SCS of the active DL BWP of the first serving cell in Table 11.5-1. | | Suggested text #3  When a UE receives in slot on the active DL BWP of a ~~first~~ serving cell a PDCCH providing DCI format 2\_9 that indicates a change in a current start/end state of DTX Active Time or DRX Active Time for a target ~~second~~ serving cell, the UE operates on the target ~~second~~  serving cell according to the indicated state of DTX Active Time or of DRX Active Time starting from a slot on the active DL BWP or on the active UL BWP of the second serving cell, respectively, that is not before the beginning of the slot on the active DL BWP of the first serving cell where is a number of slots for the SCS of the active DL BWP of the first serving cell in Table 11.5-1. | | Comment #4  Based on the following agreement, UE can drop SP/P CSI reporting outside cell DRX active time, instead of SP/P PUCCH, or PUSCH.  Agreement in RAN1#112bis  From RAN1 point of view, Rel-18 UE supporting cell DRX is not expected to transmit the following signals/channels to the gNB during non-active periods of cell DRX. The list of signals/channels may be updated based on RAN2/RAN4 input and other signals/channels are not precluded from further discussions.  Periodic/Semi-persistent CSI report  Periodic/Semi-persistent SRS  FFS: SRS for positioning  FFS:  HARQ feedback for SPS PDSCH  FFS whether there will be exception case(s) for UE transmitting listed signals/channels during non-active periods of DRX  FFS Whether the listed signals/channels can be configurable by gNB  FFS: Whether the same or different UE behavior is applicable with or without C-DRX  FFS: RAN1 to consider impact on system if the channels/signals are not transmitted during non-active period | | Original text #4  Outside DRX Active Time of a serving cell, the UE does not transmit on the serving cell  - periodic or semi-persistent PUCCH or PUSCH  - periodic or semi-persistent SRS except for SRS in resources provided by *SRS-posResourceSet* | | Suggested text #4  Outside DRX Active Time of a serving cell, the UE does not transmit on the serving cell  - periodic or semi-persistent ~~PUCCH or PUSCH~~ CSI report  - periodic or semi-persistent SRS except for SRS in resources provided by *SRS-posResourceSet* | | Comment #5  In legacy spec, “DRX” refers to UE C-DRX. When cell DTX or cell DRX is introduced for NES, it would be better to use the term “cell DTX or cell DRX” (instead of “DTX or DRX”)to distinguish from UE C-DRX. | | Comment #6  Based on RAN2’s previous agreements, other channel such as SPS PDSCH, CG PUSCH, PDCCH with DL assignment/UL grant will also be dropped during cell DTX/DRX non-active time period. For these impacted signal/channels, will we leave it to be captured in RAN2 spec, or we can also capture it in RAN1 ? | |  | |  | |  | |  | |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |