3GPP TSG-RAN WG2 #109bis-e R2-20xxxxx

Electronic Meeting, April 20th – 30th 2020

Agenda Item: 5.4.1.4

Source: Ericsson

Title: Summary of [AT109bis-e][012][NR15] Inter Node Coord

Document for: Discussion, Decision

# 1 Introduction

This document is to kick off the following email discussion:

* [AT109bis-e][012][NR15] Inter Node Coord (Ericsson, Google)

Scope: Treat all docs under AI 5.4.1.4

Part 1: Determine which issues that need resolution, find agreeable proposals. Deadline: April 23 0700 UTC

Part 2: For the parts that are agreeable, discussion will continue to agree on CRs.

# 2 Discussion

Companies are requested to add their comments for each of the treated CRs of this email discussion in the boxes below (one for each CR to be treated).

### 2.1 Remaining issues on MN-SN measurement coordination in INM ([R2-2003195](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003195))

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Nokia | Yes, but… | The issue is valid while it seems the enhancement is not essential. There are currently other shared aspects where it is up to MN implementation for example to allocate the right amount of measurement identities between MN and SN independently. It is thus the MN that takes priority to reserve needed measurement identities no matter if the SN request is supported or not. |
| Ericsson | Agree | As for the power sharing and the band combination coordination, we think the same principle can be applied also for the measurement identities.  |
| NEC | Agree with observations, but | The situation summarized in observations could happen. However, this seems not so essential issue to be solved in Rel-15 as Nokia commented. To us, it looks similar to what RAN2 discussed for maxMeasFreqsSCG for which RAN2 agreed that the MN fully controls (without any negotiation/ coordination).However, we are open for further discussions if some suppports, wth restricting the possible CRs from Rel-16 (not Rel-15). |
| ZTE | Agree | We agree the issue is valid, since the measurement identity coordination is introduced at the late stage of Rel-15. We are fine to consider a more complete solution/enhancement in Rel-15. Compare to maxMeasFreqsSCG, we think the number of used measurement identities may fluctuate in a wider range. So that is why negotiation of measurement identities seems more useful than negotiation of measured frequencies. |
| Huawei | Disagree | Agree with Nokia and NEC that this is not essential.MN will take control of the assignment of measIDs, and will guarantee enough measIDs for itself. Even if SN wants more, it is not sure whether MN will satisfy the demand. On the other hand, if SN wants to indicate that it was allocated more measIDs than needed, it does not make much difference to MN because MN already has adequate measIDs.We don’t think the mechanism can simply mimic band combination and power coordination. For power coordination, it has already been agreed that semi-static sharing, dynamic sharing are both supported. For band combination, things are more complicated because Scell addition/release and mobility are involved.In our understanding, the measId coordination could be implemented in a semi-static way, which is much easier than dynamic coordination. |
| Samsung | Disagree | We agree with others that this is not essential.We note that long time ago we agreed not to introduce the SN initiated re-negotiation for the coordination of frequencies to measure. We don’t think the changes introduced recently require a change regarding this |
| vivo | Agree | We think this coordination is useful as it is for the case of power coordination. We consider this as a must have enhancement. |
| Qualcomm | Agree but | There is benefit in SN request for measurement identities when many measurements are configured. However, it is difficult to justify as a correction so can be considered as a Rel-16 enhancement. |

### 2.1.1 Correction on MN-SN measurements coordination in INM – Stage 3 ([R2-2003193](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003193), [R2-2003194](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003194))

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Nokia | Yes, but… | The issue is valid while it seems the enhancement is not essential. There are currently other shared aspects where it is up to MN implementation for example to allocate the right amount of measurement identities between MN and SN independently. It is thus the MN that takes priority to reserve needed measurement identities no matter if the SN request is supported or not. |
| Ericsson | Agree | As for the power sharing and the band combination coordination, we think the same principle can be applied also for the measurement identities. |
| NEC |  | general comment is same as 2.1.When we focus on the CR, a question is wheter there is any specific difference between maxMeasFreqsSCG (no request) and maxInter/intraMeasIdentitiesSCG? Why only the latter should be able to be requested for change (but not for the former)? |
| ZTE | Agree | Same comment as 2.1. |
| Huawei | Disagree | Same comment as 2.1. |
| Samsung | Disagree | See 2.1 |
| vivo | Agree | See comments above |
| Qualcomm | Agree | Same as 2.1 |

### 2.2.2 Correction on MN-SN measurements coordination in INM – Stage 2 ([R2-2003191](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003191), [R2-2003192](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003192))

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Nokia | Yes, but… | The issue is valid while it seems the enhancement is not essential. There are currently other shared aspects where it is up to MN implementation for example to allocate the right amount of measurement identities between MN and SN independently. It is thus the MN that takes priority to reserve needed measurement identities no matter if the SN request is supported or not. |
| Ericsson | Agree | As for the power sharing and the band combination coordination, we think the same principle can be applied also for the measurement identities.On top of this, our understanding is that the second sentence proposed is anyway needed because is based on what has been agreed in the last meeting. |
| NEC |  | same comment as 2.2.1 |
| ZTE | Yes, but… | The current stage2 CR mainly focus on the negotiation of measurement identities. But we still need to update the sentence to capture the latest situation. See below highlighted part.Measurements can be configured independently by the MN and by the SN (intra-RAT measurements on serving and non-serving frequencies). The MN indicates the maximum number of frequency layers and measurement identities of intra-frequency and inter-frequency meaurement that can be used in the SN to ensure that UE capabilities are not exceeded. The SN can also request the MN for new maximum values of the number of measurement identities that it can configure. To assist MN or SN to identify the measurement type, in all MR-DC cases, the SN indicates to the MN the list of SCG serving frequencies. And in NR-DC, the MN indicates to SN the list of MCG serving frequencies.  |
| Huawei | Disagree | Same comment as 2.1. |
| Samsung | Disagree | See 2.1 |
| vivo | Agree | Same as in section 2.1 |
| Qualcomm | Agree | Same as 2.1 |

**Rapporteur input**: According to the inputs provided by companies, it is acknowledged that the issue is valid but the changes may not be needed at this later stage of Rel-16. However, since it seems that there is quite a good support, this proposal may be eventually pursued as a Rel-16 enhancement. Therefore, we suggest:

1. The tdocs R2-2003193, R2-2003194, and R2-2003195 are not pursued in Rel-15 and can be considered in TEI16.

Further, according to ZTE comment, it looks like that the agreements we took in the last RAN2#109-e meeting have been not reflected in stage 2. Therefore, our proposal is to revise R2-2003191 and R2-2003192 according to ZTE suggestion.

1. Revise R2-2003191 and R2-2003192 to capture agreements on the measurement identities coordination agreed in the RAN2#109-e meeting.

## 2.3 Introduce RRC version for source configuration ([R2-2003753](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003753))

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Nokia | Disagree for now | Not sure we understand the reason for proposing an OCTET STRING. Is the proposal to do something similar to:HandoverPreparationInformation-v920-IEs ::= SEQUENCE { ue-ConfigRelease-r9 ENUMERATED { rel9, rel10, rel11, rel12, v10j0, v11e0, v1280, rel13, …, rel14, rel15} OPTIONAL, -- Cond HO2 nonCriticalExtension HandoverPreparationInformation-v9d0-IEs OPTIONAL} |
| Ericsson | Disagree | To be honest we struggle to understand why such field is needed and what is the benefits behind it. Our understanding is that the CR is not needed, unless the motivation is further clarified.  |
| NEC | Disagree | we would like to ask more explation for the need of this change. In addition, it looks the proposal is from Rel-16, so no need to discuss this here? |
| ZTE | Disagree | The motivation is unclear to us, and we are wondering about the consequence if this is not agreed? |
| Huawei | Disagree | This is not a correction and should not be discussed in Rel-15. |
| Samsung | Disagree | Alike others, we don’t see the need |
| vivo | Disagree | Same view as ZTE. |
| Qualcomm | Neutral | At a high level, this sounds useful, given that a similar IE was used in LTE.  |

**Rapporteur input**: According to the collected replies, there is no support to pursue this CR. Therefore, we suggest that the CR R2-2003753 is not pursued.

1. The CR R2-2003753 is not pursued.

# Conclusion

Based on the discussion in the previous sections we propose the following:

1. The tdocs R2-2003193, R2-2003194, and R2-2003195 are not pursued in Rel-15 and can be considered in TEI16.
2. Revise R2-2003191 and R2-2003192 to capture agreements on the measurement identities coordination agreed in the RAN2#109-e meeting.
3. The CR R2-2003753 is not pursued.

# References

[1]