3GPP TSG-RAN WG2 #109bis-e R2-20xxxxx

Electronic Meeting, April 20th – 30th 2020

Agenda Item: 5.4.3

Source: OPPO

Title: [AT109bis-e][016][NR15] UE Cap Miscellaneous III (Oppo, ZTE, Nokia, Huawei)

Document for: Discussion, Decision

# 1 Introduction

This document is to kick off the following email discussion:

* [AT109bis-e][016][NR15] UE Cap Miscellaneous III (Oppo, ZTE, Nokia, Huawei)

Scope: Treat R2-2002694, R2-2002695, R2-2002637, R2-2002636, R2-2002989, R2-2002678, R2-2003541, R2-2003542

Part 1: Determine which issues that need resolution, find agreeable proposals. Deadline: April 23 0700 UTC

Part 2: For the parts that are agreeable, discussion will continue to agree on CRs.

# 2 Discussion

Companies are requested to add their comments for each of the treated CRs of this email discussion in the boxes below (one for each CR to be treated).

### 2.1 Clarification on *BandParameters* (*R2-2002694, R2-2002695, R2-2002637, R2-2002636*)

In the related contributions, the proposal is to add a field description in Rel-15 to clarify the relationship between the original *bandList* and *bandList*-v1540, and further extend it to *bandList*-v16xy.

Although two options are provided in R2-2002694,

* CRs are prepared based on option-1 (proposed as baseline in 2694), i.e., the UE shall include the same number of entries, and listed in the same order in different versions of *bandList*.
* In option-2, the CR only mandates the same order but not the same number of entries.

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| OPPO | Agree | Apparently the |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2 Removing bandwidth class F ([*R2-2002989*](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2002682))

RAN4 dummy bandwidth class F so that the CR is to remove that by clarification in 38.306.

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.3 Clarify the *bwp-WithoutRestriction* ([*R2-2002678*](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2002682))

In the description for IE of *bwp-WithoutRestriction* , the sentence of “The Bandwidth restriction in terms of DL BWP for PCell and PSCell means that the bandwidth of a UE-specific RRC configured DL BWP may not include the bandwidth of CORESET #0 (if configured) and SSB.” Is misleading, since it should be for “BWP operation without bandwidth restriction”.

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.4 Clarify the *bwp-SwitchingDelay* ([*R2-2003541,*](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2002682) *R2-2003542*)

In the description of the field *bwp-SwitchingDelay*, it says “Defines whether the UE supports DCI and timer-based active BWP switching delay type1 or type2 specified in clause 8.6.2 of TS 38.133 [5]. It is mandatory to report type 1 or type 2”. It mandates a UE to report the support of type1 or type2 for BWP switching delay. The proposal is to add “if the UE reports bwp-DiffNumerology, bwp-SameNumerology or bwp-WithoutRestriction.” to avoid the case of basic BWP operation.

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

In the previous sections we made the following observations:

Based on the discussion in the previous sections we propose the following:

# References

[1]