**3GPP TSG-RAN WG2 Meeting #109e-bis R2-20xxxxx**

**Electronic meeting, April 20 – April 30**

**Agenda item:** 6.1.1

**Source:** Qualcomm Incorporated (Rapporteur)

**Title:** [AT109bis-e][018][IAB] IAB terminology (Qualcomm)

**Document for:** Discussion

# Introduction

This document handles aspects related to IAB-terminology and notation as part of offline email discussion:

* [AT109bis-e][018][IAB] Stage-2 (Qualcomm, Huawei)

Scope: Treat Stage-2: Issues, corrections and CRs (add CRs to x.300 if needed).

Specifically: [R2-2003014](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2003014.zip), [R2-2002728](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002728.zip), [R2-2003178](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2003178.zip)

Part 1: Treat meeting input and comments.

Deadline: April 24 0700 UTC

Part 2: Update of CRs, e.g. to include agreements this meeting

The discussion on IAB terminology and notation should finish during Part 1 of the offline.

The deadline therefore is: Deadline: April 24 0700 UTC

The discussion is based on R2-2002728. This paper proposes a few modifications to the IAB terminology and notation based on discussions in RAN3 after last meeting.

# Discussion

The following captures a set of rules on IAB terminology and notation:

* In running CR 38300, the *IAB-donor* is defined as a gNB that provides network access to UEs via a network of backhaul and access links.
  + There is **no** *IAB-donor gNB* or *IAB-donor-gNB*.
  + IAB-donor-DU and IAB-donor-CU are hyphenated in the same manner as the gNB-CU and gNB-DU.
* The IAB-node holds gNB-DU functionality with IAB-specific enhancements, referred to as *IAB-DU*.
  + There is **no** *IAB-node-DU* since this might imply that there would also be an *IAB-node-CU*.
  + The IAB-DU of a specific IAB-node, e.g., IAB-node 1, can be referred to as IAB-node-1’s IAB-DU, or IAB-DU 1.
* The IAB-node holds UE functionality with IAB-specific enhancements, referred to as *IAB-MT*.
  + There is **no** *IAB-node-MT* (since this might imply that there would also be an IAB-node-DU).
  + The IAB-MT of a specific IAB-node, e.g., IAB-node 1, can be referred to as IAB-node-1’s IAB-MT, or IAB-MT 1.
* The parent-node IAB-DU and child-node IAB-MT may be referred to as parent IAB-DU and child IAB-MT, respectively.
* Hyphenation follows commonly known rules.

**Proposal: RAN2 to agree on the above IAB terminology and notation.**

**Q: Do you agree with this proposal?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with proposal | Comment |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

…