3GPP TSG-RAN WG2 #109bis-e R2-20xxxxx

Electronic Meeting, April 20th – 30th 2020

Agenda Item: 6.10.7

Source: Ericsson

Title: [AT109bis-e][039][DCCA] Fast MCG Link Recovery

Document for: Discussion, Decision

# 1 Introduction

This document is to kick off the following email discussion:

* [AT109bis-e][039][DCCA] Fast MCG Link Recovery (Ericsson)

Scope: Treat topics in 6.10.6, based on R2-2003199 and ASN.1 issues and RRC corrections. Can start discussion on non-controversial proposals immediately, if any. Wait for on-line discussion for controversial proposal.

Part 1: Determine which issues that need resolution, find agreeable proposals. Deadline: April 24 0700 UTC

# 2 Discussion

## 2.1 Summary of [Post109e#27][DCCA] Fast MCG recovery ([R2-2003199](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003199))

Regarding the fast MCG recovery, the email discussion in R2-2003199 covered two main aspects related to the SN change as result of fast MCG recovery procedure and the support of the inter-RAT HO and other handover scenarios as described in Table B-1 of TS 37.340. According to this, companies are request to provide inputs about the summary of the email discussion.

|  |  |  |
| --- | --- | --- |
| Company | Proposal  (Agree/Disagree) | Comments |
| Nokia | P1, P2, P3 – agree  P4 – Disagree in its current wording | P4 ends: “(inter-RAT HO is excluded)”. This is misleading. The origin is probably Q5 of the discussion (that lead to P4) where inter-RAT handover was out of scope.  Therefore, we propose the following re-wording:  Proposal 4 **Apart from inter-RAT HO,** according to Table B-1 of TS 37.340, all handover scenario that have a DC option in the column “from” are supported in fast MCG recovery. |
| Qualcomm | Agree P1-P3, and disagree P4 (with wording changes is fine) | We agree with Nokia’s suggested change. And on top of that, we suggest below change:  Proposal 4 **Apart from inter-RAT HO,** according to Table B-1 of TS 37.340, all handover scenario that have a DC option in the column “from” are supported in fast MCG recovery **via split SRB1**.  The reason is that some scenarios (from NE-DC) can’t be supported via SRB3 because there is no SRB3 in NE-DC:  • Case 2: NE-DC to LTE-EPC;  • Case 3: NE-DC to LTE-5GC;  Case 7: NE-DC to UTRAN-FDD (i.e. SRVCC from 5G to 3G) |
| BT | Agree - P2, P3  Disagree – P1  Disagree – P4 with current wording | We agree with proposals 2 and 3.  We don’t agree with proposal 1 as it is. The fact that fast MCG recovery is left to network implementation may cause problems for MNOs in areas with more than one infra-vendor. From the previous discussion, it is clear that not all of them share the same view. For that reason, we consider that RAN2 shall capture in a stage-2 spec note the restrictions when fast MCG recovery is active.  Proposal 4, we agree with QC. |
| ZTE | Agree P1~P3,  P4 with Nokia’s suggestion. | For P4, we agree with the proposed wording from Nokia.  Regarding the comments from Qualcomm, maybe there is no need to add ”via split SRB1” because it narrows the supported scenarios, which is not the intention of this proposal, For instance, “ via SRB3” is supported for the following cases:  • (NG)EN-DC to LTE/EPC  • (NG)EN-DC to LTE/5GC  • NR-DC to NR  • EN-DC to EN-DC  • NGEN-DC to NGEN-DC  • NR-DC to NR-DC |
|  |  |  |
|  |  |  |

## 2.2 Other contributions for fast MCG recovery

The following contributions addressed topic that have been treated during the email discussion and thus we propose to not formulate any specific proposal.

[R2-2002647](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002647.zip) Remaining issues in Fast MCG Recovery Qualcomm Incorporated discussion LTE\_NR\_DC\_CA\_enh-Core

[R2-2002700](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002700.zip) Support of Inter-RAT handover upon MCG failure recovery ZTE Corporation, Sanechips discussion Rel-16 LTE\_NR\_DC\_CA\_enh-Core

[R2-2002992](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002992.zip) CR37340 on fast MCG recovery support vivo CR Rel-16 37.340 16.1.0 0191 - B LTE\_NR\_DC\_CA\_enh-Core

However, in R2-2002700, the proposal 3 and 4 were not really discussed in the email discussion and therefore companies are asked to provide their input on those. The mentioned proposals are as follow:

**Proposal 3   Inter-RAT handover towards GERAN/UTRAN via SRB3 is supported upon MCG failure recovery, including the following scenarios:**

         **Case 6: EN-DC to GERAN/UTRAN;**

         **Case 7: NE-DC to UTRAN-FDD (i.e. SRVCC from 5G to 3G)**

         **Case 8: NR-DC to UTRAN-FDD (i.e. SRVCC from 5G to 3G)**

**Proposal 4   UE can include UTRAN-FDD measurement results in MCG Failure Information message.**

|  |  |  |
| --- | --- | --- |
| Company | Proposal  (Agree/Disagree) | Comments |
| Nokia | P3 - Agree  P4 - Agree |  |
| Qualcomm | P3 with change  P4 -with clarification | As we indicated in Q1, some scenarios are not supported unless we allow SRB3 in NE-DC. Thus, we suggest below change:  **Proposal 3   Inter-RAT handover ~~towards GERAN/UTRAN~~ via SRB3 is supported upon MCG failure recovery, including the following scenarios:**  **• Case 1: (NG)EN-DC to NR;**  **• Case 4: NR-DC to LTE-EPC;**  **• Case 5: NR-DC to LTE-5GC;**  **Case 6: EN-DC to GERAN/UTRAN;**  ~~~~**~~Case 7: NE-DC to UTRAN-FDD (i.e. SRVCC from 5G to 3G)~~**           **Case 8: NR-DC to UTRAN-FDD (i.e. SRVCC from 5G to 3G)**  For P4, although we think it is not important, we can accept it. But we think the UE can include UTRAN-FDD measurements in MCG failure information only when the UE supports the SRVCC capability (i.e. handoverUTRA-FDD) |
| BT | Agree – P4  Depends – P3 | As we highlighted above, RAN6 will be close so, for proposal 3 we need to make sure there is no impact in GERAN/UTRAN. |
| ZTE | Agree P3 with Qualcomm’s suggestion,  Agree P4. | Seems Qualcomm’s suggestion is to merge our proposal 2&3 and remove the NE-DC cases in which SRB3 is not supported. We agree.  For P4, we agree with Qualcomm that this is only needed when the UE supports 5G->3G SRVCC. (Based on the discussion in SRVCC WID, we think the network can configure UTRA-FDD measurement only if the UE supports SRVCC). |
|  |  |  |
|  |  |  |

## 2.3 ASN.1 issues and RRC Corrections

According to chairman notes, the following contributions are classified as ASN.1 issues and RRC Corrections.

[R2-2003425](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2003425.zip) [Z301] Correcction for SCG RLC failure during fast MCG recovery ZTE Corporation, Sanechips discussion Rel-16 LTE\_NR\_DC\_CA\_enh-Core

[R2-2002790](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002790.zip) Correction on the Configuration of T316 [C103] [C104] CATT draftCR Rel-16 38.331 16.0.0 F LTE\_NR\_DC\_CA\_enh-Core Late

[R2-2002984](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_109bis-e\Docs\R2-2002984.zip) Erroneous instances of “the procedure ends” impacting reception over SRB3 Nokia, Nokia Shanghai Bell CR Rel-16 38.331 16.0.0 1538 - F LTE\_NR\_DC\_CA\_enh-Core

Companies are encouraged to provide comments on those:

### 2.3.1 [Z301] Correction for SCG RLC failure during fast MCG recovery ([R2-2003425](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003425))

|  |  |  |
| --- | --- | --- |
| Company | Proposal  (Agree/Disagree) | Comments |
| Nokia | We would prefer Alt1, i.e.:  Alt1: The UE shall not trigger the failure information procedure | We prefer Alt1. This is in line with the current specification that disallows use of the SCG for FailureInformation. Otherwise we risk SCG RLF -> RRC re-establishment just before the UE would receive response to MCGFailureInfo. |
| Qualcomm | Prefer Alt-1 | Same view as Nokia |
| ZTE | Prefer Alt-2 | Regarding Nokia’s comment, we think there is no big issue to transmit the SCG FailureInformation over SCG leg of split SRB1. UE triggers FailureInformation because problem occurs on SCell, but the quality of PSCell is still good. So it won’t cause SCG RLF by just sending this message.  For Alt-1, we are not sure whether the UE can resend the FailureInformation after MCG is recovered. For Alt-2, it allows the network can take action (i.e. release/reconfigure the problem SCell) in time. |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.3.2 Correction on the Configuration of T316 [C103] [C104] ([R2-2002790](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2002790))

|  |  |
| --- | --- |
| Company | Comments |
| Nokia | Some sympathy for the intention. The current way is indeed a bit ugly |
| Qualcomm | Same view as CATT and Nokia. We also think the current way (i.e. T316 configured in the *RLF-TimersAndConstants)* will bring some unnecessary issues because T316 is also used to indicated ON/OFF of fast MCG recovery. |
| ZTE | We are ok to move T316 outside RLF-TimerAndContants, and we think it is better to use “SetupRelease{}” for this field, so network can disable the function, or maintain the value when the field is absent. |
|  |  |
|  |  |
|  |  |

### 2.3.3 Erroneous instances of “the procedure ends” impacting reception over SRB3 ([R2-2002984](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2002984))

|  |  |
| --- | --- |
| Company | Comments |
| Nokia | (Nokia CR) – we agree. |
| Qualcomm | Agree |
| ZTE | For the yellow highlighted bullets, we assume the UE will generate a *RRCReconfigurationComplete* message embedded in MN RRCReconfigurationComplete message, and submit to network via SRB1. However, it seems there is no description in section 5.3.5.3 to capture this?  1> else if the *RRCReconfiguration* message was received via SRB3 (UE in NR-DC):  2> if the *RRCReconfiguration* message was received within *DLInformationTransferMRDC*:  3> if the *RRCReconfiguration* message was received within the *nr-SCG* within *mrdc-SecondaryCellGroup* (NR SCG RRC Reconfiguration):  4> if *reconfigurationWithSync* was included in *spCellConfig* in *nr-SCG*:  5> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];  4> else  5> the procedure ends;  3> else  4> submit the *RRCReconfigurationComplete* message via SRB1 to lower layers for transmission using the new configuration;  2> else  3> submit the *RRCReconfigurationComplete* message via SRB3 to lower layers for transmission using the new configuration; |
|  |  |
|  |  |
|  |  |

# Conclusion

In the previous sections we made the following observations:

Based on the discussion in the previous sections we propose the following:

# References

[1]