**3GPP TSG-RAN WG2 Meeting #109bis-eR2-2002782**

**eMeeting, 20th – 30th April, 2020**

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **1730** | **rev** | **1** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of NeedForGap capability for NR measurement |
|  |  |
| ***Source to WG:*** | MediaTek Inc. |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core, TEI16 |  | ***Date:*** | 2020/04/20 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In release 15, the capability for requirement of measurement gap on NR measurement is not introduced due to time limitation. This results in the network configures measurement gap in most case even if the UE is capable of doing gapless in some scenario. It is proposed to have this capability in release 16. |
|  |  |
| ***Summary of change:*** | Add the capability description for the requirement of measurement gap on NR measurement. |
|  |  |
| ***Consequences if not approved:*** | The network always has to configure measurement gap for NR measurement. It will result in performance lost. |
|  |  |
| ***Clauses affected:*** | 4.3.6.xx (New) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.331 CR 4197 |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

1st change

### 4.3.6 Measurement parameters

#### 4.3.6.1 *interFreqNeedForGaps* and *interRAT-NeedForGaps*

These fields define for each supported E-UTRA band whether measurement gaps are required to perform inter-frequency measurements on each supported E-UTRA radio frequency band and inter-RAT measurements on each supported RAT/band combination. A UE also indicates for each band combination as in the supportedBandCombination whether measurement gaps are required to perform inter-frequency measurements on each supported E-UTRA radio frequency band and inter-RAT measurements on each supported RAT/band combination.

<Skip unrelated part>

4.3.6.36 *measGapPatterns-r15*

This field defines whether the UE that supports NR supports gap patterns 4 to 11 in LTE standalone as specified in TS 36.133 [16], and for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC as specified in TS38.133 [37].

4.3.6.37 *dl-ChannelQualityReporting-r16*

This field defines whether the UE supports DL channel quality reporting of the serving cell or configured carrier for FDD in RRC\_CONNECTED as specified in TS 36.331 [5]. This feature is only applicable if the UE supports *ce-ModeA-r13* or if the UE supports any *ue-Category-NB*.

Editor's note: Whether to have a common or separate capability with MTC, and how to name it if common.

4.3.6.xx *interRAT-NeedForGapsNR*

This field defines for each supported E-UTRA band or band combination whether measurement gaps are required to perform SSB based inter-RAT measurements on each supported NR band.