**3GPP TSG-RAN WG2 Meeting#109bis electronic R2-200xxxx**

**20th - 30th April, 2020**

**Source: ZTE Corporation, Sanechips**

**Title: draft\_Report of offline [AT109bis-e][108][RACS] Stage 3 CRs (ZTE)**

**Agenda item:** **6.5.1**

**Document for:** **Discussion and Decision**

# Introduction

This is the report for the following offline discussion:

* **[AT109bis-e][108][RACS] Stage 3 CRs (ZTE)**

Scope: discuss the 36.331 and 38.331 CRs in [R2-2003290](file:///C:\Data\3GPP\Extracts\R2-2003290_38.331_(REL_16)_CR1553_Correction%20to%20transfer%20of%20UE%20capabilities%20at%20HO%20forRACS%20(38.331).docx) and [R2-2003305](file:///C:\Data\3GPP\Extracts\R2-2003305.docx) and the additional proposals in [R2-2002881](file:///C:\Data\3GPP\Extracts\R2-2002881.doc) and [R2-2003471](file:///C:\Data\3GPP\Extracts\R2-2003471%20UE%20capability%20indication%20for%20segmentation.doc)

Intended outcome: In-principle agreed 36.331 and 38.331 CRs

Deadline for companies' feedback: Thursday 2020-04-23 10:00 UTC

Deadline for rapporteur version for agreement: Friday 2020-04-24 10:00 UTC

# Stage 3 CRs

## **38.331 CR (R2-2003290)**

RAN2 understand that it is optional to include UE radio access capabilities in the *HandoverPreparationInformation* message when RACS is supported and UE Radio Capability ID is used and sent an LS from RAN2#109-e to SA2 [1] about that.

Based on the ASN.1, it is already optional, but there is a note specifying which UE capabilites shall be sent, so the note needs to be updated for the RACS case. The following changes are proposed [2].

------------------------------------------------------------------------------------------------------------------------------------------------------

– *HandoverPreparationInformation*

This message is used to transfer the NR RRC information used by the target gNB during handover preparation or UE context retrieval, e.g. in case of resume or re-establishment, including UE capability information. This message is also used for transferring the information between the CU and DU.

\*\*\*\*\*\*\*\*\*omitted unchanged parts\*\*\*\*\*\*\*\*\*

NOTE 1: The following table indicates per source RAT whether RAT capabilities are included or not when UE Radio Capability ID as specified in 23.502 [X] is not used for the UE. If UE Radio Capability ID is used for the UE, all UE radio access capabilities are optional.

|  |  |  |  |
| --- | --- | --- | --- |
| **Source RAT** | **NR capabilites** | **E-UTRA capabilities** | **MR-DC capabilities** |
| NR | Included | May be included | May be included |
| E-UTRAN | Included | May be included | May be included |

NOTE 2: The following table indicates, in case of inter-RAT handover from E-UTRA, which additional IEs are included or not:

|  |  |  |  |
| --- | --- | --- | --- |
| **Source system** | **sourceConfig** | **rrm-Config** | **as-Context** |
| E-UTRA/EPC | Not included | May be included | Not included |
| E-UTRA/5GC | May be included, but only *radioBearerConfig* is included in the *RRCReconfiguration*. | May be included | Not included |

------------------------------------------------------------------------------------------------------------------------------------------------------

**Q1) Do companies agree with the above change in TS38.331?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments** |
| Ericsson | Agree with intention. | After further consideration we think that a NOTE is not the most appropriate way to capture this. NOTEs are informative but this behavior described in the addition to the NOTE seem to talk about normative behavior.  The tables below the NOTE says that the capabilities are included (always). The NOTE however says that the capabilities are optionally included when the RACS ID is used.  Perhaps a better way would be something along the lines of the following:   |  |  |  |  | | --- | --- | --- | --- | | **Source RAT** | **NR capabilites** | **E-UTRA capabilities** | **MR-DC capabilities** | | NR | May be included if UE Radio Capability ID is not used for the UE. Included otherwise. | May be included | May be included | | E-UTRAN | May be included if UE Radio Capability ID is not used for the UE. Included otherwise. | May be included | May be included | |
|  |  |  |
|  |  |  |
|  |  |  |

## **36.331 CR (R2-2003305)**

Similarly, RAN2 understand that it is optional to include UE radio access capabilities in the *HandoverPreparationInformation* message when transferring EUTRA RRC information used by the target eNB or target ng-eNB if RACS is supported and UE Radio Capability ID is used. The following changes are proposed [3] to update the note about presence of the UE radio capabilities in *HandoverPreparationInformation* message.

------------------------------------------------------------------------------------------------------------------------------------------------------

– *HandoverPreparationInformation*

This message is used to transfer the E-UTRA RRC information used by the target eNB or target ng-eNB during handover preparation or UE context retrieval, e.g. in case of resume or re-establishment, including UE capability information.

Direction: source eNB/ source RAN to target eNB or target ng-eNB

\*\*\*\*\*\*\*\*\*omitted unchanged parts\*\*\*\*\*\*\*\*\*

NOTE 1: The source typically sets the *ue-ConfigRelease* to the release corresponding with the current dedicated radio configuration. The source may however also consider the common radio resource configuration e.g. in case interoperability problems would appear if the UE temporary continues extensions of this part of the configuration in a target PCell not supporting them.

NOTE 2: The following table indicates per source RAT whether RAT capabilities are included or not when UE Radio Capability ID as specified in 23.502 [X] is not used for the UE. If UE Radio Capability ID is used for the UE, all UE radio access capabilities are optional for handover from E-UTRAN or NR.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Source RAT** | **E-UTRA capabilites** | **UTRA capabilities** | **GERAN capabilities** | **MR DC capabilities** | **NR capabilities** |
| UTRAN | Included | May be included, ignored by eNB if received | May be included | Excluded | Excluded |
| GERAN CS | Excluded | May be included, ignored by eNB if received | Included | Excluded | Excluded |
| GERAN PS | Excluded | May be included, ignored by eNB if received | Included | Excluded | Excluded |
| E-UTRAN | Included | May be included | May be included | May be included | May be included |
| NR | Included | Excluded | Excluded | May be included | May be included |

------------------------------------------------------------------------------------------------------------------------------------------------------

**Q2) Do companies agree with the above change in TS36.331?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments** |
| Ericsson | Agree with intention. | See comment above. |
|  |  |  |
|  |  |  |
|  |  |  |

# New proposals

## **Issue 1: Transmission of UE capability information message in SRB2 if segmented**

With the assumption that the segmented *UECapabilityInformation* message may block the transfer of other important SRB1 message e.g. measurement report, it has been proposed in [3] that UE capability information message should be transmitted in SRB1 if not segmented and in SRB2 if segmented to avoid the future blocking problem i.e. not transmitting the important UL message.

**Q3) Do companies agree that the UE capability information message should be transmitted in SRB2 if it is segmented to avoid future blocking problem?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments** |
| Ericsson | No | It is too late. |
|  |  |  |
|  |  |  |
|  |  |  |

## **Issue 2: Indicating UE’s support for segmentation**

With the understanding that knowing UE’s support for capability information segmentation might be helpful for the network to decide how to enquire the UE capabilities, it has been proposed in [5] that the UE should report the capability of supporting segmentation to the gNB/eNB before the gNB/eNB sends the *UECapabilityEnquiry* message.

**Q4) Do companies agree that UE should indicate support for segmentation to the network before network sends the *UECapabilityEnquiry* message?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments** |
| Ericsson | No | It is too late. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

***To be added.***

# References

1. R2-2001891 LS on RACS and signaling of UE capabilities at handover(contact: Ericsson)
2. R2-2003290 Correction to transfer of UE capabilities at HO for RACS(38.331) ZTE Corporation, Ericsson,MediaTek Inc.,Sanechips
3. R2-2003305 Correction to transfer of UE capabilities at HO for RACS (36.331) MediaTek Inc., Ericsson, ZTE Corporation, Sanechips
4. R2-2002881 Transfer of segmented UECapabilityInformation by SRB2 Samsung
5. R2-2003471 UE capability indication for segmentation Huawei, HiSilicon