RAN1 Agreements for WUS Resource location based on Resource 0 Location

|  |  |  |  |
| --- | --- | --- | --- |
| freqLocation of WUS resource 0 | n0 | n2 | n4 |
| WUS resource locations | |  |  |  |  | | --- | --- | --- | --- | | *f* | 2 | 0 |  | |  | 3 | 1 |  | |  |  |  | *t* | | Alt1:   |  |  |  |  | | --- | --- | --- | --- | | *f* | 3 | 1 |  | |  | 2 | 0 |  | |  |  |  | *t* |   Alt2:   |  |  |  |  | | --- | --- | --- | --- | | *f* |  |  |  | |  | 2 | 0 |  | |  | 3 | 1 | *t* |   Alt1 if NB is below  center carrier; otherwise Alt2. | |  |  |  |  | | --- | --- | --- | --- | | *f* |  |  |  | |  | 3 | 1 |  | |  | 2 | 0 | *t* | |