RAN1 Agreements for WUS Resource location based on Resource 0 Location

|  |  |  |  |
| --- | --- | --- | --- |
| freqLocation of WUS resource 0 | n0 | n2 | n4 |
| WUS resource locations  |

|  |  |  |  |
| --- | --- | --- | --- |
| *f* |  2 | 0 |  |
|  | 3 | 1 |  |
|  |  |  | *t* |

 | Alt1:

|  |  |  |  |
| --- | --- | --- | --- |
| *f* |  3 | 1 |  |
|  | 2 | 0 |  |
|  |  |  | *t* |

Alt2:

|  |  |  |  |
| --- | --- | --- | --- |
| *f* |  |  |  |
|  | 2 | 0 |  |
|  | 3 | 1 | *t* |

Alt1 if NB is below center carrier; otherwise Alt2. |

|  |  |  |  |
| --- | --- | --- | --- |
| *f* |  |  |  |
|  | 3 | 1 |  |
|  | 2 | 0 | *t* |

 |