3GPP TSG-RAN WG2 Meeting #109bis-e Draft-R2-2003928

Online, April 20th – 30th , 2020

**Agenda item: 7.1.8**

**Source: Qualcomm**

**Title: Report for [AT109bis-e][413][eMTC] Mobility enhancements - Open issues (Qualcomm)**

**Document for: Report**

# 1 Scope of the email discussion

This document contains the summary of the documents in Agenda item 7.1.8 regarding two issues (1) early implementable of Relaxed serving cell measurement when using WUS from Rel-15 [1] and (2) RSS [2], [3], [4] as per below email discussion:

* [AT109bis-e][413][eMTC] Mobility enhancements - Open issues (Qualcomm)

Scope: Remaining open issues on mobility enhancements including [R2-2003188](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003188.zip).

Intended outcome: Report including a list of proposals categorized as agreeable, need further discussion etc.. The outcome can be provided in R2-2003928.

Deadline: Friday, Apr. 24th 10:00 UTC

# 2 Discussion

## Early implementation of Relaxed serving cell measurement

Relaxed serving cell measurement when using WUS was discussed in Rel-15 and it was introduced for NB-IoT from Rel-15 but it could not be concluded for eMTC due to lack of time. As clarified in [1], it is introduced from Release 16. This feature has no UE capability indication and is linked to support for WUS. [1] proposes that a Release 15 UE supporting WUS can also make use of this power saving feature provided network broadcasts *numDRX-CyclesRelaxed-r16* and the UE meets the conditions specified for relaxed serving cell measurement by RAN4 in TS 36.133.

**Question 1: Do companies see any issue in allowing early implementation of relaxed serving cell measurement (i.e., *numDRX-CyclesRelaxed-r16*) when WUS is used from Rel-15?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
|  |  |  |
|  |  |  |

**Question 2: If answer to Question 1 is NO, please elaborate how to realize the early implementation of relaxed serving cell measurement (i.e., *numDRX-CyclesRelaxed-r16*) for Rel-15 UEs?**

Option A): Update the early implementable table in TS 36.331 (as proposed in [1])

Option B): TEI-15 CR

Option C): Any other

|  |  |  |
| --- | --- | --- |
| **Company** | **Which option** | **Comment** |
|  |  |  |
|  |  |  |

## RSS

For RSS, email discussion was concluded with a text proposal and a proposal to further discuss whether dedicated signalling is needed for the configuration of RSS in [2]. In RAN2#109bis-e meeting, it is agreed to take the text proposal in [3] as baseline.

According to RAN1 parameter list [5], if a neighbour cell list is not present in neighbour cell list, then UE assumes the RSS power bias is same as that used for serving cell or camped on cell. The UE can also assume same when neighbour cell list is absent from SIB4 or SIB5 (i.e., NCL is not present so a neighbour cell is NOT present in NCL).

|  |  |  |  |
| --- | --- | --- | --- |
| RSS NCL power bias | Power bias in dB relative to CRS's q\_offset of cells in the neighbor cell list for CE mode A/B in RRC\_IDLE and RRC\_CONNECTED and where one value indicates that RSS is not used for that neighbor cell. | -6, -3, 0, 3, 6, 9, 12, rssNotUsed | Cell specific |

|  |  |  |  |
| --- | --- | --- | --- |
| rss-measurement-non-NCL-enabled | A one bit indicator indicating whether RSS of neighbour cells that are NOT in the Neighbour Cell List can be used for measurements for CE mode A/B in RRC\_IDLE and RRC\_CONNECTED. When indicated as Enabled, the UE assumes that the RSS power bias is the same as that used for the serving cell or the camped on cell, for all neighbour cells that are NOT in the Neighbour Cell List. | Enabled | Cell specific |

However, there is proposal whether to use default value of zero if a neighbour cell is missing in neighbour cell list.

**Question 3: For all neighbour cells that are NOT in the Neighbour Cell List (NCL), what value of RSS power bias UE assumes?**

Option A) Follow what RAN1 has indicated (i.e., assume that the RSS power bias is the same as that used for the serving cell or the camped on cell).

Option B) use default value 0.

Option C) *rss-MeasPowerBias-r16* is provided as default value in SIB2

|  |  |  |
| --- | --- | --- |
| **Company** | **Which option** | **Comments** |
|  |  |  |
|  |  |  |

To apply the RSS power bias of a neighbour cell, UE needs to know the q\_offset value of the neighbour cell. The value of q\_offset is present in NCL in SIB. However, RSS power bias (*rss-MeasPowerBias-r16*) is OPTIONAL in the NCL and neighbour cell list may be present, for example in SIB4 and SIB5, as per proposed text [3] but the RSS power bias may be absent.

**Question 4: If a neighbour cell is in the Neighbour Cell List (NCL) but RSS power bias is NOT in the NCL, what value of RSS power bias UE assumes?**

Option A) same as that used for the serving cell or the camped on cell

Option B) use default value 0.

Option C) *rss-MeasPowerBias-r16* is provided as default value in SIB2 (as captured in [3])

|  |  |  |
| --- | --- | --- |
| **Company** | **Which option** | **Comments** |
|  |  |  |
|  |  |  |

RAN2 has received the latest feature list from RAN1, see [5]. Specially the UE may need to meet certain conditions to use of RSS in connected mode, for example, the RSS of the neighbour cell may be in different narrowband than the unicast narrowband. Also, the configured measurement gap may not work for neighbour cells as the RSS occasion may not fall in the measurement gap. Reconfiguring measurement gap to align with RSS occasion for one neighbour cell may not work for other neighbour cells and can interfere with existing tasks that UE is required to do to meet RRM requirements. Therefore, there is high probability that UE may not benefit much from RSS in RRC\_CONNECTED. Currently this is still work in progress in RAN4. Furthermore, according to latest RAN1 feature list [5], a separate UE capability may be needed for IDLE mode and RRC\_CONNECTED mode. It is up to RAN4 to decide whether eNB needs to know UE supports RSS-based measurement and whether RSS-based measurement is mandatory.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Feature group | Prerequisite feature groups | Need for the eNB to know if the feature is supported | Need of FDD/TDD differentiation | Capability interpretation for mixture of FDD/TDD | Note | Mandatory/Optional |
| RSS-based measurement improvement | Rel-15 RSS | Up to RAN4 | Yes | N/A | It is up to RAN2/RAN4 whether to have separate capabilities for Idle and Connected.  FFS: Whether it might also be relevant to consider separate capabilities for CE mode A and B  FFS: Consider removing this row since it will be part of the RAN4 UE feature list. | Up to RAN4 |

**Question 5: Should RAN2 wait RAN4 progress to capture UE capability signalling to use RSS in RRC\_IDLE and RRC\_CONNECTED?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |

In addition, the RSS configuration of the neighbour cell has to be provided in SIB as indicated by RAN1. If UE has acquired the RSS configuration from the SIB, then it can use that information when in RRC\_CONNECTED. This is already clear in the field description provided in [3] and, if needed, additional clarification can be added. In addition, if the dedicated signalling is missing, UE has to use the RSS parameters provided in SIB anyway. So, there is no guarantee that UE in RRC\_CONNECTED does not have to use RSS parameters provided in SIB. UE also needs q\_offset of each neighbour cell to apply the RSS power bias which significantly increases the dedicated signalling overhead.

It is possible that UE may declare RLF and perform RRC re-establishment to a target cell without acquiring SIB4 and SIB5 of the target cell. It is possible that network may handover the UE in RRC\_CONNECTED to a target cell. The UE may not acquire the SIB4 and SIB5 of the target cell in RRC\_CONNECTED since the UE may be provided with SIB1 and SIB2 of the target cell in handover command message. In this case, a neighbour cell may not be in the stored NCL but it may be present in NCL broadcast by the target cell. What UE assumes in this case needs to be clarified. In addition, RSS may be collocated with source cell (i.e., RSS information is not present in source cell) and the UE needs to know whether it is collocated with the target cell.

**Question 6: In RRC\_CONNECTED mode, how does UE update the neighbour cell list (NCL) for a new target cell?**

Option A) RSS configuration for the target cell are provided in HO command message.

Option B) RSS information for intra-frequency and inter-frequency neighbour cell list is provided in SIB2 instead of SIB4 and SIB5.

Option C) RSS information is provided as part of a list of measurement objects in RRC reconfiguration message [4].

Option D) Do nothing. If UE has NOT stored the RSS power bias of a neighbour cell, the UE behaviour can be same as if the neighbour cell is not present in NCL. An indication whether RSS is collocated or not is provided to UE via SIB2.

Option E) Wait for further RAN4 progress

Option D) Any other

|  |  |  |
| --- | --- | --- |
| **Company** | **Which option** | **Please elaborate the solution** |
|  |  |  |
|  |  |  |

**Question 7: Any other issue?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **If yes, please elaborate the issue** |
|  |  |  |
|  |  |  |

# 3 Conclusion

To be updated…

# 3 References

[1] R2-2003188 Permit early implementation of relaxed serving cell measurement.

[2] R2-2003141 Report on Email discussion RSS Configurations.

[3] R2-2003138 Introduction of RSS Configurations

[4] R2-2003814 Addressing FFSs for RSS configuration.

[5] R2-2002519 LS on updated Rel-16 LTE and NR parameter lists.