**3GPP TSG-RAN WG2 Meeting 109bis-e *R2-2003986***

Online, 20 – 24 Apr, 2020

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | DraftCR | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on SSB configuration in RRC spec |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_pos-Core |  | ***Date:*** | 2020-04-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | With the conclusion of the following email discussion* [Post109e#31][NR/Pos] Details of spatial relation for positioning (Huawei)

Scope: Continue the discussion from R2-2001936 and resolve open issues. Intended outcome: Summary for next meetingWe have agreed that for the SSB configuraiton for SRS, the UE can obtain the SSB configuarion either by full configuration in RRC or by indexing of PCI and SSB index to the SSB-configuration provided by LPP message for either DL-only positioning or multi-RTT. Update during 109bis-eDuring the meeting, the following agreements have been made on the above discussion:Agreements:Spatial relation of SRS is recommended by the LMF and decided by the gNB. It is up to gNB implementation whether to follow the LMF recommendation. The gNB informs the LMF of its decision.UE does not report RSRP of DL-PRS in RRC procedures for SRS configuration. Keep the current SSB configuration for the DL-only positioning in the LPP message. Keep the current configuration of SSB in RRC for UL-only positioning. This means that the RRC configuration can carry the full SSB configuration or SSB index and PCI.For the assistance information in NRPPa for SSB configuration for UL-only positioning, it should include both TF configuration and SSB index in the NRPPa message.Based on the above agreement, RRC spec needs to be chagned accordingly.  |
|  |  |
| ***Summary of change:*** | 1/ Change the need code of ssb-Configuration to need M to need S2/ Add the field description for PhysicalCellId, ssb-index and ssb-Configuration.  |
|  |  |
| ***Consequences if not approved:*** | UE may not receive neighbor SSB Configuration, thus causing ineffiecieint SRS transmission. |
|  |  |
| ***Clauses affected:*** | 6.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** | R2-2003056 |

===============================================================FIRST CHANGE===================================================

#### – *SRS-Config*

The IE *SRS-Config* is used to configure sounding reference signal transmissions. The configuration defines a list of SRS-Resources and a list of SRS-ResourceSets. Each resource set defines a set of SRS-Resources. The network triggers the transmission of the set of SRS-Resources using a configured aperiodicSRS-ResourceTrigger (L1 DCI).

*SRS-Config* information element

-- ASN1START

-- TAG-SRS-CONFIG-START

SRS-Config ::= SEQUENCE {

 srs-ResourceSetToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSetId OPTIONAL, -- Need N

 srs-ResourceSetToAddModList SEQUENCE (SIZE(1..maxNrofSRS-ResourceSets)) OF SRS-ResourceSet OPTIONAL, -- Need N

 srs-ResourceToReleaseList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-ResourceId OPTIONAL, -- Need N

 srs-ResourceToAddModList SEQUENCE (SIZE(1..maxNrofSRS-Resources)) OF SRS-Resource OPTIONAL, -- Need N

 tpc-Accumulation ENUMERATED {disabled} OPTIONAL, -- Need S

 ...,

 [[

 srs-PosResourceSetToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets)) OF SRS-PosResourceSetId-r16 OPTIONAL, -- Need N

 srs-PosResourceSetToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets)) OF SRS-PosResourceSet-r16 OPTIONAL, -- Need N

 srs-PosResourceToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources)) OF SRS-PosResourceId-r16 OPTIONAL, -- Need N

 srs-PosResourceToAddModList-r16 SEQUENCE (SIZE(1..maxNrofSRS-PosResources)) OF SRS-PosResource-r16 OPTIONAL -- Need N

 ]]

}

SRS-ResourceSet ::= SEQUENCE {

 srs-ResourceSetId SRS-ResourceSetId,

 srs-ResourceIdList SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-ResourceId OPTIONAL, -- Cond Setup

 resourceType CHOICE {

 aperiodic SEQUENCE {

 aperiodicSRS-ResourceTrigger INTEGER (1..maxNrofSRS-TriggerStates-1),

 csi-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 slotOffset INTEGER (1..32) OPTIONAL, -- Need S

 ...,

 [[

 aperiodicSRS-ResourceTriggerList SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-2))

 OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL -- Need M

 ]]

 },

 semi-persistent SEQUENCE {

 associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 ...

 },

 periodic SEQUENCE {

 associatedCSI-RS NZP-CSI-RS-ResourceId OPTIONAL, -- Cond NonCodebook

 ...

 }

 },

 usage ENUMERATED {beamManagement, codebook, nonCodebook, antennaSwitching},

 alpha Alpha OPTIONAL, -- Need S

 p0 INTEGER (-202..24) OPTIONAL, -- Cond Setup

 pathlossReferenceRS CHOICE {

 ssb-Index SSB-Index,

 csi-RS-Index NZP-CSI-RS-ResourceId

 } OPTIONAL, -- Need M

 srs-PowerControlAdjustmentStates ENUMERATED { sameAsFci2, separateClosedLoop} OPTIONAL, -- Need S

 ...

}

SRS-PosResourceSet-r16 ::= SEQUENCE {

 srs-PosResourceSetId-r16 SRS-PosResourceSetId-r16,

 srs-PosResourceIdList-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-PosResourceId-r16 OPTIONAL, -- Cond Setup

 resourceType-r16 CHOICE {

 aperiodic-r16 SEQUENCE {

 aperiodicSRS-ResourceTriggerList-r16 SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-1))

 OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL, -- Need M

 slotOffset-r16 INTEGER (1..32) OPTIONAL, -- Need S

 ...

 },

 semi-persistent-r16 SEQUENCE {

 ...

 },

 periodic-r16 SEQUENCE {

 ...

 }

 },

 alpha-r16 Alpha OPTIONAL, -- Need S

 p0-r16 INTEGER (-202..24) OPTIONAL, -- Cond Setup

 pathlossReferenceRS-Pos-r16 CHOICE {

 ssb-Index-16 SSB-Index,

 csi-RS-Index-r16 NZP-CSI-RS-ResourceId,

 ssb-r16 SSB-InfoNcell-r16,

 dl-PRS-r16 DL-PRS-Info-r16

 } OPTIONAL, -- Need M

 ...

}

SRS-ResourceSetId ::= INTEGER (0..maxNrofSRS-ResourceSets-1)

SRS-PosResourceSetId-r16 ::= INTEGER (0..maxNrofSRS-PosResourceSets-1)

SRS-Resource ::= SEQUENCE {

 srs-ResourceId SRS-ResourceId,

 nrofSRS-Ports ENUMERATED {port1, ports2, ports4},

 ptrs-PortIndex ENUMERATED {n0, n1 } OPTIONAL, -- Need R

 transmissionComb CHOICE {

 n2 SEQUENCE {

 combOffset-n2 INTEGER (0..1),

 cyclicShift-n2 INTEGER (0..7)

 },

 n4 SEQUENCE {

 combOffset-n4 INTEGER (0..3),

 cyclicShift-n4 INTEGER (0..11)

 }

 },

 resourceMapping SEQUENCE {

 startPosition INTEGER (0..5),

 nrofSymbols ENUMERATED {n1, n2, n4},

 repetitionFactor ENUMERATED {n1, n2, n4}

 },

 freqDomainPosition INTEGER (0..67),

 freqDomainShift INTEGER (0..268),

 freqHopping SEQUENCE {

 c-SRS INTEGER (0..63),

 b-SRS INTEGER (0..3),

 b-hop INTEGER (0..3)

 },

 groupOrSequenceHopping ENUMERATED { neither, groupHopping, sequenceHopping },

 resourceType CHOICE {

 aperiodic SEQUENCE {

 ...

 },

 semi-persistent SEQUENCE {

 periodicityAndOffset-sp SRS-PeriodicityAndOffset,

 ...

 },

 periodic SEQUENCE {

 periodicityAndOffset-p SRS-PeriodicityAndOffset,

 ...

 }

 },

 sequenceId INTEGER (0..1023),

 spatialRelationInfo SRS-SpatialRelationInfo OPTIONAL, -- Need R

 ...

}

SRS-PosResource-r16::= SEQUENCE {

 srs-PosResourceId-r16 SRS-PosResourceId-r16,

 transmissionComb-r16 CHOICE {

 n2-r16 SEQUENCE {

 combOffset-n2-r16 INTEGER (0..1),

 cyclicShift-n2-r16 INTEGER (0..7)

 },

 n4-r16 SEQUENCE {

 combOffset-n4-16 INTEGER (0..3),

 cyclicShift-n4-r16 INTEGER (0..11)

 },

 n8-r16 SEQUENCE {

 combOffset-n8-r16 INTEGER (0..7),

 cyclicShift-n8-r16 INTEGER (0..5)

 },

 **...**

},

 resourceMapping-r16 SEQUENCE {

 startPosition-r16 INTEGER (0..13),

 nrofSymbols-r16 ENUMERATED {n1, n2, n4, n8, n12}

 },

 freqDomainShift-r16 INTEGER (0..268),

 freqHopping-r16 SEQUENCE {

 c-SRS-r16 INTEGER (0..63)

 },

 groupOrSequenceHopping-r16 ENUMERATED { neither, groupHopping, sequenceHopping },

 resourceType-r16 CHOICE {

 aperiodic-r16 SEQUENCE {

 ...

 },

 semi-persistent-r16 SEQUENCE {

 periodicityAndOffset-sp-r16 SRS-PeriodicityAndOffset-r16,

 ...

 },

 periodic-r16 SEQUENCE {

 periodicityAndOffset-p-r16 SRS-PeriodicityAndOffset-r16,

 ...

 }

 },

 sequenceId-r16 INTEGER (0..65535),

 spatialRelationInfoPos-r16 SRS-SpatialRelationInfoPos-r16 OPTIONAL, -- Need R

 ...

}

SRS-SpatialRelationInfo ::= SEQUENCE {

 servingCellId ServCellIndex OPTIONAL, -- Need S

 referenceSignal CHOICE {

 ssb-Index SSB-Index,

 csi-RS-Index NZP-CSI-RS-ResourceId,

 srs SEQUENCE {

 resourceId SRS-ResourceId,

 uplinkBWP BWP-Id

 }

 }

}

SRS-SpatialRelationInfoPos-r16 ::= SEQUENCE {

 servingCellId-r16 ServCellIndex OPTIONAL, -- Need S

 referenceSignal-r16 CHOICE {

 ssb-IndexServing-r16 SSB-Index,

 csi-RS-IndexServing-r16 NZP-CSI-RS-ResourceId,

 srs-SpatialRelation-r16 SEQUENCE {

 resourceSelection-r16 CHOICE {

 srs-ResourceID-r16 SRS-ResourceID

 srs-PosResourceID-r16 SRS-PosResourceID-r16

 }

 uplinkBWP-r16 BWP-Id

 },

 ssbNcell-r16 SSB-InfoNcell-r16,

 dl-PRS-r16 DL-PRS-Info-r16

 }

}

SSB-Configuration-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueNR,

 halfFrameIndex-r16 ENUMERATED {zero, one},

 ssbSubcarrierSpacing-r16 SubcarrierSpacing,

 ssb-periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2,spare1 } OPTIONAL, -- Need S

 smtc-r16 SSB-MTC OPTIONAL, -- Need S

 sfn-Offset-r16 INTEGER (0..maxNumFFS),

 sfn-SSB-Offset-r16 INTEGER (0..15),

 ss-PBCH-BlockPower-r16 INTEGER (-60..50) OPTIONAL –- Cond Pathloss

}

SSB-InfoNcell-r16 ::= SEQUENCE {

 physicalCellId-r16 PhysCellId,

 ssb-IndexNcell-r16 SSB-Index,

 ssb-Configuration-r16 SSB-Configuration-r16 OPTIONAL -- Need S

}

DL-PRS-Info-r16 ::= SEQUENCE {

 trp-Id-r16 INTEGER (0..255),

 dl-PRS-ResourceSetId-r16 INTEGER (0..7),

 dl-PRS-ResourceId-r16 INTEGER (0..63) OPTIONAL –- Cond Pathloss

}

SRS-ResourceId ::= INTEGER (0..maxNrofSRS-Resources-1)

SRS-PosResourceId-r16 ::= INTEGER (0..maxNrofSRS-PosResources-1)

SRS-PeriodicityAndOffset ::= CHOICE {

 sl1 NULL,

 sl2 INTEGER(0..1),

 sl4 INTEGER(0..3),

 sl5 INTEGER(0..4),

 sl8 INTEGER(0..7),

 sl10 INTEGER(0..9),

 sl16 INTEGER(0..15),

 sl20 INTEGER(0..19),

 sl32 INTEGER(0..31),

 sl40 INTEGER(0..39),

 sl64 INTEGER(0..63),

 sl80 INTEGER(0..79),

 sl160 INTEGER(0..159),

 sl320 INTEGER(0..319),

 sl640 INTEGER(0..639),

 sl1280 INTEGER(0..1279),

 sl2560 INTEGER(0..2559)

}

SRS-PeriodicityAndOffset-r16 ::= CHOICE {

 sl1 NULL,

 sl2 INTEGER(0..1),

 sl4 INTEGER(0..3),

 sl5 INTEGER(0..4),

 sl8 INTEGER(0..7),

 sl10 INTEGER(0..9),

 sl16 INTEGER(0..15),

 sl20 INTEGER(0..19),

 sl32 INTEGER(0..31),

 sl40 INTEGER(0..39),

 sl64 INTEGER(0..63),

 sl80 INTEGER(0..79),

 sl160 INTEGER(0..159),

 sl320 INTEGER(0..319),

 sl640 INTEGER(0..639),

 sl1280 INTEGER(0..1279),

 sl2560 INTEGER(0..2559),

 sl5120 INTEGER(0..5119),

 sl10240 INTEGER(0..10239),

 sl40960 INTEGER(0..40959),

 sl81920 INTEGER(0..81919),

 ...

}

-- TAG-SRS-CONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *SRS-Config* field descriptions |
| ***tpc-Accumulation***If the field is absent, UE applies TPC commands via accumulation. If disabled, UE applies the TPC command without accumulation (this applies to SRS when a separate closed loop is configured for SRS) (see TS 38.213 [13], clause 7.3). |

|  |
| --- |
| *SRS-Resource* field descriptions |
| ***cyclicShift-n2***Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***cyclicShift-n4***Cyclic shift configuration (see TS 38.214 [19], clause 6.2.1). |
| ***freqHopping***Includes parameters capturing SRS frequency hopping (see TS 38.214 [19], clause 6.2.1). |
| ***groupOrSequenceHopping***Parameter(s) for configuring group or sequence hopping (see TS 38.211 [16], clause 6.4.1.4.2). |
| ***periodicityAndOffset-p***Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). |
| ***periodicityAndOffset-sp***Periodicity and slot offset for this SRS resource. All values are in "number of slots". Value *sl1* corresponds to a periodicity of 1 slot, value *sl2* corresponds to a periodicity of 2 slots, and so on. For each periodicity the corresponding offset is given in number of slots. For periodicity *sl1* the offset is 0 slots (see TS 38.214 [19], clause 6.2.1). |
| ***ptrs-PortIndex***The PTRS port index for this SRS resource for non-codebook based UL MIMO. This is only applicable when the corresponding *PTRS-UplinkConfig* is set to CP-OFDM. The *ptrs-PortIndex* configured here must be smaller than the *maxNrofPorts* configured in the *PTRS-UplinkConfig* (see TS 38.214 [19], clause 6.2.3.1). |
| ***resourceMapping***OFDM symbol location of the SRS resource within a slot including *nrofSymbols* (number of OFDM symbols), *startPosition* (value 0 refers to the last symbol, value 1 refers to the second last symbol, and so on) and *repetitionFactor* (see TS 38.214 [19], clause 6.2.1 and TS 38.211 [16], clause 6.4.1.4). The configured SRS resource does not exceed the slot boundary. |
| ***resourceType***Periodicity and offset for semi-persistent and periodic SRS resource (see TS 38.214 [19], clause 6.2.1). |
| ***sequenceId***Sequence ID used to initialize pseudo random group and sequence hopping (see TS 38.214 [19], clause 6.2.1). |
| ***spatialRelationInfo***Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS (see TS 38.214 [19], clause 6.2.1). |
| ***spatialRelationInfoPos***Configuration of the spatial relation between a reference RS and the target SRS. Reference RS can be SSB/CSI-RS/SRS/DL-PRS (see TS 38.214 [19], clause 6.2.1). |
| ***transmissionComb***Comb value (2 or 4 or 8) and comb offset (0..combValue-1) (see TS 38.214 [19], clause 6.2.1). |

|  |
| --- |
| *SRS-ResourceSet* field descriptions |
| ***alpha***alpha value for SRS power control (see TS 38.213 [13], clause 7.3). When the field is absent the UE applies the value 1. |
| ***aperiodicSRS-ResourceTriggerList***An additional list of DCI "code points" upon which the UE shall transmit SRS according to this SRS resource set configuration (see TS 38.214 [19], clause 6.1.1.2). When the field is not included during a reconfiguration of *SRS-ResourceSet* of *resourceType* set to *aperiodic*, UE maintains this value based on the Need M; that is, this list is not considered as an extension of *aperiodicSRS-ResourceTrigger* for purpose of applying the general rule for extended list in clause 6.1.3. |
| ***aperiodicSRS-ResourceTrigger***The DCI "code point" upon which the UE shall transmit SRS according to this SRS resource set configuration (see TS 38.214 [19], clause 6.1.1.2). |
| ***associatedCSI-RS***ID of CSI-RS resource associated with this SRS resource set in non-codebook based operation (see TS 38.214 [19], clause 6.1.1.2). |
| ***csi-RS***ID of CSI-RS resource associated with this SRS resource set. (see TS 38.214 [19], clause 6.1.1.2). |
| ***p0***P0 value for SRS power control. The value is in dBm. Only even values (step size 2) are allowed (see TS 38.213 [13], clause 7.3). |
| ***pathlossReferenceRS***A reference signal (e.g. a CSI-RS config or a SS block) to be used for SRS path loss estimation (see TS 38.213 [13], clause 7.3). |
| ***pathlossReferenceRS-Pos***A reference signal (e.g. a CSI-RS config or a SS block or a DL PRS config) to be used for SRS path loss estimation (see TS 38.213 [13], clause 7.3). |
| ***resourceType***Time domain behavior of SRS resource configuration, see TS 38.214 [19], clause 6.2.1. The network configures SRS resources in the same resource set with the same time domain behavior on periodic, aperiodic and semi-persistent SRS. |
| ***slotOffset***An offset in number of slots between the triggering DCI and the actual transmission of this *SRS-ResourceSet*. If the field is absent the UE applies no offset (value 0). |
| ***srs-PowerControlAdjustmentStates***Indicates whether hsrs,c(i) = fc(i,1) or hsrs,c(i) = fc(i,2) (if twoPUSCH-PC-AdjustmentStates are configured) or separate close loop is configured for SRS. This parameter is applicable only for Uls on which UE also transmits PUSCH. If absent or release, the UE applies the value sameAs-Fci1 (see TS 38.213 [13], clause 7.3). |
| ***srs-ResourceIdList***The IDs of the SRS-Resources used in this *SRS-ResourceSet*. If this *SRS-ResourceSet* is configured with usage set to codebook, the *srs-ResourceIdList* contains at most 2 entries. If this *SRS-ResourceSet* is configured with *usage* set to *nonCodebook*, the *srs-ResourceIdList* contains at most 4 entries. |
| ***srs-ResourceSetId***The ID of this resource set. It is unique in the context of the BWP in which the parent *SRS-Config* is defined. |
| ***usage***Indicates if the SRS resource set is used for beam management, codebook based or non-codebook based transmission or antenna switching. See TS 38.214 [19], clause 6.2.1. Reconfiguration between codebook based and non-codebook based transmission is not supported. |
| ***halfFrameIndex***Indicates whether SSB is in the first half or the second half of the frame. Value zero indicates the first half and value 1 indicates the second half. |
| ***sfn-Offset***Iindicates the SFN0 offset between the SSB-Cell and the serving cell in the unit of micro-seconds. |
| ***sfn-SSB-Offset*** Indicates the 4 LSBs of the SFN of the cell in which SSB is transmitted |
| ***trp-Id***indicates the TRP ID, see TS 37.355 [xx] |
| ***dl-PRS-ResourceSetId***The ID of the DL PRS resource set, see TS 37.355 [xx] |
| ***dl-PRS-ResourceId***The ID of the DL PRS resource, see TS 37.355 [xx] |
| ***resourceSelection*** Indicates whether the configured SRS spatial relation resource is a *SRS-Resource* or *SRS-PosResource*.  |
| ***ssb-IndexNcell***Indicates SSB index belonging to a non-serving cell |
| ***csi-RS-IndexServingcell***Indicates CSI-RS index belonging to a serving cell |
| ***ssb-IndexSevingcell***Indicates SSB index belonging to a serving cell |

|  |
| --- |
| *SSB-InfoNCell* field descriptions |
| ***physicalCellId***This field specifies the physical cell ID of the neighbour cell for which SSB configuration is provided.  |
| ***ssb-IndexNcell***This field specifies the index of the SSB for a neighbour cell. See TS 38.213 [13]. |
| ***ssb-Configuration***This field specifies the full configuration of the SSB. If this field is absent, the UE obtains the configuration for the SSB from *nr-SSB-Config* received as part of DL PRS assistance datain LPP*,* see TS 37.355 [49], by indexing using the fields *physicalCellId* and *ssb-IndexNCell*. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *Setup* | This field is mandatory present upon configuration of *SRS-ResourceSet* or *SRS-Resource* and optionally present, Need M, otherwise. |
| *NonCodebook* | This field is optionally present, Need M, in case of non-codebook based transmission, otherwise the field is absent. |
| *Pathloss* | The field is mandatory present if *pathlossReferenceRS-Pos* is included; otherwise it is optionally present, Need R |

==============================================END OF CHANGES=================================================================