**3GPP TSG-RAN WG2 Meeting #110-e *R2-200xxxx***

**Online, 1–12 June 2020**

**Agenda item: 5.3.1.1**

**Source: Samsung**

**Title: Report of [AT110e][013][NR15] User Plane Corrections (Samsung)**

**Document for: Discussion and Agreement**

# 1 Introduction

This is to report the result of the following email discussion in RAN2#110-e Meeting [1].

**[AT110e][013][NR15] User Plane Corrections (Samsung)**

 Scope: Treat R2-2004423, R2-2004424, R2-2004940, R2-2004942, R2-2005555, R2-2005557. R2-2005471, and possibly in part 2 R2-2005556, R2-2005558, R2-2005559, R2-2005560, R2-2005561, R2-2005472 (proponents are responsible to explain and drive)

 Part 1: Decision whether to make corrections or not, identify agreeable corrections. Deadline: June 4, 0700 UTC.

 Part 2: Others: For agreeable parts, continuation to agree CRs. Deadline: June 10, 0700 UTC.

# 2 Discussion

## 2.1 Obtaining of PH values

The following contributions were submitted to capture the missing parts (i.e. LTE PH from E-UTRA MAC entity) from the existing text:

[R2-2004423](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004423.zip) Clarification on obtaining of PH values Samsung CR Rel-15 38.321 15.8.0 0738 - F NR\_newRAT-Core

[R2-2004424](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004424.zip) Clarification on obtaining of PH values Samsung CR Rel-16 38.321 16.0.0 0739 - A NR\_newRAT-Core

**Question 1: Do you agree with the proposed change?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with CR? | Additional comments/suggestion |
| Samsung | Yes | The CR merely tries to correct the mistake, so it would not result any NBC issue.  |
| OPPO | Yes |  |
|  |  |  |

**Conclusion:**

…

## 2.2 Preamble selection for beam failure recovery

The following contributions were submitted to change the existing behaviour for preamble selection when dedicated preamble is configured for beam failure recovery:

[R2-2004940](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004940.zip) Clarification on preamble selection for beam failure recovery Google Inc. CR Rel-15 38.321 15.8.0 0749 - F NR\_newRAT-Core

[R2-2004942](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004942.zip) Clarification on preamble selection for beam failure recovery Google Inc. CR Rel-16 38.321 16.0.0 0750 - A NR\_newRAT-Core

**Question 2: Do you agree with the proposed change?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with CR? | Additional comments/suggestion |
| Samsung | No | RAN2 already discussed the issue long time back, and concluded to perform CBRA if no beams meet the condition, as in the current specification. |
| OPPO | No |  |
|  |  |  |

**Conclusion:**

…

## 2.3 BWP inactivity timer operation

The following contributions were submitted to clarify whether *bwp-InactivityTimer* is started (or not) if the MAC entity receives PDCCH which results BWP switching (to default BWP):

[R2-2005555](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005555.zip) Discussion on clarification of BWP inactivity timer operation ASUSTeK discussion Rel-15 NR\_newRAT-Core

[R2-2005556](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005556.zip) Clarification of BWP inactivity timer operation ASUSTeK CR Rel-15 38.321 15.8.0 0753 - F NR\_newRAT-Core

**Question 3: Do you agree with the proposed change?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with CR? | Additional comments/suggestion |
| Samsung | No | From the discussion paper, interpretation b is correct (i.e. not to (re-)start *bwp-InactivityTimer* if the MAC entity receives PDCCH, which results BWP switching to default/initial BWP. However this behaviour is obvious from the existing text, and thus no changes are needed. |
| OPPO | No | The spec is already clear that when PDCCH indicating BWP switching, and if the active BWP after switching happens to be default or initial BWP, UE does not start bwp-InactivityTimer |
|  |  |  |

**Conclusion:**

…

## 2.4 Presence of IEs in BeamFailureRecoveryConfig

The following contributions were submitted to clarify whether network should always configure *rsrp-ThresholdSSB* and *rach-ConfigBFR* (which contains *powerRampingStep*, *preambleReceivedTargetPower*, *preambleTransMax*, and *ra-ResponseWindow*) in *BeamFailureRecoveryConfig* for CFRA BFR:

[R2-2005557](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005557.zip) Discussion on presence of IEs in BeamFailureRecoveryConfig ASUSTeK discussion Rel-15 NR\_newRAT-Core

[R2-2005558](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005558.zip) Clarification on presence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-15 38.331 15.9.0 1679 - F NR\_newRAT-Core

[R2-2005559](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005559.zip) Clarification on presence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-16 38.331 16.0.0 1680 - A NR\_newRAT-Core

**Question 4: Do you agree with the proposed change?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with CR? | Additional comments/suggestion |
| Samsung | No | The proposed changes are correct: both *rsrp-ThresholdSSB* and *rach-ConfigBFR* should be present for CFRA BFR. However, it is already clear from the field descriptions of RRC and the procedures in MAC (e.g. MAC simply says '*ra-ResponseWindow* configured in *BeamFailureRecoveryConfig*' for CFRA BFR without condition). |
| OPPO | No | We actually think network will not always configure these parameters as they are optional in current 331. So, we prefer to clarify that if these parameters are not configured in BeamFailureRecoveryConfig, UE can use those configured in RACH-ConfigCommon. It seems the CRs in 2.5 are reasonable. |
|  |  |  |

**Conclusion:**

…

## 2.5 Handling on absence of IEs in BeamFailureRecoveryConfig

The following contributions were submitted to clarify which values would be used if *rach-ConfigBFR* (which contains *powerRampingStep*, *preambleReceivedTargetPower*, *preambleTransMax*, and *ra-ResponseWindow*) and/or *rsrp-ThresholdSSB* is not configured in *BeamFailureRecoveryConfig* (i.e. to use the values in *RACH-ConfigCommon*):

[R2-2005560](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005560.zip) Handling on absence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-15 38.321 15.8.0 0754 - F NR\_newRAT-Core

[R2-2005561](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005561.zip) Handling on absence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-16 38.321 16.0.0 0755 - A NR\_newRAT-Core

**Question 5: Do you agree with the proposed change?**

|  |  |  |
| --- | --- | --- |
| Company | Agree with CR? | Additional comments/suggestion |
| Samsung | No | The proposed changes are correct, but the values in *RACH-ConfigCommon* are the only available values if *beamFailureRecoveryConfig* is not configured, so no ambiguity exists. |
| OPPO | Yes | See comments above. |
|  |  |  |

**Conclusion:**

…

# 3 Conclusion

[R2-2004423](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004423.zip) Clarification on obtaining of PH values Samsung CR Rel-15 38.321 15.8.0 0738 - F NR\_newRAT-Core

[R2-2004424](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004424.zip) Clarification on obtaining of PH values Samsung CR Rel-16 38.321 16.0.0 0739 - A NR\_newRAT-Core

**=> …**

[R2-2004940](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004940.zip) Clarification on preamble selection for beam failure recovery Google Inc. CR Rel-15 38.321 15.8.0 0749 - F NR\_newRAT-Core

[R2-2004942](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004942.zip) Clarification on preamble selection for beam failure recovery Google Inc. CR Rel-16 38.321 16.0.0 0750 - A NR\_newRAT-Core

**=> …**

[R2-2005557](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005557.zip) Discussion on presence of IEs in BeamFailureRecoveryConfig ASUSTeK discussion Rel-15 NR\_newRAT-Core

[R2-2005558](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005558.zip) Clarification on presence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-15 38.331 15.9.0 1679 - F NR\_newRAT-Core

[R2-2005559](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005559.zip) Clarification on presence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-16 38.331 16.0.0 1680 - A NR\_newRAT-Core

**=> …**

[R2-2005560](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005560.zip) Handling on absence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-15 38.321 15.8.0 0754 - F NR\_newRAT-Core

[R2-2005561](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005561.zip) Handling on absence of IEs in BeamFailureRecoveryConfig ASUSTeK CR Rel-16 38.321 16.0.0 0755 - A NR\_newRAT-Core

**=> …**

# 4 References

[1] R2-110e Chair Notes 20-06-01 1200 UTC.docx