**3GPP TSG- Meeting #**

**1 June - 12 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **1762** | **rev** | **1** | **Current version:** | **15.8.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarification on L2 and RAN4 features of NGEN-DC and NE-DC |
|  |  |
| ***Source to WG:*** | OPPO |
| ***Source to TSG:*** | RAN2 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-05-18 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In 36.306, for L2 and RAN4 feature, it is unclear whether the capablity applicable to EN-DC also applies to NGEN-DC, although it has been clarified in 36.331 as follows***reportCGI-NR-EN-DC***Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is configured with (NG)EN-DC.***reportCGI-NR-NoEN-DC***Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is not configured with (NG)EN-DC.***inDeviceCoexInd-ENDC***Indicates whether the UE supports in-device coexistence indication for (NG)EN-DC operation. This field can be included only if *inDeviceCoexInd* is included. The UE supports *inDeviceCoexInd-ENDC* in the same duplexing modes as it supports *inDeviceCoexInd*.***supportedBandListEN-DC***Includes the NR bands supported by the UE in (NG)EN-DC. The field is included in case the parameter *en-DC* or *ng-EN-DC* is present and set to *supported* and not otherwise. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [89].so this CR is to clarify the support of NGEN-DC for related IEs for L2 and RAN4 features in 36.306. |
|  |  |
| ***Summary of change:*** | Clarify the support of NGEN-DC and NE-DC in field description of related capabilities.**Impact analysis**Impacted 5G architecture options:NGEN-DC, NE-DCImpacted functionality:UE capabilityInter-operability: 1. If UE implements according to the CR and the network does not, there would be no inter-operabiity issue if the network is implemented according to 36.331;
2. If the network implements according to the CR and the UE does not, , there would be no inter-operabiity issue if the network is implemented according to 36.331.
 |
|  |  |
| ***Consequences if not approved:*** | The current issue remains, i.e., it is unclear whether the UE supporting NGEN-DC can indicate the support of related L2 features*.* |
|  |  |
| ***Clauses affected:*** | 4.3.11.4, 4.3.11.5, 4.3.15.15, 4.3.34.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| CHANGE START |

#### 4.3.15.15 *inDeviceCoexInd-ENDC-r15*

This parameter defines whether the UE supports in-device coexistence indication for (NG)EN-DC operation as specified in TS 36.331 [5]. A UE that supports in-device coexistence indication for (NG)EN-DC operation shall also support in-device coexistence indication.

#### 4.3.34.2 *supportedBandListEN-DC-r15*

Only applicable if the UE supports E-UTRA NR Dual Connectivity or NG-RAN E-UTRA-NR Dual Connectivity. This field includes the supported NR bands as defined in TS 38.101-1 [33] and TS 38.101-2 [34]. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [36].

|  |
| --- |
| CHANGE END |