3GPP TSG-RAN WG2 Meeting #110-e R2-20XXXX

Electronic meeting, 1st - 12th June, 2020

**Agenda item: 5.4.3.1**

**Source: vivo (rapporteur)**

**Title: [AT110e][019][NR15] UE cap CGI Reporting**

**Document for: Discussion and decision**

# Introduction

This is a summary document of the following email discussion:

* [AT110e][019][NR15] UE cap CGI Reporting (vivo)

 Scope: Treat R2-2005618, R2-2005619, R2-2005620, R2-2005621, R2-2005622, R2-2004994, R2-2004995, R2-2004996 (proponents are responsible to explain and drive)

 Part 1: Decision whether to make corrections or not, identify agreeable corrections. Deadline: June 4, 0700 UTC.

 Part 2: For agreeable parts, continuation to agree CRs. Deadline: June 10, 0700 UTC

This summary focus on some remaining issues on CGI reporting in threefold:

* Additional CGI reporting UE capability
* Correction on CGI reporting UE capability
* Correction on UE capability constraints

# Additional CGI reporting capability [1]

In the RAN2#105 meeting, the agreements related to ANR reached are following:

Agreements

1: Introduce extra UE optional capabilities in EN-DC for ANR configured by LTE towards 2G/3G/4G neighbour cells when DRX configurations are different between MN and SN.

2: Existing FGIs (17/18/19) are required to be redefined to include the case of the UE is configured with EN-DC with same DRX configurations between MN and SN.

3: RAN2 confirms autonomous gap is not supported for the following cases:

• ANR (towards NR neighbour cells) configured by NR PCell in NR SA

• ANR (towards NR neighbour cells) configured by NR PSCell in EN-DC

• ANR (towards NR neighbour cells) configured by LTE PCell in EN-DC

• ANR (towards NR neighbour cells) configured by LTE PCell in LTE SA

4 RAN2 understands there would be interruption time on all NR SCG cells if UE starts autonomous gap in EN-DC and SN does not know this.

The extra UE optional capabilities in EN-DC were discussed in the RAN2#105 meeting, the background is quoted as following [1].

*During online discussion, some companies raised one issue in EN-DC. Since NR sub6 and LTE are actually quite similar, in some (especially early) UE implementation, some RF / Baseband hardware is shared in LTE and NR sub6 for early product launch. Then if DRX offsets are not aligned in MN and SN, such UEs must wait for both LTE and NR being idle (i.e. common idle period in DRX cycles in MN and SN) before measuring CGI. This is hardware specific or chip set vendor specific limitation, which requires different UE capability with EN-DC or LTE SA. Note that UE capability of per-FR and independent gap is introduced with similar reason.*

As a result, three UE optional capabilities, i.e. *utra-GERAN-CGI-Reporting-ENDC* /*eutra-CGI-Reporting-ENDC* /*reportCGI-NR-EN-DC-r15* are introduced in TS36.306 for ANR configured by LTE towards *GERAN* / *UTRA* /E-UTRA/NR neighbour cells when DRX configurations are different between MN and SN.

In the TS37.340, it states that “*In MR-DC, both the MN and the SN can configure CGI reporting. The MN can configure CGI reporting for intra-RAT and inter-RAT cells but the SN can only configure CGI reporting of intra-RAT cells”.* Hence, one UE optional capabilities, i.e. *nr-CGI-Reporting-ENDC* is introduced in TS38.306 for ANR configured by NR SN towards NR neighbour cells when EN-DC is configured.

The same issue discussed above also exists when ANR is configured by LTE SN towards E-UTRA neighbor cells in NE-DC case. To solve the issue, the rapporteur therefore proposes the following:

**Proposal 1: In TS36.306, introduce new UE optional capability (e.g. *eutra-CGI-Reporting-NEDC*) in NE-DC for ANR configured by LTE towards E-UTRA neighbour cells when DRX configurations are different between MN and SN.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm Incorporated | We support the direction. We think the new UE capability should also cover the case when DRX configurations are the same between MN and SN. |
|  |  |
|  |  |

Similarly, the issue discussed in above also exists when ANR is configured by NR toward E-UTRA/NR neighbour cells in NE-DC and NR-DC cases. To solve the issue, the rapporteur therefore proposes the following:

**Proposal 2: In TS38.306, introduce additional UE capabilities (e.g. *eutra-CGI-Reporting- NEDC-NRDC, nr-CGI-Reporting-NEDC-NRDC*) in NE-DC/NR-DC for ANR configured by NR towards E-UTRA/NR neighbour cells when DRX configurations are different between MN and SN.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm Incorporated | We understand that those capabilities MN configured and SN configured CGI reporting in case of NR-DC, and MN configured CGI reporting in case of NE-DC.We think we should differentiate between NR-DC and NE-DC because UE implementation is quite different between NR-DC (single RAT) and NE-DC (multi-RAT).In addition, each capability parameter should cover the cases when DRX configurations are different and the same. |
|  |  |
|  |  |

# Correction on CGI reporting UE capability [1]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ***eutra-CGI-Reporting***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the EN-DC is not configured. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***nr-CGI-Reporting***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when EN-DC is not configured. | UE | Yes | No | No |

In TS38.306, the description of *eutra-CGI-Reporting* and *nr-CGI-Reporting states that the two capabilities are applied when EN-DC is not configured.* In Rel-15, when discussing these two capabilities, they were just for SA scenario. But with the introduction of later drop, new additional MR-DC cases should be excluded. The descriptions of the two capabilities needs to be updated accordingly, i.e. they are applied when MR-DC is not configured. Therefore,

**Proposal 3: In TS38.306, update the description of eutra-CGI-Reporting and nr-CGI-Reporting to make it clear that they are applied when MR-DC is not configured.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm Incorporated | Agree. |
|  |  |
|  |  |

# Correction on UE capability constraints [2]

For CGI reporting configuration, it is only allowed to configure CGI reporting for one neighbor cell at one time

ReportCGI-EUTRA ::= SEQUENCE {

 cellForWhichToReportCGI EUTRA-PhysCellId,

 ...,

 [[

 useAutonomousGaps-r16 ENUMERATED {setup} OPTIONAL -- Need R

 ]]

}

ReportCGI ::= SEQUENCE {

 cellForWhichToReportCGI PhysCellId,

 ...,

 [[

 useAutonomousGaps-r16 ENUMERATED {setup} OPTIONAL -- Need R

 ]]

}

But in TS 38306, a number of neighbor cells “#cell for CGI reporting”, as shown below, is use for CGI reporting for neighbor cell. This description is not aligned with TS3x.331 CGI reporting configuration procedure and the meaning is not very clear:

| Parameter | Description | Value |
| --- | --- | --- |
| #DRBs | The number of DRBs that a UE shall support. | 16 per UE.NOTE: 8 per MAC entity with duplication. |
| #minCellperMeasObjectNR | The minimum number of neighbour cells (excluding black list cells) that a UE shall be able to store associated with a MeasObjectNR. | 32 |
| #minBlackCellRangesperMeasObjectNR | The minimum number of blacklist cell PCI ranges that a UE shall be able to store associated with a MeasObjectNR. | 8 |
| #minCellperMeasObjectEUTRA | The minimum number of neighbour cells that a UE shall be able to store associated with a MeasObjectEUTRA. | 32 |
| #minCellTotal | The minimum number of neighbour cells (excluding black list cells) that UE shall be able to store in total from all measurement objects configured. | 256 with counting CSI-RS and SSB as 2. |
| #cell for CGI reporting  | the limit regarding the cells NR can configure includes the cell for which the UE is requested to report CGI. | (# minCellperMeasObjectRAT - 1), where RAT represents NR and EUTRA. |
| #maxDeprioritisationFreq | The UE shall be able to store a depriotisation request for up to 8 frequencies (applicable when receiving another frequency specific deprioritisation request via *RRCRelease* before T325 expiry). | 8 |

This description is confusing as it may give the impression that the” cell for CGI reporting” can be more than one at once. Further this description does not express that the configuration is per frequency. In contrast, the UE capability constraints for CGI reporting is described in TS 36331 as highlighted below:

| Parameter | Description | Value | NB-IoT |
| --- | --- | --- | --- |
| #DRBs | The number of DRBs that a UE shall support | 8, 15 | (0, 1, 2)NOTE1 |
| #RLC-AM | The number of RLC AM entities that a UE shall support | 10, 17 | (2, 3)NOTE1 |
| #minCellperMeasObjectEUTRA | The minimum number of neighbour cells (excluding black list cells) that a UE shall be able to store within a MeasObjectEUTRA. NOTE. | 32 | N/A |
| #minBlackCellRangesperMeasObjectEUTRA | The minimum number of blacklist cell PCI ranges that a UE shall be able to store within a MeasObjectEUTRA | 32 | N/A |
| #minCellperMeasObjectUTRA | The minimum number of neighbour cells that a UE shall be able to store within a MeasObjectUTRA. NOTE. | 32 | N/A |
| #minCellperMeasObjectGERAN | The minimum number of neighbour cells that a UE shall be able to store within a measObjectGERAN. NOTE. | 32 | N/A |
| #minCellperMeasObjectCDMA2000 | The minimum number of neighbour cells that a UE shall be able to store within a measObjectCDMA2000. NOTE. | 32 | N/A |
| #minCellTotal | The minimum number of neighbour cells (excluding black list cells) that UE shall be able to store in total in all measurement objects configured | 256 | N/A |
| NOTE: In case of CGI reporting, the limit regarding the cells E-UTRAN can configure includes the cell for which the UE is requested to report CGI i.e. the amount of neighbour cells that can be included is at most (# minCellperMeasObjectRAT - 1), where RAT represents EUTRA/UTRA/GERAN/CDMA2000 respectively. |
| NOTE1: #DRBs based on UE capability, #RLC-AM =#DRBs + 2. |

This description clearly highlights that there is only one *cellForWhichToReportCGI* in the *MeasObject*. Therefore, it is proposed as:

**Proposal 4: Align UE capability Constraint for CGI reporting in TS38.306 with the corresponding description in TS36331.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm Incorporated | Agree. In the CR, the note should be numbered and the pointer to the note should put in the rows of minCellperMeasObjectNR and minCellperMeasObjectEUTRA. |
|  |  |
|  |  |

# Conclusions

To be added.

# References

[1] [R2-2005618](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CRAN2%5C2005_R2_110-e%5CDocs%5CR2-2005618.zip) Introduction of CGI reporting capabilities, vivo

[2] [R2-2004994](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004994.zip), Correction on UE capability constraints, vivo