**3GPP TSG-RAN** **WG2 Meeting #110-e R2-200xxxx**

**Electronic, June 1 – 12, 2020**

**Source: Samsung**

**Title: Summary of email discussion [AT110e][022][NR15] UE cap Miscellaneous II**

**Document for: Decision**

**Agenda Item: 5.4.3.1**

# Introduction

This document summarizes the following offline discussion for UE capabilities.

**Miscellaneous II**

* [AT110e][022][NR15] UE cap Miscellaneous II (Samsung)

Scope: Treat R2-2004831, R2-2004458, R2-2004459, R2-2005397, R2-2005398 (proponents are responsible to explain and drive)

Part 1: Decision whether to make corrections or not, identify agreeable corrections. Deadline: June 4, 0700 UTC.

Part 2: For agreeable parts, continuation to agree CRs. Deadline: June 10, 0700 UTC

xDD differentiation SUL/SDL bands

[R2-2004831](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004831.zip) xDD differentiation of UE capabilities for SUL/SDL bands Samsung discussion Rel-15 NR\_newRAT-Core

BCS and BW

[R2-2004458](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004458.zip) Clarification on BCS and UE BW capabilities Nokia, Nokia Shanghai Bell discussion Rel-15 NR\_newRAT-Core

[R2-2004459](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004459.zip) Draft LS to RAN4 on clarification on BCS and UE BW capabilities Nokia, Nokia Shanghai Bell LS out Rel-15 NR\_newRAT-Core To:RAN4

Serving cell number for ENDC power class

[R2-2005397](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005397.zip) Correction to the serving cell number for ENDC power class Huawei, HiSilicon CR Rel-15 38.306 15.9.0 0287 1 F NR\_newRAT-Core R2-2003461

[R2-2005398](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005398.zip) Correction to the serving cell number for ENDC power class Huawei, HiSilicon CR Rel-16 38.306 16.0.0 0288 1 A NR\_newRAT-Core R2-2003462

Chair: Can take LS from R4 into account once ready in R4, if it is to be provided

# Discussion: Part 1 (by June 4, 0700 UTC)

It is proposed to try to come to a set of agreeable proposals out of the documents listed above. For each set of CRs, companies are requested provide their views.

## xDD differentiation for SUL/SDL bands ([R2-2004831](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004831.zip))

This contribution proposes to clarify the xDD differentiation of capabilities for SDL and SUL bands for Rel-15, these SDL and SUL bands follow the xDD differentiation of capabilities for TDD and FDD, respectively

According to clause 5.2 in 38.101-1 v15.90, NR operating bands in FR1 are defined in Table 5.2-1. There are 2 SDL bands (i.e. n75, n76) and 6 SUL bands (i.e. n80, n81, n82, n83, n84, n86) and these bands have corresponding TDD or FDD bands i.e. all SDL/SUL bands have corresponding bands.

1. SDL bands

* n75, n76: have corresponding TDD bands, n50 and n51, respectively.

1. SUL bands

* n80, n81, n82, n83, n84, n86: have corresponding FDD bands, n66, n8, n20, n1, n66, and n5, respectively.

In other words, capabilities for SDL bands follows the TDD-differentiation (i.e. common containers of Phy-ParametersXDD-Diff and MeasAndMobParametersXDD-Diff, tdd-Add-UE-NR/MRDC-Capabilities, etc) and capabilities for SUL bands follows the FDD-differentiation (i.e. common containers of Phy-ParametersXDD-Diff and MeasAndMobParametersXDD-Diff, fdd-Add-UE-NR/MRDC-Capabilities).

**Q1. Do you agree that xDD differentiation of capabilities for SDL and SUL bands for Rel-15 follows the xDD differentiation of capabilities for TDD and FDD bands, respectively?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree / Disagree** | **Comments** |
| Samsung | Agree | It is natural that Rel-15 SUL/SDL bands can be associated with the TDD and FDD bands, respectively. |
|  |  |  |
|  |  |  |
|  |  |  |

RAN4 defined the new SUL/SDL bands in Rel-16. According to clause 5.2 in 38.101-1 v16.30, NR operating bands in FR1 are defined in Table 5.2-1. There are 3 SDL bands (i.e. n29, n75, n76) and 8 SUL bands (i.e. n80, n81, n82, n83, n84, n86, n89, n95) i.e. new bands for n29, n89, n95 are introduced in Rel-16. However, there are no clear rule that mapping SDL/SUL banbs to the corresponding TDD/FDD bands. Each new band have different corresponding band, so it seems that the Proposal 1 above cannot be applied.

1. SDL bands

* n29: no corresponding band

1. SUL bands

* n89: have corresponding FDD band (i.e. n5)
* n95: have corresponding TDD band (i.e. n34)

It is unclear how the capability parameters can be differentiated by xDD for SUL/SDL bands which can be signalled for this problematic bands above. If there are no exception case (n29 and n95), the simplest way would be the xDD differentiation for capabilities for SUL/SDL bands follow the signalling rule of the corresponding bands (i.e. SDL follows the corresponding TDD band, SUL follows the corresponding FDD band).

**Q2. How to differentiate by xDD the UE capabilities for the newly added SUL SDL bands in Rel-16?**

|  |  |
| --- | --- |
| **Company name** | **Comments** |
| Samsung | It would be better to ask this aspect to RAN4 because RAN2 cannot solve this issue without further information.  Send LS to RAN4 to ask how capability parameters can be differentiated by xDD for newly added SUL/SDL bands (i.e. n29, n89 and n95) in Rel-16. |
|  |  |
|  |  |
|  |  |

## Clarification on BCS and UE BW capabilities ([R2-2004458](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004458.zip), [R2-2004459](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2004459.zip))

In R2-2004458 [2], it is proposed to clarify the UE behaviour observed in the field on interpretation of BCS and UE BW while reporting UE capabilities:

The UE indicates its supported BCSs for each supported band combination in UE capabilities as shown in below excerpt from TS 38.306:

**supportedBandwidthCombinationSet**

*For NR SA and for inter-band EN-DC, the field defines the bandwidth combinations for the NR part of the band combination. For intra-band EN-DC, the field indicates the supported bandwidth combination set applicable to the NR and LTE band combinations. The first (left-most) bit in the bitmap corresponds to the BCS#0 and so on. If the bit is set to 1, the UE supports the corresponding BCS.*

However, the UE also has an additional capability description in *FeatureSetDownlinkPerCC::supportedBandwidthDL* to indicate the supported BW for a particular band per a band combination configuration, as well as the capabilities for supported channel BWs per band in *BandNR::channelBWs-DL*, as shown below (for downlink only in this case):

| ***supportedBandwidthDL***  Indicates maximum DL channel bandwidth supported for a given SCS that UE supports within a single CC, which is defined in Table 5.3.5-1 in TS 38.101-1 [2] for FR1 and Table 5.3.5-1 in TS 38.101-2 [3] for FR2.  For FR1, all the bandwidths listed in TS38.101-1 Table 5.3.5-1 for each band shall be mandatory with a single CC unless indicated optional. For FR2, the set of mandatory CBW is 50, 100, 200 MHz. When this field is included in a band combination with a single band entry and a single CC entry (i.e. non-CA band combination), the UE shall indicate the maximum channel bandwidth for the band according to TS 38.101-1 [2] and TS 38.101-2 [3].  NOTE: To determine whether the UE supports a channel bandwidth of 90 MHz, the network may ignore this capability for and validate instead the *channelBW-90mhz* and the *supportedBandwidthCombinationSet*. For serving cells with other channel bandwidths the network validates the *channelBWs-DL*, the *supportedBandwidthCombinationSet* and *supportedBandwidthDL*. |
| --- |

| ***channelBWs-DL***  Indicates for each subcarrier spacing the UE supported channel bandwidths. Absence of the *channelBWs-DL* (without suffix) for a band or absence of specific scs-XXkHz entry for a supported subcarrier spacing means that the UE supports the channel bandwidths among [5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100] and [50, 100, 200] that were defined in clause 5.3.5 of TS 38.101-1 version 15.7.0 [2] and TS 38.101-2 version 15.7.0 [3] for the given band or the specific SCS entry.  For FR1, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 5, 10, 15, 20, 25, 30, 40, 50, 60 and 80MHz. For FR2, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 50, 100 and 200MHz. The third / rightmost bit (for 200MHz) shall be set to 1.  For FR1, the leading/leftmost bit in *channelBWs-DL-v1590* indicates 70MHz, and all the remaining bits in *channelBWs-DL-v1590* shall be set to 0.  NOTE: To determine whether the UE supports a specific SCS for a given band, the network validates the *supportedSubCarrierSpacingDL* and the *scs-60kHz*. To determine whether the UE supports a channel bandwidth of 90 MHz, the network may ignore this capability for and validate instead the *channelBW-90mhz* and the *supportedBandwidthCombinationSet*. For serving cells with other channel bandwidths the network validates the *channelBWs-DL*, the *supportedBandwidthCombinationSet* and *supportedBandwidthDL*. |
| --- |

According to the observations and the example in R2-2004458 [2], the specifications seem unclear what exactly means for a UE to support a particular BCS: In LTE, UE was mandated to support all the bandwidths defined for the BCS, but in NR it appears (given that the current description in the specification) that some UEs consider this is not the case. If the UE cannot support all CH BWs belonging to a certain BCS from 3GPP point of view, then it is unclear how to interpret the disparity between the supported channel bandwidths and the BCS.

**Q3. Do you agree that UE shall support all the channel bandwidths for that BCS if a UE indicates support for a BCS defined for a band combination? and if not how should the discrepancy be interpreted?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree / Disagree** | **Comments** |
| Samsung | Agree | UE reported BCS0 and then the UE should support all specified aggregated bandwidths, we can refer to the description in TR-38.817-01, excerpt here:  **Considering NR bands in standalone operation:**   * BCSs are specified for CA configuration in NR bands in standalone operation * UE should support all specified aggregated bandwidths which are smaller than the indicated aggregated bandwidth and are part of same BCS indicated * UE should support all specified lower order CA configurations which have same BCS as indicated * BCS with same number (e.g. BCS0) need to be aligned between lower and higher order fallback configuration |
|  |  |  |
|  |  |  |
|  |  |  |

## Serving cell number for ENDC power class ([R2-2005397](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005397.zip), [R2-2005398](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005398.zip))

These CRs propose to update the field description for *powerClass* in TS 38.306 to support EN-DC combinations with 3 UL CCs.

RAN4 has already specified the EN-DC combinations with 3CC uplink serving cells. The EN-DC combinations with 3 UL CCs are added in TS 38.101-3 and the NOTE4 (Power class 3 is the default power class unless otherwise stated) should also be applied to these EN-DC combinations with 3 UL CCs. To align with RAN4 spec, the description for powerClass needs update, and RAN4 is working on the LS to be sent to RAN2.

See the below proposed change in these CRs.

| ***powerClass***  Indicates power class the UE supports when operating according to this band combination. If the field is absent, the UE supports the default power class. If this power class is higher than the power class that the UE supports on the individual bands of this band combination (*ue-PowerClass* in *BandNR*), the latter determines maximum TX power available in each band. The UE sets the power class parameter only in band combinations with two or more FR1 uplink serving cells. | BC | No | No | FR1 only |
| --- | --- | --- | --- | --- |

As chairman commented in the chairman note, these CRs can be confirmed/treated when LS from R4 is received but in this offline discussion RAN2 can provides the view based on internal checking for this issue.

**Q4. Do you agree to update the description for *powerClass* for band combinations with up to three FR1 uplink serving cells?**

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree / Disagree** | **Comments** |
| Samsung | Agree | It reflects the RAN4 agreements, we are fine for adding further clarification as suggested in these CRs. |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion: Part 2 (by June 10, 0700 UTC)

xxxxxxxxxx

# Conclusion

xxxxxxxxxx

# Reference

1. R2-2004831, xDD differentiation of UE capabilities for SUL/SDL bands, Samsung.
2. R2-2004458 Clarification on BCS and UE BW capabilities, Nokia, Nokia Shanghai Bell.
3. R2-2004459 Draft LS to RAN4 on clarification on BCS and UE BW capabilities, Nokia, Nokia Shanghai Bell.
4. R2-2005397 Correction to the serving cell number for ENDC power class, CR Rel-15, 38.306 15.9.0 0287, Huawei, HiSilicon.
5. R2-2005398 Correction to the serving cell number for ENDC power class, CR Rel-16, 38.306 16.0.0 0288, Huawei, HiSilicon.