**3GPP TSG-RAN WG2 Meeting #110-e** **R2-200xxxx**

**eMeeting, 1st – 12th , June, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.331** | **CR** | **4197** | **rev** | **5** | **Current version:** | **16.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction of NeedForGap capability for NR measurement | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | MediaTek Inc. | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core, TEI16 | | | | |  | ***Date:*** | | | 2020/06/01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In release 15, the capability for requirement of measurement gap on NR measurement is not introduced due to time limitation. This results in the network configures measurement gap in most case even if the UE is capable of doing gapless in some scenario. It is proposed to have this capability in release 16. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the ASN.1 capability bits for the requirement of measurement gap (NeedForGap) on NR measurement. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The network always has to configure measurement gap for NR measurement. It will result in performance lost. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.6 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 36.306 CR 1730 | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

### 6.3.6 Other information elements

<Skip unrelated Parts>

– *UE-EUTRA-Capability*

The IE *UE-EUTRA-Capability* is used to convey the E-UTRA UE Radio Access Capability Parameters, see TS 36.306 [5], and the Feature Group Indicators for mandatory features (defined in Annexes B.1 and C.1) to the network. The IE *UE-EUTRA-Capability* is transferred in E-UTRA or in another RAT.

NOTE 0: For (UE capability specific) guidelines on the use of keyword OPTIONAL, see Annex A.3.5.

***UE-EUTRA-Capability* information element**

-- ASN1START

UE-EUTRA-Capability ::= SEQUENCE {

accessStratumRelease AccessStratumRelease,

ue-Category INTEGER (1..5),

pdcp-Parameters PDCP-Parameters,

phyLayerParameters PhyLayerParameters,

rf-Parameters RF-Parameters,

measParameters MeasParameters,

featureGroupIndicators BIT STRING (SIZE (32)) OPTIONAL,

interRAT-Parameters SEQUENCE {

utraFDD IRAT-ParametersUTRA-FDD OPTIONAL,

utraTDD128 IRAT-ParametersUTRA-TDD128 OPTIONAL,

utraTDD384 IRAT-ParametersUTRA-TDD384 OPTIONAL,

utraTDD768 IRAT-ParametersUTRA-TDD768 OPTIONAL,

geran IRAT-ParametersGERAN OPTIONAL,

cdma2000-HRPD IRAT-ParametersCDMA2000-HRPD OPTIONAL,

cdma2000-1xRTT IRAT-ParametersCDMA2000-1XRTT OPTIONAL

},

nonCriticalExtension UE-EUTRA-Capability-v920-IEs OPTIONAL

}

<Skip unrelated Parts>

UE-EUTRA-Capability-v1560-IEs ::= SEQUENCE {

pdcp-ParametersNR-v1560 PDCP-ParametersNR-v1560,

irat-ParametersNR-v1560 IRAT-ParametersNR-v1560,

appliedCapabilityFilterCommon-r15 OCTET STRING OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

tdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

nonCriticalExtension UE-EUTRA-Capability-v1570-IEs OPTIONAL

}

UE-EUTRA-Capability-v1570-IEs ::= SEQUENCE {

rf-Parameters-v1570 RF-Parameters-v1570 OPTIONAL,

irat-ParametersNR-v1570 IRAT-ParametersNR-v1570 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v16xy-IEs OPTIONAL

}

UE-EUTRA-Capability-v16xy-IEs ::= SEQUENCE {

highSpeedEnhParameters-v16xy HighSpeedEnhParameters-v16xy OPTIONAL,

neighCellSI-AcquisitionParameters-v16xy NeighCellSI-AcquisitionParameters-v16xy OPTIONAL,

mbms-Parameters-v16xy MBMS-Parameters-v16xy OPTIONAL,

mac-Parameters-v16xy MAC-Parameters-v16xy OPTIONAL,

phyLayerParameters-v16xy PhyLayerParameters-v16xy OPTIONAL,

otherParameters-v16xy Other-Parameters-v16xy,

dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

mmtel-Parameters-v16xy MMTEL-Parameters-v16xy,

irat-ParametersNR-r16 IRAT-ParametersNR-r16 OPTIONAL,

measParameters-v16xy MeasParameters-v16xy OPTIONAL,

rf-Parameters-v16xy RF-Parameters-v16xy OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v16xy UE-EUTRA-CapabilityAddXDD-Mode-v16xy,

tdd-Add-UE-EUTRA-Capabilities-v16xy UE-EUTRA-CapabilityAddXDD-Mode-v16xy,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

<Skip unrelated Parts>

RF-Parameters-v1530 ::= SEQUENCE {

sTTI-SPT-Supported-r15 ENUMERATED {supported} OPTIONAL,

supportedBandCombination-v1530 SupportedBandCombination-v1530 OPTIONAL,

supportedBandCombinationAdd-v1530 SupportedBandCombinationAdd-v1530 OPTIONAL,

supportedBandCombinationReduced-v1530 SupportedBandCombinationReduced-v1530 OPTIONAL,

powerClass-14dBm-r15 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1570 ::= SEQUENCE {

dl-1024QAM-ScalingFactor-r15 ENUMERATED {v1, v1dot2, v1dot25},

dl-1024QAM-TotalWeightedLayers-r15 INTEGER (0..10)

}

RF-Parameters-v16xy ::= SEQUENCE {

supportedBandCombination-v16xy SupportedBandCombination-v16xy OPTIONAL,

supportedBandCombinationAdd-v16xy SupportedBandCombinationAdd-v16xy OPTIONAL,

supportedBandCombinationReduced-v16xy SupportedBandCombinationReduced-v16xy OPTIONAL

}

<Skip unrelated Parts>

SupportedBandCombination-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-r10

SupportedBandCombinationExt-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParametersExt-r10

SupportedBandCombination-v1090 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1090

SupportedBandCombination-v10i0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v10i0

SupportedBandCombination-v1130 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1130

SupportedBandCombination-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1250

SupportedBandCombination-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1270

SupportedBandCombination-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1320

SupportedBandCombination-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1380

SupportedBandCombination-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1390

SupportedBandCombination-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1430

SupportedBandCombination-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1450

SupportedBandCombination-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1470

SupportedBandCombination-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v14b0

SupportedBandCombination-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1530

SupportedBandCombination-v16xy ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v16xy

SupportedBandCombinationAdd-r11 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-r11

SupportedBandCombinationAdd-v11d0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v10i0

SupportedBandCombinationAdd-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1250

SupportedBandCombinationAdd-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1270

SupportedBandCombinationAdd-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1320

SupportedBandCombinationAdd-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1380

SupportedBandCombinationAdd-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1390

SupportedBandCombinationAdd-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1430

SupportedBandCombinationAdd-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1450

SupportedBandCombinationAdd-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1470

SupportedBandCombinationAdd-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v14b0

SupportedBandCombinationAdd-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1530

SupportedBandCombinationAdd-v16xy ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v16xy

SupportedBandCombinationReduced-r13 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-r13

SupportedBandCombinationReduced-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1320

SupportedBandCombinationReduced-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1380

SupportedBandCombinationReduced-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1390

SupportedBandCombinationReduced-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1430

SupportedBandCombinationReduced-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1450

SupportedBandCombinationReduced-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1470

SupportedBandCombinationReduced-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v14b0

SupportedBandCombinationReduced-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1530

SupportedBandCombinationReduced-v16xy ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v16xy

BandCombinationParameters-r10 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r10

BandCombinationParametersExt-r10 ::= SEQUENCE {

supportedBandwidthCombinationSet-r10 SupportedBandwidthCombinationSet-r10 OPTIONAL

}

BandCombinationParameters-v1090 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1090

BandCombinationParameters-v10i0::= SEQUENCE {

bandParameterList-v10i0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v10i0 OPTIONAL

}

BandCombinationParameters-v1130 ::= SEQUENCE {

multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1130 OPTIONAL,

...

}

BandCombinationParameters-r11 ::= SEQUENCE {

bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-r11,

supportedBandwidthCombinationSet-r11 SupportedBandwidthCombinationSet-r10 OPTIONAL,

multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

bandInfoEUTRA-r11 BandInfoEUTRA,

...

}

BandCombinationParameters-v1250::= SEQUENCE {

dc-Support-r12 SEQUENCE {

asynchronous-r12 ENUMERATED {supported} OPTIONAL,

supportedCellGrouping-r12 CHOICE {

threeEntries-r12 BIT STRING (SIZE(3)),

fourEntries-r12 BIT STRING (SIZE(7)),

fiveEntries-r12 BIT STRING (SIZE(15))

} OPTIONAL

} OPTIONAL,

supportedNAICS-2CRS-AP-r12 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

commSupportedBandsPerBC-r12 BIT STRING (SIZE (1.. maxBands)) OPTIONAL,

...

}

BandCombinationParameters-v1270 ::= SEQUENCE {

bandParameterList-v1270 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1270 OPTIONAL

}

BandCombinationParameters-r13 ::= SEQUENCE {

differentFallbackSupported-r13 ENUMERATED {true} OPTIONAL,

bandParameterList-r13 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r13,

supportedBandwidthCombinationSet-r13 SupportedBandwidthCombinationSet-r10 OPTIONAL,

multipleTimingAdvance-r13 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r13 ENUMERATED {supported} OPTIONAL,

bandInfoEUTRA-r13 BandInfoEUTRA,

dc-Support-r13 SEQUENCE {

asynchronous-r13 ENUMERATED {supported} OPTIONAL,

supportedCellGrouping-r13 CHOICE {

threeEntries-r13 BIT STRING (SIZE(3)),

fourEntries-r13 BIT STRING (SIZE(7)),

fiveEntries-r13 BIT STRING (SIZE(15))

} OPTIONAL

} OPTIONAL,

supportedNAICS-2CRS-AP-r13 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

commSupportedBandsPerBC-r13 BIT STRING (SIZE (1.. maxBands)) OPTIONAL

}

BandCombinationParameters-v1320 ::= SEQUENCE {

bandParameterList-v1320 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1320 OPTIONAL,

additionalRx-Tx-PerformanceReq-r13 ENUMERATED {supported} OPTIONAL

}

BandCombinationParameters-v1380 ::= SEQUENCE {

bandParameterList-v1380 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1380 OPTIONAL

}

BandCombinationParameters-v1390 ::= SEQUENCE {

ue-CA-PowerClass-N-r13 ENUMERATED {class2} OPTIONAL

}

BandCombinationParameters-v1430 ::= SEQUENCE {

bandParameterList-v1430 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1430 OPTIONAL,

v2x-SupportedTxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL,

v2x-SupportedRxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL

}

BandCombinationParameters-v1450 ::= SEQUENCE {

bandParameterList-v1450 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1450 OPTIONAL

}

BandCombinationParameters-v1470 ::= SEQUENCE {

bandParameterList-v1470 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1470 OPTIONAL,

srs-MaxSimultaneousCCs-r14 INTEGER (1..31) OPTIONAL

}

BandCombinationParameters-v14b0 ::= SEQUENCE {

bandParameterList-v14b0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v14b0 OPTIONAL

}

BandCombinationParameters-v1530 ::= SEQUENCE {

bandParameterList-v1530 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1530 OPTIONAL,

spt-Parameters-r15 SPT-Parameters-r15 OPTIONAL

}

BandCombinationParameters-v16xy ::= SEQUENCE {

measGapInfoNR MeasGapInfoNR OPTIONAL

}

-- If an additional band combination parameter is defined, which is supported for MR-DC,

-- it shall be defined in the IE CA-ParametersEUTRA in TS 38.331 [82].

<Skip unrelated Parts>

MeasParameters ::= SEQUENCE {

bandListEUTRA BandListEUTRA

}

MeasParameters-v1020 ::= SEQUENCE {

bandCombinationListEUTRA-r10 BandCombinationListEUTRA-r10

}

MeasParameters-v1130 ::= SEQUENCE {

rsrqMeasWideband-r11 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v11a0 ::= SEQUENCE {

benefitsFromInterruption-r11 ENUMERATED {true} OPTIONAL

}

MeasParameters-v1250 ::= SEQUENCE {

timerT312-r12 ENUMERATED {supported} OPTIONAL,

alternativeTimeToTrigger-r12 ENUMERATED {supported} OPTIONAL,

incMonEUTRA-r12 ENUMERATED {supported} OPTIONAL,

incMonUTRA-r12 ENUMERATED {supported} OPTIONAL,

extendedMaxMeasId-r12 ENUMERATED {supported} OPTIONAL,

extendedRSRQ-LowerRange-r12 ENUMERATED {supported} OPTIONAL,

rsrq-OnAllSymbols-r12 ENUMERATED {supported} OPTIONAL,

crs-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL,

csi-RS-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1310 ::= SEQUENCE {

rs-SINR-Meas-r13 ENUMERATED {supported} OPTIONAL,

whiteCellList-r13 ENUMERATED {supported} OPTIONAL,

extendedMaxObjectId-r13 ENUMERATED {supported} OPTIONAL,

ul-PDCP-Delay-r13 ENUMERATED {supported} OPTIONAL,

extendedFreqPriorities-r13 ENUMERATED {supported} OPTIONAL,

multiBandInfoReport-r13 ENUMERATED {supported} OPTIONAL,

rssi-AndChannelOccupancyReporting-r13 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1430 ::= SEQUENCE {

ceMeasurements-r14 ENUMERATED {supported} OPTIONAL,

ncsg-r14 ENUMERATED {supported} OPTIONAL,

shortMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

perServingCellMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

nonUniformGap-r14 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1520 ::= SEQUENCE {

measGapPatterns-r15 BIT STRING (SIZE (8)) OPTIONAL

}

MeasParameters-v1530 ::= SEQUENCE {

qoe-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

qoe-MTSI-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

ca-IdleModeMeasurements-r15 ENUMERATED {supported} OPTIONAL,

ca-IdleModeValidityArea-r15 ENUMERATED {supported} OPTIONAL,

heightMeas-r15 ENUMERATED {supported} OPTIONAL,

multipleCellsMeasExtension-r15 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v16xy ::= SEQUENCE {

bandInfoNR-v16xy SEQUENCE (SIZE (1..maxBands)) OF MeasGapInfoNR OPTIONAL

}

MeasGapInfoNR ::= SEQUENCE {

interRAT-BandListNR-EN-DC InterRAT-BandListNR OPTIONAL,

interRAT-BandListNR-SA InterRAT-BandListNR OPTIONAL

}

BandListEUTRA ::= SEQUENCE (SIZE (1..maxBands)) OF BandInfoEUTRA

BandCombinationListEUTRA-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandInfoEUTRA

BandInfoEUTRA ::= SEQUENCE {

interFreqBandList InterFreqBandList,

interRAT-BandList InterRAT-BandList OPTIONAL

}

InterFreqBandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterFreqBandInfo

InterFreqBandInfo ::= SEQUENCE {

interFreqNeedForGaps BOOLEAN

}

InterRAT-BandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterRAT-BandInfo

InterRAT-BandListNR ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF InterRAT-BandInfoNR

InterRAT-BandInfo ::= SEQUENCE {

interRAT-NeedForGaps BOOLEAN

}

InterRAT-BandInfoNR ::= SEQUENCE {

interRAT-NeedForGapsNR BOOLEAN

}

<Skip unrelated Parts>

-- ASN1STOP

| ***UE-EUTRA-Capability* field descriptions** | ***FDD/ TDD diff*** |
| --- | --- |
| ***accessStratumRelease***  Set to rel15 in this version of the specification. NOTE 7. | - |
| ***additionalRx-Tx-PerformanceReq***  Indicates whether the UE supports the additional Rx and Tx performance requirement for a given band combination as specified in TS 36.101 [42]. | - |
| ***alternativeTBS-Indices***  Indicates whether the UE supports alternative TBS indices *I*TBS 26A and 33A as specified in TS 36.213 [23]. | - |
| ***alternativeTBS-Index***  Indicates whether the UE supports alternative TBS index ITBS 33B as specified in TS 36.213 [23]. | No |
| ***alternativeTimeToTrigger***  Indicates whether the UE supports alternativeTimeToTrigger. | No |
| ***altMCS-Table***  Indicates whether the UE supports the 6-bit MCS table as specified in TS 36.212 [22] and TS 36.213 [23]. | - |
| ***aperiodicCSI-Reporting***  Indicates whether the UE supports aperiodic CSI reporting with 3 bits of the CSI request field size as specified in TS 36.213 [23], clause 7.2.1 and/or aperiodic CSI reporting mode 1-0 and mode 1-1 as specified in TS 36.213 [23], clause 7.2.1. The first bit is set to "1" if the UE supports the aperiodic CSI reporting with 3 bits of the CSI request field size. The second bit is set to "1" if the UE supports the aperiodic CSI reporting mode 1-0 and mode 1-1. | No |
| ***aperiodicCsi-ReportingSTTI***  Indicates whether the UE supports aperiodic CSI reporting for short TTI as specified in TS 36.213 [23], clause 7.2.1. | No |
| ***appliedCapabilityFilterCommon***  Contains the filter, applied by the UE, common for all MR-DC related capability containers that are requested and as defined by *UE-CapabilityRequestFilterCommon* IE in TS 38.331 [82]. | - |
| ***assistInfoBitForLC***  Indicates whether the UE supports assistance information bit for local cache. | - |
| ***aul***  Indicates whether the UE supports AUL as specified n TS 36.321 [6]. | - |
| ***bandCombinationListEUTRA***  One entry corresponding to each supported band combination listed in the same order as in *supportedBandCombination.* | - |
| ***BandCombinationParameters-v1090, BandCombinationParameters-v10i0, BandCombinationParameters-v1270***  If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | - |
| ***BandCombinationParameters-v1130***  The field is applicable to each supported CA bandwidth class combination (i.e. CA configuration in TS 36.101 [42], clause 5.6A.1) indicated in the corresponding band combination. If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | - |
| ***bandEUTRA***  E‑UTRA band as defined in TS 36.101 [42]. In case the UE includes *bandEUTRA-v9e0* or *bandEUTRA-v1090*, the UE shall set the corresponding entry of *bandEUTRA* (i.e. without suffix) or *bandEUTRA-r10* respectively to *maxFBI*. | - |
| ***bandInfoNR-v16xy***  One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to a E-UTRA band listed in *supportedBandListEUTRA* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig*. | - |
| ***bandListEUTRA***  One entry corresponding to each supported E‑UTRA band listed in the same order as in *supportedBandListEUTRA*. | - |
| <Skip unrelated Parts> |  |
| ***interFreqSI-AcquisitionForHO***  Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring inter-frequency cell. | Yes |
| ***interRAT-BandList***  One entry corresponding to each supported band of another RAT listed in the same order as in the *interRAT-Parameters*. The NR bands reported in *SupportedBandListNR* are excluded from this list. | - |
| ***interRAT-BandListNR-EN-DC***  One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListEN-DC-r15*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value for the same NR band. | - |
| ***interRAT-BandListNR-SA***  One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListNR-SA*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value for the same NR band. | - |
| ***interRAT-NeedForGaps***  Indicates need for DL measurement gaps when operating on the E‑UTRA band given by the entry in *bandListEUTRA or on the E-UTRA band combination given by the entry in bandCombinationListEUTRA* and measuring on the inter-RAT band given by the entry in the *interRAT-BandList*. | - |
| ***interRAT-NeedForGapsNR***  Indicates need for measurement gaps when operating on the E‑UTRA band given by the entry in *supportedBandListEUTRA or on the E-UTRA band combination given by the entry in supportedBandCombination-r10 or supportedBandCombinationAdd-r11* or *supportedBandCombinationReduced-r13* and measuring on the NR band given by the entry in the *InterRAT-BandListNR*. | - |
| ***interRAT-ParametersWLAN***  Indicates whether the UE supports WLAN measurements configured by *MeasObjectWLAN* with corresponding quantity and report configuration in the supported WLAN bands. | - |
| <Skip unrelated Parts> |  |
| ***supportedBandCombination***  Includes the supported CA band combinations, if any, and may include all the supported non-CA bands. | - |
| ***supportedBandCombinationAdd-r11***  Includes additional supported CA band combinations in case maximum number of CA band combinations of *supportedBandCombination* is exceeded. | - |
| ***SupportedBandCombinationAdd-v11d0,*** ***SupportedBandCombinationAdd-v1250,*** ***SupportedBandCombinationAdd-v1270, SupportedBandCombinationAdd-v1320, SupportedBandCombinationAdd-v1380, SupportedBandCombinationAdd-v1390, SupportedBandCombinationAdd-v1430, SupportedBandCombinationAdd-v1450, SupportedBandCombinationAdd-v1470, SupportedBandCombinationAdd-v14b0, SupportedBandCombinationAdd-v1530***  If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. | - |
| ***SupportedBandCombinationAdd-v16xy***  If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *SupportedBandCombinationAdd-r11* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* |  |
| ***SupportedBandCombinationExt, SupportedBandCombination-v1090, SupportedBandCombination-v10i0, SupportedBandCombination-v1130, SupportedBandCombination-v1250, SupportedBandCombination-v1270, SupportedBandCombination-v1320, SupportedBandCombination-v1380, SupportedBandCombination-v1390, SupportedBandCombination-v1430, SupportedBandCombination-v1450, SupportedBandCombination-v1470, SupportedBandCombination-v14b0, SupportedBandCombination-v1530***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. | - |
| ***SupportedBandCombination-v16xy***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombination-r10* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* |  |
| ***supportedBandCombinationReduced***  Includes the supported CA band combinations, and may include the fallback CA combinations specified in TS 36.101 [42], clause 4.3A. This field also indicates whether the UE supports reception of *requestReducedFormat*. | - |
| ***SupportedBandCombinationReduced-v1320, SupportedBandCombinationReduced-v1380, SupportedBandCombinationReduced-v1390, SupportedBandCombinationReduced-v1430, SupportedBandCombinationReduced-v1450, SupportedBandCombinationReduced-v1470, SupportedBandCombinationReduced-v14b0, SupportedBandCombinationReduced-v1530***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. | - |
| ***SupportedBandCombinationReduced-v16xy***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombinationReduced-r13* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* |  |
| ***SupportedBandGERAN***  GERAN band as defined in TS 45.005 [20]. | No |

<Skip unrelated Parts>