**3GPP TSG-RAN2 Meeting #110 electronic *R2-200xxxx***

**Online, June 1 – June 12 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **-** | **rev** | **-** | **Current version:** | **15.9.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR on introduction of BCS to asymmetric channel bandwidths (38.331) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon, Telus | | | | | | | | | |
| ***Source to TSG:*** | RAN2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_n66\_BW | | | | |  | ***Date:*** | | | 2020-05-22 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Based on RAN4 LS R4-2002852, RAN4 agreed to introduce channel bandwidth combination set to asymmetric channel bandwidths defined in clause 5.3.6, in TS 38.101-1 with following agreements:  • UE shall support asymmetric channel bandwidth combination set 0 which was defined in Rel-15 by default.  • For n66, support of asymmetric channel bandwidth combination set 1 is optional in Rel16.  Based on the RAN4 LS R4-2008893, from RAN4 point of view the support for asymmetric channel bandwidth combination set 1 for n66 can be release independent from Release 15. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add *asymmetricBandwidthCombinationSet* in per band level to indicate the asymmetric channel bandwidth combination set. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UE cannot report the asymmetric channel bandwidth combination set which may lead to failure configuration. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.306 CR xxxx | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---------------------------------------------START OF CHANGE-------------------------------------------

### 6.3.3 UE capability information elements

– *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

***RF-Parameters* information element**

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

supportedBandCombinationList BandCombinationList OPTIONAL,

appliedFreqBandListFilter FreqBandList OPTIONAL,

...,

[[

supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

]],

[[

supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

]],

[[

supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

]],

[[

supportedBandCombinationList-v16xy BandCombinationList-v16xy OPTIONAL

]]

}

BandNR ::= SEQUENCE {

bandNR FreqBandIndicatorNR,

modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

extendedCP ENUMERATED {supported} OPTIONAL,

multipleTCI ENUMERATED {supported} OPTIONAL,

bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

pusch-256QAM ENUMERATED {supported} OPTIONAL,

ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

channelBWs-DL CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

}

} OPTIONAL,

channelBWs-UL CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

}

} OPTIONAL,

...,

[[

maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

]],

[[

pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

]],

[[

maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

]],

[[

channelBWs-DL-v1590 CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

}

} OPTIONAL,

channelBWs-UL-v1590 CHOICE {

fr1 SEQUENCE {

scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

},

fr2 SEQUENCE {

scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

}

} OPTIONAL

]],

[[

asymmetricBandwidthCombinationSet-v15xy BIT STRING (SIZE (1..32)) OPTIONAL

]]

}

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| ***RF-Parameters* field descriptions** |
| ***appliedFreqBandListFilter***  In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationList***  A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |

---------------------------------------------END OF CHANGE---------------------------------------------