**3GPP TSG-RAN WG2 #110-e *R2-2006351***

**E-meeting, 01 – 12 June 2020**

**Agenda item:** 6.1.5

**Source:** Samsung (rapporteur)

**Title:** TP for TS 38.331 on IP Address allocation for IAB nodes

**Document for:** Discussion and decision

# Text Proposal for TS 38.331

**------------------------------------------------1st Change -----------------------------------------------------**

### 5.3.5 RRC reconfiguration

#### 5.3.5.1 General



Figure 5.3.5.1-1: RRC reconfiguration, successful



Figure 5.3.5.1-2: RRC reconfiguration, failure

The purpose of this procedure is to modify an RRC connection, e.g. to establish/modify/release RBs, to perform reconfiguration with sync, to setup/modify/release measurements, to add/modify/release SCells and cell groups, to add/modify/release conditional handover configuration, to add/modify/release conditional PSCell change configuration. As part of the procedure, NAS dedicated information may be transferred from the Network to the UE.

RRC reconfiguration to perform reconfiguration with sync includes, but is not limited to, the following cases:

- reconfiguration with sync and security key refresh, involving RA to the PCell/PSCell, MAC reset, refresh of security and re-establishment of RLC and PDCP triggered by explicit L2 indicators;

- reconfiguration with sync but without security key refresh, involving RA to the PCell/PSCell, MAC reset and RLC re-establishment and PDCP data recovery (for AM DRB) triggered by explicit L2 indicators.

In (NG)EN-DC and NR-DC, SRB3 can be used for measurement configuration and reporting, to (re-)configure MAC, RLC, physical layer and RLF timers and constants of the SCG configuration, and to reconfigure PDCP for DRBs associated with the S-KgNB or SRB3, and to reconfigure SDAP for DRBs associated with S-KgNB in NGEN-DC and NR-DC, and to add/modify/release conditional PSCell change configuration, provided that the (re-)configuration does not require any MN involvement. In (NG)EN-DC and NR-DC, only *measConfig*, *radioBearerConfig, conditionalReconfiguration* and/or *secondaryCellGroup* are included in *RRCReconfiguration* received via SRB3.

#### 5.3.5.2 Initiation

The Network may initiate the RRC reconfiguration procedure to a UE in RRC\_CONNECTED. The Network applies the procedure as follows:

- the establishment of RBs (other than SRB1, that is established during RRC connection establishment) is performed only when AS security has been activated;

- the addition of Secondary Cell Group and SCells is performed only when AS security has been activated;

- the *reconfigurationWithSync* is included in *secondaryCellGroup* only when at least one RLC bearer is setup in SCG;

- the *reconfigurationWithSync* is included in *masterCellGroup* only when AS security has been activated, and SRB2 with at least one DRB are setup and not suspended;

- the *conditionalReconfiguration* is included only when AS security has been activated, and SRB2 with at least one DRB are setup and not suspended.

#### 5.3.5.3 Reception of an *RRCReconfiguration* by the UE

The UE shall perform the following actions upon reception of the *RRCReconfiguration,* or upon execution of the conditional configuration (CHO or CPC):

1> if the *RRCReconfiguration* is applied due to a conditional configurationexecution upon cell selection while timer T311 is running, as defined in 5.3.7.3:

2> remove all the entries within *VarConditionalConfig*, if any;

NOTE: This step is performed so the UE only performs conditional configuration execution while timer T311 is running once for a given failure detection.

1> if the *RRCReconfiguration* includes the *daps-SourceRelease*:

2> reset source MAC and release the source MAC configuration;

2> for each DRB with a DAPS PDCP entity:

3> release the RLC entity and the associated logical channel for the source;

3> reconfigure the PDCP entity to normal PDCP as specified in TS 38.323 [5];

2> for each SRB:

3> release the PDCP entity for the source;

3> release the RLC entity and the associated logical channel for the source;

2> release the physical channel configuration for the source;

2> discard the keys used in source (the KgNB key, the S-KgNB key, the S-KeNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key), if any;

1> if the *RRCReconfiguration* is received via other RAT (i.e., inter-RAT handover to NR):

2> if the *RRCReconfiguration* does not include the *fullConfig* and the UE is connected to 5GC (i.e., delta signalling during intra 5GC handover):

3> re-use the source RAT SDAP and PDCP configurations if available (i.e., current SDAP/PDCP configurations for all RBs from source E-UTRA RAT prior to the reception of the inter-RAT HO *RRCReconfiguration* message);

1> else:

2> if the RRCReconfiguration includes the fullConfig:

3> perform the full configuration procedure as specified in 5.3.5.11;

1> if the *RRCReconfiguration* includes the *masterCellGroup*:

2> perform the cell group configuration for the received *masterCellGroup* according to 5.3.5.5;

1> if the *RRCReconfiguration* includes the *masterKeyUpdate*:

2> perform AS security key update procedure as specified in 5.3.5.7;

1> if the *RRCReconfiguration* includes the *sk-Counter*:

2> perform security key update procedure as specified in 5.3.5.7;

1> if the *RRCReconfiguration* includes the *secondaryCellGroup*:

2> perform the cell group configuration for the SCG according to 5.3.5.5;

1> if the *RRCReconfiguration* includes the *mrdc-SecondaryCellGroupConfig:*

2> if the *mrdc-SecondaryCellGroupConfig* is set to *setup*:

3> if the *mrdc-SecondaryCellGroupConfig* includes *mrdc-ReleaseAndAdd*:

4> perform MR-DC release as specified in clause 5.3.5.10;

3> if the received *mrdc-SecondaryCellGroup* is set to *nr-SCG*:

4> perform the RRC reconfiguration according to 5.3.5.3 for the *RRCReconfiguration* message included in *nr-SCG*;

3> if the received *mrdc-SecondaryCellGroup* is set to *eutra-SCG*:

4> perform the RRC connection reconfiguration as specified in TS 36.331 [10], clause 5.3.5.3 for the *RRCConnectionReconfiguration* message included in *eutra-SCG*;

2> else (*mrdc-SecondaryCellGroupConfig* is set to *release*):

3> perform MR-DC release as specified in clause 5.3.5.10;

1> if the *RRCReconfiguration* message includes the *radioBearerConfig*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCReconfiguration* message includes the *radioBearerConfig2*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCReconfiguration* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> if the *RRCReconfiguration* message includes the *dedicatedNAS-MessageList*:

2> forward each element of the *dedicatedNAS-MessageList* to upper layers in the same order as listed;

1> if the *RRCReconfiguration* message includes the *dedicatedSIB1-Delivery*:

2> perform the action upon reception of *SIB1* as specified in 5.2.2.4.2;

NOTE 0: If this *RRCReconfiguration* is associated to the MCG and includes *reconfigurationWithSync* in *spCellConfig* and *dedicatedSIB1-Delivery*, the UE initiates (if needed) the request to acquire required SIBs, according to clause 5.2.2.3.5, only after the random access procedure towards the target SpCell is completed.

1> if the *RRCReconfiguration* message includes the *dedicatedSystemInformationDelivery*:

2> perform the action upon reception of System Information as specified in 5.2.2.4;

1> if the *RRCReconfiguration* message includes the *otherConfig*:

2> perform the other configuration procedure as specified in 5.3.5.9;

1> if the *RRCReconfiguration* message includes the *bap-Config*:

2> perform the BAP configuration procedure as specified in 5.3.5.12;

1> if the *RRCReconfiguration* message includes the *conditionalReconfiguration*:

2> perform conditional configuration as specified in 5.3.5.13;

1> if the *RRCReconfiguration* message includes the *sl-ConfigDedicatedNR*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.5.8;

1> if the *RRCReconfiguration* message includes the *sl-ConfigDedicatedEUTRA*:

2> if *sl-V2X-ConfigDedicated* is included in *sl-ConfigDedicatedEUTRA*

3> perform the V2X sidelink communication dedicated configuration procedure as specified in 5.3.10.15a in TS 36.331 [10];

2> if *sl-V2X-SPS-Config* is included in *sl-ConfigDedicatedEUTRA*

3> perform V2X sidelink SPS reconfiguration as specified in 5.3.10.5 in TS 36.331 [10];

1> if the *RRCReconfiguration* message includes the *iab-IP-Address*:

 2> if *iab-IP-AddressToReleaseList* is included:

 3> for each *IAB-IP-AddressIndex-r16* received in the *iab-IP-AddressToReleaseList*

4> release the corresponding IP address;

2> if *iab-IP-AddressToAddModList* is included:

3> for each *IAB-IP-AddressIndex-r16* received in the *iab-IP-AddressToAddModList*

4> add the IP address in accordance with the received *IAB-IP-Address* as specified in 5.7.x.5;

1> set the content of the *RRCReconfigurationComplete* message as follows:

2> if the *RRCReconfiguration* includes the *masterCellGroup* containing the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each MCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each MCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *RRCReconfiguration* includes the *secondaryCellGroup* containing the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each SCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each SCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *RRCReconfiguration* message includes the *mrdc-SecondaryCellGroupConfig* with *mrdc-SecondaryCellGroup* set to *eutra-SCG*:

3> include in the *eutra-SCG-Response* the E-UTRA *RRCConnectionReconfigurationComplete* message in accordance with TS 36.331 [10] clause 5.3.5.3;

2> if the *RRCReconfiguration* message includes the *mrdc-SecondaryCellGroupConfig* with *mrdc-SecondaryCellGroup* set to *nr-SCG*:

3> include in the *nr-SCG-Response* the *RRCReconfigurationComplete* message;

2> if the *RRCReconfiguration* message was included in an *RRCResume* message:

3> include the *RRCReconfigurationComplete* message in the *nr-SCG-Response* within the *scg-Response* in the *RRCResumeComplete* message;

2> if the *RRCReconfiguration* message was included in E-UTRA *RRCConnectionResume* message:

3> include the *RRCReconfigurationComplete* message in the E-UTRA MCG RRC message *RRCConnectionResumeComplete* in accordance with TS 36.313 [10], clause 5.3.3.4a;

2> if the *RRCReconfiguration* is applied due to a conditional configuration execution and included a s*econdaryCellGroupConfig*:

3> if the applied *RRCReconfiguration* message was received via SRB1:

4> if the applied *RRCReconfiguration* message was received via E-UTRAN:

5> FFS;

Editor's note: FFS How the *RRCReconfigurationComplete* is transmitted when the UE is in EN-DC e.g. *ULInformationTransferMRDC* or *RRCConnectionReconfigurationComplete.*

4> else:

5> submit the *RRCReconfigurationComplete* to lower layers for transmissionvia SRB1;

Editor's note: FFS on whether to inform MN upon the CPC execution if CPC configured via SRB3

2> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable* in the *RRCReconfigurationComplete* message;

2> if the UE has Bluetooth logged measurements available and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailableBT* in the *RRCReconfigurationComplete* message;

2> if the UE has WLAN logged measurements available and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailableWLAN* in the *RRCReconfigurationComplete* message;

2> if the UE has connection establishment failure information available in *VarConnEstFailReport* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport*:

3> include *connEstFailInfoAvailable* in the *RRCReconfigurationComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

3> include *rlf-InfoAvailable* in the *RRCReconfigurationComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> include *rlf-InfoAvailable* in the *RRCReconfigurationComplete* message;

1> if the UE is configured with E-UTRA *nr-SecondaryCellGroupConfig* (UE in (NG)EN-DC):

2> if the *RRCReconfiguration* message was received via E-UTRA SRB1 as specified in TS 36.331 [10]; or

2> if the *RRCReconfiguration* message was received via SRB3 within *DLInformationTransferMRDC*

3> submit the *RRCReconfigurationComplete* via E-UTRA embedded in E-UTRA RRC message *RRCConnectionReconfigurationComplete* as specified in TS 36.331 [10], clause 5.3.5.3/5.3.5.4;

3> if *reconfigurationWithSync* was included in *spCellConfig* of an SCG:

4> initiate the Random Access procedure on the SpCell, as specified in TS 38.321 [3];

3> else:

4> the procedure ends;

NOTE 1: The order the UE sends the *RRCConnectionReconfigurationComplete* message and performs the Random Access procedure towards the SCG is left to UE implementation.

2> else (*RRCReconfiguration* was received via SRB3) but not within *DLInformationTransferMRDC*:

3> submit the *RRCReconfigurationComplete* message via SRB3 to lower layers for transmission using the new configuration;

NOTE 2: In (NG)EN-DC and NR-DC, in the case *RRCReconfiguration* is received via SRB1 or within *DLInformationTransferMRDC* via SRB3, the random access is triggered by RRC layer itself as there is not necessarily other UL transmission. In the case *RRCReconfiguration* is received via SRB3 but not within *DLInformationTransferMRDC*, the random access is triggered by the MAC layer due to arrival of *RRCReconfigurationComplete*.

1> else if the *RRCReconfiguration* message was received via SRB1 within the *nr-SCG* within *mrdc-SecondaryCellGroup* (UE in NR-DC, *mrdc-SecondaryCellGroup* was received in *RRCReconfiguration* via SRB1):

2> if *reconfigurationWithSync* was included in *spCellConfig* in *nr-SCG*:

3> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

2> else

3> the procedure ends;

NOTE 2a: The order in which the UE sends the *RRCReconfigurationComplete* message and performs the Random Access procedure towards the SCG is left to UE implementation.

1> else if the *RRCReconfiguration* message was received via SRB3 (UE in NR-DC):

2> if the *RRCReconfiguration* message was received within *DLInformationTransferMRDC*:

3> if the *RRCReconfiguration* message was received within the *nr-SCG* within *mrdc-SecondaryCellGroup* (NR SCG RRC Reconfiguration):

4> if *reconfigurationWithSync* was included in *spCellConfig* in *nr-SCG*:

5> initiate the Random Access procedure on the PSCell, as specified in TS 38.321 [3];

4> the procedure ends;

3> submit the *RRCReconfigurationComplete* message via SRB1 to lower layers for transmission using the new configuration;

3> the procedure ends;

2> submit the *RRCReconfigurationComplete* message via SRB3 to lower layers for transmission using the new configuration;

1> else(*RRCReconfiguration* was received via SRB1):

2> submit the *RRCReconfigurationComplete* message via SRB1 to lower layers for transmission using the new configuration;

2> if this is the first *RRCReconfiguration* message after successful completion of the RRC re-establishment procedure:

3> resume SRB2 and DRBs that are suspended;

1> if *reconfigurationWithSync* was included in *spCellConfig* of an MCG or SCG, and when MAC of an NR cell group successfully completes a Random Access procedure triggered above;

2> stop timer T304 for that cell group;

2> stop timer T310 for source if running;

2> apply the parts of the CSI reporting configuration, the scheduling request configuration and the sounding RS configuration that do not require the UE to know the SFN of the respective target SpCell, if any;

2> apply the parts of the measurement and the radio resource configuration that require the UE to know the SFN of the respective target SpCell (e.g. measurement gaps, periodic CQI reporting, scheduling request configuration, sounding RS configuration), if any, upon acquiring the SFN of that target SpCell;

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an MCG:

3> if T390 is running:

4> stop timer T390 for all access categories;

4> perform the actions as specified in 5.3.14.4.

3> if *RRCReconfiguration* does not include *dedicatedSIB1-Delivery* and

3> if the active downlink BWP, which is indicated by the *firstActiveDownlinkBWP-Id* for the target SpCell of the MCG, has a common search space configured by *searchSpaceSIB1*:

4> acquire the *SIB1*, which is scheduled as specified in TS 38.213 [13], of the target SpCell of the MCG;

4> upon acquiring *SIB1*, perform the actions specified in clause 5.2.2.4.2;

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an MCG; or:

2> if the *reconfigurationWithSync* was included in *spCellConfig* of an SCG and the CPC was configured

3> remove all the entries within *VarConditionalConfig*, if any;

3> for each *measId* of the source SpCell configuration, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

4> for the associated *reportConfigId*:

5> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

4> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *cho-TriggerConfig*:

5> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

4> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if *reconfigurationWithSync* was included in *masterCellGroup*; and

2> if the UE transmitted a *UEAssistanceInformation* message during the last 1 second, and the UE is still configured to provide UE assistance information:

3> initiate transmission of a *UEAssistanceInformation* message to re-send the UE assistance information that UE is still configured to provide with the same contents;

2> if *SIB12* is provided by the target PCell; and the UE transmitted a *SidelinkUEInformationNR* message indicating a change of NR sidelink communication related parameters relevant in target PCell (i.e. change of *sl-RxInterestedFreqList* or *sl-TxResourceReqList*) during the last 1 second preceding reception of the *RRCReconfiguration* message including *reconfigurationWithSync*:

3> initiate transmission of the *SidelinkUEInformationNR* message in accordance with 5.8.3.3;

2> the procedure ends.

NOTE 3: The UE is only required to acquire broadcasted *SIB1* if the UE can acquire it without disrupting unicast data reception, i.e. the broadcast and unicast beams are quasi co-located.

**------------------------------------------------2st Change -----------------------------------------------------**

## 5.7 Other

**>>>>>>>>>>>>>>> Unchanged parts are skipped<<<<<<<<<<<<<<<<**

### 5.7.x IAB IP Address Information

#### 5.7.x.1 General



Figure 5.7.x.1-1: IAB IP Address Information procedure

The IAB IP Address Information procedure is used by IAB-MT to request the IAB-donor-CU to allocate IP address or inform the IAB-donor-CU of the IP address for the collocated IAB-DU.

#### 5.7.x.2 Initiation

Upon initiation of the procedure, the IAB-MT shall:

1> initiate transmission of the *IABIPAddressInformation* message in accordance with 5.7.x.3;

#### 5.7.x.3 Actions related to transmission of *IABIPAddressInformation* message

The IAB-MT shall set the contents of *IABIPAddressInformation* message as follows:

1> if the procedure is used to request IP address:

2> if IPv4 address is requested:

3> set the *iab-IPv4-AddressNumReq* to the number of IPv4 address requested per specific usage;

2> else if IPv6 address is requested:

3> set the *iab-IPv6-AddressNumReq* to the number of IPv6 address requested per specific usage;

2> else if IPv6 address prefix is requested:

3> set the *iab-IPv6-AddressPrefixReq* to true per specific usage;

 1> if the procedure is used to report IP address:

 2> if IPv4 address is reported:

3> include *iPv4-Address* in *iab-IPv4-AddressReport;*

4> if this IPv4 address is used for F1-C traffic:

5> include this address in *f1-C-Traffic-IP-Address*.

4> else if this IPv4 address is used for F1-U traffic:

5> include this address in *f1-U-Traffic-IP-Address*.

4> else if this IPv4 address is used for non-F1 traffic:

5> include this address in *non-f1-Traffic-IP-Address*.

2> else if IPv6 address is reported:

3> include *iPv6-Address* in *iab-IPv6-AddressReport;*

4> if this IPv6 address is used for F1-C traffic:

5> include this address in *f1-C-Traffic-IP-Address*.

4> if this IPv6 address is used for F1-U traffic:

5> include this address in *f1-U-Traffic-IP-Address*.

4> if this IPv6 address is used for non-F1 traffic:

5> include this address in *non-f1-Traffic-IP-Address*.

2> else if IPv6 address prefix is reported:

3> include *iPv6-Prefix* in *iab-IPv6-PrefixReport;*

4> if this IPv6 address prefix is used for F1-C traffic:

5> include this prefix in *f1-C-Traffic-IP-Address*.

4> if this IPv6 address prefix is used for F1-U traffic:

5> include this prefix in *f1-U-Traffic-IP-Address*.

4> if this IPv6 address prefix is used for non-F1 traffic:

5> include this prefix in *non-f1-Traffic-IP-Address*.

1> submit the *IABIPAddressInformation* message to lower layers for transmission, upon which the procedure ends.

#### 5.7.x.4 IP Address Release

The IAB-MT shall:

1> if the release is triggered by reception of the *iab-IP-AddressToReleaseList*:

 2> for each *iab-IP-AddressIndex* value included in *iab-IP-AddressToReleaseList:*

3> release the corresponding IP address.

#### 5.7.x.5 IP Address Addition/Modification

The IAB-MT shall:

 1> for each *iab-IP-AddressIndex* value included in the *iab-IP- AddressToAddModList* that is not part of the current IAB-MT configuration:

 2> add the IP address, corresponding to the *iab-IP-AddressIndex.*

2> if *iPv4-Address* is included:

3> if *f1-C* is included in *iab-IP-Usage:*

4> store the received IPv4 address for F1-C traffic.

3> else if *f1-U* is included in *iab-IP-Usage*:

4> store the received IPv4 address for F1-U traffic.

3> else if *non-F1* is included in *iab-IP-Usage*:

4> store the received IPv4 address for non-F1 traffic.

2> else if *iPv6-Address* is included:

3> if *f1-C* is included in *iab-IP-Usage*:

4> store the received IPv6 address for F1-C traffic.

3> else if *f1-U* is included in *iab-IP-Usage*:

4> store the received IPv6 address for F1-U traffic.

3> else if *non-F1* is included in *iab-IP-Usage*:

4> store the received IPv6 address for non-F1 traffic.

2> else if *iPv6-Prefix* is included in *iab-IP-AddressToAddModList*:

3> if *f1-C* is included in *iab-IP-Usage*:

4> store the received IPv6 address prefix for F1-C traffic.

3> else if *f1-U* is included in *iab-IP-Usage*:

4> store the received IPv6 address prefix for F1-U traffic.

3> else if *non-F1* is included in *iab-IP-Usage*:

4> store the received IPv6 address prefix for non-F1 traffic.

 1> for each *iab-IP-AddressIndex* value included in the *iab-IP- AddressToAddModList* that is part of the current IAB-MT configuration:

 2> modify the IP address configuration in accordance with the *iab-IP-Address-Allocation.***------------------------------------------------3st Change -----------------------------------------------------**

## 6.2 RRC messages

### 6.2.1 General message structure

**>>>>>>>>>>>>>>> Unchanged parts are skipped<<<<<<<<<<<<<<<<**

*– UL-DCCH-Message*

The *UL-DCCH-Message* class is the set of RRC messages that may be sent from the UE to the network on the uplink DCCH logical channel.

-- ASN1START

-- TAG-UL-DCCH-MESSAGE-START

UL-DCCH-Message ::= SEQUENCE {

 message UL-DCCH-MessageType

}

UL-DCCH-MessageType ::= CHOICE {

 c1 CHOICE {

 measurementReport MeasurementReport,

 rrcReconfigurationComplete RRCReconfigurationComplete,

 rrcSetupComplete RRCSetupComplete,

 rrcReestablishmentComplete RRCReestablishmentComplete,

 rrcResumeComplete RRCResumeComplete,

 securityModeComplete SecurityModeComplete,

 securityModeFailure SecurityModeFailure,

 ulInformationTransfer ULInformationTransfer,

 locationMeasurementIndication LocationMeasurementIndication,

 ueCapabilityInformation UECapabilityInformation,

 counterCheckResponse CounterCheckResponse,

 ueAssistanceInformation UEAssistanceInformation,

 failureInformation FailureInformation,

 ulInformationTransferMRDC ULInformationTransferMRDC,

 scgFailureInformation SCGFailureInformation,

 scgFailureInformationEUTRA SCGFailureInformationEUTRA

 },

 messageClassExtension CHOICE {

 c2 CHOICE {

 ulDedicatedMessageSegment-r16 ULDedicatedMessageSegment-r16,

 dedicatedSIBRequest-r16 DedicatedSIBRequest-r16,

 mcgFailureInformation-r16 MCGFailureInformation-r16,

 ueInformationResponse-r16 UEInformationResponse-r16,

 sidelinkUEInformationNR-r16 SidelinkUEInformationNR-r16,

 sidelinkUEInformationEUTRA-r16 SidelinkUEInformationEUTRA-r16,

 ueAssistanceInformationEUTRA-r16 UEAssistanceInformationEUTRA-r16,

 iabIPAddressInformation-r16 IABIPAddressInformation-r16, spare8 NULL,spare7 NULL, spare6 NULL,

 spare5 NULL, spare4 NULL, spare3 NULL, spare2 NULL, spare1 NULL

 },

 messageClassExtensionFuture-r16 SEQUENCE {}

 }

}

-- TAG-UL-DCCH-MESSAGE-STOP

-- ASN1STOP

**------------------------------------------------4st Change -----------------------------------------------------**

### 6.2.2 Message definitions

**>>>>>>>>>>>>>>> Unchanged parts are skipped<<<<<<<<<<<<<<<<**

#### – *RRCReconfiguration*

The *RRCReconfiguration* message is the command to modify an RRC connection. It may convey information for measurement configuration, mobility control, radio resource configuration (including RBs, MAC main configuration and physical channel configuration) and AS security configuration.

Signalling radio bearer: SRB1 or SRB3

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

*RRCReconfiguration message*

-- ASN1START

-- TAG-RRCRECONFIGURATION-START

RRCReconfiguration ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcReconfiguration RRCReconfiguration-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCReconfiguration-IEs ::= SEQUENCE {

 radioBearerConfig RadioBearerConfig OPTIONAL, -- Need M

 secondaryCellGroup OCTET STRING (CONTAINING CellGroupConfig) OPTIONAL, -- Need M

 measConfig MeasConfig OPTIONAL, -- Need M

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCReconfiguration-v1530-IEs OPTIONAL

}

RRCReconfiguration-v1530-IEs ::= SEQUENCE {

 masterCellGroup OCTET STRING (CONTAINING CellGroupConfig) OPTIONAL, -- Need M

 fullConfig ENUMERATED {true} OPTIONAL, -- Cond FullConfig

 dedicatedNAS-MessageList SEQUENCE (SIZE(1..maxDRB)) OF DedicatedNAS-Message OPTIONAL, -- Cond nonHO

 masterKeyUpdate MasterKeyUpdate OPTIONAL, -- Cond MasterKeyChange

 dedicatedSIB1-Delivery OCTET STRING (CONTAINING SIB1) OPTIONAL, -- Need N

 dedicatedSystemInformationDelivery OCTET STRING (CONTAINING SystemInformation) OPTIONAL, -- Need N

 otherConfig OtherConfig OPTIONAL, -- Need M

 nonCriticalExtension RRCReconfiguration-v1540-IEs OPTIONAL

}

RRCReconfiguration-v1540-IEs ::= SEQUENCE {

 otherConfig-v1540 OtherConfig-v1540 OPTIONAL, -- Need M

 nonCriticalExtension RRCReconfiguration-v1560-IEs OPTIONAL

}

RRCReconfiguration-v1560-IEs ::= SEQUENCE {

 mrdc-SecondaryCellGroupConfig SetupRelease { MRDC-SecondaryCellGroupConfig } OPTIONAL, -- Need M

 radioBearerConfig2 OCTET STRING (CONTAINING RadioBearerConfig) OPTIONAL, -- Need M

 sk-Counter SK-Counter OPTIONAL, -- Need N

 nonCriticalExtension RRCReconfiguration-v16xy-IEs OPTIONAL

}

RRCReconfiguration-v16xy-IEs ::= SEQUENCE {

 otherConfig-v16xy OtherConfig-v16xy OPTIONAL, -- Need M

 bap-Config-r16 SetupRelease { BAP-Config-r16 } OPTIONAL, -- Need M

 conditionalReconfiguration-r16 ConditionalReconfiguration-r16 OPTIONAL, -- Need M

 daps-SourceRelease-r16 ENUMERATED{true} OPTIONAL, -- Need N

 sl-ConfigDedicatedNR-r16 SetupRelease {SL-ConfigDedicatedNR-r16} OPTIONAL, -- Need M

sl-ConfigDedicatedEUTRA-r16 SetupRelease {SL-ConfigDedicatedEUTRA-r16} OPTIONAL, -- Need Miab-IP-AddressConfiguration-r16 IAB-IP-AddressConfiguration-r16 OPTIONAL, -- Need M

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Editor's Note: Whether an explicit indication is needed to configure/deconfigure the on-demand SIB request for CONNECTED UEs is FFS.

MRDC-SecondaryCellGroupConfig ::= SEQUENCE {

 mrdc-ReleaseAndAdd ENUMERATED {true} OPTIONAL, -- Need N

 mrdc-SecondaryCellGroup CHOICE {

 nr-SCG OCTET STRING (CONTAINING RRCReconfiguration),

 eutra-SCG OCTET STRING

 }

}

BAP-Config-r16 ::= SEQUENCE {

 bap-Address-r16 BIT STRING (SIZE (10)) OPTIONAL, -- Need M

 defaultUL-BAP-routingID-r16 BAP-Routing-ID-r16 OPTIONAL, -- Need M

 defaultUL-BH-RLC-Channel-r16 BH-RLC-ChannelID-r16 OPTIONAL, -- Need M

 flowControlFeedbackType-r16 ENUMERATED {perBH-RLC-Channel, perRoutingID, both} OPTIONAL, -- Need R

...

}

MasterKeyUpdate ::= SEQUENCE {

 keySetChangeIndicator BOOLEAN,

 nextHopChainingCount NextHopChainingCount,

 nas-Container OCTET STRING OPTIONAL, -- Cond securityNASC

 ...

}

IAB-IP-AddressConfiguration-r16 ::= SEQUENCE {

 iab-IP-AddressToAddModList-r16 SEQUENCE (SIZE(1..maxIAB-IP-Address-r16)) OF IAB-IP-AddressConfiguration-r16 OPTIONAL, -- Need N

 iab-IP-AddressToReleaseList-r16 SEQUENCE (SIZE(1..maxIAB-IP-Address-r16)) OF IAB-IP-AddressIndex-r16 OPTIONAL, -- Need N

 ...

}IAB-IP-AddressConfiguration-r16 ::= SEQUENCE {

 iab-IP-AddressIndex-r16 IAB-IP-AddressIndex-r16,

 iab-IP-Address-r16 IAB-IP-Address-r16 OPTIONAL, -- Need M

iab-IP-Usage-r16 IAB-IP-Usage-r16 OPTIONAL, -- Need M

donor-DU-BAP-Address-r16 BIT STRING (SIZE(10)) OPTIONAL, -- Need M

...

}

-- TAG-RRCRECONFIGURATION-STOP

-- ASN1STOP

|  |
| --- |
| *RRCReconfiguration-IEs* field descriptions |
| ***bap-Config***This field is used to configure the BAP entity for IAB-node. |
| ***bap-Address***Indicates the BAP address of an IAB-node. |
| ***conditionalReconfiguration***Configuration of candidate target SpCell(s) and execution condition(s) for conditional handover or conditional PSCell change. For conditional PSCell change, this field may only be present in an *RRCReconfiguration* message for intra-SN PSCell change. The network does not configure a UE with both conditional PCell change and conditional PSCell change simultaneously. The field is absent if *dapsConfig* is configured for any DRB or the cell indicated in *masterCellGroup* is different from the serving cell. |
| ***daps-SourceRelease***Indicates the UE to release the source. |
| ***dedicatedNAS-MessageList***This field is used to transfer UE specific NAS layer information between the network and the UE. The RRC layer is transparent for each PDU in the list.  |
| ***dedicatedSIB1-Delivery***This field is used to transfer *SIB1* to the UE. The field has the same values as the corresponding configuration in *servingCellConfigCommon*. |
| ***dedicatedSystemInformationDelivery***This field is used to transfer *SIB6*, *SIB7*, *SIB8* to the UE in RRC\_IDLE and RRC\_INACTIVE. For UEs in RRC\_CONNECTED, this field is used to transfer the SIBs requested on-demand. |
| ***defaultUL-BAP-routingID***This field is used for IAB-node to configure the default uplink Routing ID *during IAB-node bootstrapping for F1-C and non-F1 traffic*. |
| ***defaultUL-BH-RLC-Channel***This field is used for IAB-node to configure the default uplink *bh-RLC-Channel during IAB-node bootstrapping for F1-C and non-F1 traffic*. |
| ***donor-DU-BAP-Address***This field is used to indicate the BAP address of the IAB-donor-DU which anchors the IP address/prefix. |
| ***flowControlFeedbackType***This field is only used for IAB-node that support hop-by-hop flow control to configure the type of flow control feedback. Value *perBH-RLC-Channel* indicates the IAB-node shall provide flow control feedback per BH RLC channel, value *perRoutingID* indicates the IAB-node shall provide flow control feedback per routing ID, and value *both* indicates that the IAB-node shall provide flow control feedback both per BH RLC channel and per routing ID. |
| ***fullConfig***Indicates that the full configuration option is applicable for the *RRCReconfiguration* message for intra-system intra-RAT HO. For inter-RAT HO from E-UTRA to NR, *fullConfig* indicates whether or not delta signalling of SDAP/PDCP from source RAT is applicable. This field is absent if *dapsConfig* is configured for any DRB or when the *RRCReconfiguration* message is transmitted on SRB3, and in an *RRCReconfiguration* message contained in another *RRCReconfiguration* message (or *RRCConnectionReconfiguration* message, see TS 36.331 [10]) transmitted on SRB1. |
| ***iab-IP-Address***This field is used to provide the IP address allocation for IAB-node.  |
|  ***iab-IP-AddressToAddModList***List of IP addresses allocated for IAB-node to be added and modified.  |
| ***iab-IP-AddressToReleaseList***List of IP address allocated for IAB-node to be released. |
| ***iab-IP-Usage***This field is used to indicate the usage of the assigned IP address.  |
| ***keySetChangeIndicator***Indicates whether UE shall derive a new KgNB. If *reconfigurationWithSync* is included, value *true* indicates that a KgNB key is derived from a KAMF key taken into use through the latest successful NAS SMC procedure, or N2 handover procedure with KAMF change, as described in TS 33.501 [11] for KgNB re-keying. Value *false* indicates that the new KgNB key is obtained from the current KgNB key or from the NH as described in TS 33.501 [11]. |
| ***masterCellGroup***Configuration of master cell group. |
| ***mrdc-ReleaseAndAdd***This field indicates that the current SCG configuration is released and a new SCG is added at the same time. |
| ***mrdc-SecondaryCellGroup***Includes an RRC message for SCG configuration in NR-DC or NE-DC.For NR-DC (nr-SCG), *mrdc-SecondaryCellGroup* contains the *RRCReconfiguration* message as generated (entirely) by SN gNB. In this version of the specification, the RRC message can only include fields *secondaryCellGroup* and *measConfig*.For NE-DC (eutra-SCG), *mrdc-SecondaryCellGroup* includes the E-UTRA *RRCConnectionReconfiguration* message as specified in TS 36.331 [10]. In this version of the specification, the E-UTRA RRC message can only include the field *scg-Configuration*. |
| ***nas-Container***This field is used to transfer UE specific NAS layer information between the network and the UE. The RRC layer is transparent for this field, although it affects activation of AS security after inter-system handover to NR. The content is defined in TS 24.501 [23]. |
| ***nextHopChainingCount***Parameter NCC: See TS 33.501 [11] |
| ***otherConfig***Contains configuration related to other configurations. |
| ***radioBearerConfig***Configuration of Radio Bearers (DRBs, SRBs) including SDAP/PDCP. In EN-DC this field may only be present if the *RRCReconfiguration* is transmitted over SRB3. |
| ***radioBearerConfig2***Configuration of Radio Bearers (DRBs, SRBs) including SDAP/PDCP. This field can only be used if the UE supports NR-DC or NE-DC. |
| ***secondaryCellGroup***Configuration of secondary cell group ((NG)EN-DC or NR-DC). This field can only be present in an *RRCReconfiguration* message is transmitted on SRB3, and in an *RRCReconfiguration* message contained in another *RRCReconfiguration* message (or *RRCConnectionReconfiguration* message, see TS 36.331 [10]) transmitted on SRB1. |
| ***sk-Counter***A counter used upon initial configuration of S-KgNB or S-KeNB, as well as upon refresh of S-KgNB or S-KeNB. This field is always included either upon initial configuration of an NR SCG or upon configuration of the first RB with *keyToUse* set to *secondary*, whichever happens first. This field is absent if there is neither any NR SCG nor any RB with *keyToUse* set to *secondary*. |
| ***sl-ConfigDedicatedNR***This field is used to provide the dedicated configurations for NR sidelink communication. |
| ***sl-ConfigDedicatedEUTRA***This field is used to provide the dedicated configurations for V2X sidelink communication. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *nonHO* | The field is absent in case of reconfiguration with sync within NR or to NR; otherwise it is optionally present, need N. |
| *securityNASC* | This field is mandatory present in case of inter system handover. Otherwise the field is optionally present, need N. |
| *MasterKeyChange* | This field is mandatory present in case *masterCellGroup* includes *ReconfigurationWithSync* and *RadioBearerConfig* includes *SecurityConfig* with *SecurityAlgorithmConfig*, indicating a change of the AS security algorithms associated to the master key. If *ReconfigurationWithSync* is included for other cases, this field is optionally present, need N. Otherwise the field is absent. |
| *FullConfig* | The field is mandatory present in case of inter-system handover from E-UTRA/EPC to NR. It is optionally present, Need N, during reconfiguration with sync and also in first reconfiguration after reestablishment; or for intra-system handover from E-UTRA/5GC to NR. It is absent otherwise. |

**>>>>>>>>>>>>>>> Unchanged parts are skipped<<<<<<<<<<<<<<<<**– *IABIPAddressInformation*

The *IABIPAddressInformation* message is used by IAB-MT to request the network to allocate IP addresses for an IAB node or inform the network about IP addresses allocated to the collocated IAB-DU.

Signalling radio bearer: SRB1 or SRB3

RLC-SAP: AM

Logical channel: DCCH

Direction: IAB-MT to Network

***IABIPAddressInformation message***

-- ASN1START

-- TAG-IABIPADDRESSInformation-START

IABIPAddressInformation-r16 ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 iabIPAddressInformation-r16 IABIPAddressInformation-r16-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

IABIPAddressInformation-r16-IEs ::= SEQUENCE {

iab-IP-Request-r16 SEQUENCE {

 iab-IPv4-AddressNumReq-r16 IAB-IPAddressNumReq-r16 OPTIONAL,

 iab-IPv6-AddressReq-r16 CHOICE {

 iab-IPv6-AddressNumReq-r16 IAB-IPAddressNumReq-r16,

 iab-IPv6-AddressPrefixReq-r16 IAB-IPAddressPrefixReq-r16,

 ...

 } OPTIONAL,

} OPTIONAL,

iab-IP-Report-r16 SEQUENCE {

 iab-IPv4-AddressReport-r16 IAB-IP-AddressAndTraffic-r16, OPTIONAL,

 iab-IPv6-Report-r16 ::= CHOICE {

 iab-IPv6-AddressReport-r16 IAB-IP-AddressAndTraffic-r16, OPTIONAL,

 iab-IPv6-PrefixReport-r16 IAB-IP-PrefixAndTraffic-r16, OPTIONAL

 ...

 }

} OPTIONAL,

...

}

IAB-IPAddressNumReq-r16 ::= SEQUENCE {

 all-Traffic-NumReq-r16 INTEGER (1..8) OPTIONAL,

f1-C-Traffic-NumReq-r16 INTEGER (1..8) OPTIONAL,

f1-U-Traffic-NumReq-r16 INTEGER (1..8) OPTIONAL,

non-F1-Traffic-NumReq-r16 INTEGER (1..8) OPTIONAL,

...

}

IAB-IPAddressPrefixReq-r16 ::= SEQUENCE {

 all-Traffic-PrefixReq-r16 ENUMERATED (true) OPTIONAL,

f1-C-Traffic-PrefixReq-r16 ENUMERATED (true) OPTIONAL,

f1-U-Traffic-PrefixReq-r16 ENUMERATED (true) OPTIONAL,

non-F1-Traffic-PrefixReq-r16 ENUMERATED (true) OPTIONAL,

...

}

IAB-IP-AddressAndTraffic-r16 ::= SEQUENCE {

 all-Traffic-IAB-IP-Address-r16 SEQUENCE (size(1..8)) of IAB-IP-Address-r16 OPTIONAL,

 f1-C-Traffic-IP-Address-r16 SEQUENCE (size(1..8)) of IAB-IP-Address-r16 OPTIONAL,

 f1-U-Traffic-IP-Address-r16 SEQUENCE (size(1..8)) of IAB-IP-Address-r16 OPTIONAL,

 non-F1-Traffic-IP-Address-r16 SEQUENCE (size(1..8)) of IAB-IP-Address-r16 OPTIONAL

}

IAB-IP-PrefixAndTraffic-r16 ::= SEQUENCE {

 all-Traffic-IAB-IP-Address-r16 IAB-IP-Address-r16 OPTIONAL,

 f1-C-Traffic-IP-Address-r16 IAB-IP-Address-r16 OPTIONAL,

 f1-U-Traffic-IP-Address-r16 IAB-IP-Address-r16 OPTIONAL,

 non-F1-Traffic-IP-Address-r16 IAB-IP-Address-r16 OPTIONAL

}

-- TAG-IABIPADDRESSInformation-STOP

-- ASN1STOP

|  |
| --- |
| ***IABIPAddressInformation-IEs* field descriptions** |
| ***all-Traffic-PrefixReq***This field is used to request the IPv6 address prefix for all traffic. The length of allocated IPv6 prefix is fixed to 64. |
| ***all-Traffic-NumReq***This field is used to request the numbers of IP address for all traffic. |
| ***IAB-IP-AddressAndTraffic***This field is used to report to IAB-donor-CU the IP addresses per specific usage assigned by OAM for IAB-DU. |
| ***IAB-IP-PrefixAndTraffic***This field is used to report to IAB-donor-CU the IPv6 prefixes per specific usage assigned by OAM for IAB-DU. |
| ***iab-IPv4-AddressNumReq***This field is used to request the numbers of IPv4 address per specific usage. The specifc usages include F1-C traffic, F1-U traffic and non-F1 traffic. |
| ***iab-IPv6-AddressReq***This field is used to request the numbers or the prefix of IPv6 address per specific usage. The specifc usages include F1-C traffic, F1-U traffic and non-F1 traffic. |
| ***f1-C-Traffic-PrefixReq***This field is used to request the IPv6 address prefix for F1-C traffic. The length of allocated IPv6 prefix is fixed to 64. |
| ***f1-C-Traffic-NumReq***This field is used to request the numbers of IP address for F1-C traffic. |
| ***f1-U-Traffic-PrefixReq***This field is used to request the IPv6 address prefix for F1-U traffic. The length of allocated IPv6 prefix is fixed to 64. |
| ***f1-U-Traffic-NumReq***This field is used to request the numbers of IP address for F1-U traffic. |
| ***non-F1-Traffic-PrefixReq***This field is used to request the IPv6 address prefix for non-F1 traffic. The length of allocated IPv6 prefix is fixed to 64. |
| ***non-F1-Traffic-NumReq***This field is used to request the numbers of IP address for non-F1 traffic. |

**------------------------------------------------4st Change -----------------------------------------------------**

### 6.3.2 Radio resource control information elements

– *IAB-IP-Address*

The IE *IAB-IP-Address* is used to indicate the IP address/prefix.

***IAB-IP-Address*** ***information element***

-- ASN1START

-- TAG-IAB-IP-ADDRESS-START

IAB-IP-Address-r16 ::= CHOICE {

 iPv4-Address-r16 BIT STRING (SIZE(32)),

 iPv6-Address-r16 BIT STRING (SIZE(128)),

 iPv6-Prefix-r16 BIT STRING (SIZE(64)),

 ...

}

-- TAG-IAB-IP-ADDRESS-STOP

-- ASN1STOP

|  |
| --- |
| ***IAB-IP-Address* field descriptions** |
| ***iPv4-Address***This field is used to provide the allocated IPv4 address. |
| ***iPv6-Address***This field is used to provide the allocated IPv6 address. |
| ***iPv6-Prefix***This field is used to provide the allocated IPv6 prefix. |

– *IAB-IP-AddressIndex*

The IE *IAB-IP-AddressIndex* is used to identify a configuration of an IP address.

***IAB-IP-AddressIndex information element***

-- ASN1START

-- TAG-IAB-IP-ADDRESSINDEX-START

IAB-IP-AddressIndex-r16 ::= INTEGER (1..maxIAB-IP-Address-r16),

-- TAG-IAB-IP-ADDRESSINDEX-STOP

-- ASN1STOP

– *IAB-IP-Usage*

The IE *IAB-IP-Usage* is used to indicate the usage of the requested IP address/prefix.

***IAB-IP-Usage information element***

-- ASN1START

-- TAG-IAB-IP-USAGE-START

IAB-IP-Usage-r16 ::= ENUMERATED {f1-c, f1-U, non-F1, spare0}

-- TAG-IAB-IP-USAGE-STOP

-- ASN1STOP

**------------------------------------------------5st Change -----------------------------------------------------**

6.4 RRC multiplicity and type constraint values

– Multiplicity and type constraint definitions

-- ASN1START

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-START

ffsValue INTEGER ::= 65536 -- Placehold for all FFS values, to be removed

maxAI-DCI-PayloadSize-r16 INTEGER ::= 128 --Maximum size of the DCI payload scrambled with ai-RNTI

maxAI-DCI-PayloadSize-r16-1 INTEGER ::= 127 --Maximum size of the DCI payload scrambled with ai-RNTI minus 1

maxBandComb INTEGER ::= 65536 -- Maximum number of DL band combinations

maxBandsUTRA-FDD-r16 INTEGER ::= 64 -- Maximum number of bands listed in UTRA-FDD UE caps

maxBH-RLC-channelID INTEGER ::= 65536 -- Maximum value of BH RLC Channel ID

maxBT-IdReport-r16 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r16 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCBR-Config-r16 INTEGER ::= 8 -- Maximum number of CBR range configurations for sidelink communication

 -- congestion control

maxCBR-Config-1-r16 INTEGER ::= 7

maxCBR-Level-r16 INTEGER ::= 16 -- Maximum nuber of CBR levels

maxCBR-Level-1-r16 INTEGER ::= 15

maxCellBlack INTEGER ::= 16 -- Maximum number of NR blacklisted cell ranges in SIB3, SIB4

maxCellHistory-r16 INTEGER ::= 16 -- Maximum number of visited cells reported

maxCellInter INTEGER ::= 16 -- Maximum number of inter-Freq cells listed in SIB4

maxCellIntra INTEGER ::= 16 -- Maximum number of intra-Freq cells listed in SIB3

maxCellMeasEUTRA INTEGER ::= 32 -- Maximum number of cells in E-UTRAN

maxCellMeasIdle-r16 INTEGER ::= 65535 -- Maximum number of cells per carrier for idle/inactive measurements is FFS

maxCellMeasUTRA-FDD-r16 INTEGER ::= 32 -- Maximum number of cells in FDD UTRAN

maxCellWhite INTEGER ::= 16 -- Maximum number of NR whitelisted cell ranges in SIB3, SIB4

maxEARFCN INTEGER ::= 262143 -- Maximum value of E-UTRA carrier frequency

maxEUTRA-CellBlack INTEGER ::= 16 -- Maximum number of E-UTRA blacklisted physical cell identity ranges

 -- in SIB5

maxEUTRA-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxLogMeasReport-r16 INTEGER ::= 520 -- Maximum number of entries for logged measurements

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands that a cell belongs to

maxNARFCN INTEGER ::= 3279165 -- Maximum value of NR carrier frequency

maxNR-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFreqIdle-r16 INTEGER ::= 8 -- Maximum number of carrier frequencies for idle/inactive measurements

maxNrofServingCells INTEGER ::= 32 -- Max number of serving cells (SpCells + SCells)

maxNrofServingCells-1 INTEGER ::= 31 -- Max number of serving cells (SpCell + SCells) per cell group

maxNrofAggregatedCellsPerCellGroup INTEGER ::= 16

maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DU

maxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5

maxNrofAvailabilityCombinationsPerSet-r16-1 INTEGER ::= 511 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5 minus 1

maxNrofSCells INTEGER ::= 31 -- Max number of secondary serving cells per cell group

maxNrofCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the cell lists in a measurement

 -- object

maxNrofCG-SL-r16 INTEGER ::= 8 -- Max number of configured sidelink grant

maxNrofSS-BlocksToAverage INTEGER ::= 16 -- Max number for the (max) number of SS blocks to average to determine cell

 -- measurement

maxNrofCondCells-r16 INTEGER ::= 8 -- Max number of conditional candidate SpCells

maxNrofCSI-RS-ResourcesToAverage INTEGER ::= 16 -- Max number for the (max) number of CSI-RS to average to determine cell

 -- measurement

maxNrofDL-Allocations INTEGER ::= 16 -- Maximum number of PDSCH time domain resource allocations

maxNrofSR-ConfigPerCellGroup INTEGER ::= 8 -- Maximum number of SR configurations per cell group

maxLCG-ID INTEGER ::= 7 -- Maximum value of LCG ID

maxLC-ID INTEGER ::= 32 -- Maximum value of Logical Channel ID

maxLC-ID-Iab-r16 INTEGER ::= 65536 -- Maximum value of BH Logical Channel ID extension

maxLTE-CRS-Patterns-r16 INTEGER ::= 3 -- Maximum number of additional LTE CRS rate matching patterns

maxNrofTAGs INTEGER ::= 4 -- Maximum number of Timing Advance Groups

maxNrofTAGs-1 INTEGER ::= 3 -- Maximum number of Timing Advance Groups minus 1

maxNrofBWPs INTEGER ::= 4 -- Maximum number of BWPs per serving cell

maxNrofCombIDC INTEGER ::= 128 -- Maximum number of reported MR-DC combinations for IDC

maxNrofSymbols-1 INTEGER ::= 13 -- Maximum index identifying a symbol within a slot (14 symbols, indexed

 -- from 0..13)

maxNrofSlots INTEGER ::= 320 -- Maximum number of slots in a 10 ms period

maxNrofSlots-1 INTEGER ::= 319 -- Maximum number of slots in a 10 ms period minus 1

maxNrofPhysicalResourceBlocks INTEGER ::= 275 -- Maximum number of PRBs

maxNrofPhysicalResourceBlocks-1 INTEGER ::= 274 -- Maximum number of PRBs minus 1

maxNrofPhysicalResourceBlocksPlus1 INTEGER ::= 276 -- Maximum number of PRBs plus 1

maxNrofControlResourceSets-1 INTEGER ::= 11 -- Max number of CoReSets configurable on a serving cell minus 1

maxNrofControlResourceSets-1-r16 INTEGER ::= 15 -- Max number of CoReSets configurable on a serving cell extended in minus 1

maxNrofCoresetPools-r16 INTEGER ::= 2 -- Maximum number of CORESET pools

maxCoReSetDuration INTEGER ::= 3 -- Max number of OFDM symbols in a control resource set

maxNrofSearchSpaces-1 INTEGER ::= 39 -- Max number of Search Spaces minus 1

maxSFI-DCI-PayloadSize INTEGER ::= 128 -- Max number payload of a DCI scrambled with SFI-RNTI

maxSFI-DCI-PayloadSize-1 INTEGER ::= 127 -- Max number payload of a DCI scrambled with SFI-RNTI minus 1

maxIAB-IP-Address-r16 INTEGER ::= 32 -- Max number of assigned IP address

maxINT-DCI-PayloadSize INTEGER ::= 126 -- Max number payload of a DCI scrambled with INT-RNTI

maxINT-DCI-PayloadSize-1 INTEGER ::= 125 -- Max number payload of a DCI scrambled with INT-RNTI minus 1

maxNrofRateMatchPatterns INTEGER ::= 4 -- Max number of rate matching patterns that may be configured

maxNrofRateMatchPatterns-1 INTEGER ::= 3 -- Max number of rate matching patterns that may be configured minus 1

maxNrofRateMatchPatternsPerGroup INTEGER ::= 8 -- Max number of rate matching patterns that may be configured in one group

maxNrofCSI-ReportConfigurations INTEGER ::= 48 -- Maximum number of report configurations

maxNrofCSI-ReportConfigurations-1 INTEGER ::= 47 -- Maximum number of report configurations minus 1

maxNrofCSI-ResourceConfigurations INTEGER ::= 112 -- Maximum number of resource configurations

maxNrofCSI-ResourceConfigurations-1 INTEGER ::= 111 -- Maximum number of resource configurations minus 1

maxNrofAP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrOfCSI-AperiodicTriggers INTEGER ::= 128 -- Maximum number of triggers for aperiodic CSI reporting

maxNrofReportConfigPerAperiodicTrigger INTEGER ::= 16 -- Maximum number of report configurations per trigger state for aperiodic

 -- reporting

maxNrofNZP-CSI-RS-Resources INTEGER ::= 192 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources

maxNrofNZP-CSI-RS-Resources-1 INTEGER ::= 191 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources minus 1

maxNrofNZP-CSI-RS-ResourcesPerSet INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per resource set

maxNrofNZP-CSI-RS-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per cell

maxNrofNZP-CSI-RS-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resources per cell minus 1

maxNrofNZP-CSI-RS-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of resource sets per resource configuration

maxNrofNZP-CSI-RS-ResourcesPerConfig INTEGER ::= 128 -- Maximum number of resources per resource configuration

maxNrofZP-CSI-RS-Resources INTEGER ::= 32 -- Maximum number of Zero-Power (ZP) CSI-RS resources

maxNrofZP-CSI-RS-Resources-1 INTEGER ::= 31 -- Maximum number of Zero-Power (ZP) CSI-RS resources minus 1

maxNrofZP-CSI-RS-ResourceSets-1 INTEGER ::= 15

maxNrofZP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrofZP-CSI-RS-ResourceSets INTEGER ::= 16

maxNrofCSI-IM-Resources INTEGER ::= 32 -- Maximum number of CSI-IM resources. See CSI-IM-ResourceMax in 38.214.

maxNrofCSI-IM-Resources-1 INTEGER ::= 31 -- Maximum number of CSI-IM resources minus 1. See CSI-IM-ResourceMax

 -- in 38.214.

maxNrofCSI-IM-ResourcesPerSet INTEGER ::= 8 -- Maximum number of CSI-IM resources per set. See CSI-IM-ResourcePerSetMax

 -- in 38.214

maxNrofCSI-IM-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-IM resources per cell

maxNrofCSI-IM-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-IM resources per cell minus 1

maxNrofCSI-IM-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of CSI IM resource sets per resource configuration

maxNrofCSI-SSB-ResourcePerSet INTEGER ::= 64 -- Maximum number of SSB resources in a resource set

maxNrofCSI-SSB-ResourceSets INTEGER ::= 64 -- Maximum number of CSI SSB resource sets per cell

maxNrofCSI-SSB-ResourceSets-1 INTEGER ::= 63 -- Maximum number of CSI SSB resource sets per cell minus 1

maxNrofCSI-SSB-ResourceSetsPerConfig INTEGER ::= 1 -- Maximum number of CSI SSB resource sets per resource configuration

maxNrofFailureDetectionResources INTEGER ::= 10 -- Maximum number of failure detection resources

maxNrofFailureDetectionResources-1 INTEGER ::= 9 -- Maximum number of failure detection resources minus 1

maxNrofFreqSL-r16 INTEGER ::= 8 -- Maximum number of carrier frequncy for for NR sidelink communication

maxNrofSL-BWPs-r16 INTEGER ::= 4 -- Maximum number of BWP for for NR sidelink communication

maxFreqSL-EUTRA-r16 INTEGER ::= 8 -- Maximum number of EUTRA anchor carrier frequncy for NR sidelink

 -- communication

maxNrofSL-MeasId-r16 INTEGER ::= 84 -- Maximum number of sidelink measurement identity (RSRP)

maxNrofSL-ObjectId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement objects (RSRP)

maxNrofSL-ReportConfigId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement reporting configuration(RSRP)

maxNrofSL-PoolToMeasureEUTRA-r16 INTEGER ::= 8 -- Maximum number of resoure pool for V2X sidelink measurement to measure

 -- for each measurement object (for CBR)

maxNrofSL-PoolToMeasureNR-r16 INTEGER ::= 8 -- Maximum number of resoure pool for NR sidelink measurement to measure for

 -- each measurement object (for CBR)

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequncy for NR sidelink

 -- communication

maxNrofSL-QFIs-r16 INTEGER ::= 2048 -- Maximum number of QoS flow for NR sidelink communication per UE

maxNrofSL-QFIsPerDest-r16 INTEGER ::= 64 -- Maximum number of QoS flow per destination for NR sidelink communication

maxNrofObjectId INTEGER ::= 64 -- Maximum number of measurement objects

maxNrofPageRec INTEGER ::= 32 -- Maximum number of page records

maxNrofPCI-Ranges INTEGER ::= 8 -- Maximum number of PCI ranges

maxPLMN INTEGER ::= 12 -- Maximum number of PLMNs broadcast and reported by UE at establisghment

maxNrofCSI-RS-ResourcesRRM INTEGER ::= 96 -- Maximum number of CSI-RS resources for an RRM measurement object

maxNrofCSI-RS-ResourcesRRM-1 INTEGER ::= 95 -- Maximum number of CSI-RS resources for an RRM measurement object minus 1

maxNrofMeasId INTEGER ::= 64 -- Maximum number of configured measurements

maxNrofQuantityConfig INTEGER ::= 2 -- Maximum number of quantity configurations

maxNrofCSI-RS-CellsRRM INTEGER ::= 96 -- Maximum number of cells with CSI-RS resources for an RRM measurement

 -- object

maxNrofSL-Dest-r16 INTEGER ::= 32 -- Maximum number of destination for NR sidelink communication

maxNrofSL-Dest-1-r16 INTEGER ::= 31 -- Highest index of destination for NR sidelink communication

maxNrofSLRB-r16 INTEGER ::= 512 -- Maximum number of radio bearer for NR sidelink communication per UE

maxSL-LCID-r16 INTEGER ::= 512 -- Maximum number of RLC bearer for NR sidelink communication per UE

maxSL-SyncConfig-r16 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxNrofRXPool-r16 INTEGER ::= 16 -- Maximum number of Rx resource poolfor NR sidelink communication

maxNrofTXPool-r16 INTEGER ::= 8 -- Maximum number of Tx resourcepoolfor NR sidelink communication

maxNrofPoolID-r16 INTEGER ::= 16 -- Maximum index of resource pool for NR sidelink communication

maxNrofSRS-PathlossReferenceRS-r16-1 INTEGER ::= ffsValue --

maxNrofSRS-ResourceSets INTEGER ::= 16 -- Maximum number of SRS resource sets in a BWP.

maxNrofSRS-ResourceSets-1 INTEGER ::= 15 -- Maximum number of SRS resource sets in a BWP minus 1.

maxNrofSRS-PosResourceSets-r16 INTEGER ::= 16 -- Maximum number of SRS Positioning resource sets in a BWP.

maxNrofSRS-PosResourceSets-1-r16 INTEGER ::= 15 -- Maximum number of SRS Positioning resource sets in a BWP minus 1.

maxNrofSRS-Resources INTEGER ::= 64 -- Maximum number of SRS resources.

maxNrofSRS-Resources-1 INTEGER ::= 63 -- Maximum number of SRS resources in an SRS resource set minus 1.

maxNrofSRS-PosResources-r16 INTEGER ::= 64 -- Maximum number of SRS Positioning resources.

maxNrofSRS-PosResources-1-r16 INTEGER ::= 63 -- Maximum number of SRS Positioning resources in an SRS Positioning

 -- resource set minus 1.

maxNrofSRS-ResourcesPerSet INTEGER ::= 16 -- Maximum number of SRS resources in an SRS resource set

maxNrofSRS-TriggerStates-1 INTEGER ::= 3 -- Maximum number of SRS trigger states minus 1, i.e., the largest code

 -- point.

maxNrofSRS-TriggerStates-2 INTEGER ::= 2 -- Maximum number of SRS trigger states minus 2.

maxRAT-CapabilityContainers INTEGER ::= 8 -- Maximum number of interworking RAT containers (incl NR and MRDC)

maxSimultaneousBands INTEGER ::= 32 -- Maximum number of simultaneously aggregated bands

maxNrofSlotFormatCombinationsPerSet INTEGER ::= 512 -- Maximum number of Slot Format Combinations in a SF-Set.

maxNrofSlotFormatCombinationsPerSet-1 INTEGER ::= 511 -- Maximum number of Slot Format Combinations in a SF-Set minus 1.

maxNrofTrafficPattern-r16 INTEGER ::= 8 -- Maximum number of Traffic Pattern for NR sidelink communication.

maxNrofPUCCH-Resources INTEGER ::= 128

maxNrofPUCCH-Resources-1 INTEGER ::= 127

maxNrofPUCCH-ResourceSets INTEGER ::= 4 -- Maximum number of PUCCH Resource Sets

maxNrofPUCCH-ResourceSets-1 INTEGER ::= 3 -- Maximum number of PUCCH Resource Sets minus 1.

maxNrofPUCCH-ResourcesPerSet INTEGER ::= 32 -- Maximum number of PUCCH Resources per PUCCH-ResourceSet

maxNrofPUCCH-P0-PerSet INTEGER ::= 8 -- Maximum number of P0-pucch present in a p0-pucch set

maxNrofPUCCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUCCH power control.

maxNrofPUCCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUCCH power

 -- control minus 1.

maxNrofPUCCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1 extended.

maxNrofPUCCH-ResourceGroups-r16 INTEGER ::= 4 -- Maximum number of PUCCH resources groups.

maxNrofPUCCH-ResourcesPerGroup-r16 INTEGER ::= ffsValue -- Maximum number of PUCCH resources in a PUCCH group.

maxNrofPUCCH-ResourcesPerGroup-1-r16 INTEGER ::= ffsValue -- Maximum number of PUCCH resources in a PUCCH group minus 1.

maxNrofServingCells-r16 INTEGER ::= ffsValue -- Maximum number of serving cells in simultaneousTCI-UpdateList.

maxNrofP0-PUSCH-AlphaSets INTEGER ::= 30 -- Maximum number of P0-pusch-alpha-sets (see 38,213, clause 7.1)

maxNrofP0-PUSCH-AlphaSets-1 INTEGER ::= 29 -- Maximum number of P0-pusch-alpha-sets minus 1 (see 38,213, clause 7.1)

maxNrofPUSCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUSCH power control.

maxNrofPUSCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUSCH power

 -- control minus 1.

maxNrofPUSCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- extended

maxNrofPUSCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- minus 1

maxNrofNAICS-Entries INTEGER ::= 8 -- Maximum number of supported NAICS capability set

maxBands INTEGER ::= 1024 -- Maximum number of supported bands in UE capability.

maxBandsMRDC INTEGER ::= 1280

maxBandsEUTRA INTEGER ::= 256

maxCellReport INTEGER ::= 8

maxDRB INTEGER ::= 29 -- Maximum number of DRBs (that can be added in DRB-ToAddModLIst).

maxFreq INTEGER ::= 8 -- Max number of frequencies.

maxFreqIDC-r16 INTEGER ::= 128 -- Max number of frequencies for IDC indication.

maxCombIDC-r16 INTEGER ::= 128 -- Max number of reported UL CA for IDC indication.

maxFreqIDC-MRDC INTEGER ::= 32 -- Maximum number of candidate NR frequencies for MR-DC IDC indication

maxNrofCandidateBeams INTEGER ::= 16 -- Max number of PRACH-ResourceDedicatedBFR that in BFR config.

maxNrofCandidateBeams-r16 INTEGER ::= 64 -- Max number of candidate beam resources in BFR config.

maxNrofCandidateBeamsExt-r16 INTEGER ::= 9999 -- FFS

maxNrofPCIsPerSMTC INTEGER ::= 64 -- Maximun number of PCIs per SMTC.

maxNrofQFIs INTEGER ::= 64

maxNrofResourceAvailabilityPerCombination-r16 INTEGER ::= 256 -- FFS

maxNrOfSemiPersistentPUSCH-Triggers INTEGER ::= 64 -- Maximum number of triggers for semi persistent reporting on PUSCH

maxNrofSR-Resources INTEGER ::= 8 -- Maximum number of SR resources per BWP in a cell.

maxNrofSlotFormatsPerCombination INTEGER ::= 256

maxNrofSpatialRelationInfos INTEGER ::= 8

maxNrofSpatialRelationInfos-r16 INTEGER ::= 64

maxNrofIndexesToReport INTEGER ::= 32

maxNrofIndexesToReport2 INTEGER ::= 64

maxNrofSSBs-r16 INTEGER ::= 64 -- Maximum number of SSB resources in a resource set.

maxNrofSSBs-1 INTEGER ::= 63 -- Maximum number of SSB resources in a resource set minus 1.

maxNrofS-NSSAI INTEGER ::= 8 -- Maximum number of S-NSSAI.

maxNrofTCI-StatesPDCCH INTEGER ::= 64

maxNrofTCI-States INTEGER ::= 128 -- Maximum number of TCI states.

maxNrofTCI-States-1 INTEGER ::= 127 -- Maximum number of TCI states minus 1.

maxNrofUL-Allocations INTEGER ::= 16 -- Maximum number of PUSCH time domain resource allocations.

maxQFI INTEGER ::= 63

maxRA-CSIRS-Resources INTEGER ::= 96

maxRA-OccasionsPerCSIRS INTEGER ::= 64 -- Maximum number of RA occasions for one CSI-RS

maxRA-Occasions-1 INTEGER ::= 511 -- Maximum number of RA occasions in the system

maxRA-SSB-Resources INTEGER ::= 64

maxSCSs INTEGER ::= 5

maxSecondaryCellGroups INTEGER ::= 3

maxNrofServingCellsEUTRA INTEGER ::= 32

maxMBSFN-Allocations INTEGER ::= 8

maxNrofMultiBands INTEGER ::= 8

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxReportConfigId INTEGER ::= 64

maxNrofCodebooks INTEGER ::= 16 -- Maximum number of codebooks suppoted by the UE

maxNrofCSI-RS-Resources INTEGER ::= 7 -- Maximum number of codebook resources supported by the UE

maxNrofSRI-PUSCH-Mappings INTEGER ::= 16

maxNrofSRI-PUSCH-Mappings-1 INTEGER ::= 15

maxSIB INTEGER::= 32 -- Maximum number of SIBs

maxSI-Message INTEGER::= 32 -- Maximum number of SI messages

maxPO-perPF INTEGER ::= 4 -- Maximum number of paging occasion per paging frame

maxAccessCat-1 INTEGER ::= 63 -- Maximum number of Access Categories minus 1

maxBarringInfoSet INTEGER ::= 8 -- Maximum number of Access Categories

maxCellEUTRA INTEGER ::= 8 -- Maximum number of E-UTRA cells in SIB list

maxEUTRA-Carrier INTEGER ::= 8 -- Maximum number of E-UTRA carriers in SIB list

maxPLMNIdentities INTEGER ::= 8 -- Maximum number of PLMN identites in RAN area configurations

maxDownlinkFeatureSets INTEGER ::= 1024 -- (for NR DL) Total number of FeatureSets (size of the pool)

maxUplinkFeatureSets INTEGER ::= 1024 -- (for NR UL) Total number of FeatureSets (size of the pool)

maxEUTRA-DL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxEUTRA-UL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxFeatureSetsPerBand INTEGER ::= 128 -- (for NR) The number of feature sets associated with one band.

maxPerCC-FeatureSets INTEGER ::= 1024 -- (for NR) Total number of CC-specific FeatureSets (size of the pool)

maxFeatureSetCombinations INTEGER ::= 1024 -- (for MR-DC/NR)Total number of Feature set combinations (size of the

 -- pool)

maxInterRAT-RSTD-Freq INTEGER ::= 3

maxHRNN-Len-r16 INTEGER ::= ffsValue -- Maximum length of HRNNs, value is FFS

maxNPN-r16 INTEGER ::= 12 -- Maximum number of NPNs broadcast and reported by UE at establishment

maxNrOfMinSchedulingOffsetValues-r16 INTEGER ::= 2 -- Maximum number of min. scheduling offset (K0/K2) configurations

maxK0-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K2)

maxDCI-2-6-Size-r16 INTEGER ::= 140 -- Maximum size of DCI format 2-6

maxDCI-2-6-Size-1-r16 INTEGER ::= 139 -- Maximum DCI format 2-6 size minus 1

maxNrofUL-Allocations-r16 INTEGER ::= 64 -- Maximum number of PUSCH time domain resource allocations

maxNrofP0-PUSCH-Set-r16 INTEGER ::= 2 -- Maximum number of P0 PUSCH set(s)

maxCI-DCI-PayloadSize-r16 INTEGER ::= 126 -- Maximum number of the DCI size for CI

maxCI-DCI-PayloadSize-r16-1 INTEGER ::= 125 -- Maximum number of the DCI size for CI minus 1

maxWLAN-Id-Report-r16 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r16 INTEGER ::= 4 -- Maximum number of WLAN name

maxRAReport-r16 INTEGER ::= 8 -- Maximum number of RA procedures information to be included in the

 -- RA report

maxTxConfig-r16 INTEGER ::= 64

maxTxConfig-1-r16 INTEGER ::= 63

maxPSSCH-TxConfig-r16 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxNrofCLI-RSSI-Resources-r16 INTEGER ::= 64 -- Maximum number of CLI-RSSI resources for UE

maxNrofCLI-RSSI-Resources-r16-1 INTEGER ::= 63 -- Maximum number of CLI-RSSI resources for UE minus 1

maxNrofSRS-Resources-r16 INTEGER ::= 32 -- Maximum number of SRS resources for CLI measurement for UE

maxCLI-Report-r16 INTEGER ::= 8

maxNrofConfiguredGrantConfig-r16 INTEGER ::= 12 -- Maximum number of configured grant configurations per BWP

maxNrofConfiguredGrantConfig-r16-1 INTEGER ::= 11 -- Maximum number of configured grant configurations per BWP minus 1

maxNrofConfiguredGrantConfigMAC-r16 INTEGER ::= 32 -- Maximum number of configured grant configurations per MAC entity

maxNrofConfiguredGrantConfigMAC-r16-1 INTEGER ::= 31 -- Maximum number of configured grant configurations per MAC entity minus 1

maxNrofSPS-Config-r16 INTEGER ::= 8 -- Maximum number of SPS configurations per BWP

maxNrofSPS-Config-r16-1 INTEGER ::= 7 -- Maximum number of SPS configurations per BWP minus 1

maxNrofDormancyGroups INTEGER ::= 5 --

maxNrofPUCCH-ResourceGroups-1-r16 INTEGER ::= 3 --

maxNrofServingCellsTCI-r16 INTEGER ::= ffsValue --

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-STOP

-- ASN1STOP