3GPP TSG-RAN WG2 Meeting #110-e draftR2-2005926

Online, 1st – 12th June 2020

**Agenda item: 7.2.5**

**Source: Huawei (offline email discussion rapporteur)**

**Title: Report of [AT110-e][306][NBIOT] R16 RAN1 features list and UE capabilities (Huawei)**

**Document for: Report**

# 1 Introduction

This document is the report of the following e-mail discussion:

* [AT110-e][306][NBIOT] R16 RAN1 features list and UE capabilities (Huawei)

Status: Not Started.

Scope: [R2-2005030](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005030.zip).

Intended outcome: Report in R2-2005926

Deadline: June 5 1000 UTC

The discussion is based on the proposals in [2].

# 2 Discussion

## 2.1 Assistance information for inter-RAT cell selection to/from NB-IoT

**Proposal S1-1:** There is no need to introduce an optional feature for support of assistance information for inter-RAT cell selection to/from NB-IoT in TS 36.306

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.2 AS RAI enhancement for UE connected to 5GC

**Proposal S2-1:** *rai-Support-r14* applies to both EPC and 5GC without EPC/5GC differentiation.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S2-2:** Introduce an optional feature for support of AS RAI enhancement for UE connected to 5GC in TS 36.306.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.3 Group Wake Up signal

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Index | Feature group | Components | Prerequisite feature groups | Need of FDD/TDD differentiation | Note | Mandatory/Optional |
| 2-1 | UE-group wake-up signal (Group WUS) with a wake-up time before the first associated PO (without group resource alternation) |  | Rel-15 NWUS | FDD only |  | Optional with capability signalling |
| 2-2 | UE-group WUS with a wake-up time before the first associated PO (with group resource alternation) |  | 2-1 | FDD only | If UE does not support group resource alternation and the eNB enables group resource alternation, UE falls back to Rel-15 NWUS when Rel-15 NWUS is configured or no NWUS when Rel-15 NWUS is not configured. | Optional with capability signalling |

**Proposal S3-1:** For NB-IoT and eMTC, clarify in TS 36.331 and TS 36.306 that the capability *groupWakeUpSignal-r16* corresponds to GWUS without group alternation.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S3-2:** For NB-IoT and eMTC, introduce a new capability *groupWakeUpSignalAlternation-r16* corresponding to GWUS with group alternation, conditional to support of *groupWakeUpSignal-r16*.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S3-3:** For eMTC, introduce a new capability *groupWakeUpSignalAlternationTDD-r16* corresponding to GWUS with group alternation, conditional to support of *groupWakeUpSignalTDD-r16*.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S3-4:** Update TS 36.304 to specify that if the UE does not support GWUS with group alternation and the eNB enables group alternation, then the UE does not use GWUS.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.4 PUR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Index | Feature group | Components | Prerequisite feature groups | Need of FDD/TDD differentiation | Note | Mandatory/Optional |
| 2-3 | Transmission in preconfigured UL resources (PUR)  (with potential UE-specific cyclic shift for DMRS) |  |  | FDD only | RAN2 has agreed that PUR with UP and CP solutions have separate indications, but this is not captured in this RAN1 UE feature list. | Optional with capability signalling |
| 2-4 | PUR with serving cell RSRP for TA validation |  | 2-3 | FDD only | RAN2 has agreed that PUR with UP and CP solutions have separate indications, but this is not captured in this RAN1 UE feature list.  TA validation mechanisms based on ‘Serving cell changes’, ‘TA timer for idle mode’ and ‘TA always valid’ are mandatory for PUR UEs. | Optional with capability signalling |
| 2-5 | PUR with L1 ACK |  | 2-3 | FDD only | RAN2 has agreed that PUR with UP and CP solutions have separate indications, but this is not captured in this RAN1 UE feature list. | Optional with capability signalling |

**Proposal S4-1:** For NB-IoT and eMTC, introduce a new general capability *pur-RSRP-Validation-r16*, conditional to support of *pur-CP-EPC-r16* and/or *pur-CP-5GC-r16* and/or *pur-UP-EPC-r16* and/or *pur-UP-EPC-r16.*

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S4-2:** For NB-IoT and eMTC, introduce a new physical layer capability *pur-CP-L1Ack-r16*, conditional to support of *pur-CP-EPC-r16* and/or *pur-CP-5GC-r16*.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.5 MultiTB scheduling

| Index | Feature group | Components | Prerequisite feature groups | Need of FDD/TDD differentiation | Note | Mandatory/Optional |
| --- | --- | --- | --- | --- | --- | --- |
| 2-6 | Multi-TB scheduling for unicast in DL with a single DCI  (Interleaved transmission) |  | Two HARQ processes | FDD only |  | Optional with capability signalling |
| 2-7 | Multi-TB scheduling for unicast in DL with a single DCI (Non-interleaved transmission) |  | Two HARQ processes | FDD only |  | Optional with capability signalling |
| 2-8 | Multi-TB scheduling for unicast in UL with a single DCI  (Interleaved transmission) |  | Two HARQ processes | FDD only |  | Optional with capability signalling |
| 2-9 | Multi-TB scheduling for unicast in UL with a single DCI  (Non-interleaved transmission) |  | Two HARQ processes | FDD only |  | Optional with capability signalling |
| 2-10 | Multi-TB scheduling for unicast in DL in a single DCI  (HARQ bundling for HARQ-ACK feedback to interleaved transmission) |  | 2-6 | FDD only |  | Optional with capability signalling |

**Proposal S5-1:** For NB-IoT, remove the conditions in TS 36.331 and TS 36.306 that a UE that supports *multiTB-DL-Interleaving-r16* (*multiTB-UL-Interleaving-r16)* shall also support general *multiTB-DL-r16* (*multiTB-UL-r16).*

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.6 Resource reservation for NR

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Index | Feature group | Components | Prerequisite feature groups | Need of FDD/TDD differentiation | Note | Mandatory/Optional |
| 2-12 | DL resource reservation with subframe-level granularity of NB-IoT non-anchor carriers. |  |  | FDD only |  | Optional with capability signalling |
| 2-12a | DL resource reservation with slot-level and symbol-level granularity of NB-IoT non-anchor carriers. |  | 2-12 | FDD only |  | Optional with capability signalling |
| 2-13 | UL resource reservation with subframe-level granularity of NB-IoT non-anchor carriers. |  |  | FDD only |  | Optional with capability signalling |
| 2-13a | UL resource reservation with slot-level and symbol(s)-level granularity of NB-IoT non-anchor carriers. |  | 2-13 | FDD only |  | Optional with capability signalling |

**Proposal S6-1:** Rename the two already defined capabilities to *ul-ResourceReservationSubframeLevel-r16* and *dl-ResourceReservationSubframeLevel-r16*.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S6-2:** Introduce two new physical layer capabilities *ul-ResourceReservationSlotLevel-r16* and *dl-ResourceReservationSlotLevel-r16*, conditional to support of resource reservation with subframe level granularity.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

## 2.7 NRS presence on non-anchor carrier

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Index | Feature group | Components | Prerequisite feature groups | Need of FDD/TDD differentiation | Note | Mandatory/Optional |
| 2-16 | NRS on a non-anchor carrier for paging | 1. Presence of NRS on a set of subframes on a non-anchor carrier when no paging NPDCCH is transmitted | Paging non-anchor carrier | FDD only |  | Optional without capability signalling |

**Proposal S7-1:** Introduce a new optional feature “NRS presence on non-anchor paging carriers” in TS 36.306.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

**Proposal S7-2:** Clarify in the description of the already agreed optional feature “RRM measurements on non-anchor paging carriers” that it is dependent on support of ‘NRS presence on non-anchor paging carriers”.

**Company views**

|  |  |  |
| --- | --- | --- |
| **Company** | **do you agree**  **(yes/no)** | **Comments** |
|  |  |  |
|  |  |  |

Conclusion:

Proposal:

# 3 Summary

**Conclusions:**

**Potential easy agreements**

To be completed

**For further discussion**

To be completed

# 4 List of referenced documents

1. [R2-2005080](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005080.zip) Updates for Rel-16 additional enhancements NB-IoT BlackBerry UK Limited CR Rel-16 36.306 16.0.0 1746 - C NB\_IOTenh3-Core

1. [R2-2005030](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_110-e/Docs/R2-2005030.zip" \o "https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_109bis-e/Docs/R2-2003248.zip) RAN1 features list and UE capabilities issues Huawei, HiSilicon discussion Rel-16 NB\_IOTenh3-Core