**3GPP TSG-RAN WG2 Meeting #110-e *draft-*R2-2005825**

**Online, June 1st – June 12 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.304** | **CR** | **0789** | **rev** | **1** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Corrections to WUS group for eMTC |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | LTE\_eMTC5-Core |  |  | 2020-05-12 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | To capture the remaining RAN2 agreements related to GWUS monitoring |
|  |  |
| ***Summary of change:*** | New section for WUS Resource identification for BL UE and UE in enhanced coverage. |
|  |  |
| ***Consequences if not approved:*** | Rel-16 eMTC enhancements for GWUS will not be complete. |
|  |  |
| ***Clauses affected:*** | 7.5.1, 7.5.x(new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.331 CR 4239 |
| ***affected:*** | **X** |  |  Test specifications | TS 36.300 CR 1277 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |   |

First Change

## 7.5 Paging with Group Wake Up Signal

### 7.5.1 General

When the UE supports GWUS and GWUS configuration (*gwus-Config*) is provided in system information, the UE shall monitor GWUS using the GWUS parameters provided in System Information.

A UE supporting GWUS can be configured to monitor a WUS Group and a common WUS. Upon detecting either of them UE shall monitor POs as defined in clause 7.4.

For NB-IoT, E-UTRAN may configure up to 2 WUS resources (numbered 0 and 1). The time offset, *g*0, from the end of WUS resource 0 to the start of corresponding PO is determined as defined in subclause 7.4. When both *wus-Config* and g*wus-Config* are present, WUS resource 0 shares radio resources with *wus-Config.*The time offset from the end of WUS resource 1 to the start of corresponding PO is sum of the time offset *g*0 and the maximum WUS duration.

For BL UEs and UEs in enhanced coverage, E-UTRAN may configure up to 4 WUS resources. The resource number, time and frequency location of these resources is determined as specified in subclause 7.5.x

Next change

### 7.5.x WUS Resource Location for BL UEs and UEs in Enhanced coverage

A BL UE or UE in enhanced coverage determines the time/frequency location of WUS resources based on the number of configured WUS resources and the frequency location of WUS Resource 0 (. If *wus-Config* is present, frequency location for WUS Resource 0 is defined by *frequencyLocation* parameter in *wus-Config*. Otherwise, frequency location for WUS Resource 0 is defined by *resourceLocationWithoutWUS* in *gwus-Config*. The frequency location of other WUS Resources (Resource ID 1,2,3), based on frequency location of of WUS Resource 0, is given in Table 7.5.x-1.

Table 7.5.x-1: WUS Resource frequency location

|  |  |
| --- | --- |
| ***WUS Resource******()*** | ***Frequency location of WUS Resource ID 0*** |
| ***n0*** | ***n2***  | ***n4 (Note 1)*** |
| ***NB frequency < centre frequency*** | ***NB frequency > centre frequency***  |
| WUS Resource 1,3 | n2 | n4 | n0 | n2 |
| WUS Resource 2 | n0 | n2 | n2 | n4 |
| WUS Resource 2(Note 2) | n4 | n4 | n0 | n0 |
| Note 1: This column is applicable if wus-Config is present.Note 2: This row is applicable if resourceLocationWIthWUS is primary3FDM |

The time offset, *g*0, from the end of WUS resource 0 and WUS resource 1 to the start of corresponding PO is determined as defined in subclause 7.4. The time offset from the end of WUS resource 2 and WUS resource 3 to the start of corresponding PO is sum of the time offset *g*0 and the maximum WUS duration for all value of resourceLocation in resourcePattern except primary3FDM . The time offset, *g*0, for WUS resource 2 is same as WUS resource 0 and 1 if *resourceLocationWIthWUS* is set to *primary3FDM*.

 ID (rp-ID) and the configured number of WUS resources as follows:

If *resourceLocationWithWUS* is configured

rp-ID = 2\*(maxWR – 1) if *resourceLocationWithWUS* is set to *primary*

rp-ID= 2\*maxWR - 1 if *resourceLocationWithWUS* is set to *secondary*

rp-ID=7 if *resourceLocationWithWUS* is set to *primary3FDM*.

If *resourceLocationWithoutWUS* is configured

rp-ID = 2\*(maxWR-1)

where maxWR is *maxWR* is the total number of WUS resources configured in *numGroupsList* for the gap.

corresponding to the resource pattern ID determineddefined

Table 7.5.x-2: WUS Resources applicable for Resource Pattern

|  |  |
| --- | --- |
|  | **Resource Pattern\_ID** |
| ***0*** | ***1*** | ***2*** | ***3*** | ***4*** | ***5*** | ***6*** | ***7*** |
| **WUS Resource*****()*** | ***0*** | X |  | X |  | X |  | X | X |
| ***1*** |  | X | X | X | X | X | X | X |
| ***2*** |  |  |  | X | X | X | X | X |
| ***3*** |  |  |  |  |  | X | X |  |

If = 0 is not used, the first entry in the *numGroupsList* corresponds to = 1. Otherwise, is the index of the WUS resources in *numGroupsList*.

End of Changes