3GPP TSG-RAN WG2 #110-e DRAFT R2-2005830

Electronic Meeting, June 1-12, 2020

Agenda Item: 7.1.6

Source: Qualcomm

Title: [AT110-e][410][eMTC] ASN.1 review for eMTC (Phase 2)

Document for: Discussion, Decision

# 1 Introduction

This document is the report of the following email discussion:

* [AT110-e][410][eMTC] R16 ASN.1 Review (Qualcomm)

Scope: Remaining RIL issues (TBD)

Intended outcome: Report in R2-2005830

Deadline: Friday, June 5th 10:00 UTC

This document summarizes the discussion on LTE ASN.1 issues specific to Rel-16 eMTC from phase 2 RILs in v65. (See R2-200xx ASN.1 review file and/or R2-200xx spreadsheet of RILs.)

# 2 Discussion

As a starting point, following tables are populated with the RILs (from phase 2 only).

## 2.1 RIL issues not for discussion unless flagged

The following table shows the RILS with the status from RRC/spec rapporteur currently set to PropAgree, PropReject, and PropNoAct. They are intended to be agreed in block unless they are flagged via email or by comment in this document, in which case they will move to the discussion section.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ID** | **Work Item** | **Class** | **TDoc** | **Status** | **Proposed Conclusion** | **Description** | **Proposed Change** | **Comments**  **Companies are requested to input their views on this column** | **Proposed conclusion (from email discussion)**  **Column to be used by email rapporteur.** |
| E904 | eMTC/NB-IoT | 4 | None | PropAgree | v54: Change to Class 4. Ghange as suggested | Not sure why there is a reference to TS 36.321 in field description of newUE-Identity (also in other places, -NB versions)? There is no special handling captured in TS 36.321 for this case, it is a normal C-RNTI used in RRC\_CONNECTED. | Remove references to TS 36.321 from newUE-Identity-r16 field descriptions here and in other locations. | Huawei: v54: this also applies to NB-IoT and should be class 4 | [rapp]: captured in eMTC RRC CR v0. |
| B100 | LTE\_eMTC5-Core, NB\_IOTenh3-Core | 2 | None | PropAgree | v50: As suggested | E134 for 38.331 was agreed, i.e. to use non-critical extension on message level (in this case in the extension addition group in SIB4) and introduce “parallel list” with the new field. Reason: extension of list elements in SIB should not use “…” as it costs pprox.. 3 bytes per list element. The same should be adopted here for rss-MeasPowerBias-r16 as well. | Introduce rss-MeasPowerBias-r16 by a parallel list as shown below. |  | [rapp]: captured in eMTC RRC CR v0. |
| H814 | eMTC | 2 | None | PropAgree | v54, as suggested | why e2?. this represents a number should be n2, n4… |  | Qualcomm v33: The values were inspired from SPS, similar to the field name was inspired from SPS: implicitReleaseAfter ENUMERATED {e2, e3, e4, e8}. Qualcomm v46: Also it was exactly as your proposed change in H113. But ok to change to nX, nY | [rapp]: captured in eMTC RRC CR v0. |
| H822 | eMTC | 4 | None | PropAgree | v54. Changed to class 4. as suggested and/or (aslo NB-IoT) | RAN2#108 agreed that for NB-IoT and eMTC, the existing capability wakeUpSignalMinGap-eDRX-r15 also applies to Rel-16 WUS. | The UE shall also indicate support of WUS or GWUS for paging | Qualcomm v39: Agree. We assume “or” above means “and/or” | [rapp]: captured in eMTC RRC CR v0. |
| H849 | eMTC | 3 | None | PropAgree | v54: as suggested | RRC connection re-establishment also applies to the Control Plane CIoT 5GS optimisation. | Change to EPS/5GS | Qualcomm v39: Agree. But this could be a simple editorial fix in RRC CR discussion. | [rapp]: captured in eMTC RRC CR v0. |

## 2.2 RIL issues for discussion

Following table shows the RILs to be discussed in eMTC ASN.1 review. Companies are requested to add their comments in the “Comments” column.

NOTE 1: Keep in mind the current “status” and “proposed conclusion” column while providing your comment, i.e., comments should take these as baseline conclusion, where available.

NOTE 2: If you are unable to see the whole table, change the display to “draft” or “web layout” from “view” menu option.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ID** | **Work Item** | **Class** | **TDoc** | **Status** | **Proposed Conclusion** | **Description** | **Proposed Change** | **Comments**  **Companies are requested to input their views on this column** | **Proposed conclusion (from email discussion)**  **Column to be used by email rapporteur.** |
| Q605 | eMTC | 3 | R2-2004627 /R2-2004634 | DiscMeet | v55: discuss in meeting whether Rel-15 CR is agreeable. | WI open issue. RAN2 has agreed “Early implementation of relaxed serving cell measurement by Rel-15 UEs when configured with WUS is permitted. FFS whether to agree in TEI15.” | Introduce this field from Rel-15 (add as wus-Config-v15xy in rel-15 AEG with a rel-15 CR, mirror in rel-16, and remove from current AEG). CRs will be submitted as indicated in [Tdoc]. | Qualcomm v55: proposal is to agree Rel-15 CR and merge Rel16 draftCR to eMTC RRC CR. |  |
| Q607 | eMTC | 3 | None | DiscMeet | v61: discuss with other eMTC-specific ASN.1 issues | This is signalling of upto 29 bits. Networks may want to reserve whole frequency range corresponding to certain time resources given by periodicityStartPost. To reduce overhead, it is better to make it optional and specify “if absent, whole frequency range is reserved”. | Make resourceReservationFreq optional and clarify “if absent, whole frequency range is reserved”. |  |  |
| H817 | eMTC | 4 | None | DiscMeet | v54: To be discussed with other remaining capability issues | WI Open issue: TS 36.306: Editor’s note: In RRC the 4 PUR capabilities are part of MAC parameters for eMTC, but are part of general parameters for NB-IoT. Need to align one way or another. |  |  |  |
| H818 | eMTC | 3 | None | DiscMail | v55: discuss in context of eMTC RRC CR | The six capabilities agreed at RAN2#109e for coexistence with NR are missing. |  |  |  |
| H820 | eMTC | 4 | None | DiscMeet | v54: To be discussed with other remaining capability issues. | WI Open issue: TS 36.306: Editor's note: Field names need to be aligned across TS 36.331 and TS 36.306. See Also NB-IoT (RIL#852) |  |  |  |
| H821 | eMTC | 4 | None | DiscMeet | v54: To be discussed with other remaining capability issues | RAN2#108 agreed that Rel-15 WUS and Rel-16 Group WUS are not supported for eMTC UEs in RRC\_INACTIVE. | Clarify in the field description. Clarification is TS 36.304 also needed. |  |  |

## 2.3 RIL issues for discussion in NB-IoT ASN.1 review (for information only)

Following issues are common to NB-IoT and eMTC and will be discussed in NB-IoT ASN.1 review.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ID** | **Work Item** | **Class** | **TDoc** | **Status** | **Proposed Conclusion** | **Description** | **Proposed Change** | **Comments** | **N/A** |
| E906 | eMTC/NBIoT | 4 | None | DiscMeet | v54: Changed to class 4. To be discussed in WI session with other PUR open issues. | Is it clear what configuration will be provided at this step, compared to storing pur-Config? E.g., MAC layer would need to be provided with PUR-RNTI here, the current MAC CR says RNTI is released after PUR occasion. Also some information related to the exact next PUR occasion should be provided. Or is it implicitly assumed these are the configuration provided? | Suggest to be more explicit here, i.e. reference to PUR-RNTI, PUR occasion. To be further discussed in WI, open issues Tdoc will be submitted including further discussion. | Qualcommv46: Agree some discussion and resolution is needed. For example, latest MAC spec CR says: “- when pur-TimeAlignmentTimer configuration is received from upper layers: - start or restart the pur-TimeAlignmentTimer.” Does this mean every PUR occasion the pur TAT restarts? (Given these and some other E90x RILs are joint issues, should class be changed to 4?) Huawei: v54: also think should be class 4 |  |
| E907 | eMTC/NBIoT | 4 | None | DiscMeet | v54: Change to class 4. To be discussed in WI session with other PUR open issues. | For CP solution same as for UP solution, should we be more explicit? See E906 | See E906 | Qualcomm v46: same comment as E906. |  |
| H811 | eMTC | 4 | None | DiscMeet | v54: to be discussed in WI session with other PUR open issues | WI Open issue: For the requested PUR TBS in eMTC and NB-IoT, the minimum value is b328.FFS: other details. Also NB-IoT (RIL#841) |  |  |  |
| H815 | eMTC | 3 | None | DiscMail | v54: To be discussed with other remaining ASN.1 issues | It is not clear what an empty PUR occasion is. Propose to align with NB-IoT ‘Number of consecutive PUR occasions that can be skipped before implicit release of PUR configuration’ |  |  |  |
| H823 | NBIoT/eMTC | 4 | None | DiscMail | v54: To be discussed with other remaining ASN.1 issues | It is not specified which parameters are used in that case. Also NB-IoT (RIL#859) | Clarify in the field description that if the field is absent, the parameters in wus-Config apply |  |  |
| H859 | NBIoT/eMTC | 4 | None | DiscMail | v54: To be discussed with other remaining ASN.1 issues | It is not specified which parameters are used in that case. Also eMTC (RIL#823) | Clarify in the field description that if the field is absent, the parameters in wus-Config apply |  |  |
| H810 | eMTC | 4 | None | DiscMeet | v54: To be discussed in WI session with other PUR open issues | WI Open issue: FFS: 2-level offset need and details for pur-StartTime-r16. Also NB-IoT (RIL#840) |  |  |  |

# Conclusion

In the previous sections we made the following observations:

Based on the discussion in the previous sections following is proposed:

# References

[1] R2-200xx ASN.1 review file, v65

[2] R2-200xx Spreadsheet containing RILs vXX