**3GPP TSG-RAN2 Meeting # 110-e *R2-200xxxx***

**Electronic meeting, June 1st –12th, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.305** | **CR** | **0024** | **rev** | **1** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update B1I signal ICD file to v3.0 in BDS system in A-GNSS |
|  |  |
| ***Source to WG:*** | CATT, CAICT, Huawei, ZTE Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI16 |  | ***Date:*** | 2020-6-2 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Update B1I signal ICD file from v2.0 to v3.0 in the network-assisted BDS System, as part of A-GNSS positioning methods in LTE and NR. The modification of B1I ICD, BDS-SIS-ICD-B1I-3.0 includes:- an increase in the number of satellite vehicles supported, - Identification of Expanded BDS Integrity and differential correction information (BDEpID)- the No. of some tables and sections are changed which are the editor modification. |
|  |  |
| ***Summary of change:*** | 1. ICD specification of B1I signal in BDS is updated to v3.0 in section 2 as reference.
 |
|  |  |
| ***Consequences if not approved:*** | The assistance data of B1I signal in A-BDS won’t support the SV-ID larger than 37, but the real satellite system already supports SV-ID more than 37 in B1I signal. |
|  |  |
| ***Clauses affected:*** | 2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS37.355 CR0259TS36.305 CR0088 |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **Start of change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501 "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 22.071: "Location Services (LCS); Service description, Stage 1".

[4] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[5] IS-GPS-200, Revision D, Navstar GPS Space Segment/Navigation User Interfaces, March 7th, 2006.

[6] IS-GPS-705, Navstar GPS Space Segment/User Segment L5 Interfaces, September 22, 2005.

[7] IS-GPS-800, Navstar GPS Space Segment/User Segment L1C Interfaces, September 4, 2008.

[8] Galileo OS Signal in Space ICD (OS SIS ICD), Draft 0, Galileo Joint Undertaking, May 23rd, 2006.

[9] Global Navigation Satellite System GLONASS Interface Control Document, Version 5, 2002.

[10] IS-QZSS, Quasi Zenith Satellite System Navigation Service Interface Specifications for QZSS, Ver.1.0, June 17, 2008.

[11] Specification for the Wide Area Augmentation System (WAAS), US Department of Transportation, Federal Aviation Administration, DTFA01-96-C-00025, 2001.

[12] RTCM 10402.3, RTCM Recommended Standards for Differential GNSS Service (v.2.3), August 20, 2001.

[13] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[14] 3GPP TS 38.331: "NR Radio Resource Control (RRC) protocol specification".

[15] OMA-AD-SUPL-V2\_0: "Secure User Plane Location Architecture Approved Version 2.0".

[16] OMA-TS-ULP-V2\_0\_4: "UserPlane Location Protocol Approved Version 2.0.4".

[17] 3GPP TS 36.214: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer – Measurements".

[18] 3GPP TS 36.302: "Evolved Universal Terrestrial Radio Access (E-UTRA); Services provided by the physical layer".

[19] 3GPP TS 36.355: "Evolved Universal Terrestrial Radio Access (E-UTRA); LTE Positioning Protocol (LPP)"

[20] BDS-SIS-ICD-B1I-3.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B1I (Version 3.0)", February, 2019.

[21] IEEE 802.11: "Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications"

[22] Bluetooth Special Interest Group: "Bluetooth Core Specification v4.2", December 2014.

[23] ATIS-0500027: "Recommendations for Establishing Wide Scale Indoor Location Performance", May 2015.

[24] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical channels and modulation".

[25] 3GPP TS 36.305: "Stage 2 functional specification of User Equipment (UE) positioning in E‑UTRA".

[26] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[27] 3GPP TS 38.455: "NG-RAN; NR Positioning Protocol A (NRPPa)".

[28] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[29] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[30] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[31] RTCM 10403.3, "RTCM Recommended Standards for Differential GNSS Services (v.3.3)", October 7, 2016.

[32] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[33] 3GPP TS 29.572: "Location Management Services; Stage 3".

[34] BDS-SIS-ICD-B1C-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B1C (Version 1.0)", December, 2017

[35] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[36] IS-QZSS-L6-001, Quasi-Zenith Satellite System Interface Specification – Centimetre Level Augmentation Service, Cabinet Office, November 5, 2018.

[37] 3GPP TS 38.215: "NR; Physical layer – Measurements".

[38] 3GPP TS 38.401: "3rd Generation Partnership Project; Technical Specification Group Radio Access Network; NG-RAN; Architecture description".

|  |
| --- |
| **The end** |