**3GPP TSG-RAN2 Meeting # 110bis electronic  *R2-2005954***

**1 June - 12 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.306** | **CR** | **Draft-CR** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR on PC5 capability on PC5-RRC and Uu-RRC (focusing on RAN1/RAN4 capability) |
|  |  |
| ***Source to WG:*** | OPPO |
| ***Source to TSG:*** | RAN2 |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core |  | ***Date:*** | 2020-6-2 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In RAN2#109-E, the following agreements were reachedAgreements on UE capabilities: 1: In Uu-RRC, capture SL per-band capability as a sidelink band list within RF-parameters in UE-NR-Capability (pending final RAN1 conclusion on L1 feature list).2: In Uu-RRC, introduce supported LTE / NR PC5 band combination(s) for each NR Uu band combination by referring to a list of PC6 band combinations.3: In Uu-RRC, when rat-Type=nr, UE reports NR-PC5 capability for NR standalone / NR-DC controlled NR-PC5 via UE-NR-Capability.4: In Uu-RRC, introduce supported NR PC5 band combination(s) for each LTE Uu band combination.5: For PC5-RRC, include frequencyBandListFilter in UECapabilityEnquirySidelink to indicate the requested frequency band of sidelink capability report on PC5-RRC. RAN2 to confirm that rat-Type in not included in UECapabilityEnquirySidelink.In RAN2#109bis-E, the following agreements were reachedAgreements on capabilities: 1: For LTE-Uu controlling NR-PC5, define the NR PC5 band combination in UE-EUTRA-Capability.2: For NR-Uu controlling LTE-PC5, define the NR PC5 band combination in UE-NR-Capability.3: Working assumption: The band combination of mixed LTE-PC5 and NR-PC5 will be reported, in addition to pure LTE-PC5 band combination and NR-PC5 band combination.4: RRC\_CONNECTED UE reports the received SL capability via PC5-RRC to network.5: RAN2 not pursue UE reporting the SL capability to network for network to transfer the SL capability to the counterpart UE.6: For layer-2 buffer size, leave the decision of maximum data rate discussion to RAN1, and only focus on RTT in RAN2.7: Disallow autonomous update of UE capability on PC5.8: For SL capability report on Uu-RRC, introduce MAC parameters: a) LCP restriction, b) Logical channel SR-delay timer, c) Multiple CGs.9: For SL capability report on PC5-RRC, introduce PDCP parameter: a) Out of order delivery.In RAN2#110-E, the following agreements are reached:Agreements on UE capabilities: 1a: For SL capability report on Uu-RRC, introduce RLC parameters: a) 12-bit SN length for UM, b) 18-bit SN for AM, and MAC parameter: multiple SR configuration. 1b: RRC specification will update SRB0, i.e. to 6bits.2: RAN2 will wait for RAN1 decision on the capability of range-based HARQ feedback.3: For SL capability report on Uu-RRC agreed in RAN2, they are per-UE capability.4: For SL capability report on Uu-RRC agreed in RAN2, allow FDD/TDD differentiation only for a) Logical channel SR-delay timer, and c) multiple SR configuration.5: For SL capability report on Uu-RRC agreed in RAN2, no need for FR1/FR2 differentiation.6: For SL capability report on Uu-RRC agreed in RAN2, conditionally (i.e., if UE supports NR sidelink) mandatory feature without capability signalling includes PDCP parameters: 1) 12-bit SN, 2) 18-bit SN, and RLC parameter: 1) 6-bit SN for UM, 2) 12-bit SN for AM. 18-bit PDCP SN can be revisited after PDCP discussion (if required).7: For SL capability report on Uu-RRC agreed in RAN2, optional feature with capability signaling includes RLC parameter: 1) 12-bit SN for UM, 2) 18-bit SN for AM; and MAC parameter: 1) LCP restriction, 2) Logical channel SR-delay timer, 3) Multiple CGs, 4) multiple SR configuration.8: For SL capability report on PC5-RRC, introduce RLC parameters: a) 12-bit SN length for UM, b) 18-bit SN for AM.9: For SL capability report on PC5-RRC agreed in RAN2, they are per-UE capability.10: For SL capability report on PC5-RRC agreed in RAN2, no need for either FDD/TDD or FR1/FR2 differentiation.11: For SL capability report on PC5-RRC agreed in RAN2, conditionally (i.e., if UE supports NR sidelink) mandatory feature without capability signalling includes PDCP parameters: 1) 12-bit SN, 2) 18-bit SN, and RLC parameter: 1) 6-bit SN for UM, 2) 12-bit SN for AM. 18-bit PDCP SN can be revisited after PDCP discussion (if required).12: For SL capability report on PC5-RRC agreed in RAN2, optional feature with capability signaling includes PDCP parameter: out-of-order delivery, RLC parameter: 1) 12-bit SN for UM, 2) 18-bit SN for AM.13: Maximum number of destinations is not considered in the definition of layer-2 buffer size.14: RRC\_CONNECTED UE reports the received SL capability (carrying RX UE capability received via UECapabilityInformationSidelink) via PC5-RRC to network using a container within SidelinkUEInformationNR message.15: RAN2 not pursue the timer to handle the failure case of UE capability transfer via sidelink.16: RAN2 not purse signaling overhead optimization for capability transfer procedure for TX-UE forwarding peer-UE SL capability to network via Uu-RRC.17: RAN2 not pursue signalling overhead optimization for capability transfer procedure via PC5-RRC. |
|  |  |
| ***Summary of change:*** | 1. Capture the RAN1/4 capability for Sidelink in 4.2.X.5;
2. Clarify the sidelink capability in A.Y
 |
|  |  |
| ***Consequences if not approved:*** | UE capability transfer via Uu-RRC and PC5-RRC is missing for Rel-16 NR V2X WI. |
|  |  |
| ***Clauses affected:*** | 4.2.X.5, A.Y |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start Change*

#### 4.2.X.5 Sidelink Physical Layer Parameters

##### 4.2.X.5.1 S*upportedBandListSidelink* parameters

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***gnb-ScheduledSidelinkMode3SidelinkEUTRA*** Indicates whether transmitting V2X sidelink communication mode 3 scheduled by NR Uu. If supported, this parameter indicates the support of the capabilities and includes the parameters as follows:* the UE can be scheduled by gNB using DCI format 3\_1 for V2X sidelink mode 3 transmission.
* ***gnb-ScheduledMode3DelaySidelinkEUTRA***, which indicates the minimum value UE supports for the additional time indicated in the NR DCI scheduling V2X sidelink mode 3. Value ms0 corresponds to 0 ms, ms0dot25 corresponds to 0.25 ms, and so on.

This field is only applicable if the UE supports V2X sidelink communication. | Band | No | No | No |
| ***gnb-ScheduledSidelinkMode4SidelinkEUTRA*** Indicates whether the UE can be scheduled by gNB for V2X sidelink mode 4 transmission. This field is only applicable if the UE supports V2X sidelink communication. | Band | No | No | No |

*Next Change*

# Annex A.Y: Sidelink capabilities applicable to Uu and PC5

Annex A.Y specifies for each sidelink related capability, in which interface (i.e., *UECapabilityInformation* in Uu RRC and *UECapabilityInformation*Sidelink in PC5 Uu) a UE supporting sidelink shall report the concerned capability:

* *UECapabilityInformation*: the concerned sidelink capability is reported within *UECapabilityInformation*;
* *UECapabilityInformationSidelink*: the concerned sidelink capability is reported within *UECapabilityInformationSidelink;*

Table A.Y-1: Sidelink capability reported in *UECapabilityInformation*/ *UECapabilityInformationSidelink*

|  |  |  |
| --- | --- | --- |
| Sidelink Capability  | *UECapabilityInformation* | *UECapabilityInformationSidelink* |
| gnb-ScheduledSidelinkMode3SidelinkEUTRA  | X |  |
| gnb-ScheduledSidelinkMode4SidelinkEUTRA  | X |  |