**3GPP TSG-RAN WG2** **Meeting #111 *R2-200xxxx***

**Electronic, 17 – 28 August 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **1985** | **rev** | **1** | **Current version:** | **15.10.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification on the SRB configuration for fullConfig during RRC Resume procedure | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE corporation, Sanechips | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2020-08-06 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The following Note has been added to clarify the SRB configuration handling when fullConfig is included for reconfiguration with sync and reconfiguration after re-establishment.  *NOTE 2: This is to get the SRBs (SRB1 and SRB2 for reconfiguration with sync and SRB2 for reconfiguration after re-establishment) to a known state from which the reconfiguration message can do further configuration.*  However, for the RRC Resume procedure, the fullConfig can also be included and the SRB configuration handling is not quite clear.  For RRC Resume procedure, UE has already apply the default configuration for SRB1 when initiating RRCResumeRequest message. If SRB1 is included in the *srb-ToAddModList* when fullConfig is configured in RRCResume, UE has to create a new PDCP entity with the default which seems to be unnecessary.  Thus, it is suggested to clarify in the Note 2 that for resume with fullconfig, the following operation is to get the SRB2 for resume to a know state from which the reconfiguration can do further configuration.  1> for each *srb-Identity* value included in the *srb-ToAddModList* (SRB reconfiguration):  2> apply the default SRB configuration defined in 9.2.1 for the corresponding SRB; | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify in the Note 2 that for resume with fullconfig, the following operation is to get the SRB2 for resume to a know state from which the reconfiguration can do further configuration.   1. for each *srb-Identity* value included in the *srb-ToAddModList* (SRB reconfiguration):   2> apply the default SRB configuration defined in 9.2.1 for the corresponding SRB;  **Impact Analysis**  Impacted 5G architecture options:  SA, NE-DC, NR-DC    Impacted functionality:  RRC Resume procedure    Inter-operability:  No inter-operability is forseen. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The SRB configuration handling for RRC Resume with fullconfig is not clear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.5.11 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

Start of change

#### 5.3.5.11 Full configuration

The UE shall:

1> release/ clear all current dedicated radio configurations except for the following:

- the MCG C-RNTI;

- the AS security configurations associated with the master key;

NOTE 1: Radio configuration is not just the resource configuration but includes other configurations like *MeasConfig*. In case NR-DC or NE-DC is configured, this also includes the entire NR or E-UTRA SCG configuration which are released according to the MR-DC release procedure as specified in 5.3.5.10. The radio configuration does not include SRB1/SRB2 configurations and DRB configurations as configured by *radioBearerConfig* or *radioBearerConfig2*.

1> if the *spCellConfig* in the *masterCellGroup* includes the *reconfigurationWithSync* (i.e., SpCell change):

2> release/ clear all current common radio configurations;

2> use the default values specified in 9.2.3 for timers T310, T311 and constants N310, N311;

1> else (full configuration after re-establishment or during RRC resume):

2> use values for timers T301, T310, T311 and constants N310, N311, as included in *ue-TimersAndConstants* received in *SIB1*;

1> apply the default L1 parameter values as specified in corresponding physical layer specifications except for the following:

- parameters for which values are provided in *SIB1*;

1> apply the default MAC Cell Group configuration as specified in 9.2.2;

1> for each *srb-Identity* value included in the *srb-ToAddModList* (SRB reconfiguration):

2> apply the default SRB configuration defined in 9.2.1 for the corresponding SRB;

NOTE 2: This is to get the SRBs (SRB1 and SRB2 for reconfiguration with sync and SRB2 for resume and reconfiguration after re-establishment) to a known state from which the reconfiguration message can do further configuration.

1> for each *pdu-Session* that is part of the current UE configuration:

2> release the SDAP entity (clause 5.1.2 in TS 37.324 [24]);

2> release each DRB associated to the *pdu-Session* as specified in 5.3.5.6.4;

NOTE 3: This will retain the *pdu-Session* but remove the DRBs including *drb-identity* of these bearers from the current UE configuration. Setup of the DRBs within the AS is described in clause 5.3.5.6.5 using the new configuration. The *pdu-Session* acts as the anchor for associating the released and re-setup DRB. In the AS the DRB re-setup is equivalent with a new DRB setup (including new PDCP and logical channel configurations).

1> for each *pdu-Session* that is part of the current UE configuration but not added with same *pdu-Session* in the *drb-ToAddModList*:

2> if the procedure was triggered due to reconfiguration with sync:

3> indicate the release of the user plane resources for the *pdu-Session* to upper layers after successful reconfiguration with sync;

2> else:

3> indicate the release of the user plane resources for the *pdu-Session* to upper layers immediately;

End of change