**3GPP TSG-RAN WG2 Meeting #111 Electronic *R2-2008207***

**17 – 28 August 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.304** | **CR** |  | **rev** |  | **Current version:** | **16.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Idle mode corrections for NPN |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, CATT, Vivo |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NG\_RAN\_PRN-Core, NR\_unlic-Core |  | ***Date:*** | 2020-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | 16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | This CR contains the agreed NPN related corrections from RAN2#111-e. |
|  |  |
| ***Summary of change:*** | 1. R2-2006634: Changes related to "CAG-ID" (issue 1 in the CR) are endorsed
2. Change the naming “CAG ID” in clause 4.1,4.2, 5.1.1.2, 5.2.4.4, 5.3.1 to “CAG-ID”.
3. R2-2006852: Change 2d) is endorsed.
4. A clarification is added to clause 5.2.4.4 that in unlicensed bands the *"UE should continue to consider other cells on the same frequency for cell reselection"* after the candidate cell is excluded being not suitable due the listed reasons.
5. R2-2008114: 2nd change ("this cell does not~~is a SNPN cell that~~ belongs to a SNPN that is not equal to the registered or selected SNPN of the UE in SNPN access mode") is endorsed.
6. Secondly, update the description in 5.2.4.4 that *“this cell is a SNPN cell that belongs to a SNPN that is not equal to the registered or selected SNPN of the UE in SNPN access mode”* to avoid uncertainty of UE behavior due to the unspecified definition of SNPN cell
7. R2-2006852: Remove the redundant texts from 5.2.4.4
8. The following text is removed from clause 5.2.4.4: "For a UE operating in SNPN AM and in shared spectrum channel access, if the highest ranked cell or best cell according to absolute priority reselection rules is a cell which is not suitable due to not broadcasting the registered or selected SNPN ID, the UE shall not consider this cell as candidate for cell reselection but should continue to consider other cells on the same frequency for cell reselection."
9. The 1st occurrence of the following sentence is removed from clause 5.2.4.4 of 38.304: "If the UE is redirected under NR control to a frequency for which the timer is running, any limitation on that frequency shall be removed"
10. R2-200.
11. A.
12. R2-200.
13. A.
14. R2-200.
15. A.

**Impact analysis**Impacted functionality: Cell selection and reselection in case of NPNs.Inter-operability: As this network has no network impact, implementation of this CR by a UE will not cause compatibility issues |
|  |  |
| ***Consequences if not approved:*** | The specification of NPN feature remains unclear and contains errors. |
|  |  |
| ***Clauses affected:*** | 4.1, 4.2, 5.1.1.2, 5.2.4.4, 5.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*First Modified Subclause*

## 4.1 Overview

The RRC\_IDLE state and RRC\_INACTIVE state tasks can be subdivided into three processes:

- PLMN selection (for UE not operating in SNPN access mode) or SNPN selection (for UE operating in SNPN access mode);

- Cell selection and reselection;

- Location registration and RNA update.

PLMN selection, SNPN selection, cell reselection procedures, and location registration are common for both RRC\_IDLE state and RRC\_INACTIVE state. RNA update is only applicable for RRC\_INACTIVE state. When UE selects a new PLMN or SNPN, UE transitions from RRC\_INACTIVE to RRC\_IDLE, as specified in TS 24.501 [14].

When a UE is switched on, a public land mobile network (PLMN) or a SNPN is selected by NAS. For the selected PLMN/SNPN, associated RAT(s) may be set, as specified in TS 23.122 [9]. The NAS shall provide a list of equivalent PLMNs, if available, that the AS shall use for cell selection and cell reselection.

With cell selection, the UE searches for a suitable cell of the selected PLMN or selected SNPN, chooses that cell to provide available services, and monitors its control channel. This procedure is defined as "camping on the cell".

The UE shall, if necessary, then register its presence, by means of a NAS registration procedure, in the tracking area of the chosen cell. As an outcome of a successful Location Registration, the selected PLMN/SNPN then becomes the registered PLMN/SNPN, as specified in TS 23.122 [9].

If the UE finds a more suitable cell, according to the cell reselection criteria, it reselects onto that cell and camps on it. If the new cell does not belong to at least one tracking area to which the UE is registered, location registration is performed. In RRC\_INACTIVE state, if the new cell does not belong to the configured RNA, an RNA update procedure is performed.

If necessary, the UE shall search for higher priority PLMNs at regular time intervals as described in TS 23.122 [9] and search for a suitable cell if another PLMN has been selected by NAS.

For UE not operating in SNPN access mode, search of available CAGs may be triggered by NAS to support manual CAG selection. The AS shall report available CAG-ID(s) together with their HRNN (if broadcast) and PLMN(s) to the NAS.

*Next change*

## 4.2 Functional division between AS and NAS in RRC\_IDLE state and RRC\_INACTIVE state

Table 4.2-1 presents the functional division between UE non-access stratum (NAS) and UE access stratum (AS) in RRC\_IDLE state and RRC\_INACTIVE states. The NAS part is specified in TS 23.122 [9] and the AS part in the present document.

Table 4.2-1: Functional division between AS and NAS in RRC\_IDLE state and RRC\_INACTIVE state

| RRC\_IDLE and RRC\_INACTIVE state Process | UE Non-Access Stratum | UE Access Stratum |
| --- | --- | --- |
| PLMN Selection  | **For a UE not operating in SNPN access mode, perform the following:**Maintain a list of PLMNs in priority order according to TS 23.122 [9]. Select a PLMN using automatic or manual mode as specified in TS 23.122 [9] and request AS to select a cell belonging to this PLMN. For each PLMN, associated RAT(s) may be set.Evaluate reports of available PLMNs and any associated CAG-IDs from AS for PLMN selection.Maintain a list of equivalent PLMN identities.To support manual CAG selection, provide request to search for available CAGs and evaluate reports of available CAGs from AS for CAG selection.**For a UE operating in SNPN access mode, perform the following:**Maintain a list of SNPNs according to TS 23.122 [9]. Select a SNPN using automatic or manual mode as specified in TS 23.122 [9] and request AS to select a cell belonging to this SNPN.Evaluate reports of available SNPNs from AS for SNPN selection. | For a UE not operating in SNPN access mode, search for available PLMNs.If associated RAT(s) is (are) set for the PLMN, search in this (these) RAT(s) and other RAT(s) for that PLMN as specified in TS 23.122 [9].For a UE operating in SNPN access mode, search for available SNPNs only consider NR cells.Perform measurements to support PLMN/SNPN selection.Synchronise to a broadcast channel to identify found PLMNs/SNPNs.Report available PLMNs and any associated CAG-IDs with associated RAT(s) to NAS on request from NAS or autonomously.For a UE operating in SNPN access mode, report available SNPNs to NAS autonomously.**To support manual CAG selection, perform the following:**Search for cells broadcasting a CAG-ID.Read the HRNN (if broadcast) for each CAG-ID if a cell broadcasting a CAG-ID is found.Report CAG-ID(s) of found cell(s) broadcasting a CAG-IDtogether with the associated manual CAG selection allowed indicator, HRNN and PLMNto NAS.On selection of a CAG by NAS, select any acceptable or suitable cell belonging to the selected CAG and give an indication to NAS that access is possible (for the registration procedure)To support manual SNPN selection, report available SNPNs together with associated HRNNs (if available) to NAS on request from NAS. |
| Cell Selection | Control cell selection for example by indicating RAT(s) associated with the selected PLMN to be used initially in the search of a cell in the cell selection.Maintain a list of "Forbidden Tracking Areas" and provide the list to AS.For a UE not operating in SNPN access mode: Maintain Allowed CAG list and optional CAG-only indication along with associated PLMN ID(s) on which the UE is allowed access and provide these lists to AS. To support manual CAG selection, select a CAG and request AS to select a cell belonging to this CAG. | Perform measurements needed to support cell selection.Detect and synchronise to a broadcast channel. Receive and handle broadcast information. Forward NAS system information to NAS.Search for a suitable cell. The cells broadcast one or more 'PLMN identity' or 'SNPN identity' (for a UE operating in SNPN access mode) in the system information. Respond to NAS whether such cell is found or not.If associated RATs is (are) set for the PLMN, perform the search in this (these) RAT(s) and other RATs for that PLMN as specified in TS 23.122 [9].If a cell is found which satisfies cell selection criteria, camp on that cell. |
| Cell Reselection | For a UE not operating in SNPN access mode,maintain a list of equivalent PLMN identities and provide the list to AS.Maintain a list of "Forbidden Tracking Areas" and provide the list to AS.For a UE not operating in SNPN access mode, maintain Allowed CAG list and optional CAG-only indication along with associated PLMN ID(s) on which the UE is allowed access and provide these lists to AS. | Perform measurements needed to support cell reselection.Detect and synchronise to a broadcast channel. Receive and handle broadcast information. Forward NAS system information to NAS.Change cell if a more suitable cell is found. |
| Location registration | Register the UE as active after power on.Register the UE's presence in a registration area, for instance regularly or when entering a new tracking area.Deregister UE when shutting down.Maintain a list of "Forbidden Tracking Areas".Control and restrict location registration for a UE in eCall Only Mode. | Report registration area information to NAS. |
| RAN Notification Area Update | Not applicable. | Register the UE's presence in a RAN-based notification area (RNA), periodically or when entering a new RNA. |

*Next change*

#### 5.1.1.2 NR case

The UE shall scan all RF channels in the NR bands according to its capabilities to find available PLMNs and available CAGs. On each carrier, the UE shall search for the strongest cell and read its system information, in order to find out which PLMN(s) the cell belongs to and any associated CAG(s). For operation with shared spectrum channel access, the UE may also read the system information of multiple strongest cell(s). If the UE can read one or several PLMN identities in the strongest cell or the multiple strongest cell(s) in case of operation with shared spectrum channel access, each found PLMN (see the PLMN reading in TS 38.331 [3]) shall be reported to the NAS as a high quality PLMN (but without the RSRP value) and any associated CAG-ID, provided that the following high-quality criterion is fulfilled:

1. For an NR cell, the measured RSRP value shall be greater than or equal to -110 dBm.

Found PLMNs that do not satisfy the high-quality criterion but for which the UE has been able to read the PLMN identities are reported to the NAS together with their corresponding RSRP values and any associated CAG-ID. The quality measure reported by the UE to NAS shall be the same for each PLMN found in one cell.

The search for PLMNs may be stopped on request from the NAS. The UE may optimise PLMN search by using stored information e.g. frequencies and optionally also information on cell parameters from previously received measurement control information elements.

Once the UE has selected a PLMN, the cell selection procedure shall be performed in order to select a suitable cell of that PLMN to camp on.

To support manual CAG selection, the UE shall upon request by NAS report available CAG-ID (s) together with their manual CAG selection allowed indicator (if broadcast), HRNN (if broadcast) and PLMN(s) to the NAS. If NAS has selected a CAG and provided this selection to AS, the UE shall search for an acceptable or suitable cell belonging to the selected CAG to camp on.

*Next change*

#### 5.2.4.4 Cells with cell reservations, access restrictions or unsuitable for normal camping

For the highest ranked cell (including serving cell) according to cell reselection criteria specified in clause 5.2.4.6, for the best cell according to absolute priority reselection criteria specified in clause 5.2.4.5, the UE shall check if the access is restricted according to the rules in clause 5.3.1.

If that cell and other cells have to be excluded from the candidate list, as stated in clause 5.3.1, the UE shall not consider these as candidates for cell reselection. This limitation shall be removed when the highest ranked cell changes.

If the highest ranked cell or best cell according to absolute priority reselection rules is an intra-frequency or inter-frequency cell which is not suitable due to one or more of the following reasons:

- this cell belongs to a PLMN which is not indicated as being equivalent to the registered PLMN, or

- this cell is a CAG cell that belongs to a PLMN which is equivalent to the registered PLMN but with no CAG-ID that is present in the UE's allowed CAG list being broadcasted, or

- this cell is not a CAG cell and the CAG-only indication in the UE is set, or

- this cell does not belong to a SNPN that is equal to the registered or selected SNPN of the UE in SNPN access mode,

the UE shall not consider this cell and, for operation in licensed spectrum, other cells on the same frequency as candidates for reselection for a maximum of 300 seconds.

For operation with shared spectrum channel access, when the highest ranked cell or best cell is not a candidate for reselection per the previous paragraph, the UE should continue to consider other cells on the same frequency for cell reselection, however if the second highest ranked cell on this frequency is also not suitable due to one or more of the above reasons, the UE may consider this frequency to be the lowest priority for a maximum of 300 seconds.

If the highest ranked cell or best cell according to absolute priority reselection rules is an inter-frequency or inter-frequency cell which is not suitable due to being part of the "list of 5GS forbidden TAs for roaming", the UE shall not consider this cell and other cells on the same frequency as candidates for reselection for a maximum of 300 seconds.

If the UE enters into state *any cell selection*, any limitation shall be removed.

If the highest ranked cell or best cell according to absolute priority reselection rules is an inter-RAT cell which is not suitable due to being part of the "list of forbidden TAs for roaming" or belonging to a PLMN which is not indicated as being equivalent to the registered PLMN, the UE shall not consider this cell and other cells on the same frequency, as candidates for reselection for a maximum of 300 seconds. If the UE enters into state *any cell selection*, any limitation shall be removed. If the UE is redirected under NR control to a frequency for which the timer is running, any limitation on that frequency shall be removed.

*Next change*

### 5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *MIB or SIB1* message as specified in TS 38.331 [3] by means of following fields:

- *cellBarred* (IE type: "barred" or "not barred")
Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")
Indicated in *SIB1* message*.* In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

- *cellReservedForOtherUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs.

*- cellReservedForFutureUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

NOTE: IAB-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse*, *cellReservedForOtherUse* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. IAB-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable IAB-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

- *iab-Support* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

When cell status is indicated as "not barred" and "not reserved" for operator use and not "true" for other use and not "true" for future use,

- All UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell broadcasts any CAG-IDs or NIDs and the cell status is indicated as "not barred" and "not reserved" for operator use and "true" for other use, and not "true" for future use:

- All NPN-capable UEs shall treat this cell as candidate during the cell selection and cell reselection procedures, other UEs shall treat this cell as if cell status is "barred".

*Next Modified Subclause*

*End of Changes*