3GPP TSG-RAN WG2 #111e Tdoc draftR2-2008199

Electronic meeting, August 17th – 28th 2020

Agenda Item: 8.12.1

Source: Rapporteur (Ericsson)

Title: Summary of [AT111][108][REDCAP] Scope and skeleton update

Document for: Discussion, Decision

# 1 Introduction

This document summarizes the following discussion during RAN2#111-e:

* [AT111e][108][REDCAP] Scope and skeleton update (Ericsson)

Scope: Discuss the SI scope in [R2-2006910](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2//TSGR2_111-e/Docs//R2-2006910.zip) and the skeleton update in [R2-2007366](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2//TSGR2_111-e/Docs//R2-2007366.zip)

Initial intended outcome: summary of the offline discussion with e.g.:

* + - List of agreeable proposals (if any)
		- List of proposals that require online discussions

and skeleton update

Initial deadline (for companies' feedback): Monday 2020-08-24 16:00 UTC

Initial deadline (for rapporteur's summary in R2-2008189): Monday 2020-08-24 18:00 UTC

The discussion in based on [R2-2006910](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2//TSGR2_111-e/Docs//R2-2006910.zip) [2] and there are questions related to the TR skeleton [3] as well.

As background for the discussion on the study item scope, the SID includes the following objectives [1]:

*The study item includes the following objectives:*

*Identify and study potential UE complexity reduction features, including [RAN1, RAN2]:*

* *Reduced number of UE RX/TX antennas*
* *UE Bandwidth reduction*

*Note: Rel-15 SSB bandwidth should be reused and L1 changes minimized*

* *Half-Duplex-FDD*
* *Relaxed UE processing time*
* *Relaxed UE processing capability*

*The study includes evaluations of the impact to coverage, network capacity and spectral efficiency*

*Note1: The work defined above should not overlap with LPWA use cases. The lowest data rate and bandwidth capability considered should be no less than an LTE Category 1bis modem.*

*Study UE power saving and battery lifetime enhancement for reduced capability UEs in applicable use cases (e.g. delay tolerant) [RAN2, RAN1]:*

* *Reduced PDCCH monitoring by smaller numbers of blind decodes and CCE limits [RAN1].*
* *Extended DRX for RRC Inactive and/or Idle [RAN2]*
* *RRM relaxation for stationary devices [RAN2]*

*Study functionality that will enable the performance degradation of such complexity reduction to be mitigated or limited, including [RAN1]:*

* *Coverage recovery to compensate for potential coverage reduction due to the device complexity reduction.*
	+ *Note: For FR1, coverage analysis for wearables can include consideration of potential reduced antenna efficiency due to device size limitations as part of the antenna gains. The extent of additional recovery of coverage loss due to reduced antenna efficiency is to be limited to 3 dB*
* *The study includes evaluations of the impact to network capacity and spectral efficiency*

*Study standardization framework and principles for how to define and constrain such reduced capabilities – considering definition of a limited set of one or more device types and considering how to ensure those device types are only used for the intended use cases [RAN2, RAN1].*

*Study functionality that will allow devices with reduced capabilities to be explicitly identifiable to networks and network operators, and allow operators to restrict their access, if desired [RAN2, RAN1].*

*Note2: Potential overlap with coverage enhancements study is discussed and resolved in RAN#87 or later.*

*Note3: Coexistence with Rel-15 and Rel-16 UE should be ensured*

*Note4: This SI should focus on SA mode and single connectivity*

Companies are asked to provide input on the described scope in questions below. Please indicate especially if some objective is not clear, or if there are some aspects missing from the proposed scope of discussion.

# 2 Discussion

## 2.1 UE complexity reduction features

As discussed in [1] and in other submitted contributions, RAN1 has the main responsibility of defining the features which describe a RedCap UE, where a number of agreements have been made already.

For RAN2, it mainly remains to be discussed which particular aspects of RAN2 protocols and procedures are impacted and whether changes are needed. Companies are welcome to provide their initial views on what RAN2 should further consider or discuss related to the UE complexity reduction features.

The RAN1 agreements before RAN2#111-e are listed in the Appendix for reference. It should be noted the final feature list is not yet completed and the evaluation from RAN2 side is subject to change.

**Question 1 (Expected RAN2 impact): What are expected impacts in RAN2 protocols and procedures due to introduction of RedCap UEs in NR/5GS? What other aspects, not already covered by the objectives in the SID [3], RAN2 should consider in their work?**

*Note: The discussion can be based on already agreed features in RAN1 and based on expectations on possible not yet agreed RedCap features.*

|  |  |
| --- | --- |
| **Company** | **View** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Question 2 (RAN2 input on features): Do you think there is need for RAN2 to provide other input to RAN1 regarding the UE complexity reduction features. If yes, please elaborate on what input you think is needed.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

##

## 2.2 UE power saving and battery lifetime enhancement

Two RAN2-specific objectives related to UE power saving are mentioned in the SID [3]: 1) Extended DRX for RRC Inactive and/or Idle, and 2) RRM relaxation for stationary devices.

Discussion paper [1] contains proposal for RAN2 to provide solutions and analysis to TR 38.875 on extended DRX for RRC Inactive and Idle modes and RRM relaxation for stationary RedCap devices. This is inline with the SI scope and companies are asked to confirm the understanding of this scope and provide additional comments, if any:

**Question 3 (Power saving scope): Do you agree that for UE power saving and battery lifetime enhancement, RAN2 should focus only on studying extended DRX for RRC Inactive and Idle modes and RRM relaxation for stationary RedCap devices, and provide input on these objectives to TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

The SID only mentions "RRM relaxation for stationary devices", and it is not explicitly stated whether such relaxation should apply to neighboring cells and/or the serving cell. Also, it is not explicitly stated whether relaxation should apply in RRC\_IDLE and/or RRC\_INACTIVE and/or RRC\_CONNECTED. Companies are asked to provide preliminary input on what they think should be the scope of the RRM relaxation objective.

**Question 4 (RRM relaxation scope): Which cells and RRC states RAN2 should focus on when studying RRM relaxation for stationary RedCap devices?**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Neighboring/serving cell** | **RRC state(s)** | **Comments** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## 2.3 Standardization framework and principles for constraints for reduced capabilities

One of the objectives in the SI is to "study standardization framework and and principles for how to define and constrain such reduced capabilities". Proposal in [1] is for RAN2 to focus on providing RAN2 view on how and how many RedCap UE types should be defined and for RAN2 to further study how to possibly constrain or extend the capability signaling framework for RedCap UEs or use cases.

**Question 5 (UE types): Do you agree that RAN2 should study if, how and how many UE types should be defined for RedCap UEs from RAN2 point of view and provide input to RAN1 and TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 6 (Capability framework): Do you agree that RAN2 should discuss whether there is need to constrain or extend the existing capability signaling framework due to introduction of RedCap UEs in NR/5GS, and provide possible input in TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 7 (Constraining of reduced capabilities): Do you agree that RAN2 should discuss whether and how it can be ensured RedCap UEs are used only for intended use cases, and provide possible input in TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.4 Functionality for identification of restricted capability UEs

The network should be able to identify RedCap UEs from "normal" NR UEs e.g. to control access of such UEs to the system. Couple of different ways to achieve this are discussed in the submitted contributions and according to the SI [3], RAN2 should study the options and provide view on which would be the best way. Correspondingly, proposal in [1] is for RAN2 to provide input to TR 38.875 on the possible identification mechanisms, and on the possible access restriction mechanisms. Companies are asked to confirm the understanding of the RAN2 scope.

**Question 8 (Identification of UEs in RAN): Do you agree that RAN2 should discuss and provide input to TR 38.875 on mechanisms how to identify RedCap UEs and how to control the access of RedCap UEs in RAN?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.5 TR skeleton for TR 38.875

The TR skeleton for TR 38.875 is provided in [2]. This version is based on the initial version v0.0.1 endorsed in RAN1#101-e and further revised.

The above questions cover the sections in TR 38.875 where RAN2 input is expected. Companies are asked to provide input on the TR skeleton, e.g. if there are sections which should be added, changed or removed, etc.

**Question 9: Please provide input, if any, on the TR skeleton in [2].**

|  |  |
| --- | --- |
| **Company** | **Input** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.6 Organization of the RAN2 work during the study phase

If RAN2 identifies need to update the skeleton or provide other text input already from RAN2#111-e, it should be possible to send LS to RAN1 e.g. containing RAN2 changes on the skeleton, if needed. This can be evaluated once the discussion has progressed.

Otherwise, RAN2 should consider whether to start email discussions on the different aspects discussed above, to facilitate the eventual input to TR 38.875.

**Question 10: Do you agree that RAN2 should initiate email discussions Post-RAN2#111-e on the different aspects and objectives discussed above, where the scope is drafting input to TR 38.875, to be agreed in RAN2#112.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes / no** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Summary and proposals

TBD

# References

1. [R2-2006910](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2//TSGR2_111-e/Docs//R2-2006910.zip), Scope of RedCap SI, Ericsson, RAN2#111-e, Electronic meeting, August 2020.

1. [R2-2007366](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2//TSGR2_111-e/Docs//R2-2007366.zip), R38.875 skeleton updates for Study on support of reduced capability NR devices, Ericsson, RAN2#111-e, Electronic meeting, August 2020.

1. [RP-201386](https://www.3gpp.org/ftp/TSG_RAN/TSG_RAN/TSGR_88e/Docs/RP-201386.zip), Revised SID on Study on support of reduced capability NR devices, Ericsson, RAN#88e, Electronic meeting, June 29 – July 3, 2020.

# Appendix: RAN1 agreements from RAN1#101-e

RAN1 made the following agreements related to **use case requirements**:

|  |
| --- |
| Agreements:* For safety related sensors, latency requirements apply to traffic initiated from RRC\_CONNECTED.
 |

RAN1 made the following agreements related to **study of UE complexity reduction**:

|  |
| --- |
| Agreements:* For FR1, study at least 20MHz maximum UE bandwidth at least for initial access
	+ Other bandwidths FFS
* For FR2, study 50MHz and 100 MHz maximum UE bandwidth at least for initial access
	+ Other bandwidths FFS

Agreements:* For FR1, study two antenna configurations for RedCap UEs, namely 1Rx/1Tx and 2Rx/1Tx.
* For FR2, study two antenna configurations for RedCap UEs, namely 1Rx/1Tx and 2Rx/1Tx.

Agreements:* Study HD-FDD operation Type A and Type B (as defined in LTE) in RAN1, where study of Type A is prioritized.

Agreements:* For UE complexity reduction through relaxed UE processing time, study a more relaxed UE processing time in terms of N1/N2 compared to capability #1.

Agreements:* Use the TR 36.888 methodology for UE cost/complexity evaluation as a starting point and determine what major updates are needed.
* Cost/complexity breakdowns can be separate for FR1 and FR2 if found beneficial.
* Include antenna parts at least in the cost/complexity breakdown for FR2.
* Potential benefits in terms of reduced device size can be mentioned where applicable in the TR (e.g. in the section on reduced number of antennas), but the SI will not aim to quantify such benefits.

Agreements:The reference NR device for evaluation of cost/complexity reduction supports the following:* All mandatory Rel-15 features (with or without capability signaling)
* Single RAT
* Operation in a single band at a time
* Maximum bandwidth:
	+ For FR1: 100 MHz for DL and UL
	+ For FR2: 200 MHz for DL and UL
* Antennas:
	+ For FR1 FDD: 2Rx/1Tx
	+ For FR1 TDD: 4Rx/1Tx
	+ For FR2: 2Rx/1Tx
* Power class: PC3
* Processing time: Capability 1
* Modulation:
	+ For FR1: support 256QAM for DL and 64QAM for UL
	+ For FR2: support 64QAM for DL and 64QAM for UL
* Access: Direct DL/UL access between UE and gNB

Note: The study will consider impacts on the cost/complexity reduction from support of multiple RF bands within FR1 or FR2. |

RAN1 made the following agreements related to **study of UE power saving**:

|  |
| --- |
| Agreements:* Study the impact of BD and CCE limits reduction on power saving and PDCCH blocking probability (quantitatively) and impacts on latency and scheduling flexibility (at least qualitatively).

Agreements:* Reuse the power consumption models and scaling factors for FR1 and FR2 provided in TR 38.840 (sections 8.1.1, 8.1.2, 8.1.3) as appropriate.
* For evaluation of UE power saving, for wearables, use the traffic models FTP model 3 and VoIP from TR 38.840 to characterize the wearables service types including IM, VoIP, heartbeat, etc. with proper modification of at least packet size and mean inter-arrival time. Values are FFS.
* For evaluation of UE power saving, for industrial wireless sensor use cases, use a traffic model based on the service performance requirements for the process monitoring use case in TS 22.104 Table 5.2-2. At least 64 bytes UL message (plus headers, e.g. MAC, RLC, etc.) transmitted periodically with a periodicity 100 ms should be considered (other values are encouraged).
 |

RAN1 made the following agreements related to **study of coverage loss/recovery**:

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Agreements:* If/when coverage evaluations outside the CE SI are needed,
	+ The basic evaluation methodology is based on link-level simulation for FR1.
		- ­Step 1: Obtain the required SINR for the physical channels under target scenarios and service/reliability requirements.
		- ­Step 2: Obtain the baseline performance based on required SINR and link budget template.
		- ­Note: aspects related to identifying target performance and coverage bottlenecks based on target performance metric is to be handled separately
	+ The evaluation methodology for FR2 is the same as FR1.

Agreements:* If/when link-level coverage evaluations outside the CE SI are needed,
	+ The CE SI link-level simulation assumptions can be used as a starting point.
	+ For calibration purposes, the following settings can be used:

|  |  |  |
| --- | --- | --- |
| **Parameters** | **FR1 values** | **FR2 values** |
| Scenario and frequency | Urban:2.6 GHz (TDD) (primary choice)4 GHz (TDD) (secondary choice)Rural:700 MHz (FDD) | Indoor: 28 GHz (TDD) |
| Frame structure for TDD | For 2.6 GHz:DDDDDDDSUU (S: 6D:4G:4U)For 4 GHz:DDDSUDDSUU(S: 10D:2G:2U) | DDDSU(S: 10D:2G:2U) |
| Channel model | TDL-C | TDL-A |
| UE velocity | 3 km/h | 3 km/h |

 |

RAN1 made the following agreements related to **study of performance impacts**:

|  |
| --- |
| Agreements:* The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique.
 |