**3GPP TSG-RAN WG2 Meeting #111 electronic R2-2008493**

**Online, August 17th - 28th, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.305** | **CR** | *0029* | **rev** | **1** | **Current version:** | **16.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on Stage-2 for gNB and LMF information transfer | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos-Core | | | | |  | ***Date:*** | | | 2020-7-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 1. In RAN3#108, RAN3 agreed to introduce the number of SRS resources/resource sets in POSITIONING INFORMATION REQUEST message, so as to provide assistance from LMF in order to facilitate gNB to configure SRS resource. It is better that stage-2 captures such information.  2. The describetion of the Geographical coordinate of the TRPs served by the gNB is per DL-PRS Resource ID. Addtionally, RAN3#108 aggreed the Cartesian coordinations and the corresponding describtion in stage-2 should be revised.  3. TRP measurement request information includes information that is not aligned with NRPPa and has been updated: | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Assistance data that may be transferred from gNB to the LMF:  * Change description of Geographical coordinates of TRP  1. Requested UL-SRS transmission characteristics  * Add the number of requested SRS resources and SRS resource sets in the message between LMF and gNB.  1. TRP Measurement request information  * Delete the PCI, CGI of the TRP; * Update the the timing informatin of TRPs * Delete the start time, and dureation of the measurements. * Add the Measurement quantities.   **Impact analysis**  **Impacted functionality**  Information that may be transfered between gNB and LMF  **Inter-operability:**   1. If the network is implemented according to the CR and the UE is not, there is no inter-oprability issue 2. If the UE is implemented according to the CR and the network is not, there is no inter-oprability issue. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | If changes are not approved, the stage-2 description is not aligned with NRPPa and may cause misunderstanding. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.10.2.3, 8.10.2.4, 8.11.2.3, 8.12.2.3, 8.13.2.3, 8.14.2.3, 8.13.2.0, 8.14.2.0 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR … CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

CHANGE Begin

#### 8.10.2.3 Information that may be transferred from the gNB to LMF

The assistance data that may be transferred from gNB to the LMF is listed in Table 8.10.2.3-1.

Table 8.10.2.3-1: Assistance data that may be transferred from gNB to the LMF

|  |
| --- |
| Information |
| PCI, GCI, and TRP IDs of the TRPs served by the gNB |
| Timing information of TRPs served by the gNB |
| DL-PRS configuration of the TRPs served by the gNB |
| SSB information of the TRPs (the time/frequency occupancy of SSBs) |
| Spatial direction information of the DL-PRS Resources of the TRPs served by the gNB |
| Geographical coordinates information of the DL-PRS Resources of the TRPs served by the gNB |

====================== Unchanged parts omitted =====================

#### 8.10.2.4 Information that may be transferred from the LMF to gNBs

The requested UL-SRS transmission characteristics information that may be signalled from the LMF to the gNB is listed in Table 8.10.2.4-1.

Table 8.10.2.4-1: Requested UL-SRS transmission characteristics information that may be transferred from LMF to gNB.

|  |
| --- |
| Information |
| Number Of Transmissions/duration for which the UL-SRS is requested |
| Bandwidth |
| Resource type (periodic, semi-persistent) |
| Number of requested SRS resource sets and SRS resources per set |
| Pathloss reference:  - PCI, SSB Index  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |
| Spatial relation info  - PCI, SSB Index  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |

The TRP measurement request information that may be signalled from the LMF to the gNBs is listed in Table 8.10.2.4-2.

Table 8.10.2.4-2: TRP Measurement request information that may be transferred from LMF to gNBs.

|  |
| --- |
| Information |
| TRP ID of the TRP to receive UL-SRS |
| UE-SRS configuration |
| UL timing information of the reference TRP (the serving TRP, on which the UE-SRS is configured), for reception of SRS by candidate TRPs |
| Report characteristics for the measurements |
| Measurement Quantities |

NEXT CHANGE

#### 8.11.2.3 Information that may be transferred from the gNB to LMF

The assistance data that may be transferred from gNB to the LMF is listed in table 8.11.2.3-1.

Table 8.11.2.3-1: Assistance data that may be transferred from gNB to the LMF

|  |
| --- |
| Information |
| PCI, GCI, and TRP IDs of the TRPs served by the gNB |
| Timing information of TRPs served by the gNB |
| DL-PRS configuration of the TRPs served by the gNB |
| SSB information of the TRPs (the time/frequency occupancy of SSBs) |
| Spatial direction information of the DL-PRS Resources of the TRPs served by the gNB |
| Geographical coordinates information of the TRPs served by the gNB |

NEXT CHANGE

#### 8.12.2.3 Information that may be transferred from the gNB to LMF

The assistance data that may be transferred from gNB to the LMF is listed in Table 8.12.2.3-1.

Table 8.12.2.3-1: Assistance data that may be transferred from gNB to the LMF

|  |
| --- |
| Information |
| PCI, GCI, and TRP IDs of the TRPs served by the gNB |
| Timing information of TRPs served by the gNB |
| DL-PRS configuration of the TRPs served by the gNB |
| SSB information of the TRPs (the time/frequency occupancy of SSBs) |
| Spatial direction information of the DL-PRS Resources of the TRPs served by the gNB |
| Geographical coordinates information of the TRPs served by the gNB |

NEXT CHANGE

#### 8.13.2.3 Information that may be transferred from the LMF to gNBs

The requested UL-SRS transmission characteristics information that may be signalled from the LMF to the gNB is listed in Table 8.13.2.3-1.

Table 8.13.2.3-1: Requested UL-SRS transmission characteristics information that may be transferred from LMF to gNB.

|  |
| --- |
| Information |
| Number Of Transmissions/duration for which the UL-SRS is requested |
| Bandwidth |
| Resource type (periodic, semi-persistent) |
| Pathloss reference:  - PCI, SSB Index, SSB configuration (time/frequency occupancy of SSBs)  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |
| Spatial relation info  - PCI, SSB Index, SSB configuration (time/frequency occupancy of SSBs)  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |

The TRP measurement request information that may be signalled from the LMF to the gNB is listed in table 8.13.2.3-2.

Table 8.13.2.3-2: TRP Measurement request information that may be transferred from LMF to gNB.

|  |
| --- |
| Information |
| TRP ID of the TRP to receive UL-SRS |
| UE-SRS configuration |
| UL timing information together with timing uncertainty, for reception of SRS by candidate TRPs |
| Report characteristics for the measurements |
| Measurement Quantities |

NEXT CHANGE

#### 8.14.2.3 Information that may be transferred from the LMF to gNB

The requested UL-SRS transmission characteristics information that may be signalled from the LMF to the gNB is listed in Table 8.14.2.3-1.

Table 8.14.2.3-1: Requested UL-SRS transmission characteristics information that may be transferred from LMF to gNB.

|  |
| --- |
| Information |
| Number Of Transmissions/duration for which the UL-SRS is requested |
| Bandwidth |
| Resource type (periodic, semi-persistent) |
| Number of requested SRS resource sets and SRS resources per set |
| Pathloss reference:  - PCI, SSB Index, SSB configuration (time/frequency occupancy of SSBs)  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |
| Spatial relation info  - PCI, SSB Index, SSB configuration (time/frequency occupancy of SSBs)  - DL-PRS ID, DL-PRS Resource Set ID, DL-PRS Resource ID |

The TRP measurement request information that may be signalled from the LMF to the gNB is listed in table 8.14.2.3-2.

Table 8.14.2.3-2: TRP Measurement request information that may be transferred from LMF to gNB.

|  |
| --- |
| Information |
| TRP ID of the TRP to receive UL-SRS |
| UE-SRS configuration |
| UL timing information together with timing uncertainty, for reception of SRS by candidate TRPs |
| Report characteristics for the measurements |
| Measurement Quantities |

NEXT CHANGE

#### 8.13.2.0 Assistance Data that may be transferred from the gNB to the LMF

The assistance data that may be transferred from the gNB to the LMF is listed in Table 8.13.2.0-1.

Table 8.13.2.0-1: Assistance data that may be transferred from gNB to the LMF

|  |
| --- |
| Information |
| PCI, GCI, and TRP IDs of the TRPs served by the gNB |
| SSB information of the TRPs (the time/frequency occupancy of SSBs) |
| Geographical coordinates information of the DL-PRS Resources of the TRPs served by the gNB |

NEXT CHANGE

#### 8.14.2.0 Assistance Data that may be transferred from the gNB to the LMF

The assistance data that may be transferred from the gNB to the LMF is listed in Table 8.14.2.0-1.

Table 8.14.2.0-1: Assistance data that may be transferred from gNB to the LMF

|  |
| --- |
| Information |
| PCI, GCI, and TRP IDs of the TRPs served by the gNB |
| SSB information of the TRPs (the time/frequency occupancy of SSBs) |
| Geographical coordinates information of the DL-PRS Resources of the TRPs served by the gNB |

CHANGE END