**3GPP TSG-RAN2 Meeting #112 electronic R2-2101874**

**Online, Jan 25th - Feb 5th, 2021**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.306** | **CR** | **0521** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR on the Capability of PUCCH Transmissions for HARQ-ACK-38306 |
|  |  |
| ***Source to WG:*** | ZTE Corporation, Sanechips,Intel |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_L1enh\_URLLC |  | ***Date:*** | 2021-1-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |

|  |  |
| --- | --- |
| ***Reason for change:*** | The component 6 of RAN1 feature 11-4/4a as below was not included in the corresponding field description.**11-4/4a component 6**Supported maximum number of actual PUCCH transmissions for HARQ-ACK within a slot.Candidate values for the component 6 of FG11-4 is: For NCP, {4, 5, 6, 7} for 2-symbol\*7 sub-slot configuration; For ECP, the candidate value is {4, 5, 6} for 2-symbol\*6 sub-slot configuration. |
|  |  |
| ***Summary of change:*** | Update the field description of twoHARQ-ACK-Codebook-type1-r16/ twoHARQ-ACK-Codebook-type2-r16 to include the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot.**Impact analysis**Impacted 5G architecture options:NR SA, NR-DC, (NG)EN-DC/NE-DCImpacted functionality:URLLCInter-operability:1. If UE implements according to the CR and the network does not, the network is unable to get the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot.
2. If the network implements according to the CR and the UE is not, the UE is unable to report the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot.
 |
|  |  |
| ***Consequences if not approved:*** | The network may misunderstand the capability and give the wrong configuration to the UE. |
|  |  |
| ***Clauses affected:*** | 4.2.7.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

####

Start change

#### 4.2.7.7 *FeatureSetUplink* parameters

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* omitted unchanged parts \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***twoHARQ-ACK-Codebook-type1-r16***Indicates whether the UE supports two HARQ-ACK codebooks with up to one subslot based HARQ-ACK codebook (i.e. slot-based + slot-based, or slot-based + subslot based) simultaneously constructed for supporting HARQ-ACK codebooks with different priorities at a UE.- *sub-SlotConfig-NCP-r16* indicates the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot for NCP with 2-symbol\*7 sub-slot configuration;- *sub-SlotConfig-ECP-r16* indicates the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot for ECP with 2-symbol\*6 sub-slot configuration;For the 7-symbol\*2 sub-slot configuration of NCP or the 6-symbol\*2 sub-slot configuration of ECP, the value of the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot is {2}.Note: If a UE reports both *multiPUCCH-r16* and *twoHARQ-ACK-Codebook-type1-r16*, it can support two slot-based HARQ-ACK codebooks, and one slot-based and one-sub-slot-based HARQ-ACK codebooks. If a UE reports *twoHARQ-ACK-Codebook-type1-r16* but doesn’t report *multiPUCCH-r16*, it can only support two slot-based HARQ-ACK codebooks. | FS | No | N/A | N/A |
| ***twoHARQ-ACK-Codebook-type2-r16***Indicates whether the UE supports two subslot based HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different priorities at a UE.- *sub-SlotConfig-NCP-r16* indicates the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot for NCP with 2-symbol\*7 sub-slot configuration;- *sub-SlotConfig-ECP-r16* indicates the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot for ECP with 2-symbol\*6 sub-slot configuration;For the 7-symbol\*2 sub-slot configuration of NCP or the 6-symbol\*2 sub-slot configuration of ECP, the value of the maximum number of actual PUCCH transmissions for HARQ-ACK within a slot is {2}.  | FS | No | N/A | N/A |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* omitted unchanged parts \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

End of change