3GPP TSG-RAN WG2 Meeting #113 draftR2-2102015

Elbonia, Online, 25 January – 5 February 2021

**Agenda item: 8.10.3.2**

**Source: Nokia, Nokia Shanghai Bell**

**Title: Report from [113-e][105][NTN] Idle mode aspects (Nokia)**

**WID/SID: NR\_NTN\_solutions-Core - Release 17**

**Document for: Discussion and Decision**

# 1 Brief scope of the paper

This document aims at collecting companies’ views regarding the Rel-17 NTN Idle mode:

* [AT113-e][105][NTN] Idle mode aspects (Nokia)

Scope: Discuss:

1. Continue the discussion on P1 and P2 from [R2-2100527](file:///C:\Data\3GPP\Extracts\R2-2100527_Report%20from%20%5bPost112-e%5d%5b153%5d%5bNTN%5d%20Idle%20mode%20aspects%20(Nokia).docx)
2. Usage and provision of the cell expire time and upcoming cell info
3. ephemeris assisted cell (re)selection

based on the corresponding proposals in [R2-2100347](file:///C:\Data\3GPP\Extracts\R2-2100347%20NTN%20Idle%20mode.docx) (P1~P4), [R2-2101196](file:///C:\Data\3GPP\Extracts\R2-2101196_Discussion%20on%20cell%20selection%20and%20reselection%20in%20NTN.docx), [R2-2100382](file:///C:\Data\3GPP\Extracts\R2-2100382.docx) (P1) and [R2-2100163](file:///C:\Data\3GPP\Extracts\R2-2100163%20NTN%20Idle%20inactive%20mode%20procedures.doc) (P1 and P2)

Initial intended outcome: Summary of the offline discussion with e.g.:

* + - List of proposals for agreement (if any)
    - List of proposals that require online discussions
    - List of proposals that should not be pursued (if any)

Initial deadline (for companies' feedback): Monday 2021-02-01 17:00 UTC

Initial deadline (for rapporteur's summary in R2-2102015): Monday 2021-02-01 23:00 UTC

Proposals marked "for agreement" in R2-2102015 not challenged until Tuesday 2020-02-02 11:00 UTC will be declared as agreed by the session chair. For the rest the discussion will continue online.

The following sections elaborate on the topics listed in the scope above.

# 2 Proposal 1 and Proposal 2 from R2-2100527

As an outcome of [1] the following was proposed, among the others:

|  |
| --- |
| Proposal 1: UE is made aware of the network type (TN or NTN) in an implicit way.  Proposal 2: NTN scenario information (e.g. LEO/GEO) is not signalled explicitly, but inferred from the contents of the ephemeris. FFS which exact parameters are sufficient and whether this behavior needs to be specified. |

During the online discussion at RAN2#113, the following views have been exchanged with regards to these:

|  |
| --- |
| Proposal 1: UE is made aware of the network type (TN or NTN) in an implicit way.   * ZTE is fine for the serving cell but we could have an explicit indication for the neighbour cell. * LG still wonders whether this works. * Continue the discussion as part of offline 105   Proposal 2: NTN scenario information (e.g. LEO/GEO) is not signalled explicitly, but inferred from the contents of the ephemeris. FFS which exact parameters are sufficient and whether this behavior needs to be specified.   * Samsung/QC prefer an explicit indication to avoid that the UE needs to derive this. * Continue the discussion as part of offline 105 |

Despite large majority supporting each of these proposals during [1], it was not feasible to converge during the online handling of the resulting report [1]. Regarding Proposal 1, it is commonly understood there are multiple ways how this can be ensured, even if separate PLMNs for TN and NTN cannot be guaranteed (as argued e.g. by LG or BT [1]). For example, the existence of NTN-specific SIB or ephemeris is an easy way to infer the cell is of NTN type. In addition, we believe the introduction of a new parameter (network type in this case) shall be properly justified, so the proponents of an explicit indication shall actually describe why this is needed. Otherwise, before convincing the substantial majority, RAN2 shall proceed towards the end of the WI with the agreement there is no such explicit indication (as the need for having such new parameter has not been widely acknowledged).

As pointed out by ZTE and quoted in the box above, there may be a distinction between the serving cell and the neighbours as the UE may not know which SIBs are available per each neighbour cell, while it will anyway acquire serving cell’s SIB1 and know if e.g. NTN-specific SIB is available. Thus, it shall be considered whether we can at least agree no indication for the serving cell (i.e. in MIB/SIB1) is needed?

|  |  |  |
| --- | --- | --- |
| **Question 1: Do you agree there is no explicit indication of network type (TN/NTN) for serving cell in MIB/SIB1?** | | |
| **Company** | **Yes/No** | **Motivation** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary for Question 1:

<blank>

Then, a related question shall be asked concerning the neighbour cells, as suggested by ZTE. It is argued [1] that SIBs 2-5, where the cell reselection information could be provided, there is a need to indicate which cells are of NTN type, so that the UE knows which cells to consider in reselection process. As this is related to cell reselection procedure (discussed separately below) and also such information can be conveyed in the ephemeris (when its content are decided eventually), we think it is perhaps not essential to consider it here and now. On the other hand, for completeness (with Question 1), companies are at least asked to indicate if NTN type for neighbour cells shall be indicated explicitly. If yes, please indicate how. If not, please indicate why.

|  |  |  |
| --- | --- | --- |
| **Question 2: Should the network type (NTN or TN) be indicated explicitly for neighbour cells? If yes, please indicate how. If not, please indicate why.** | | |
| **Company** | **Yes/No** | **Motivation** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary for Question 2:

<blank>

Regarding Proposal 2 (*NTN scenario information (e.g. LEO/GEO) is not signalled explicitly, but inferred from the contents of the ephemeris. FFS which exact parameters are sufficient and whether this behavior needs to be specified*), we would like to highlight there was a massive support for such approach in [1], namely 24 out of 26 companies were OK to progress with no explicit signalling of NTN scenario type. As described in [1], there are numerous ways to distinguish the scenarios, based on some scenario-specific parameters (such as compensation values, etc.) or contents of the ephemeris. Even if the ephemeris for neighbour cells will be of reduced size and limited in detail, compared to the serving cell’s ephemeris, it shall still be sufficient to recognize the scenario and allow the UE to identify if the cell is e.g. LEO or GEO. Furthermore, the usual approach shall be to confirm the issue and convince all RAN2 companies new parameter(s) for such indication is/are needed. So far, based on [1] and related discussions, the overwhelming majority in RAN2 believes the UE can recognize the scenario in multiple ways. Thus, we suggest RAN2 proceeds with such agreement for the time being and revise it only if during the remainder of the WI it is identified and proven implicit indication is insufficient.

|  |  |  |
| --- | --- | --- |
| **Question 3: Do you agree implicit indication of NTN scenario is enough for Rel-17 work? It can be revised if during the remainder of the WI it is proven implicit indication is not sufficient.** | | |
| **Company** | **Yes/No** | **Motivation** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary for Question 3:

<blank>

# 3 Cell reselection related enhancements

Another part of this e-mail thread is to discuss the subset of proposals in [2][3][4][5] which are related to cell expiry time and upcoming cell info, to be used for cell (re)selection and other IDLE mode procedures. A related aspect is that such information, if agreed, could be provided via ephemeris. In [1] there were mixed views provided whether such timing information on when the cell is going to stop/another is going to start serving the area is essential for cell reselection, with a slight majority saying it is not needed. However, the level of interest in having such mechanism, based on the submitted papers, still appears to be quite high.

In [2] and [3] the authors suggest the awareness of cell expiry time shall be considered for cell selection/reselection and triggering the intra-frequency/inter-frequency measurements. Both papers argue RSRP/RSRQ measurements are insufficient for cell reselection and also suggest to consider UE’s location [2] or the distance between the UE and the satellite or cell center [3].

Even though lots of details in this area have been discussed multiple times (e.g. in [1]), we would like to make another attempt, with tiny step at a time and starting from a different angle.

|  |  |  |
| --- | --- | --- |
| **Question 4: Should the UE be provided with the information on when a cell is going to stop serving the area and the timing information about new upcoming cell? Please indicate how it is provided (e.g. system information, ephemeris, etc.)** | | |
| **Company** | **Yes/No** | **Motivation** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary for Question 4:

<blank>

If you have answered ‘Yes’ to Question 4, please further indicate how such information is used (e.g. cell reselection, idle mode measurements triggering, etc.)

|  |  |
| --- | --- |
| **Question 5: How is the information on when a cell is going to stop serving the area and the timing information about new upcoming cell used? E.g. for cell reselection, idle mode measurements triggering, etc. Please indicate also the applicable scenarios (e.g. Earth-moving, Earth-fixed cells).** | |
| **Company** | **Answer** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Summary for Question 5:

<blank>

In each of the considered papers [2][3][4][5], the use of UE’s geolocation for IDLE mode procedures (such as cell reselection) is mentioned. It is either suggested on the general level [2] or with more detailed implementation details, such as using the distance between the UE and the satellite or cell center [3][4][5]. Companies are therefore asked to share their views whether UE’s geolocation shall be used for IDLE mode procedures and in what form.

|  |  |  |
| --- | --- | --- |
| **Question 6: Should the UE’s geolocation information be used for IDLE mode procedures? If yes, please indicate how is it used and for which procedures.** | | |
| **Company** | **Yes/No** | **Motivation** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary for Question 6:

<blank>

# 4 Conclusions

Based on the views expressed in the previous sections, we propose the following:

Proposals

# 5 List of referenced documents

[1] [R2-2100527](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100527.zip) *Report from [Post112-e][153][NTN] Idle mode aspects (Nokia)* 3GPP TSG-RAN WG2 Meeting #113 Electronic Elbonia, 25th of January – 5th of February 2021

[2] [R2-2100347](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100347.zip) *Idle mode aspects for NTN* 3GPP TSG-RAN WG2 Meeting #113 Electronic Elbonia, 25th of January – 5th of February 2021

[3] [R2-2101196](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2101196.zip) *Discussion on cell selection and reselection in NTN* 3GPP TSG-RAN WG2 Meeting #113 Electronic Elbonia, 25th of January – 5th of February 2021

[4] [R2-2100382](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100382.zip) *Idle mode operation in NTN* 3GPP TSG-RAN WG2 Meeting #113 Electronic Elbonia, 25th of January – 5th of February 2021

[5] [R2-2100163](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100163.zip) *Discussion on idle/inactive mode procedures in NTN* 3GPP TSG-RAN WG2 Meeting #113 Electronic Elbonia, 25th of January – 5th of February 2021

# Contact information

|  |  |
| --- | --- |
| Company | Delegate contact |
| COMPANY\_NAME | NAME ([email@address.com](mailto:email@address.com)) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |