3GPP TSG-RAN WG2 Meeting#113-e Draft\_R2-2102017

Online, January 25th - February 5th 2021

Agenda Item: 8.12.2.2

Source: Huawei

Title: Summary of offline 107 - [REDCAP] L2 capabilities and UE types

Document for: Discussion and Decision

# Introduction

This document is for the following offline discussion on L2 capabilities and UE types:

* [AT113-e][107][REDCAP] L2 capabilities and UE types (Huawei)

 Scope: based on the proposals in [R2-2101255](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2101255%20Higher%20layer%20capabilities%20and%20procedural%20impacts%20of%20RedCap%20UE.doc), [R2-2100310](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2100310_Definition%20of%20RedCap%20UEs.docx) and [R2-2100460](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2100460_UE%20type%20definition%20and%20constraining%20for%20RedCap%20UEs.doc), discuss:

1. which "reduced L2 capabilities" can be listed as possible enhancements in the TR
2. which impacts on procedures for RedCap UEs can be described in the TR
3. which pros and cons to have only one vs multiple RedCap UE types can be listed in the TR

For all the aspects (and namely for 3), the intention of this offline is to describe options and implications in the TR, not to down-select any alternatives

Initial intended outcome: Summary of the offline discussion with:

* + - List of proposals for agreement
		- List of proposals that require online discussions
		- Corresponding TP for the TR

Initial deadline (for companies' feedback): Monday 2021-02-01 11:00 UTC

Initial deadline (for rapporteur's summary in R2-2102017): Monday 2021-02-01 17:00 UTC

Proposals marked "for agreement" in R2-2102017 not challenged until Tuesday 2020-02-02 10:00 UTC will be declared as agreed by the session chair. For the rest the discussion will continue online.

This offline discussion is based on the proposals in the following contributions:

R2-2101255 Higher layer capabilities and procedural impacts of RedCap UE Huawei, HiSilicon

R2-2100310 Definition of RedCap UEs Qualcomm Incorporated

R2-2100460 UE type defination and constraining for RedCap UEs vivo, Guangdong Genius

# Discussion

The following issues will be discussed according to the scope of this offline discussion:

* Reduced L2 capabilities
* Impacts on procedures for RedCap UEs
* Pros/cons to have only one RedCap UE type v.s. multiple RedCap UE types

According to the chairman guidance, the intention of this offline is to describe options and implications in the TR.

## Reduced L2 capabilities

In RAN2#111e meeting, it was agreed that the reduction of upper layer capabilities is FFS:

FFS:

1. Whether reduction of upper layer capabilities should be considered is FFS (in any case no email discussion until the next meeting on this)

Regarding reduction of upper layer capabilities, proposals from above contributions are listed below:

|  |  |  |
| --- | --- | --- |
| **Tdoc number** | **Company name** | **Proposals** |
| R2-2100310 | Qualcomm Incorporated | Proposal 3. Make the following upper-layer UE capabilities optional for RedCap UEs:* Maximum number of DRBs;
* Total layer-2 buffer size;
* 18-bit sequence number field for PDCP and RLC AM;
* RRC processing delay.
 |
| R2-2101255 | Huawei, HiSilicon | Proposal 1: Consider to reduce the number of DRBs to be mandatorily supported for RedCap UE and allow the UE to report the number of supported DRBs.Proposal 2: Consider to reduce the length of PDCP and RLC AM SN to be mandatorily supported for RedCap UE (e.g. mandatory 12-bit SN). |

In summary, reduction for the following four higher layer capabilities are proposed:

* Maximum number of DRBs;
* Total layer-2 buffer size;
* 18-bit sequence number field for PDCP and RLC AM;
* RRC processing delay.

Companies are invited to provide comments on which the above four higher layer capabilities can be reduced.

**Question 1a.** Do you support reducing the maximum number of DRBs mandatory supported by RedCap UEs?

* Yes, how?
* No, why?

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | Yes | We are ok with reduction in number of DRBs, since some RedCap UEs like surveillance do not need many DRBs to support.This can be a capability at the UE. |
| Qualcomm | Yes | We notice that many use cases for RedCap UEs (e.g. sensors or low end wearables) do not need the current maximum number of DRBs (8), which was selected based on the need of premium eMBB UEs. Since maximum number of DRBs directly affects the buffer size requirement of a UE chip, smaller maximum number of DRBs can help reduce the buffer size and hence the cost of a RedCap UE.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 1b.** Do you support reducing the total layer-2 buffer size for RedCap UEs compared with the value required by Section 4.1.4 in TS 38.306?

* Yes, how?
* No, why?

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | We are ok with this but | L2 buffer size is anyway something that the gNB can use as a parameter in scheduling. And since there is no CA or DC, it’s even simpler now and it’s transparent to how the UE implements this. So we are not sure what needs to be changed even with a reduction in DRBs. |
| Qualcomm | Yes | Total lay-2 buffer size is used by gNB for scheduling. What we have found in field studies is that for most applications, especially those do not have high data rates, do not need the entire L2 buffer specified in 38.306 to achieve good throughput. Relaxing this requirement hence can help reduce buffer size and hence cost of RedCap UEs. This reduction can be signalled as a fraction (e.g. 50%) of the “theoretical” total L2 buffer size as a UE capability to network.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 1c.** Do you support to make support of 18-bit sequence number field for PDCP and RLC AM optional for RedCap UEs?

* Yes, how?
* No, why?

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | Yes | With no CA/DC, 18-bit is not necessary |
| Qualcomm | Yes | 18-bit SN is needed only by high data rate applications. The longer the SN is, the bigger buffer UE needs to have to support the sliding window operations in PDCP/RLC. Since RedCap UEs are not expected to have high data rates (e.g. no CA or DC), 18-bit SN field becomes unnecessary. RedCap can use the 12-bit SN instead (currently optional for R15/16). |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 1d.** Do you support relaxing the RRC processing delay for RedCap UEs?

* Yes, how?
* No, why?

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | Yes | We need to discuss the details but we agree with increased processing times. |
| Qualcomm | Yes | NR reduced RRC processing time (compared to LTE) to better support low latency applications such as URLLC. However, most RedCap use cases do not have low latency requirement. Reducing RRC processing time do not have much impact on UEs’ control-plane performance but can relax their requirement on processor. This relaxation can be signaled as a scaling factor (e.g. 1.25x) on top of R15’s mandatory RRC processing time, via UE capability signaling. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Impacts on procedures for RedCap UEs

In RAN2#111e meeting, the following agreement was made for the impacts on procedures for RedCap UEs:

Depending on RAN1 input, discussion is expected at least on the following impacts on RAN2 procedures:

 a. Impact on cell (re)selection

 b. Impact on initial access

 c. Impact on other idle mode procedures (i.e. SI acquisition, paging)

In above contributions, the following observations on procedural impacts were made and it was proposed to capture them in the TR:

|  |  |  |
| --- | --- | --- |
| **Tdoc number** | **Company name** | **Proposals** |
| R2-2101255 | Huawei, HiSilicon | Observation 1: RedCap UE may consume more power than non-RedCap UE during cell search and cell re-selection.Observation 2: If RedCap UEs share PO with non-RedCap UE, the power consumption of RedCap UEs may be impacted because of false probability and unnecessary SIB1 reading.Observation 3: RedCap UE needs measurement GAP for serving cell measurement with higher probability than non-RedCap UE.Proposal 3: Capture above observations into the TR. |

**Observation 1: RedCap UE may consume more power than non-RedCap UE during cell search and cell re-selection.**

**Question 2a. Do you agree with observation 1?**

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | yes | With reduced Rx/tx, more effort might be needed by redcap UEs to read broadcast info. |
| Qualcomm | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Observation 2: If RedCap UEs share PO with non-RedCap UE, the power consumption of RedCap UEs may be impacted because of false probability and unnecessary SIB1 reading.**

**Question 2b. Do you agree with observation 2?**

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | Yes |  |
| Qualcomm | Yes | This issue is not necessarily specific to RedCap. The paging enhancements discussed in R17 Power saving are applicable to RedCap too.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Observation 3: RedCap UE needs measurement GAP for serving cell measurement with higher probability than non-RedCap UE.**

**Question 2c. Do you agree with observation 3?**

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Yes/No*** | ***Comments*** |
| Apple | Yes | 1Tx/1Rx results in this for eg. |
| Qualcomm | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## One v.s. multiple RedCap UE type(s) (Pros/Cons)

Regarding how many type(s) should be defined for RedCap UEs, proposals from above contributions are listed below:

|  |  |  |
| --- | --- | --- |
| **Tdoc number** | **Company name** | **Proposals** |
| R2-2100310 | Qualcomm Incorporated | Proposal 1. Only a single RedCap UE type (per FR) is defined. |
| R2-2100460 | vivo, Guangdong Genius | Proposal 1: Two UE types/categories should be defined for RedCap devices to cover various use cases: high-end and low-end devices.Proposal 2: Two UE types/categories for RedCap devices can be defined based on the UE features (e.g. Bandwidth, antenna number, etc.). Detailed reduced capability could be discussed and decided in WI. |

The number of RedCap UE type(s) has been discussed in the previous RAN2 meetings and the following principle has been agreed in RAN2#111e:

1. The number of device types should be minimised, to reduce market fragmentation, and introduced only where essential to control UE accesses and differentiate them from legacy R15/R16 and non-Redcap R17 UEs, (e.g. number of Tx/Rx antennas, maximum supportable BW, etc.). The exact composition of the set of L1 capabilities of the device type can be discussed by RAN1

The discussion here is not for down-selection but for elaborating pros/cons for both options, i.e. only one UE type v.s. multiple UE types.

**Question 3.** Companies are invited to provide comments on pros/cons to have only one v.s. multiple RedCap UE type(s).

|  |  |  |
| --- | --- | --- |
| ***Company name*** | ***Only one RedCap UE type*** | ***Multiple RedCap UE types*** |
|  | * Pros:
* Cons:
 | * Pros:
* Cons:
 |
| Apple | We prefer to not fragment. Anyway the capabilities would be exchanged to know the different “types” of RedCap, and for initial access, all RedCapUEs are required to support a min BW. We do not see the need to define more types. Also, RAN1 is also discussing this, and their input needs to be considered. |  |
| Qualcomm | For access, we think a single UE type is sufficient for network to enforce access restriction (ensure RedCap is used only for its intended use cases). Once UE is connected, network can learn different capability levels of RedCap UEs from capability signaling.Have a single UE type is simple, avoid market segmentation. Although a single UE type is defined, one can still potentially support an infinite number of feature permutations in the market, through NR’s capability framework.  | Defining multiple UE types means that 3GPP would have to take on the role of product management and identify specific product segments to determine where to draw the line between different UE types. In our view, that’s outside 3GPP’s scope. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Summary

TBD

# Conclusion

This offline discussion focused on L2 capabilities and UE types for REDCAP:

**TBD**

# Contact delegates

|  |  |  |
| --- | --- | --- |
| **Delegate** | **Company name** | **Email** |
| Linhai He | Qualcomm | linhaihe@qti.qualcomm.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |