**3GPP TSG- Meeting #**

**,**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **3** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , Qualcomm, NTT DoCoMo | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core, TEI16 | | | | |  | ***Date:*** | | | 2021-03-31 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **C** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Multimedia Priority Service (MPS) provides priority treatment to increase the probability of an authorized Service User’s Voice, Video, and Data communication. It is important that a UE involved in an MPS session continues the MPS session with priority upon successfully reconnected in 5GS or EPS following an RRC release with redirect. A UE can be in an MPS session in one of the following three ways:   1. An authorized Service User using a UE with an MPS subscription can initiate MPS when it originates a session (See TS 22.153 clause 5.1). In the case of 5GS, the UE is assigned Access Identity 1 (AI1) and is entitled to the special Establishment Cause (mps-PriorityAccess) and priority treatment when it originates a session. In case of EPC, the UE is assigned Access Class 14 and is entitled to the special Establishment Cause (highPriorityAccess) and priority treatment when it originates a session. 2. Unauthorized Service User using a UE that does not have an MPS subscription can initiate MPS for an originating session but priority treatment is only obtained after MPS is established for the session (See TS 22.153 clause 5.1). In this case the priority treatment is based on network control of the priority session as opposed to the UE subscription to MPS. 3. A terminating UE receives priority treatment for an incoming MPS session independent of whether the terminating UE has a subscription for MPS (See TS 22.153 clause 5.4). In this case the terminating UE receives priority treatment as for the above originating cases.   This CR addresses the 2nd and 3rd cases: When the originating/terminating UE of an MPS session has to redirect (to another cell in NR or to E-UTRA), it is entitled to maintain MPS priority treatment on the ongoing MPS session. The redirection decision is performed by the gNB/eNB/ng-eNB. The UE that needs to redirect to another cell, another RAT or another core network to receive service, should be able to connect to the target network at the RRC layer with MPS priority following the release with redirection. Currently, the RRC layer at the UE without an MPS subscription is not aware of an MPS priority session in the network and does not connect to the network with MPS priority at the RRC layer following a release with redirection.  This MPS redirection procedure is applicable to an ongoing MPS session for which the gNB/eNB/ng-eNB forces the UE to release with redirection. It is assumed that the gNB/eNB/ng-eNB is aware of the MPS session via the ARP value and/or the QoS characteristics of the MPS session. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | When the network performs a release with redirection, for UEs with MPS priority session(s), the network includes an MPS priority indication in the RRCRelease message. When connecting to the target network and if the connection establishment is the result of release with redirect with *mpsPriorityIndication*, the UE sets the RRC Establishment Cause to *mps-PriorityAccess* if the target RAN is NR and to *highPriorityAccess* if the target is E-UTRA.  First change:  If the UE has an indication of MPS priority for redirection, the UE sets the RRC Establishment Cause to *highPriorityAccess* to indicate to the network that the request is to be handled with high priority.  Second change:  The UE access attempt shall not be barred if the connection establishment is the result of release with redirection with *mpsPriorityIndication* and access barring for AC=14 is not in effect.  Third change:  The UE access attempt shall not be barred if the connection establishment is the result of release with redirection with *mpsPriorityIndication* and access barring for MPS priority is not in effect.  Fourth change:  Adds the MPS priority indication to the RRCConnectionRelease message.  **Impact Analysis**:  Impacted 5G architecture option:  NR-SA  Impacted functionality:  Redirection from NR to: LTE/EPC, LTE/5GC.  Redirection from LTE/5GC to NR or LTE/EPC, LTE/EPC to NR, within LTE/5GC, within LTE/EPC.  Inter-operability:   * If the network is implemented according to the CR and the UE is not; There is no inter-operability issue. The UE will ignore the *mpsPriorityIndication* and its redirection will occur without receiving MPS priority treatment in its new RRC connection. * If the UE is implemented according to the CR and the network is not;   There is no inter-operability issue. The UE will not receive an indication from the network at the time of redirection; the UE will execute a normal redirection per standard. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | A user authorized to receive MPS priority service when using a UE that has no MPS subscription will not have MPS priority following a release with redirection. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.3.3, 5.3.3.11, 5.3.16.5, 6.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.331 CR 2413  TS 36.306 CR 1804  TS 38.306 CR 0526 | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR … CR … | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Rev 3 adds cover page editorial fixes and normative text improvements; Rev 2 points to new TS 36.331 v16.4.0; Rev1 adds the 2nd change and the TS 36.306 being affected | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | R2-2102232, R2- 2101476, R2-2103042 | | | | | | | | |

#### \*\*\*\*\* First change \*\*\*\*\*

#### 5.3.3.3 Actions related to transmission of *RRCConnectionRequest* message

The UE shall set the contents of *RRCConnectionRequest* message as follows:

1> if the UE is connected to EPC:

2> set the *ue-Identity* as follows:

3> if upper layers provide an S-TMSI:

4> set the *ue-Identity* to the value received from upper layers;

3> else:

4> draw a random value in the range 0 .. 240-1 and set the *ue-Identity* tothis value;

NOTE 1: Upper layers provide the S-TMSI if the UE is registered in the TA of the current cell.

2> if the establishment of the RRC connection is the result of release with redirect with *mpsPriorityIndication;*

3> set the establishmentCause to *highPriorityAccess*;

2> else:

3> if the UE supports *mo-VoiceCall* establishment cause and UE is establishing the RRC connection for mobile originating MMTEL voice and *SystemInformationBlockType2* includes *voiceServiceCauseIndication* and the establishment cause received from upper layers is not set to *highPriorityAccess*; or

3> if the UE supports *mo-VoiceCall* establishment cause and EPS fallback for IMS voice (see TS 23.502 [102]) was triggered in NR via *RRCRelease* with *voiceFallbackIndication* (see TS 38.331 [82]) and *SystemInformationBlockType2* includes *voiceServiceCauseIndication* and the establishment cause received from upper layers is not set to *highPriorityAccess* or *emergency*:

4> set the *establishmentCause* to *mo-VoiceCall*;

3> else if the UE supports *mo-VoiceCall* establishment cause for mobile originating MMTEL video and UE is establishing the RRC connection for mobile originating MMTEL video and *SystemInformationBlockType2* includes *videoServiceCauseIndication* and the establishment cause received from upper layers is not set to *highPriorityAccess*:

4> set the *establishmentCause* to *mo-VoiceCall*;

3> else:

4> set the *establishmentCause* in accordance with the information received from upper layers;

1> if the UE is connected to 5GC:

2> set the *ue-Identity* as follows:

3> if upper layers provide a 5G-S-TMSI:

4> except for NB-IoT, set the ue-Identity to ng-5G-S-TMSI-Part1;

4> for NB-IoT, set the *ue-Identity* to ng-5G-S-TMSI;

3> else:

4> draw a random value in the range 0 .. 240-1 and set the *ue-Identity* to this value;

2> if the establishment of the RRC connection is the result of release with redirect with *mpsPriorityIndication;*

3> set the establishmentCause to *highPriorityAccess*;

2> else set the *establishmentCause* in accordance with the information received from upper layers;

2> except for NB-IoT, apply the default NR PDCP configuration as specified in TS 38.331 [82], clause 9.2.1.1 for SRB1;

2> except for NB-IoT, use NR PDCP for all subsequent messages received and sent by the UE via SRB1;

1> if the UE is a NB-IoT UE:

2> if the UE is connected to EPC:

3> if the UE supports multi-tone transmission, include *multiToneSupport*;

3> if the UE supports multi-carrier operation, include *multiCarrierSupport*;

3> set *earlyContentionResolution* to TRUE;

2> if the UE supports DL channel quality reporting in MSG3 and *cqi-Reporting* is present in *SystemInformationBlockType2-NB*:

3> set the *cqi-NPDCCH* to include the latest results of the downlink channel quality measurements of the carrier where the random access response is received as specified in TS 36.133 [16];

NOTE 2: The downlink channel quality measurements use measurement period T1 or T2, as defined in TS 36.133 [16].

1> if the UE is initiating transmission using PUR in accordance with conditions in 5.3.3.1c:

2> configure, except *pur-TimeAlignmentTimer*, the lower layers to use transmission using PUR;

2> deliver the UL grant for transmission using PUR to the MAC entity;

The UE shall submit the *RRCConnectionRequest* message to lower layers for transmission.

The UE shall continue cell re-selection related measurements as well as cell re-selection evaluation. If the conditions for cell re-selection are fulfilled, the UE shall perform cell re-selection as specified in 5.3.3.5.

#### \*\*\*\*\* Second change \*\*\*\*\*

#### 5.3.3.11 Access barring check

1> if timer T302 or "Tbarring" is running:

2> consider access to the cell as barred;

1> else if *SystemInformationBlockType2* includes "AC barring parameter":

2> if the UE has one or more Access Classes, as stored on the USIM, with a value in the range 11..15, which is valid for the UE to use according to TS 22.011 [10] and TS 23.122 [11], and

NOTE: ACs 12, 13, 14 are only valid for use in the home country and ACs 11, 15 are only valid for use in the HPLMN/ EHPLMN.

2> for at least one of these valid Access Classes the corresponding bit in the *ac-BarringForSpecialAC* contained in "AC barring parameter" is set to *zero*:

3> consider access to the cell as not barred;

2> else if the the establishment of the RRC connection is the result of release with redirect with *mpsPriorityIndication*; and

2> the corresponding bit for Access Class 14 in the *ac-BarringForSpecialAC* contained in "AC barring parameter" is set to *zero*:

3> consider access to the cell as not barred;

2> else:

3> draw a random number '*rand*' uniformly distributed in the range: 0 ≤ *rand* < 1;

3> if '*rand*' is lower than the value indicated by *ac-BarringFactor* included in "AC barring parameter":

4> consider access to the cell as not barred;

3> else:

4> consider access to the cell as barred;

1> else:

2> consider access to the cell as not barred;

1> if access to the cell is barred and both timers T302 and "Tbarring" are not running:

2> draw a random number '*rand*' that is uniformly distributed in the range 0 ≤ *rand* < 1;

2> start timer "Tbarring" with the timer value calculated as follows, using the *ac-BarringTime* included in"AC barring parameter":

"Tbarring" = (0.7+ 0.6 \* *rand*) \* *ac-BarringTime*;

#### \*\*\*\*\* Third change \*\*\*\*\*

#### 5.3.16.5 Access barring check

The UE shall:

1> if one or more Access Identities are indicated according to TS 24.501 [95], and

1> if for at least one of these Access Identities the corresponding bit in the *uac-BarringForAccessIdentity* contained in "UAC barring parameter" is set to *zero*:

2> consider the access attempt as allowed;

1> else:

2> if the establishment of the RRC connection is the result of relase with redirect with *mpsPriorityIndication*; and

2> if the bit corresponding to Access Identity 1 in the *uac-BarringForAccessIdentity* contained in the "UAC barring parameter" is set to zero:

3> consider the access attempt as allowed;

2> else:

3> draw a random number '*rand*' uniformly distributed in the range: 0 ≤ *rand* < 1;

3> if '*rand*' is lower than the value indicated by *uac-BarringFactor* included in "UAC barring parameter":

4> consider the access attempt as allowed;

3> else:

4> consider the access attempt as barred;

1> if the access attempt is considered as barred:

2> draw a random number '*rand*' that is uniformly distributed in the range 0 ≤ *rand* < 1;

2> start timer T309 for the Access Category with the timer value calculated as follows, using the *uac-BarringTime* included in"AC barring parameter":

"Tbarring" = (0.7+ 0.6 \* *rand*) \* *uac-BarringTime*;

#### \*\*\*\*\* Fourth change \*\*\*\*\*

#### – *RRCConnectionRelease*

The *RRCConnectionRelease* message is used to command the release of an RRC connection, or to complete an UP-EDT procedure.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: E‑UTRAN to UE

*RRCConnectionRelease message*

-- ASN1START

RRCConnectionRelease ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

c1 CHOICE {

rrcConnectionRelease-r8 RRCConnectionRelease-r8-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

RRCConnectionRelease-r8-IEs ::= SEQUENCE {

releaseCause ReleaseCause,

redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need ON

idleModeMobilityControlInfo IdleModeMobilityControlInfo OPTIONAL, -- Need OP

nonCriticalExtension RRCConnectionRelease-v890-IEs OPTIONAL

}

RRCConnectionRelease-v890-IEs ::= SEQUENCE {

lateNonCriticalExtension OCTET STRING (CONTAINING RRCConnectionRelease-v9e0-IEs) OPTIONAL,

nonCriticalExtension RRCConnectionRelease-v920-IEs OPTIONAL

}

-- Late non critical extensions

RRCConnectionRelease-v9e0-IEs ::= SEQUENCE {

redirectedCarrierInfo-v9e0 RedirectedCarrierInfo-v9e0 OPTIONAL, -- Cond NoRedirect-r8

idleModeMobilityControlInfo-v9e0 IdleModeMobilityControlInfo-v9e0 OPTIONAL, -- Cond IdleInfoEUTRA

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

RRCConnectionRelease-v920-IEs ::= SEQUENCE {

cellInfoList-r9 CHOICE {

geran-r9 CellInfoListGERAN-r9,

utra-FDD-r9 CellInfoListUTRA-FDD-r9,

utra-TDD-r9 CellInfoListUTRA-TDD-r9,

...,

utra-TDD-r10 CellInfoListUTRA-TDD-r10

} OPTIONAL, -- Cond Redirection

nonCriticalExtension RRCConnectionRelease-v1020-IEs OPTIONAL

}

RRCConnectionRelease-v1020-IEs ::= SEQUENCE {

extendedWaitTime-r10 INTEGER (1..1800) OPTIONAL, -- Need ON

nonCriticalExtension RRCConnectionRelease-v1320-IEs OPTIONAL

}

RRCConnectionRelease-v1320-IEs::= SEQUENCE {

resumeIdentity-r13 ResumeIdentity-r13 OPTIONAL, -- Need OR

nonCriticalExtension RRCConnectionRelease-v1530-IEs OPTIONAL

}

RRCConnectionRelease-v1530-IEs ::= SEQUENCE {

drb-ContinueROHC-r15 ENUMERATED {true} OPTIONAL, -- Cond UP-EDTorPUR

nextHopChainingCount-r15 NextHopChainingCount OPTIONAL, -- Cond EarlySec

measIdleConfig-r15 MeasIdleConfigDedicated-r15 OPTIONAL, -- Need ON

rrc-InactiveConfig-r15 RRC-InactiveConfig-r15 OPTIONAL, -- Need OR

cn-Type-r15 ENUMERATED {epc,fivegc} OPTIONAL, -- Need OR

nonCriticalExtension RRCConnectionRelease-v1540-IEs OPTIONAL

}

RRCConnectionRelease-v1540-IEs ::= SEQUENCE {

waitTime INTEGER (1..16) OPTIONAL, -- Cond 5GC

nonCriticalExtension RRCConnectionRelease-v15b0-IEs OPTIONAL

}

RRCConnectionRelease-v15b0-IEs ::= SEQUENCE {

noLastCellUpdate-r15 ENUMERATED {true} OPTIONAL, -- Need OP

nonCriticalExtension RRCConnectionRelease-v1610-IEs OPTIONAL

}

RRCConnectionRelease-v1610-IEs ::= SEQUENCE {

fullI-RNTI-r16 I-RNTI-r15 OPTIONAL, -- Need OR

shortI-RNTI-r16 ShortI-RNTI-r15 OPTIONAL, -- Need OR

pur-Config-r16 SetupRelease {PUR-Config-r16} OPTIONAL, -- Need ON

rrc-InactiveConfig-v1610 RRC-InactiveConfig-v1610 OPTIONAL, -- Cond BLCE-IDLEeDRX

releaseIdleMeasConfig-r16 ENUMERATED {true} OPTIONAL, -- Need ON

altFreqPriorities-r16 ENUMERATED {true} OPTIONAL, -- Need ON

t323-r16 ENUMERATED {

min5, min10, min20, min30, min60, min120, min180,

min720} OPTIONAL, -- Need OR

nonCriticalExtension RRCConnectionRelease-v16xy-IEs OPTIONAL

}

RRCConnectionRelease-v16xy-IEs ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Need OR

nonCriticalExtension SEQUENCE {} OPTIONAL

}

ReleaseCause ::= ENUMERATED {loadBalancingTAUrequired,

other, cs-FallbackHighPriority-v1020, rrc-Suspend-v1320}

RedirectedCarrierInfo ::= CHOICE {

eutra ARFCN-ValueEUTRA,

geran CarrierFreqsGERAN,

utra-FDD ARFCN-ValueUTRA,

utra-TDD ARFCN-ValueUTRA,

cdma2000-HRPD CarrierFreqCDMA2000,

cdma2000-1xRTT CarrierFreqCDMA2000,

...,

utra-TDD-r10 CarrierFreqListUTRA-TDD-r10,

nr-r15 CarrierInfoNR-r15

}

RedirectedCarrierInfo-v9e0 ::= SEQUENCE {

eutra-v9e0 ARFCN-ValueEUTRA-v9e0

}

RRC-InactiveConfig-r15::= SEQUENCE {

fullI-RNTI-r15 I-RNTI-r15,

shortI-RNTI-r15 ShortI-RNTI-r15,

ran-PagingCycle-r15 ENUMERATED { rf32, rf64, rf128, rf256} OPTIONAL, --Need OR

ran-NotificationAreaInfo-r15 RAN-NotificationAreaInfo-r15 OPTIONAL, --Need ON

periodic-RNAU-timer-r15 ENUMERATED {min5, min10, min20, min30, min60,

min120, min360, min720} OPTIONAL, --Need OR

nextHopChainingCount-r15 NextHopChainingCount OPTIONAL, --Cond INACTIVE

dummy SEQUENCE{} OPTIONAL

}

RRC-InactiveConfig-v1610::= SEQUENCE {

ran-PagingCycle-v1610 ENUMERATED {rf512, rf1024}

}

RAN-NotificationAreaInfo-r15 ::= CHOICE {

cellList-r15 PLMN-RAN-AreaCellList-r15,

ran-AreaConfigList-r15 PLMN-RAN-AreaConfigList-r15

}

PLMN-RAN-AreaCellList-r15 ::= SEQUENCE (SIZE (1..maxPLMN-r15)) OF PLMN-RAN-AreaCell-r15

PLMN-RAN-AreaCell-r15 ::= SEQUENCE {

plmn-Identity-r15 PLMN-Identity OPTIONAL,

ran-AreaCells-r15 SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList-r15 ::= SEQUENCE (SIZE (1..maxPLMN-r15)) OF PLMN-RAN-AreaConfig-r15

PLMN-RAN-AreaConfig-r15 ::= SEQUENCE {

plmn-Identity-r15 PLMN-Identity OPTIONAL,

ran-Area-r15 SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig-r15

}

RAN-AreaConfig-r15 ::= SEQUENCE {

trackingAreaCode-5GC-r15 TrackingAreaCode-5GC-r15,

ran-AreaCodeList-r15 SEQUENCE (SIZE (1..32)) OF RAN-AreaCode-r15 OPTIONAL --Need OR

}

CarrierFreqListUTRA-TDD-r10 ::= SEQUENCE (SIZE (1..maxFreqUTRA-TDD-r10)) OF ARFCN-ValueUTRA

IdleModeMobilityControlInfo ::= SEQUENCE {

freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need ON

freqPriorityListGERAN FreqsPriorityListGERAN OPTIONAL, -- Need ON

freqPriorityListUTRA-FDD FreqPriorityListUTRA-FDD OPTIONAL, -- Need ON

freqPriorityListUTRA-TDD FreqPriorityListUTRA-TDD OPTIONAL, -- Need ON

bandClassPriorityListHRPD BandClassPriorityListHRPD OPTIONAL, -- Need ON

bandClassPriorityList1XRTT BandClassPriorityList1XRTT OPTIONAL, -- Need ON

t320 ENUMERATED {

min5, min10, min20, min30, min60, min120, min180,

spare1} OPTIONAL, -- Need OR

...,

[[ freqPriorityListExtEUTRA-r12 FreqPriorityListExtEUTRA-r12 OPTIONAL -- Need ON

]],

[[ freqPriorityListEUTRA-v1310 FreqPriorityListEUTRA-v1310 OPTIONAL, -- Need ON

freqPriorityListExtEUTRA-v1310 FreqPriorityListExtEUTRA-v1310 OPTIONAL -- Need ON

]],

[[ freqPriorityListNR-r15 FreqPriorityListNR-r15 OPTIONAL -- Need ON

]]

}

IdleModeMobilityControlInfo-v9e0 ::= SEQUENCE {

freqPriorityListEUTRA-v9e0 SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v9e0

}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListExtEUTRA-r12 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-r12

FreqPriorityListEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityListExtEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityEUTRA ::= SEQUENCE {

carrierFreq ARFCN-ValueEUTRA,

cellReselectionPriority CellReselectionPriority

}

FreqPriorityEUTRA-v9e0 ::= SEQUENCE {

carrierFreq-v9e0 ARFCN-ValueEUTRA-v9e0 OPTIONAL -- Cond EARFCN-max

}

FreqPriorityEUTRA-r12 ::= SEQUENCE {

carrierFreq-r12 ARFCN-ValueEUTRA-r9,

cellReselectionPriority-r12 CellReselectionPriority

}

FreqPriorityEUTRA-v1310 ::= SEQUENCE {

cellReselectionSubPriority-r13 CellReselectionSubPriority-r13 OPTIONAL -- Need ON

}

FreqPriorityListNR-r15 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR-r15

FreqPriorityNR-r15 ::= SEQUENCE {

carrierFreq-r15 ARFCN-ValueNR-r15,

cellReselectionPriority-r15 CellReselectionPriority,

cellReselectionSubPriority-r15 CellReselectionSubPriority-r13 OPTIONAL -- Need OR

}

FreqsPriorityListGERAN ::= SEQUENCE (SIZE (1..maxGNFG)) OF FreqsPriorityGERAN

FreqsPriorityGERAN ::= SEQUENCE {

carrierFreqs CarrierFreqsGERAN,

cellReselectionPriority CellReselectionPriority

}

FreqPriorityListUTRA-FDD ::= SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF FreqPriorityUTRA-FDD

FreqPriorityUTRA-FDD ::= SEQUENCE {

carrierFreq ARFCN-ValueUTRA,

cellReselectionPriority CellReselectionPriority

}

FreqPriorityListUTRA-TDD ::= SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF FreqPriorityUTRA-TDD

FreqPriorityUTRA-TDD ::= SEQUENCE {

carrierFreq ARFCN-ValueUTRA,

cellReselectionPriority CellReselectionPriority

}

BandClassPriorityListHRPD ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriorityHRPD

BandClassPriorityHRPD ::= SEQUENCE {

bandClass BandclassCDMA2000,

cellReselectionPriority CellReselectionPriority

}

BandClassPriorityList1XRTT ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriority1XRTT

BandClassPriority1XRTT ::= SEQUENCE {

bandClass BandclassCDMA2000,

cellReselectionPriority CellReselectionPriority

}

CellInfoListGERAN-r9 ::= SEQUENCE (SIZE (1..maxCellInfoGERAN-r9)) OF CellInfoGERAN-r9

CellInfoGERAN-r9 ::= SEQUENCE {

physCellId-r9 PhysCellIdGERAN,

carrierFreq-r9 CarrierFreqGERAN,

systemInformation-r9 SystemInfoListGERAN

}

CarrierInfoNR-r15 ::= SEQUENCE {

carrierFreq-r15 ARFCN-ValueNR-r15,

subcarrierSpacingSSB-r15 ENUMERATED {kHz15, kHz30, kHz120, kHz240},

smtc-r15 MTC-SSB-NR-r15 OPTIONAL -- Need OP

}

CellInfoListUTRA-FDD-r9 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-FDD-r9

CellInfoUTRA-FDD-r9 ::= SEQUENCE {

physCellId-r9 PhysCellIdUTRA-FDD,

utra-BCCH-Container-r9 OCTET STRING

}

CellInfoListUTRA-TDD-r9 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r9

CellInfoUTRA-TDD-r9 ::= SEQUENCE {

physCellId-r9 PhysCellIdUTRA-TDD,

utra-BCCH-Container-r9 OCTET STRING

}

CellInfoListUTRA-TDD-r10 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r10

CellInfoUTRA-TDD-r10 ::= SEQUENCE {

physCellId-r10 PhysCellIdUTRA-TDD,

carrierFreq-r10 ARFCN-ValueUTRA,

utra-BCCH-Container-r10 OCTET STRING

}

-- ASN1STOP

| *RRCConnectionRelease* field descriptions |
| --- |
| ***altFreqPriorities***  Indicates that the UE shall apply the alternative cell reselectionpriorities, when available. This field is not configured together with *idleModeMobilityControlInfo*. |
| ***carrierFreq or bandClass***  The carrier frequency (UTRA, E-UTRA, and NR) and band class (HRPD and 1xRTT) for which the associated cellReselectionPriority is applied. For NR, the *ARFCN-ValueNR* corresponds to a GSCN value as specified in TS 38.101 [85]. |
| ***carrierFreqs***  The list of GERAN carrier frequencies organised into one group of GERAN carrier frequencies. |
| ***cellInfoList***  Used to provide system information of one or more cells on the redirected inter-RAT carrier frequency. The system information can be used if, upon redirection, the UE selects an inter-RAT cell indicated by the *physCellId* and *carrierFreq* (GERAN and UTRA TDD) or by the *physCellId* (other RATs). The choice shall match the *redirectedCarrierInfo*. In particular, E-UTRAN only applies value *utra-TDD-r10* in case *redirectedCarrierInfo* is set to *utra-TDD-r10*. |
| ***cellList***  Indicates a list of cells configured as RAN area. For each element, in the absence of *plmn-Identity* the UE considers the registered PLMN. Total number of cells across all PLMNs does not exceed 32. |
| ***cn-Type***  The*cn-Type* is used to indicate that the UE is redirected from 5GC to EPC or 5GC when*redirectedCarrierInfo* indicates E-UTRA frequency. |
| ***drb-ContinueROHC***  This field indicates whether to continue or reset the header compression protocol context for the DRBs configured with the header compression protocol. Presence of the field indicates that the header compression protocol context continues when UE initiates UP-EDT in the same cell, while absence indicates that the header compression protocol context is reset. |
| ***dummy***  This field is not used in the specification. If received it shall be ignored by the UE. |
| ***extendedWaitTime***  Value in seconds for the wait time for Delay Tolerant access requests. |
| ***freqPriorityListX***  Provides a cell reselection priority for each frequency, by means of separate lists for each RAT (including E-UTRA). The UE shall be able to store at least 3 occurrences of *FreqsPriorityGERAN*. If E-UTRAN includes *freqPriorityListEUTRA-v9e0* and/or *freqPriorityListEUTRA-v1310* it includes the same number of entries, and listed in the same order, as in *freqPriorityListEUTRA* (i.e. without suffix). Field *freqPriorityListExt* includes additional neighbouring inter-frequencies, i.e. extending the size of the inter-frequency carrier list using the general principles specified in 5.1.2. EUTRAN only includes *freqPriorityListExtEUTRA* if *freqPriorityListEUTRA* (i.e without suffix) includes *maxFreq* entries. If E-UTRAN includes *freqPriorityListExtEUTRA-v1310* it includes the same number of entries, and listed in the same order, as in *freqPriorityListExtEUTRA-r12.* |
| ***idleModeMobilityControlInfo***  Provides dedicated cell reselection priorities. Used for cell reselection as specified in TS 36.304 [4]. For E-UTRA and UTRA frequencies, a UE that supports multi-band cells for the concerned RAT considers the dedicated priorities to be common for all overlapping bands (i.e. regardless of the ARFCN that is used). |
| ***measIdleConfig***  Indicates a one-shot measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***mpsPriorityIndication***  Indicates the UE can set the establishment cause to *highPriorityAccess* for a new connection to a new RAT following a redirect to E-UTRA. If the target RAT is NR, see TS 38.331 [82]. The eNB/ng-eNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the eNB/ng-eNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo*field in the *RRCConnectionRelease* message. |
| ***noLastCellUpdate***  Presence of the field indicates that the last used cell for (G)WUS shall not be updated. |
| ***periodic-RNAU-timer***  Refers to the timer that triggers the periodic RNAU procedure in UE. Value min5 corresponds to 5 minutes, value min10 corresponds to 10 minutes and so on. |
| ***ran-Area***  Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or RAN area code(s) to configure a UE. Total number of TACs across all PLMNs does not exceed 16. Total number of RAN-AreaCode across all PLMNs does not exceed 32. |
| ***ran-NotificationAreaInfo***  Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ranAreaConfigList***  Indicates a list of RAN area codes or RA code(s) as RAN area. For each element, in the absence of *plmn-Identity* the UE considers the registered PLMN. |
| ***ran-pagingCycle***  Refers to the UE specific cycle for RAN-initiated paging. Value rf32 corresponds to 32 radio frames, rf64 corresponds to 64 radio frames and so on. |
| ***redirectedCarrierInfo***  The r*edirectedCarrierInfo* indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an E‑UTRA or an inter-RAT carrier frequency, by means of the cell selection upon leaving RRC\_CONNECTED as specified in TS 36.304 [4]. The value *geran* can only be included after successful security activation when UE is connected to 5GC. |
| ***releaseCause***  The *releaseCause* is used to indicate the reason for releasing the RRC Connection. The cause value *cs-FallbackHighPriority* is only applicable when *redirectedCarrierInfo* is present with the value set to *utra-FDD,* *utra-TDD* or *utra-TDD-r10*. E-UTRAN should not set the *releaseCause* to *loadBalancingTAURequired* or to *cs-FallbackHighPriority* if the *extendedWaitTime* is present. The network should not set the *releaseCause* to *loadBalancingTAURequired* if the UE is connected to 5GC. The network does not set the *releaseCause* to *rrc-Suspend* if the UE is configured with a DAPS bearer, i.e. if source PCell resources after a DAPS handover have not been released. |
| ***releaseIdleMeasConfig***  Indicates that the UE shall release the idle/inactive measurement configurations, if configured. |
| ***rrc-InactiveConfig***  Indicates configuration for the RRC\_INACTIVE state. The network does not configure this field when the UE is redirected to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***smtc***  The SSB periodicity/offset/duration configuration of the redirected target NR frequency. It is based on the timing reference of EUTRAN PCell. If the field is absent, the UE uses the SMTC configured in the *measObjectNR* having the same SSB frequency and subcarrier spacing |
| ***subcarrierSpacingSSB***  Indicate subcarrier spacing of SSB of redirected target NR frequency. Only the values 15 or 30 (<6GHz), 120 kHz or 240 kHz (>6GHz) are applicable. |
| ***systemInformation***  Container for system information of the GERAN cell i.e. one or more System Information (SI) messages as defined in TS 44.018 [45], table 9.1.1. |
| ***t320***  Timer T320 as described in clause 7.3. Value minN corresponds to N minutes. |
| ***t323***  Timer T323 as described in clause 7.3. Value minN corresponds to N minutes. |
| ***utra-BCCH-Container***  Contains System Information Container message as defined in TS 25.331 [19]. |
| ***waitTime***  Wait time value in seconds. |

| Conditional presence | Explanation |
| --- | --- |
| *5GC* | The field is optionally present, Need ON, if the UE is connected to 5GC; otherwise the field is not present. |
| *BLCE-IDLEeDRX* | The field is optionally present, Need OR, if the UE is a BL UE or UE in CE and the UE is connected to 5GC and IDLE mode eDRX is configured and *ran-PagingCycle-r15* is absent; otherwise the field is not present. | |
| *EARFCN-max* | The field is mandatory present if the corresponding *carrierFreq* (i.e. without suffix) is set to *maxEARFCN*. Otherwise the field is not present. |
| *EarlySec* | When the UE is connected to 5GC, the field is mandatory present. When the UE is connected to EPC, the field is optionally present, Need ON, if the UE supports UP-EDT or UP transmission using PUR or early security reactivation and *releaseCause* is set to *rrc-Suspend*; otherwise the field is not present. | |
| *IdleInfoEUTRA* | The field is optionally present, Need OP, if the *IdleModeMobilityControlInfo* (i.e. without suffix) is included and includes *freqPriorityListEUTRA*; otherwise the field is not present. |
| *INACTIVE* | The field is mandatory present in this release. |
| *NoRedirect-r8* | The field is optionally present, Need OP, if the *redirectedCarrierInfo* (i.e. without suffix) is not included; otherwise the field is not present. |
| *Redirection* | The field is optionally present, Need ON, if the *redirectedCarrierInfo* is included and set to *geran*, *utra-FDD*, *utra-TDD* or *utra-TDD-r10*; otherwise the field is not present. |
| *UP-EDTorPUR* | The field is optionally present, Need ON, if the UE supports UP-EDT or UP transmission using PUR and *releaseCause* is set to *rrc-Suspend*; otherwise the field is not present. |

#### \*\*\*\*\* End of changes \*\*\*\*\*