**3GPP TSG-RAN WG2 Meeting #113bis-e *R2-210xxxx***

**Online, 12–20 April 2021**

**Agenda item: 6**

**Source: Mediatek inc (RAN2 Chairman)**

**Title: Report of [AT113bis-e][001][TEI16] TEI16 new and small (Chairman)**

**Document for: Discussion and Agreement**

# 1 Introduction

This is the result of the following email discussion in RAN2#113bis-e Meeting:.

* [AT113bis-e][001][TEI16] TEI16 new and small (Chairman)

Scope: Treat R2-2103042, R2-2103043, R2-2103044, R2-2103045, R2-2102623, R2-2102624, R2-2103467, R2-2103464  
Phase 1, determine agreeable parts, Phase 2, for agreeable parts Work on CRs.  
Intended outcome: Report and Agreed-in-principle CRs, if any  
Deadline: Schedule A

**Chairman views:**

1/ Now is late for R16, so completely new functionality for TEI16 would require strong support and fixing a real and important problem.

2/ However, for some TEI16 proposals is it not clear-cut whether they are new functionality or bug fixes or consistency updates. For bug-fixes and small consistency updates the bar is lower. For the proposals in this discussion it is not clear cut whether they should be regarded as new functions or not, and they they fullfill the requirement that they are small, so thus RAN2 can discuss.

Please feel free to ask questions. The proponents need to reply to questions. If possible please provide a position statement, and some brief justification, to facilitate decision whether the proposals or some modified variant of them can be accepted/agreed or not, in phase 1. Detailed dicussions on Proposals that seems agreeable is expected in phase 2.

# 2 Contact Information

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Moderator RAN2 Chair | Johan Johansson (johan.johansson@mediatek.com) |
| ZTE | eswar.vutukuri@zte.com.cn |
| Nokia | Tero Henttonen (tero.henttonen@nokia.com) |
| Qualcomm | Mouaffac Ambriss ([mambriss@qti.qualcomm.com](mailto:mambriss@qti.qualcomm.com) ) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

## 3.1 Redirection with MPS indication

[R2-2103042](file:///C:\evutukuri\work\5G\RAN2\docs\R2-2103042.zip) Redirection with MPS Indication Perspecta Labs, CISA ECD, T-Mobile, Ericsson, Qualcomm CR Rel-16 36.331 16.4.0 4579 2 C NR\_newRAT-Core, TEI16 R2-2102232

[R2-2103043](file:///C:\evutukuri\work\5G\RAN2\docs\R2-2103043.zip) Redirection with MPS Indication Perspecta Labs, CISA ECD, T-Mobile, Ericsson, Qualcomm CR Rel-16 38.331 16.4.1 2413 2 C NR\_newRAT-Core, TEI16 R2-2102233

[R2-2103044](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113bis-e\Docs\R2-2103044.zip) Redirection with MPS Indication Perspecta Labs, CISA ECD, T-Mobile, Ericsson, Qualcomm CR Rel-16 36.306 16.4.0 1804 1 C NR\_newRAT-Core, TEI16 R2-2102234

[R2-2103045](file:///C:\evutukuri\work\5G\RAN2\docs\R2-2103045.zip) Redirection with MPS Indication Perspecta Labs, CISA ECD, T-Mobile, Ericsson, Qualcomm CR Rel-16 38.306 16.4.0 0526 1 C NR\_newRAT-Core, TEI16 R2-2102235

|  |  |  |
| --- | --- | --- |
| Company | Position | Detailed Comments |
| Nokia, Nokia Shanghai Bell | TEI17 | The proposal would introduce new condition for setting highPriorityAccess establishment cause (overriding NAS behaviour). Since the modification of establishment causes might impact CT1 (see 24.501, clause 5.4.6), this may not be even TEI proposal. Anyway, as it's rather late for TEI16, this could be considered for Rel-17 (the TEI17 is planned to start from August 2021). |
| Qcom | Support |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.2 Initiation of RNA update

[R2-2103623](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113bis-e\Docs\R2-2103623.zip) Clarification on the initiation of RNA update Huawei, HiSilicon discussion Rel-16 TEI16

|  |  |  |
| --- | --- | --- |
| Company | Position | Detailed Comments |
| ZTE | Agree | We are okay with the proposed changes |
| Nokia, Nokia Shanghai Bell | Further check is needed | Access Category 2 got special treatment. At least TS24.501 reads “*barring checks will be skipped for this access attempt.*” That was the reason to treat the procedures for Access Category in a different way.  However, further check may be needed to ensure the scenario when two requests come together (RNA Update and Emergency call) is covered properly. |
| Qcom | Yes for the NR CR | We’re fine with the clarification to align with other part of spec that specified to allow RNA update when barring is lifted for access category 2 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.3 RRC Release cause for inter-RAT cell (re)selection in RRC\_INACTIVE

[R2-2103624](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113bis-e\Docs\R2-2103624.zip) Clarification on RRC Release cause for inter-RAT cell (re)selection in RRC\_INACTIVE Huawei, HiSilicon discussion Rel-16 TEI16

|  |  |  |
| --- | --- | --- |
| Company | Position | Detailed Comments |
| Chairman |  | I assume the intention here is to clarify cross-layer behaviour, and not really change behaviour (or what)? If that is the case, the discussion should consider that this is intended to be a bug-fix. |
| ZTE | Disagree | AS can inform NAS about the inter-RAT reselection and it is usually done by implementation and not limited to the case when UE falls from inactive to idle mode when inter-RAT cell reselection happens.  Thus we think this CR is not needed as NAS will not rely on the release cause to know that the inter-RAT selection happens. |
| Nokia, Nokia Shanghai Bell | Disagree | CR is not needed and this is not a correction but a behavioural change - if the cross-layer indication is missing, that could be done by changing RRC procedural text, but adding a new cause value would also impact CT1 specifications.  In fact upper layers will notify the change of RAT as AS provides information about broadcast information (e.g. SIB1 in NR and LTE) to upper layers (e.g. in NR 5.2.2.4.2 forward the cellIdentity to upper layers; forward the trackingAreaCode to upper layers). Hence, the CR is not needed. |
| QCOM | neutral | We agree with the issue, but we don’t see there is a need for spec change … behavior correction can be left to UE implementation to handle it. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.4 Combined RRC procedures

[R2-2103467](file:///C:\evutukuri\work\5G\RAN2\docs\R2-2103467.zip) On combined RRC procedures Nokia, Nokia Shanghai Bell, Ericsson discussion Rel-16 TEI16 R2-2101319

[R2-2103464](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113bis-e\Docs\R2-2103464.zip) RRC processing delays for combined procedures Nokia, Nokia Shanghai Bell, Ericsson CR Rel-16 38.331 16.4.1 1288 8 F TEI16 R2-2101320

|  |  |  |
| --- | --- | --- |
| Company | Position | Detailed Comments |
| Chairman |  | Similar proposals were discussed before, If I recall correctly, CRs were not agreed then partly due to unwillingness to change current UE implementations that treats RRC messages sequentially and without specific optimization even if said RRC messages are sent in the same Transport Block. I understand that the proponents have modified the proposal to allow that, so we can consider again. |
| ZTE | Disagree with the CR | We agree there is an issue, but the main problem with the existing spec is with lack of SR resources and hence the resulting double-RACH. However, we don’t think the CR sovles this issue.  Note that the UE releases the lower layer configuration (specifically, the SR and the PUCCH resoures are released). When the reestablishment is received, the UE submits the reestablishment complete message to the lower layers and if the subsequent reconfiguration message has not yet been received/processed by the UE, this will result in a RACH attempt. The gNB may be able to solve this problem of double RACH by sending UL grant(s) to schedule the reestablishmentComplete message but the timing of such scheduling needs to take into account potential differences in the UE processing delay to be able to avoid the double RACH issue.  Even if a combined processing delay is defined, it is not the case that the UEs are mandated to delay the submission of Reestablishment complete message until the RRCReconfiguration is processed. If this is the intention, then this should be clarified (that the UEs are required to wait until they process the reconfiguration message before submitting the reestablishmentComplete to lower layers – this will require more changes). However, this also results in unnecessary delay for the overall procedure and instead the better approach is to allow sequential processing but to include L1 SR resources to be provided in the reestablishment message similar to what is done in LTE (as proposed in R2-2004618). |
| Nokia, Nokia Shanghai Bell | Proponent | The issue here is two-fold: 1) RRC re-establishment cannot be rejected and 2) RRC re-establishment doesn't allow reconfiguration of dedicated parameters. This means network has to accept all re-establishment requests and then reconfigure the UE or use the fallback mechanism.  There are different ways to approach this, and the CR only covers P3+P4. We would first like to understand what the UE problems are - LTE has already defined combined RRC messages for a similar use case, so there should be no principal problem for UEs with this. Without this CR, the combined procedures cannot be used.  To ZTE: the double RACH can be avoided if network uses blind UL grants - this was already discussed during LTE and is widely used within deployed networks. So that shouldn't be a big issue in NR, either.  The combined procedure doesn't mean the responses are delayed - this in fact reduces the delay: UP data can anyway only continue after the first reconfiguration, and normally this would require network to first wait for the UE response, then react to that, send reconfiguration and wait for the response. Here this is combined to the same procedure, which reduces the overall delay. |
| QCOM | NO | Although the spec may allow transmission of the 2 RRC messages in the same TB, but this doesn’t mean that UE is expected to transmit one RRC Complete message (for both messages), or 2 seperate RRC Complete messages in the same TB. The UE behavior varies among UE vendors, and therefore any modification in the spec to mandate a specific UE behavior will be considered an NBC for some of the UE vendors. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 4 Conclusion

# 5 References

[1] R2-113bise Chairman notes 2021-04-11.docx