**3GPP T****SG-RAN WG2 Meeting #113bis-electronic R2-210xxxx**

**Online, April 12th – April 20th, 2021**

**Agenda item: 6.1.3.1**

**Source: vivo**

**Title:** **[AT113bis-e][015][NR16] Overlapping UCI Data and SR of equal priority and UL skipping (vivo)**

**Document for: Discussion and Decision**

# 1 Introduction

This contribution is aimed at reporting the discussion and results of the following email discussion:

* [AT113bis-e][015][NR16] Overlapping UCI Data and SR of equal priority and UL skipping (vivo)

Scope: Take into account on-line progress, Take into account R2-2102628, R2-2102626, R2-2102724, R2-2102759, R2-2102754, R2-2103381, R2-2103481, R2-2103846, R2-2103847, R2-2102775, R2-2103067, R2-2103426, R2-2103208, R2-2103439, R2-2103440, R2-2102776, R2-2103845, R2-2104054

Determine agreeable parts, make decisions for Reply LS to RAN1. For parts with incomplete conclusions, pave the way for on-line CB

Intended outcome: Report, approved LS out,

Deadline: Monday April 19 (if needed CB April 20)

The discussion scope is to gather understanding on whether the MAC layer is aware of the final PUCCH resource after UCI multiplexing with multiple UCI types in a PUCCH and to check if there is sufficient support to pursue the correction CR [R2-2103381](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103381.zip).

Then, the rapporteur would like to point out the specific deadline for this discussion with two phases,

* In phase 1, companies are invited to provide their views by April. 15th (Thursday), 2021, 18:00 UTC.
* In phase 2, the corresponding summary proposals (if consensus can be achieved), draft CR(s), and draft reply LS will be provided. Any comments on the proposals, draft CR(s), and draft reply LS are invited to be provided by April. 19th (Monday), 2021, 18:00 UTC.

# 2 Participants

|  |  |
| --- | --- |
| Participant name | E-mail |
| Yitao Mo (Stephen) | yitao.mo@vivo.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

## 3.1 Visibility of final PUCCH resource in MAC layer

During the online discussion at RAN2#113bis-e meeting, a warm discussion on the RAN1 LS question that whether MAC is aware of UCI multiplexing in PHY or not has been launched [1]. The corresponding discussion records are given as below:

|  |
| --- |
| R2-2102626 Reply LS on overlapped data and SR are of equal L1 priority (R1-2102244; contact: vivo) RAN1 LS in Rel-16 NR\_IIOT-Core To:RAN2  moved from 6.1.1  SR  - vivo think that MAC layer is not aware of the final resource of SR etc.  - Oppo think there is a dependency between L1 and MAC as L1 decides based on MAC decision, e.g. PUCCH format.  - MTK think MAC is written fuzzy e.g. doesn’t say whether info is configured or L1 chosen, e.g. in order to do UL skipping MAC need to be aware of L1, and MAC/L1 are quite tight coupled, MAC can be aware.  - Samsung think that PUCCH PUSCH conflicts are explicit and MAC cannot determine other conflicts. MAC is not aware of PUCCH resource.  - ZTE think MAC is aware, DRX Note about CSI-RS reporting refers to CSI-RS resources co-inciding with DRX active time. ZTE think MAC can be aware. Think we need to consider the chicken egg problem. CATT think there is no chicken-egg issue, and the time-line shows that UCI multiplexing is already known in the UE when MAC intra-UE-prioritzation is done, so the UE can know. Agree with ZTE that MAC is aware of L1 and there are several examples in the TS.  - Huawei don’t think MAC is aware of everything, think we can choose whether MAC need to know.  - Apple are not sure, whether we need to modify the Phy MAC interface. Chair think we never attempted to specify a MAC Phy interface.  - Ericsson think MAC cannot know the final PUCCH resource.  - LG would like the specification to be as simple as possible i.e. independent in this case.  - Lenovo think the interlayer interaction was never specified in detail, and we always left MAC a bit fuzzy. Qc agrees with this, and current MAC design doesn’t rule out.  - Nokia think MAC doesn’t need to know what is the final resource.  - IDT think the understanding 1 gives the least impact, not sure whether there will need to be any change, e.g. for retriggering maybe SR is just delayed.  - CATT think that Understanding 2 is the current behaviour. MTK agrees.  - Samsung think the impact to UE impl is different.  Chair: A TS can refer to a condition where the details are specified in another TS. This is usually done by fuzzy reference, so it seems that both interpretations are possible (without adding L1 specific details in MAC or vice versa).  Chair: Understanding 1: If we assume that MAC just generate SR and let L1 decide if/by what resource to transmit it, if the SR is not transmitted in the end then MAC may need to know this, in order to re-trigger the SR.  Chair: Understanding 2: If we assume that MAC (the UE) can first know whether SR can be transmitted or not, then the current TS works.  Attempt to progress offline, CB on-line if needed |

Thus, there are two options for LCH-based prioritization:

1. **MAC is not aware of the final PUCCH after UCI multiplexing in PHY:**

In contributions [5][8][11][12][13][14] provide an understanding that the terminologies “PUCCH resource with an SR transmission” (in section 5.4.1), “valid PUCCH resource for SR” (in section 5.4.4), and “PUCCH resource for the SR transmission occasion” (in section 5.4.4) are referred to as the PUCCH resource for SR transmission configured within the *MAC-CellGroupConfig*. This is because the MAC layer, for implementation simplicity and layer independence, should not visit/monitor the other PUCCH configurations used for other purposes (e.g. CSI reporting, UCI multiplexing for multiple UCIs in a PUCCH).

Based on this understanding, for case 2-1 depicted in Figure 1, when performing LCH-based prioritization check, the MAC layer takes the SR resource marked with dashed frame and the overlapping PUSCH for prioritization. Then, the MAC layer will checks with PHY that whether these two resources can be used for SR or PUSCH transmission. Consequently, the MAC will only deliver either SR or PUSCH MAC PDU to PHY layer, which leads to unnecessary performance degradation. For case 2-2 depicted in Figure 2, in the same logic, the MAC will deliver both SR and PUSCH MAC PDU to PHY layer. Fortunately, the current PHY spec allows the PHY to multiplex other UCI(s) i.e., HARQ-ACK/CSI in the PUSCH and does not transmit SR. In this sense, this option would not bring any negative impact on UE behavior.



Figure 1: Example of case 2-1 where the final PUCCH resource does not overlap with PUSCH



Figure 2: Example of case 4 where only the final PUCCH resource overlaps with PUSCH

1. **MAC is aware of the final PUCCH after UCI multiplexing in PHY:**

During the online discussion and also in contributions [4][15][18], some companies think that the terminologies “PUCCH resource with an SR transmission” (in section 5.4.1), “valid PUCCH resource for SR” (in section 5.4.4), and “PUCCH resource for the SR transmission occasion” (in section 5.4.4) are not so clear. It might be referred to as the final PUCCH resource after UCI multiplexing in a PUCCH via PHY layer. Besides, it is mentioned that, based on the current MAC spec, the MAC layer firstly will inquire PHy layer whether the SR can be signaled on a PUCCH resource or not, it is quite natural that the PHY layer will take UCI multiplexing into account and informs MAC layer of the final PUCCH resource for further LCH-based prioritization check.

Based on this understanding, for case 2-1 depicted in Figure 1, when performing LCH-based prioritization check, in practice, the MAC layer has to firstly indicate PHY that a SR would be transmitted and then the PHY assumes that UCI multiplexing should be performed. Then, if UCI multiplexing condition is fulfilled (e.g. processing timeline and PUCCH format can support the UCI multiplexing), the PHY can tell MAC the final PUCCH resource. Otherwise, the PHY just checks whether the initial SR resource can be used for SR transmission or not. Further, if the SR is considered as a prioritized SR transmission and the SR transmission is instructed by the MAC layer, the PHY layer has really performed the UCI multiplexing procedure for final PUCCH transmission with SR. Obviously, the PHY layer has to at first assume the UCI multiplexing hypothesis and again recall the UCI multiplexing procedure in reality if SR is delivered.

The potential UE implementation for both Understanding 1 and Understanding 2 are given in the following Figure 3. And Table 1 summarizes the pros and cons of these two understandings, based on contribution [20].



Figure 3: UE implementation via Understanding 1/2

**Table 1: Summary of pros and cons of Understanding 1 and Understanding 2**

|  |  |  |
| --- | --- | --- |
| **Cases** | **Understanding 1:**  **MAC is not aware of the final PUCCH resource** | **Understanding 2:**  **MAC is aware of the final PUCCH resource** |
| Case 2-1 | **Pros:**   * Simple UE implementation; * No MAC spec impact.   **Cons:**   * Performancedegradation since either SR or PUSCH will be unnecessarily dropped by MAC. | **Pro:**   * Both SR and PUSCH can be transmitted.   **Con:**   * Complex interaction between PHY and MAC; * NBC change might be needed. |
| cid:image001.png@01D6FBC1.DD0FD2F0  Case 4 | **Pros:**   * Simple UE implementation; * No MAC spec impact.   **Con:**   * PHY should drop the SR. | **Pro:**   * PHY doesn’t need to drop SR.   **Con:**   * Complex interaction between PHY and MAC; * NBC change might be needed. |

Anyway, the rapporteur thinks a decision is needed for the way forward although it is really hard to select either option since they are all feasible and have their advantages.

### **Q1: Which option do companies prefer for the LCH-based prioritization procedure?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Preference (Understanding 1 or Understanding 2)** | **Detailed comments** |
| vivo | Understanding 1 | In our understanding, the terminology “valid PUCCH resource for SR” in the MAC spec, which has been used since V8.4.0, is intended to link to the PUCCH resource configured within MAC configuration with a specific PUCCH format for single SR transmission. In this sense, the current MAC spec text is quite clear and Understanding 1 aligns with the current MAC behavior. From the technical point of view, Understanding 1 can work well without performance degradation in all the cases given by RAN1 except case 2-1 (which might be a very corner case). We don’t think any enhancement (e.g. Understanding 2) is needed for Rel-16 which has been frozen. Also, to get rid of potential impacts on UE implementation and MAC spec clarification, we should stick with Understanding 1. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Conclusion:**

**TBD**

## 3.2 R2-2103381 on UL skipping correction

In [R2-2103381](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2103381.zip), it pointed out that CG-UCI is not able to be multiplexed with other UCIs if *cg-UCI-Multiplexing* is not configured in case of CG PUSCH transmission in NR-U. Thus, if *cg-UCI-Multiplexing* is not configured, it is useless for MAC to generate an empty TB. Besides, retransmission of such empty TB is then later prioritized over new transmission, which is rather undesirable.

Therefore, the following correction is proposed:

|  |
| --- |
| **TS 38.321 sub-clause 5.4.3.1.3 Allocations of resources**  The MAC entity shall:  1> if the MAC entity is configured with *enhancedSkipUplinkTxDynamic* with value *true* and the grant indicated to the HARQ entity was addressed to a C-RNTI, or if the MAC entity is configured with *enhancedSkipUplinkTxConfigured* with value *true* and the grant indicated to the HARQ entity is a configured uplink grant; and  1> if the MAC entity is not configured with *lch-basedPrioritization*; and  1> if there is no UCI to be multiplexed on this PUSCH transmission as specified in TS 38.213 [6] or if there is HARQ-ACK information overlapping with this PUSCH transmission which is a configured uplink grant configured with *cg-RetransmissionTimer* but not *cg-UCI-Multiplexing*; and  1> if there is no aperiodic CSI requested for this PUSCH transmission as specified in TS 38.212 [9]; and  1> if the MAC PDU includes zero MAC SDUs; and  1> if the MAC PDU includes only the periodic BSR and there is no data available for any LCG, or the MAC PDU includes only the padding BSR:  2> not generate a MAC PDU for the HARQ entity. |

### **Q2: Do companies agree the intention of CR R2-2103381?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Detailed comments** |
| vivo | No | In our understanding, the former condition “if there is no UCI to be multiplexed on this PUSCH transmission” has covered the case mentioned in the CR. Specifically, when performing the UL skipping check, the MAC layer will instruct the PHY layer to check whether there is a UCI (e.g. HARQ-ACK) that will be multiplexed on this CG-PUSCH. Then if *cg-UCI-Multiplexing* is not configured, the PHY is aware that the HARQ-ACK will not be multiplexed on the CG PUSCH transmission based on the following highlighted quoted text from 38.213 section 9. As a result, the MAC will consider there is no UCI to be multiplexed on this CG PUSCH transmission, and no padding MAC PDU will be generated.   |  | | --- | | 38.213 section 9  *When a UE would multiplex HARQ-ACK information in a PUSCH transmission that is configured by a ConfiguredGrantConfig, and includes CG-UCI [5, TS 38.212], the UE multiplexes the HARQ-ACK information in the PUSCH transmission if the UE is provided cg-UCI-Multiplexing; otherwise, the UE does not transmit the PUSCH and multiplexes the HARQ-ACK information in a PUCCH transmission or in another PUSCH transmission.* | |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.3 Other potential impacts/enhancements

Last but not least, companies can provide their comments on the remaining issues of overlapping UCI and PUSCH with Rel-16 PUSCH skipping, if they are not covered by this discussion.

### **Q3: Are there any additional comments on the remaining issues?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Detailed comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Conclusion:**

**TBD**

# 4 Conclusion

The contribution is summarized with observations and proposals as follows,

**Phase 1:**

# 5 References

1. R2-2102626, Reply LS on overlapped data and SR are of equal L1 priority (R1-2102244; contact: vivo)
2. RAN2 113bis-e Chairman notes 2021-04-12 1600 UTC
3. R2-2102628, LS on UL skipping for PUSCH in Rel-16 (R1-2102249; contact: vivo)
4. R2-2102724, Analysis of RAN1 reply LS on overlapped SR and data, CATT
5. R2-2102759, Remaining issues on overlapped PUSCH and UCI with UL skipping, vivo
6. R2-2102754, Draft reply LS to RAN1 on overlapped data and SR are of equal L1 priority, vivo
7. R2-2103381, Correction to PUSCH skipping with UCI for NR-U, Nokia, Nokia Shanghai Bell
8. R2-2103481, MAC behaviour for overlapped UCI(s), SR and PUSCH with equal L1 priority, Huawei, HiSilicon
9. R2-2103846, Overlapped SR and PUSCH of equal L1 priority, Apple
10. R2-2103847, Treatment of overlapping SR/Data, Apple
11. R2-2102775, Discussion on overlapped data and SR with equal PHY priority, Samsung
12. R2-2103067, LCH based prioritization for SR and PUSCH, Intel Corporation
13. R2-2103426, Remaining corrections for Intra-UE prioritization, Ericsson
14. R2-2103208, Discussion on reply LS on overlapped data and SR are of equal L1 priority, OPPO
15. R2-2103439, Considerations on the intra-UE multiplexing coupled with PUCCH transmission, ZTE Corporation, Sanechips
16. R2-2103440, Correction to 38.321 on intra-UE multipexing involved PUCCH transmission, ZTE Corporation, Sanechips
17. R2-2102776, UL Skipping with LCH-based Prioritization, Samsung
18. R2-2103845, UL skipping and intra-UE prioritization, Apple
19. R2-2104054, RAN2 impact of Case 1-6 for UL skipping, Huawei, HiSilicon
20. R2-2104309, Treatment of overlapping SR/Data, Apple